(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 245)
    (zones 0)
    (modules 28)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.3)
    (user_via 0.762 0.381)
    (user_via 1.016 0.635)
    (user_via 1.27 0.889)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 SPKR)
  (net 2 SPKR_R)
  (net 3 SPKL)
  (net 4 SPKR_L)
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C3-Pad1)")
  (net 7 GND)
  (net 8 "Net-(C4-Pad1)")
  (net 9 VDD_IO)
  (net 10 +3V3)
  (net 11 +5V)
  (net 12 "Net-(D1-Pad2)")
  (net 13 "Net-(D1-Pad1)")
  (net 14 "Net-(D2-Pad2)")
  (net 15 "Net-(D2-Pad1)")
  (net 16 "Net-(D3-Pad2)")
  (net 17 "Net-(J1-Pad8)")
  (net 18 "Net-(J1-Pad7)")
  (net 19 "Net-(J1-Pad6)")
  (net 20 UART_TX)
  (net 21 "Net-(J1-Pad4)")
  (net 22 UART_RX)
  (net 23 "Net-(J1-Pad2)")
  (net 24 "Net-(J1-Pad1)")
  (net 25 LINEIN_L)
  (net 26 LINEIN_R)
  (net 27 P2_4)
  (net 28 P2_0)
  (net 29 EAN)
  (net 30 "Net-(MOD1-Pad21)")
  (net 31 "Net-(MOD1-Pad18)")
  (net 32 "Net-(MOD1-Pad17)")
  (net 33 "Net-(MOD1-Pad16)")
  (net 34 "Net-(MOD1-Pad15)")
  (net 35 "Net-(MOD1-Pad22)")
  (net 36 "Net-(MOD1-Pad36)")
  (net 37 "Net-(MOD1-Pad35)")
  (net 38 "Net-(MOD1-Pad34)")
  (net 39 "Net-(MOD1-Pad31)")
  (net 40 "Net-(MOD1-Pad30)")
  (net 41 "Net-(MOD1-Pad26)")
  (net 42 "Net-(MOD1-Pad25)")
  (net 43 "Net-(MOD1-Pad24)")
  (net 44 "Net-(MOD1-Pad14)")
  (net 45 "Net-(MOD1-Pad13)")
  (net 46 "Net-(MOD1-Pad10)")
  (net 47 "Net-(MOD1-Pad6)")
  (net 48 "Net-(MOD1-Pad5)")
  (net 49 "Net-(MOD1-Pad3)")
  (net 50 "Net-(MOD1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net EAN)
    (add_net GND)
    (add_net LINEIN_L)
    (add_net LINEIN_R)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(MOD1-Pad1)")
    (add_net "Net-(MOD1-Pad10)")
    (add_net "Net-(MOD1-Pad13)")
    (add_net "Net-(MOD1-Pad14)")
    (add_net "Net-(MOD1-Pad15)")
    (add_net "Net-(MOD1-Pad16)")
    (add_net "Net-(MOD1-Pad17)")
    (add_net "Net-(MOD1-Pad18)")
    (add_net "Net-(MOD1-Pad21)")
    (add_net "Net-(MOD1-Pad22)")
    (add_net "Net-(MOD1-Pad24)")
    (add_net "Net-(MOD1-Pad25)")
    (add_net "Net-(MOD1-Pad26)")
    (add_net "Net-(MOD1-Pad3)")
    (add_net "Net-(MOD1-Pad30)")
    (add_net "Net-(MOD1-Pad31)")
    (add_net "Net-(MOD1-Pad34)")
    (add_net "Net-(MOD1-Pad35)")
    (add_net "Net-(MOD1-Pad36)")
    (add_net "Net-(MOD1-Pad5)")
    (add_net "Net-(MOD1-Pad6)")
    (add_net P2_0)
    (add_net P2_4)
    (add_net SPKL)
    (add_net SPKR)
    (add_net SPKR_L)
    (add_net SPKR_R)
    (add_net UART_RX)
    (add_net UART_TX)
    (add_net VDD_IO)
  )
  (module BM62Adapter:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 618C188C)
    (at 170.18 128.905 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 1.27 12.49 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 5.08) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 UART_RX))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 UART_TX))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 VDD_IO))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 EAN))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 P2_0))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 P2_4))
  )
  (module BM62Adapter:MountingHole_2.5mm (layer F.Cu) (tedit 618C12DB)
    (at 153.67 111.76)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module BM62Adapter:MountingHole_2.5mm (layer F.Cu) (tedit 618C12DB)
    (at 193.04 111.76)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module BM62Adapter:BM62SPKS1MC2-0001AA (layer F.Cu) (tedit 618B737C)
    (at 133.35 115.57 90)
    (fp_text reference MOD1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value BM62 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user * (at 0 0 90) (layer F.Fab) hide)
    (fp_text user * (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User) hide)
    (pad 21 smd rect (at 2.659999 14.149987 90) (size 0.850011 1.699997) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(MOD1-Pad21)"))
    (pad 20 smd rect (at 1.389999 14.149987 90) (size 0.850011 1.699997) (layers F.Cu F.Paste F.Mask)
      (net 11 +5V))
    (pad 19 smd rect (at 0.119999 14.149987 90) (size 0.850011 1.699997) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD_IO))
    (pad 18 smd rect (at -1.150001 14.149987 90) (size 0.850011 1.699997) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(MOD1-Pad18)"))
    (pad 17 smd rect (at -2.420001 14.149987 90) (size 0.850011 1.699997) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(MOD1-Pad17)"))
    (pad 16 smd rect (at -3.690001 14.149987 90) (size 0.850011 1.699997) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(MOD1-Pad16)"))
    (pad 15 smd rect (at -4.960001 14.149987 90) (size 0.850011 1.699997) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(MOD1-Pad15)"))
    (pad 23 smd rect (at 5.199999 14.149987 90) (size 0.850011 1.699997) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 22 smd rect (at 3.929999 14.149987 90) (size 0.850011 1.699997) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(MOD1-Pad22)"))
    (pad 37 smd rect (at 7.150001 -2.700012 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 36 smd rect (at 7.150001 -1.500012 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(MOD1-Pad36)"))
    (pad 35 smd rect (at 7.150001 -0.300012 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(MOD1-Pad35)"))
    (pad 34 smd rect (at 7.150001 0.899988 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(MOD1-Pad34)"))
    (pad 33 smd rect (at 7.150001 2.099988 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 22 UART_RX))
    (pad 32 smd rect (at 7.150001 3.299988 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 20 UART_TX))
    (pad 31 smd rect (at 7.150001 4.499988 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(MOD1-Pad31)"))
    (pad 30 smd rect (at 7.150001 5.699989 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(MOD1-Pad30)"))
    (pad 29 smd rect (at 7.150001 6.899989 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 27 P2_4))
    (pad 28 smd rect (at 7.150001 8.099986 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-Pad1)"))
    (pad 27 smd rect (at 7.150001 9.299986 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad1)"))
    (pad 26 smd rect (at 7.150001 10.499987 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(MOD1-Pad26)"))
    (pad 25 smd rect (at 7.150001 11.699987 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(MOD1-Pad25)"))
    (pad 24 smd rect (at 7.150001 12.899987 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(MOD1-Pad24)"))
    (pad 14 smd rect (at -7.150001 12.899987 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(MOD1-Pad14)"))
    (pad 13 smd rect (at -7.150001 11.699987 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(MOD1-Pad13)"))
    (pad 12 smd rect (at -7.150001 10.499987 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad1)"))
    (pad 11 smd rect (at -7.150001 9.299986 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (pad 10 smd rect (at -7.150001 8.099986 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(MOD1-Pad10)"))
    (pad 9 smd rect (at -7.150001 6.899986 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 3 SPKL))
    (pad 8 smd rect (at -7.150001 5.699986 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 7 smd rect (at -7.150001 4.499988 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 1 SPKR))
    (pad 6 smd rect (at -7.150001 3.299988 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(MOD1-Pad6)"))
    (pad 5 smd rect (at -7.150001 2.099988 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(MOD1-Pad5)"))
    (pad 4 smd rect (at -7.150001 0.899988 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 28 P2_0))
    (pad 3 smd rect (at -7.150001 -0.300012 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(MOD1-Pad3)"))
    (pad 2 smd rect (at -7.150001 -1.500012 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 29 EAN))
    (pad 1 smd rect (at -7.150001 -2.700012 90) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(MOD1-Pad1)"))
    (model D:/MCCI/BM62Adapter/3d/BM62SPKA1MC2-0001AA--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module BM62Adapter:CUI_SJ1-3533N (layer F.Cu) (tedit 618B71FB)
    (at 177.8 101.6 270)
    (fp_text reference J5 (at 11.43 -6.35 90) (layer F.SilkS) hide)
    (fp_text value SJ1-3533N (at 4.445 -6.35 90) (layer F.SilkS))
    (pad 3 thru_hole oval (at 7.9 -2) (size 3.2 1.6) (drill oval 1.8 1) (layers *.Cu *.Mask)
      (net 26 LINEIN_R))
    (pad 2 thru_hole oval (at 2.4 -2) (size 3.2 1.6) (drill oval 1.8 1) (layers *.Cu *.Mask)
      (net 25 LINEIN_L))
    (pad 1 thru_hole oval (at 0 0) (size 3.2 1.6) (drill oval 1.8 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model D:/MCCI/BM62Adapter/3d/CUI_DEVICES_SJ1-3533N.step
      (offset (xyz -5.1 1 7))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 180))
    )
  )
  (module BM62Adapter:CUI_SJ1-3533N (layer F.Cu) (tedit 618B71FB)
    (at 165.1 101.6 270)
    (fp_text reference J4 (at 2.3591 -6.79794 90) (layer F.SilkS) hide)
    (fp_text value SJ1-3533N (at 5.08 -6.35 90) (layer F.SilkS))
    (pad 3 thru_hole oval (at 7.9 -2) (size 3.2 1.6) (drill oval 1.8 1) (layers *.Cu *.Mask)
      (net 2 SPKR_R))
    (pad 2 thru_hole oval (at 2.4 -2) (size 3.2 1.6) (drill oval 1.8 1) (layers *.Cu *.Mask)
      (net 4 SPKR_L))
    (pad 1 thru_hole oval (at 0 0) (size 3.2 1.6) (drill oval 1.8 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (model D:/MCCI/BM62Adapter/3d/CUI_DEVICES_SJ1-3533N.step
      (offset (xyz -5.1 1 7))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 180))
    )
  )
  (module BM62Adapter:Pin_Header_Angled_2x03_Pitch2.54mm (layer F.Cu) (tedit 5D3EA9E4)
    (at 190.5 101.6)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at 5.08 7.62) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 5.655 7.35) (layer F.Fab) hide)
    (fp_text user %R (at 5.31 2.54 90) (layer F.Fab) hide)
    (pad 5 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 6 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SPKR_L))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 LINEIN_L))
    (pad 1 thru_hole rect (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 SPKR_R))
    (pad 2 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 LINEIN_R))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BM62Adapter:Pin_Header_Angled_2x06_Pitch2.54mm (layer F.Cu) (tedit 5D3EA957)
    (at 190.5 116.84)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (fp_text reference J1 (at 5.08 -2.54) (layer F.SilkS))
    (fp_text value Conn_02x06_Odd_Even (at 5.655 14.97) (layer F.Fab) hide)
    (fp_text user %R (at 5.31 6.35 90) (layer F.Fab) hide)
    (pad 11 thru_hole oval (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +3V3))
    (pad 12 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +3V3))
    (pad 9 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 10 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 7 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)"))
    (pad 5 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 UART_TX))
    (pad 6 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad6)"))
    (pad 3 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 UART_RX))
    (pad 4 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad4)"))
    (pad 1 thru_hole rect (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_muRata_CRE1xxxxxx3C_THT (layer F.Cu) (tedit 59F5F4E9)
    (at 179.07 118.11 270)
    (descr "Isolated 1W single output DC/DC, http://power.murata.com/data/power/ncl/kdc_cre1.pdf")
    (tags "Isolated 1W single output DC/DC")
    (fp_text reference U1 (at 1 -3 90) (layer F.SilkS))
    (fp_text value CME0305S3C (at 2 11 270) (layer F.Fab) hide)
    (fp_text user %R (at 3 4) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_CRE1xxxxxx3C_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 163.83 119.38 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 7 GND))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 146.05 104.14 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +5V))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 143.51 104.14 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(MOD1-Pad24)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 140.97 104.14 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(MOD1-Pad24)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 153.67 125.73)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.54 0) (layer F.SilkS))
    (fp_text value 1K (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 153.67 121.92)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.54 0) (layer F.SilkS))
    (fp_text value 5K (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 LINEIN_R))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 153.67 123.825)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.54 0) (layer F.SilkS))
    (fp_text value 5K (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LINEIN_L))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 132.08 104.14 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D3 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value GREEN (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 135.255 104.14 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D2 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value RED (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 138.43 104.14 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D1 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 166.37 119.38 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.68 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 149.86 113.03 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 184.15 118.11 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 186.69 118.11 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.68 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 151.13 118.745)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 1.905) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.68) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 VDD_IO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 147.32 126.365)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -2.54 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 147.46 128.27)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.68 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.115 105.41 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 1.85 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 SPKL))
    (pad 1 smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 SPKR_L))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.115 111.125 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 1.85 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 SPKR))
    (pad 1 smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 SPKR_R))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "BM62 Adapter Board Rev A\nCopyright © 2021 Microsoft Corporation" (at 147.955 103.505) (layer B.SilkS))
  (gr_line (start 129.54 130.81) (end 129.54 100.33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.85 130.81) (end 129.54 130.81) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.85 100.33) (end 196.85 130.81) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.54 100.33) (end 196.85 100.33) (layer Edge.Cuts) (width 0.05))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.66 134.62) (xy 127 134.62) (xy 127 120.65) (xy 133.35 120.65) (xy 133.35 110.49)
        (xy 127 110.49) (xy 127 96.52) (xy 200.66 96.52)
      )
    )
  )
)
