(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 14)
    (no_connects 0)
    (area 92.424999 44.024999 107.575001 52.475001)
    (thickness 1.6)
    (drawings 16)
    (tracks 48)
    (zones 0)
    (modules 2)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(P1-Pad4)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(P1-Pad2)")
  (net 5 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net VCC)
  )
  (module footprints:USB_Micro-B_top_mount (layer F.Cu) (tedit 5799B0A8)
    (at 100 50)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P1 (at 0 -3.45) (layer F.SilkS))
    (fp_text value USB (at 0 4.1) (layer F.Fab))
    (pad 6 thru_hole rect (at -0.8375 0.95 90) (size 1.9 1.37) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 0.8375 0.95 90) (size 1.9 1.37) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 smd rect (at -1.3009 -1.725 90) (size 1.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.6509 -1.725 90) (size 1.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad4)"))
    (pad 3 smd rect (at -0.0009 -1.725 90) (size 1.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 0.6491 -1.725 90) (size 1.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P1-Pad2)"))
    (pad 1 smd rect (at 1.2991 -1.725 90) (size 1.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 6 smd rect (at -2.5009 -1.35 90) (size 2.1 1.475) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.4991 -1.35 90) (size 2.1 1.475) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -3.95 0.95 90) (size 1.6 1.6) (drill oval 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.95 0.95 90) (size 1.6 1.6) (drill oval 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module footprints:3DS_power_connector_area (layer F.Cu) (tedit 579AE95B)
    (at 100 52.4)
    (fp_text reference P2 (at 0 0.5) (layer F.SilkS))
    (fp_text value MAIN (at 0 -9.3) (layer F.Fab))
    (pad 2 smd rect (at 6.65 -0.75) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1 -7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1 -7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
    (pad 4 thru_hole circle (at 4.5 -7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at -4.5 -7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 smd circle (at 4.75 -2) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd circle (at -4.75 -2) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -6.65 -0.75) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
  )
  (gr_line (start 94 49) (end 92.5 49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 44.1) (end 94 49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106 49) (end 107.5 49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106 44.1) (end 106 49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 44.1) (end 106 44.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.5 52.4) (end 92.5 49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.2 52.4) (end 92.5 52.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.2 50.3) (end 97.2 52.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.1 50.3) (end 97.2 50.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.1 52.4) (end 98.1 50.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.9 52.4) (end 98.1 52.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.9 50.4) (end 101.9 52.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.8 50.4) (end 101.9 50.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.8 52.4) (end 102.8 50.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.5 52.4) (end 102.8 52.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.5 49) (end 107.5 52.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.03 49.01) (xy 107.51 49.01) (xy 107.51 52.39) (xy 102.79 52.36) (xy 102.79 50.4)
        (xy 101.9 50.43) (xy 101.87 52.39) (xy 98.13 52.39) (xy 98.1 50.32) (xy 97.2 50.32)
        (xy 97.2 52.42) (xy 92.54 52.39) (xy 92.51 49.01) (xy 94.02 49.01) (xy 93.99 44.06)
        (xy 106.03 44.09)
      )
    )
  )
)
