(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 12)
    (no_connects 0)
    (area 104.674999 45.234999 182.357208 82.662208)
    (thickness 1.6)
    (drawings 74)
    (tracks 111)
    (zones 0)
    (modules 8)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad1)")
  (net 2 "Net-(IC1-Pad3)")
  (net 3 "Net-(IC1-Pad4)")
  (net 4 "Net-(IC1-Pad5)")
  (net 5 3.3v)
  (net 6 "Net-(IC1-Pad7)")
  (net 7 "Net-(IC1-Pad8)")
  (net 8 "Net-(IC1-Pad9)")
  (net 9 "Net-(IC1-Pad10)")
  (net 10 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3.3v)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
  )
  (net_class GND ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module Buttons_Switches:Tact_Switch_RightAngle_NoOutline (layer B.Cu) (tedit 5A76B0D3)
    (at 156.5 50.59 270)
    (fp_text reference SW3 (at 7.62 0 360) (layer B.Fab))
    (fp_text value SW_PUSH_SMALL_H (at 1.016 0 540) (layer B.Fab))
    (pad 1 thru_hole circle (at 2.75 -2.25 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(IC1-Pad7)"))
    (pad 2 thru_hole circle (at 2.75 2.25 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 10 GND))
    (pad "" thru_hole circle (at 5.25 3.5 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" thru_hole circle (at 5.25 -3.5 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
  )
  (module Buttons_Switches:Tact_Switch_RightAngle_NoOutline (layer B.Cu) (tedit 5A76B0D3)
    (at 130.485 50.59 270)
    (fp_text reference SW2 (at 7.62 0 360) (layer B.Fab))
    (fp_text value SW_PUSH_SMALL_H (at 1.016 0 540) (layer B.Fab))
    (pad 1 thru_hole circle (at 2.75 -2.25 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(IC1-Pad9)"))
    (pad 2 thru_hole circle (at 2.75 2.25 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 10 GND))
    (pad "" thru_hole circle (at 5.25 3.5 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad "" thru_hole circle (at 5.25 -3.5 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
  )
  (module Buttons_Switches:SW_PUSH_6mm_NoOutline (layer B.Cu) (tedit 5A76B222)
    (at 158.805 58.57 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW4 (at 3.25 2 90) (layer B.Fab))
    (fp_text value SW_PUSH_SMALL_H (at 3.75 -6.7 90) (layer B.Fab))
    (fp_text user %R (at 3.25 -2.25 90) (layer B.Fab))
    (pad 2 thru_hole circle (at 0 -4.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad7)"))
    (pad 2 thru_hole circle (at 6.5 -4.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 1 thru_hole circle (at 6.5 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad7)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches:SW_PUSH_6mm_NoOutline (layer B.Cu) (tedit 5A76B222)
    (at 132.715 58.57 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 2 90) (layer B.Fab))
    (fp_text value SW_PUSH_SMALL_H (at 3.75 -6.7 90) (layer B.Fab))
    (fp_text user %R (at 3.25 -2.25 90) (layer B.Fab))
    (pad 2 thru_hole circle (at 0 -4.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad9)"))
    (pad 2 thru_hole circle (at 6.5 -4.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 1 thru_hole circle (at 6.5 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad9)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Logos:Kerntroller-Back-1200 v1.1 - Solder Mask" (layer B.Cu) (tedit 0)
    (at 143.51 65.405 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Trinket:Trinket_3v3_MountingHoles (layer F.Cu) (tedit 5A774D1E)
    (at 143.51 49.53)
    (fp_text reference IC1 (at 0 1.27) (layer F.Fab))
    (fp_text value Trinket3v3 (at 0 6.985) (layer F.Fab))
    (pad "" thru_hole circle (at -6.096 6.604) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -5.715 22.86) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.715 22.86) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 6.096 6.604) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -6.35 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 3 thru_hole circle (at -6.35 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole circle (at -6.35 16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad4)"))
    (pad 5 thru_hole circle (at -6.35 19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole circle (at 6.35 19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 3.3v))
    (pad 7 thru_hole circle (at 6.35 16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad8)"))
    (pad 9 thru_hole circle (at 6.35 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad9)"))
    (pad 10 thru_hole circle (at 6.35 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad10)"))
  )
  (module "Logos:Kerntroller-Back-1200 v1.1b - Partial Silk Mask" (layer B.Cu) (tedit 0)
    (at 143.51 65.405 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Logos:a-015-1200 (layer F.Cu) (tedit 0)
    (at 141.732 71.628)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "Adafruit\nTrinket M0" (at 143.51 57.404) (layer F.SilkS))
  (gr_line (start 131.9784 78.613) (end 155.03906 78.613) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.285 66.04) (end 121.285 49.53) (angle -220.3645366) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.735 66.04) (end 165.735 49.53) (angle 220.3645366) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.285 49.53) (end 165.735 49.53) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(IC1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.831 58.547) (xy 172.339 58.547) (xy 172.339 62.23) (xy 172.72 62.611) (xy 176.403 62.611)
        (xy 176.403 63.119) (xy 172.72 63.119) (xy 172.339 63.5) (xy 172.339 67.183) (xy 171.831 67.183)
        (xy 171.831 63.5) (xy 171.45 63.119) (xy 167.767 63.119) (xy 167.767 62.611) (xy 171.45 62.611)
        (xy 171.831 62.23)
      )
    )
  )
  (zone (net 3) (net_name "Net-(IC1-Pad4)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.131 64.897) (xy 159.639 64.897) (xy 159.639 68.58) (xy 160.02 68.961) (xy 163.703 68.961)
        (xy 163.703 69.469) (xy 160.02 69.469) (xy 159.639 69.85) (xy 159.639 73.533) (xy 159.131 73.533)
        (xy 159.131 69.85) (xy 158.75 69.469) (xy 155.067 69.469) (xy 155.067 68.961) (xy 158.75 68.961)
        (xy 159.131 68.58)
      )
    )
  )
  (zone (net 7) (net_name "Net-(IC1-Pad8)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.809 60.071) (xy 122.809 60.325) (xy 118.745 60.325) (xy 118.745 64.389) (xy 117.475 64.389)
        (xy 117.475 60.325) (xy 113.411 60.325) (xy 113.411 59.055) (xy 117.475 59.055) (xy 117.475 54.991)
        (xy 118.745 54.991) (xy 118.745 59.055) (xy 122.809 59.055) (xy 122.809 59.309) (xy 123.19 59.309)
        (xy 123.19 58.674) (xy 120.777 58.674) (xy 121.285 57.404) (xy 120.396 56.515) (xy 119.126 57.023)
        (xy 119.126 54.61) (xy 117.094 54.61) (xy 117.094 57.023) (xy 115.824 56.515) (xy 114.935 57.404)
        (xy 115.443 58.674) (xy 113.03 58.674) (xy 113.03 60.706) (xy 115.443 60.706) (xy 114.935 61.976)
        (xy 115.824 62.865) (xy 117.094 62.357) (xy 117.094 64.77) (xy 119.126 64.77) (xy 119.126 62.357)
        (xy 120.396 62.865) (xy 121.285 61.976) (xy 120.777 60.706) (xy 123.19 60.706) (xy 123.19 60.071)
      )
    )
  )
  (zone (net 7) (net_name "Net-(IC1-Pad8)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.159 72.771) (xy 129.159 73.025) (xy 125.095 73.025) (xy 125.095 77.089) (xy 123.825 77.089)
        (xy 123.825 73.025) (xy 119.761 73.025) (xy 119.761 71.755) (xy 123.825 71.755) (xy 123.825 67.691)
        (xy 125.095 67.691) (xy 125.095 71.755) (xy 129.159 71.755) (xy 129.159 72.009) (xy 129.54 72.009)
        (xy 129.54 71.374) (xy 127.127 71.374) (xy 127.635 70.104) (xy 126.746 69.215) (xy 125.476 69.723)
        (xy 125.476 67.31) (xy 123.444 67.31) (xy 123.444 69.723) (xy 122.174 69.215) (xy 121.285 70.104)
        (xy 121.793 71.374) (xy 119.38 71.374) (xy 119.38 73.406) (xy 121.793 73.406) (xy 121.285 74.676)
        (xy 122.174 75.565) (xy 123.444 75.057) (xy 123.444 77.47) (xy 125.476 77.47) (xy 125.476 75.057)
        (xy 126.746 75.565) (xy 127.635 74.676) (xy 127.127 73.406) (xy 129.54 73.406) (xy 129.54 72.771)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 58.166) (xy 171.45 62.23) (xy 167.386 62.23) (xy 167.386 63.5) (xy 171.45 63.5)
        (xy 171.45 67.564) (xy 172.72 67.564) (xy 172.72 63.5) (xy 176.784 63.5) (xy 176.784 62.23)
        (xy 172.72 62.23) (xy 172.72 58.166) (xy 172.466 58.166) (xy 172.466 57.785) (xy 173.101 57.785)
        (xy 173.101 60.198) (xy 174.371 59.69) (xy 175.26 60.579) (xy 174.752 61.849) (xy 177.165 61.849)
        (xy 177.165 63.881) (xy 174.752 63.881) (xy 175.26 65.151) (xy 174.371 66.04) (xy 173.101 65.532)
        (xy 173.101 67.945) (xy 171.069 67.945) (xy 171.069 65.532) (xy 169.799 66.04) (xy 168.91 65.151)
        (xy 169.418 63.881) (xy 167.005 63.881) (xy 167.005 61.849) (xy 169.418 61.849) (xy 168.91 60.579)
        (xy 169.799 59.69) (xy 171.069 60.198) (xy 171.069 57.785) (xy 171.704 57.785) (xy 171.704 58.166)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.75 64.516) (xy 158.75 68.58) (xy 154.686 68.58) (xy 154.686 69.85) (xy 158.75 69.85)
        (xy 158.75 73.914) (xy 160.02 73.914) (xy 160.02 69.85) (xy 164.084 69.85) (xy 164.084 68.58)
        (xy 160.02 68.58) (xy 160.02 64.516) (xy 159.766 64.516) (xy 159.766 64.135) (xy 160.401 64.135)
        (xy 160.401 66.548) (xy 161.671 66.04) (xy 162.56 66.929) (xy 162.052 68.199) (xy 164.465 68.199)
        (xy 164.465 70.231) (xy 162.052 70.231) (xy 162.56 71.501) (xy 161.671 72.39) (xy 160.401 71.882)
        (xy 160.401 74.295) (xy 158.369 74.295) (xy 158.369 71.882) (xy 157.099 72.39) (xy 156.21 71.501)
        (xy 156.718 70.231) (xy 154.305 70.231) (xy 154.305 68.199) (xy 156.718 68.199) (xy 156.21 66.929)
        (xy 157.099 66.04) (xy 158.369 66.548) (xy 158.369 64.135) (xy 159.004 64.135) (xy 159.004 64.516)
      )
    )
  )
  (zone (net 3) (net_name "Net-(IC1-Pad4)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.778 72.136) (xy 128.778 72.644) (xy 125.095 72.644) (xy 124.714 73.025) (xy 124.714 76.708)
        (xy 124.206 76.708) (xy 124.206 73.025) (xy 123.825 72.644) (xy 120.142 72.644) (xy 120.142 72.136)
        (xy 123.825 72.136) (xy 124.206 71.755) (xy 124.206 68.072) (xy 124.714 68.072) (xy 124.714 71.755)
        (xy 125.095 72.136)
      )
    )
  )
  (zone (net 2) (net_name "Net-(IC1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.428 59.436) (xy 122.428 59.944) (xy 118.745 59.944) (xy 118.364 60.325) (xy 118.364 64.008)
        (xy 117.856 64.008) (xy 117.856 60.325) (xy 117.475 59.944) (xy 113.792 59.944) (xy 113.792 59.436)
        (xy 117.475 59.436) (xy 117.856 59.055) (xy 117.856 55.372) (xy 118.364 55.372) (xy 118.364 59.055)
        (xy 118.745 59.436)
      )
    )
  )
  (zone (net 7) (net_name "Net-(IC1-Pad8)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.51 79.375) (xy 139.7 79.375) (xy 139.7 76.2) (xy 147.32 76.2) (xy 147.32 79.375)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.545 60.579) (xy 169.799 60.325) (xy 170.053 60.325) (xy 171.069 61.341) (xy 171.069 61.595)
        (xy 170.815 61.849) (xy 170.561 61.849) (xy 169.545 60.833)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.101 61.595) (xy 173.355 61.849) (xy 173.609 61.849) (xy 174.625 60.833) (xy 174.625 60.579)
        (xy 174.371 60.325) (xy 174.117 60.325) (xy 173.101 61.341)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.355 63.881) (xy 173.101 64.135) (xy 173.101 64.389) (xy 174.117 65.405) (xy 174.371 65.405)
        (xy 174.625 65.151) (xy 174.625 64.897) (xy 173.609 63.881)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.815 63.881) (xy 171.069 64.135) (xy 171.069 64.389) (xy 170.053 65.405) (xy 169.799 65.405)
        (xy 169.545 65.151) (xy 169.545 64.897) (xy 170.561 63.881)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.577 62.865) (xy 172.085 62.357) (xy 172.593 62.865) (xy 172.085 63.373)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.369 67.945) (xy 158.115 68.199) (xy 157.861 68.199) (xy 156.845 67.183) (xy 156.845 66.929)
        (xy 157.099 66.675) (xy 157.353 66.675) (xy 158.369 67.691)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.655 68.199) (xy 160.401 67.945) (xy 160.401 67.691) (xy 161.417 66.675) (xy 161.671 66.675)
        (xy 161.925 66.929) (xy 161.925 67.183) (xy 160.909 68.199)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.401 70.485) (xy 160.655 70.231) (xy 160.909 70.231) (xy 161.925 71.247) (xy 161.925 71.501)
        (xy 161.671 71.755) (xy 161.417 71.755) (xy 160.401 70.739)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.115 70.231) (xy 158.369 70.485) (xy 158.369 70.739) (xy 157.353 71.755) (xy 157.099 71.755)
        (xy 156.845 71.501) (xy 156.845 71.247) (xy 157.861 70.231)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.877 69.215) (xy 159.385 68.707) (xy 159.893 69.215) (xy 159.385 69.723)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.84 58.674) (xy 117.094 58.42) (xy 117.094 58.166) (xy 116.078 57.15) (xy 115.824 57.15)
        (xy 115.57 57.404) (xy 115.57 57.658) (xy 116.586 58.674)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.84 60.706) (xy 117.094 60.96) (xy 117.094 61.214) (xy 116.078 62.23) (xy 115.824 62.23)
        (xy 115.57 61.976) (xy 115.57 61.722) (xy 116.586 60.706)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.126 60.96) (xy 119.38 60.706) (xy 119.634 60.706) (xy 120.65 61.722) (xy 120.65 61.976)
        (xy 120.396 62.23) (xy 120.142 62.23) (xy 119.126 61.214)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.126 58.42) (xy 119.38 58.674) (xy 119.634 58.674) (xy 120.65 57.658) (xy 120.65 57.404)
        (xy 120.396 57.15) (xy 120.142 57.15) (xy 119.126 58.166)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.11 59.182) (xy 117.602 59.69) (xy 118.11 60.198) (xy 118.618 59.69)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.19 71.374) (xy 123.444 71.12) (xy 123.444 70.866) (xy 122.428 69.85) (xy 122.174 69.85)
        (xy 121.92 70.104) (xy 121.92 70.358) (xy 122.936 71.374)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.476 71.12) (xy 125.73 71.374) (xy 125.984 71.374) (xy 127 70.358) (xy 127 70.104)
        (xy 126.746 69.85) (xy 126.492 69.85) (xy 125.476 70.866)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.19 73.406) (xy 123.444 73.66) (xy 123.444 73.914) (xy 122.428 74.93) (xy 122.174 74.93)
        (xy 121.92 74.676) (xy 121.92 74.422) (xy 122.936 73.406)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.476 73.66) (xy 125.73 73.406) (xy 125.984 73.406) (xy 127 74.422) (xy 127 74.676)
        (xy 126.746 74.93) (xy 126.492 74.93) (xy 125.476 73.914)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 72.898) (xy 123.952 72.39) (xy 124.46 71.882) (xy 124.968 72.39)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.775 49.53) (xy 182.245 49.53) (xy 182.245 82.55) (xy 104.775 82.55)
      )
    )
  )
)
