(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 51)
    (zones 0)
    (modules 6)
    (nets 7)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.6096)
    (user_trace_width 0.762)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.254)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /SW)
  (net 2 /GND)
  (net 3 /VIN)
  (net 4 /LDO_EN)
  (net 5 /SW_INT)
  (net 6 /SW2v5)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net /LDO_EN)
    (add_net /SW)
    (add_net /SW2v5)
    (add_net /SW_INT)
    (add_net /VIN)
  )
  (module JohnLibrary:john-SOT23-5 (layer Top) (tedit 5CA75596)
    (at 135.9916 93.3704)
    (descr "SMALL OUTLINE TRANSISTOR")
    (tags "SMALL OUTLINE TRANSISTOR")
    (attr smd)
    (fp_text reference U3 (at 0.127 -2.3622) (layer F.SilkS) hide)
    (fp_text value MIC5504-3.3 (at 0.2667 -0.0127) (layer F.SilkS) hide)
    (pad 5 smd rect (at -0.94996 -1.29794) (size 0.54864 1.19888) (layers Top F.Paste F.Mask)
      (net 6 /SW2v5))
    (pad 4 smd rect (at 0.94996 -1.29794) (size 0.54864 1.19888) (layers Top F.Paste F.Mask))
    (pad 3 smd rect (at 0.94996 1.29794) (size 0.54864 1.19888) (layers Top F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at 0 1.29794) (size 0.54864 1.19888) (layers Top F.Paste F.Mask)
      (net 2 /GND))
    (pad 1 smd rect (at -0.94996 1.29794) (size 0.54864 1.19888) (layers Top F.Paste F.Mask)
      (net 3 /VIN))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Package_DFN_QFN:UDFN-4_1x1mm_P0.65mm (layer Top) (tedit 5A02F385)
    (at 135.9916 93.3704)
    (descr UDFN-4_1x1mm_P0.65mm)
    (tags UDFN-4_1x1mm_P0.65mm)
    (attr smd)
    (fp_text reference U1 (at 1.8034 -0.3048 90) (layer F.SilkS) hide)
    (fp_text value TCR3UM18ALF (at 0.47 2.34) (layer F.Fab))
    (fp_text user %R (at 0.04 0.08) (layer F.Fab))
    (pad 2 smd rect (at -0.345 0.415 90) (size 0.07 0.19) (layers Top F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd trapezoid (at -0.43 0.29 90) (size 0.18 0.18) (rect_delta 0.1799 0 ) (layers Top F.Paste F.Mask)
      (net 2 /GND))
    (pad 1 smd trapezoid (at -0.43 -0.3 180) (size 0.2 0.2) (rect_delta 0 0.19999 ) (layers Top F.Paste F.Mask)
      (net 6 /SW2v5))
    (pad 2 smd rect (at -0.54 0.325 270) (size 0.25 0.22) (layers Top F.Paste F.Mask)
      (net 2 /GND))
    (pad 5 smd rect (at 0 0.17 315) (size 0.24 0.24) (layers Top F.Paste F.Mask)
      (net 2 /GND))
    (pad 1 smd rect (at -0.54 -0.325 270) (size 0.25 0.22) (layers Top F.Paste F.Mask)
      (net 6 /SW2v5))
    (pad 4 smd rect (at 0.54 -0.325 270) (size 0.25 0.22) (layers Top F.Paste F.Mask)
      (net 3 /VIN))
    (pad 4 smd trapezoid (at 0.425 -0.29 270) (size 0.18 0.18) (rect_delta 0.1799 0 ) (layers Top F.Paste F.Mask)
      (net 3 /VIN))
    (pad 4 smd rect (at 0.34 -0.415 90) (size 0.07 0.19) (layers Top F.Paste F.Mask)
      (net 3 /VIN))
    (pad 3 smd rect (at 0.54 0.325 270) (size 0.25 0.22) (layers Top F.Paste F.Mask)
      (net 3 /VIN))
    (pad 3 smd trapezoid (at 0.43 0.29) (size 0.18 0.18) (rect_delta 0 0.17999 ) (layers Top F.Paste F.Mask)
      (net 3 /VIN))
    (pad 1 smd trapezoid (at -0.38 -0.35 180) (size 0.2 0.2) (rect_delta 0 0.19999 ) (layers Top F.Paste F.Mask)
      (net 6 /SW2v5))
    (pad 3 smd rect (at 0.345 0.415 90) (size 0.07 0.19) (layers Top F.Paste F.Mask)
      (net 3 /VIN))
    (pad 5 smd rect (at 0.17 0 315) (size 0.24 0.24) (layers Top F.Paste F.Mask)
      (net 2 /GND))
    (pad 5 smd rect (at -0.17 0 315) (size 0.24 0.24) (layers Top F.Paste F.Mask)
      (net 2 /GND))
    (pad 5 smd rect (at 0 -0.17 315) (size 0.24 0.24) (layers Top F.Paste F.Mask)
      (net 2 /GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UDFN-4_1x1mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnLibrary:john-TACTILE_SWITCH_SMD-4 (layer Bottom) (tedit 5EA2F5AB)
    (at 136.144 90.5002 270)
    (attr smd)
    (fp_text reference S1 (at 0.127 1.9812 270) (layer B.SilkS))
    (fp_text value PTS810 (at 0.3302 -1.8288 270) (layer B.SilkS) hide)
    (pad B2 smd rect (at 2.2479 -1.07442 270) (size 1.09982 0.6985) (layers Bottom B.Paste B.Mask)
      (net 2 /GND))
    (pad B1 smd rect (at -2.2479 -1.07442 270) (size 1.09982 0.6985) (layers Bottom B.Paste B.Mask)
      (net 2 /GND))
    (pad A2 smd rect (at 2.2479 1.07442 270) (size 1.09982 0.6985) (layers Bottom B.Paste B.Mask)
      (net 1 /SW))
    (pad A1 smd rect (at -2.2479 1.07442 270) (size 1.09982 0.6985) (layers Bottom B.Paste B.Mask)
      (net 1 /SW))
    (model ${PERSONAL3DMOD}/2pts810.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer Top) (tedit 5A02FF57)
    (at 136.0932 89.3064 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U2 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value ATtiny10-TS (at 0 2.9 135) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers Top F.Paste F.Mask)
      (net 4 /LDO_EN))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers Top F.Paste F.Mask)
      (net 2 /GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers Top F.Paste F.Mask)
      (net 1 /SW))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers Top F.Paste F.Mask)
      (net 5 /SW_INT))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers Top F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers Top F.Paste F.Mask)
      (net 6 /SW2v5))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer Top) (tedit 5E89F409)
    (at 140.081 93.726 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /LDO_EN))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SW_INT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (offset (xyz 0 0 -0.6096))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer Top) (tedit 5E89F3F1)
    (at 132.3086 93.7768 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0.2032 2.4384 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /SW))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VIN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (offset (xyz 0 0 -0.6096))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text PMIC (at 136.0932 87.1982) (layer B.SilkS))
  (gr_text "Oops \nElectronics" (at 136.1694 94.5134) (layer B.SilkS))
  (gr_text attiny (at 136.271 89.2048) (layer F.SilkS))
  (gr_text EN (at 138.8364 87.6046 90) (layer B.SilkS))
  (gr_text GND (at 138.7348 91.2622 90) (layer B.SilkS))
  (gr_text INT (at 138.7094 93.5736 90) (layer B.SilkS))
  (gr_text VIN (at 133.7564 93.472 90) (layer B.SilkS))
  (gr_text GND (at 133.7056 91.313 90) (layer B.SilkS))
  (gr_text SW (at 133.6802 87.7316 90) (layer B.SilkS))
  (gr_line (start 130.302 95.758) (end 130.302 86.614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.732 95.758) (end 130.302 95.758) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.732 86.614) (end 141.732 95.758) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.302 86.614) (end 141.732 86.614) (layer Edge.Cuts) (width 0.1))
  (gr_text EN (at 138.1506 88.6206 90) (layer F.SilkS))
  (gr_text INT (at 138.2522 93.4974 90) (layer F.SilkS))
  (gr_text GND (at 138.2268 91.186 90) (layer F.SilkS))
  (gr_text SW (at 133.9596 88.6714 90) (layer F.SilkS))
  (gr_text GND (at 134.0358 91.1352 90) (layer F.SilkS))
  (gr_text VIN (at 133.9342 93.345 90) (layer F.SilkS))
  (zone (net 2) (net_name /GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.8862 87.3252) (xy 141.3256 87.3252) (xy 141.3256 95.2754) (xy 130.9116 95.2754)
      )
    )
  )
)
