(kicad_pcb (version 4) (host pcbnew 4.0.4+dfsg1-stable)
  (general
    (links 51)
    (no_connects 0)
    (area 21.689287 16.3373 87.881002 50.381002)
    (thickness 1.6)
    (drawings 72)
    (tracks 278)
    (zones 0)
    (modules 18)
    (nets 30)
  )
  (page USLetter portrait)
  (title_block
    (title Pinguino_SMD-2550)
    (date 2016-07-09)
    (rev 1B)
    (company fAnDrEs)
    (comment 1 Rootdevel)
    (comment 2 Hackesapce)
    (comment 3 http://rootdevel.clockingit.com/)
    (comment 4 http://cc-electrognu.blogspot.com.co/)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.4318)
    (user_trace_width 0.508)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (trace_clearance 0.3048)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.4)
    (via_min_drill 0.3302)
    (user_via 0.508 0.3302)
    (user_via 0.8128 0.508)
    (user_via 1.016 0.4064)
    (user_via 1.2192 0.8128)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.064 2.064)
    (pad_drill 1.048)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x000f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory PCB))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 VSS)
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 VCC)
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad1)")
  (net 8 "Net-(P1-Pad2)")
  (net 9 "Net-(P1-Pad3)")
  (net 10 /PIN_13)
  (net 11 /PIN_14)
  (net 12 /PIN_15)
  (net 13 /PIN_16)
  (net 14 /PIN_17)
  (net 15 /PIN_10)
  (net 16 /PIN_11)
  (net 17 /PIN_12)
  (net 18 /PIN_7)
  (net 19 /PIN_6)
  (net 20 /PIN_5)
  (net 21 /PIN_4)
  (net 22 /PIN_3)
  (net 23 /PIN_2)
  (net 24 /PIN_1)
  (net 25 /PIN_0)
  (net 26 /PIN_8)
  (net 27 /PIN_9)
  (net 28 "Net-(R1-Pad2)")
  (net 29 "Net-(R2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.3048)
    (trace_width 0.1524)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /PIN_0)
    (add_net /PIN_1)
    (add_net /PIN_10)
    (add_net /PIN_11)
    (add_net /PIN_12)
    (add_net /PIN_13)
    (add_net /PIN_14)
    (add_net /PIN_15)
    (add_net /PIN_16)
    (add_net /PIN_17)
    (add_net /PIN_2)
    (add_net /PIN_3)
    (add_net /PIN_4)
    (add_net /PIN_5)
    (add_net /PIN_6)
    (add_net /PIN_7)
    (add_net /PIN_8)
    (add_net /PIN_9)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net VCC)
    (add_net VSS)
  )
  (net_class POWER ""
    (clearance 0.508)
    (trace_width 1.016)
    (via_dia 1.397)
    (via_drill 1.016)
    (uvia_dia 1.016)
    (uvia_drill 0.254)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 42.672 38.481)
    (fp_text reference G*** (at 0 2.65176) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -2.65176) (layer F.SilkS) hide)
  )
  (module Buttons_Switches_SMD:SW_SMD_1181 (layer B.Cu) (tedit 57AE5F40)
    (at 33.274 33.528 90)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at 0.0762 -1.1684 90) (layer B.SilkS))
    (fp_text value "SW Reset" (at 0 -2.286 90) (layer B.SilkS))
    (pad 2 smd rect (at 3 0 90) (size 2.3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(R2-Pad2)"))
    (pad 1 smd rect (at -3 0 90) (size 2.3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 VSS))
    (model Buttons_Switches_SMD.3dshapes/SW_SMD_1181.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x08 (layer F.Cu) (tedit 579E23B3)
    (at 36.8173 22.7203)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /PIN_13))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /PIN_14))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /PIN_15))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /PIN_16))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /PIN_17))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /PIN_10))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /PIN_11))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /PIN_12))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x10 (layer F.Cu) (tedit 579E2394)
    (at 31.8643 44.323)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 23.749 -0.127 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /PIN_7))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /PIN_6))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PIN_5))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /PIN_4))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /PIN_3))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /PIN_2))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /PIN_1))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /PIN_0))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /PIN_8))
    (pad 10 thru_hole circle (at 22.86 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /PIN_9))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x10.wrl
      (at (xyz 0.45 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module "Crystal SMD:Crystal_SMD_5032_2Pads" (layer F.Cu) (tedit 57E411F5)
    (at 44.6405 33.2105 90)
    (descr "Ceramic SMD crystal, 5.0x3.2mm, 2 Pads")
    (tags "crystal oscillator quartz SMD SMT 5032")
    (attr smd)
    (fp_text reference Y1 (at -0.0381 1.1303 270) (layer F.SilkS))
    (fp_text value 20Mhz (at 3.9497 -0.0127 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.05 0 90) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2.05 0 90) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Crystals.3dshapes/Crystal_SMD_5032_2Pads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 579E243C)
    (at 43.7388 25.1841 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 0.0127 180) (layer F.SilkS))
    (fp_text value 22pF (at -0.0254 -1.5621 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 579E2477)
    (at 48.4759 25.1587)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0.0127 0.0381) (layer F.SilkS))
    (fp_text value 22pF (at 0.0381 1.5621) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5890C31C)
    (at 53.4797 26.3906 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -0.1143 -0.6096 180) (layer F.SilkS))
    (fp_text value 220nF (at 2.6543 -0.2286 450) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 579E2302)
    (at 37.108 41.402)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -0.024 0) (layer F.SilkS))
    (fp_text value 100nF (at 0.1284 -1.4986 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer B.Cu) (tedit 579E4753)
    (at 33.20098 28 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 2.29362 0 270) (layer B.SilkS))
    (fp_text value "Run LED" (at -2.36902 -0.4 270) (layer B.SilkS))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 5 VCC))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer B.Cu) (tedit 579E4764)
    (at 33.25 39.15)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at -2.262 -0.0086 90) (layer B.SilkS))
    (fp_text value "Power LED" (at 2.42 -0.28 90) (layer B.SilkS))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 5 VCC))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_Mini-B (layer F.Cu) (tedit 57AE783F)
    (at 51.77536 33.51022 180)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (attr smd)
    (fp_text reference P1 (at 0.89916 0.08382 270) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at -2.88544 -0.06858 270) (layer F.SilkS))
    (pad 1 smd rect (at 3.44932 -1.6002 180) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 3.44932 -0.8001 180) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at 3.44932 0 180) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 3.44932 0.8001 180) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 3.44932 1.6002 180) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (pad 6 smd rect (at 3.35026 -4.45008 180) (size 2.24536 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (pad 6 smd rect (at -2.14884 -4.45008 180) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (pad 6 smd rect (at 3.35026 4.45008 180) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (pad 6 smd rect (at -2.14884 4.45008 180) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (pad "" np_thru_hole circle (at 0.8509 -2.19964 180) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.8509 2.19964 180) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
    (model Connect.3dshapes/USB_Mini_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 579E2429)
    (at 33.20796 33.1978)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -0.01016 -0.1016) (layer F.SilkS))
    (fp_text value 470 (at 0.14224 -1.5748 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 579E2432)
    (at 33.2232 29.6418)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -0.0254 0.1016) (layer F.SilkS))
    (fp_text value 10k (at 0 -1.524 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 579E241C)
    (at 33.2232 37.084)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -0.0254 0) (layer F.SilkS))
    (fp_text value 470 (at 0 -1.5494 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOJ-28-W (layer B.Cu) (tedit 579E4520)
    (at 45.212 33.528)
    (descr "Module CMS SOJ 32 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U***1 (at -0.2032 3.6322) (layer B.SilkS) hide)
    (fp_text value PIC18F2550 (at 4.699 0.0254) (layer B.SilkS))
    (pad 16 smd rect (at 6.985 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(P1-Pad3)"))
    (pad 17 smd rect (at 5.715 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 27 /PIN_9))
    (pad 18 smd rect (at 4.445 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 26 /PIN_8))
    (pad 19 smd rect (at 3.175 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 VSS))
    (pad 20 smd rect (at 1.905 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 5 VCC))
    (pad 24 smd rect (at -3.175 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 22 /PIN_3))
    (pad 25 smd rect (at -4.445 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 21 /PIN_4))
    (pad 26 smd rect (at -5.715 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 20 /PIN_5))
    (pad 27 smd rect (at -6.985 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 19 /PIN_6))
    (pad 28 smd rect (at -8.255 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 18 /PIN_7))
    (pad 1 smd rect (at -8.255 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -6.985 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 10 /PIN_13))
    (pad 3 smd rect (at -5.715 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 11 /PIN_14))
    (pad 4 smd rect (at -4.445 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 12 /PIN_15))
    (pad 5 smd rect (at -3.175 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 13 /PIN_16))
    (pad 9 smd rect (at 1.905 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 10 smd rect (at 3.175 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 11 smd rect (at 4.445 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 15 /PIN_10))
    (pad 12 smd rect (at 5.715 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 16 /PIN_11))
    (pad 13 smd rect (at 6.985 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 17 /PIN_12))
    (pad 14 smd rect (at 8.255 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 6 smd rect (at -1.905 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(R1-Pad2)"))
    (pad 7 smd rect (at -0.635 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 14 /PIN_17))
    (pad 8 smd rect (at 0.635 -5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 VSS))
    (pad 23 smd rect (at -1.905 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 23 /PIN_2))
    (pad 22 smd rect (at -0.635 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 24 /PIN_1))
    (pad 21 smd rect (at 0.635 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 25 /PIN_0))
    (pad 15 smd rect (at 8.255 5.842) (size 0.4572 1.27) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(P1-Pad2)"))
    (model SMD_Packages.3dshapes/SOJ-28-W.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.7 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 579CEF09)
    (at 32.639 25.273 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6256 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VSS))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.3 (layer F.Cu) (tedit 55725E31)
    (at 39.1668 33.26638 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.3")
    (attr smd)
    (fp_text reference C5 (at 0.00762 -0.0762 360) (layer F.SilkS))
    (fp_text value "10uF a 100uF" (at 0 4.445 270) (layer F.Fab))
    (pad 1 smd rect (at 2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at -2.75082 0 270) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 VSS))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 100nF (at 37.465 33.147 90) (layer F.SilkS))
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1,0000 in" (at 43.18 17.7) (layer Dwgs.User))
    (feature1 (pts (xy 55.88 20.828) (xy 55.88 16.35)))
    (feature2 (pts (xy 30.48 20.828) (xy 30.48 16.35)))
    (crossbar (pts (xy 30.48 19.05) (xy 55.88 19.05)))
    (arrow1a (pts (xy 55.88 19.05) (xy 54.753496 19.636421)))
    (arrow1b (pts (xy 55.88 19.05) (xy 54.753496 18.463579)))
    (arrow2a (pts (xy 30.48 19.05) (xy 31.606504 19.636421)))
    (arrow2b (pts (xy 30.48 19.05) (xy 31.606504 18.463579)))
  )
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1,0000 in" (at 27.225 33.528 270) (layer Dwgs.User))
    (feature1 (pts (xy 30.48 46.228) (xy 25.875 46.228)))
    (feature2 (pts (xy 30.48 20.828) (xy 25.875 20.828)))
    (crossbar (pts (xy 28.575 20.828) (xy 28.575 46.228)))
    (arrow1a (pts (xy 28.575 46.228) (xy 27.988579 45.101496)))
    (arrow1b (pts (xy 28.575 46.228) (xy 29.161421 45.101496)))
    (arrow2a (pts (xy 28.575 20.828) (xy 27.988579 21.954504)))
    (arrow2b (pts (xy 28.575 20.828) (xy 29.161421 21.954504)))
  )
  (gr_text Rootdevel.co (at 38.44 41.35) (layer B.SilkS))
  (gr_text GND (at 34.4424 25.4 90) (layer B.SilkS))
  (gr_text VCC (at 34.544 22.479 90) (layer B.SilkS))
  (gr_text I2C-SPI (at 47.117 41.656 90) (layer B.SilkS))
  (gr_text I2C-SPI (at 49.784 41.656 90) (layer B.SilkS))
  (gr_text 17-RA5 (at 46.99 25.273 90) (layer B.SilkS))
  (gr_text 16-RA3 (at 44.8056 25.2984 90) (layer B.SilkS))
  (gr_text 10 (at 49.53 25.019 90) (layer B.SilkS))
  (gr_text 15-RA2 (at 42.037 25.273 90) (layer B.SilkS))
  (gr_text SPI-Rx (at 54.737 41.275 90) (layer B.SilkS))
  (gr_text Tx (at 52.197 41.783 90) (layer B.SilkS))
  (gr_text RA1 (at 39.37 25.4 90) (layer B.SilkS))
  (gr_text RA0 (at 36.83 25.4 90) (layer B.SilkS))
  (gr_text PWM (at 54.737 25.146 90) (layer B.SilkS))
  (gr_text PWM (at 52.197 25.146 90) (layer B.SilkS))
  (gr_text 11 (at 52.2224 24.765) (layer F.SilkS))
  (gr_text 12 (at 54.737 24.765) (layer F.SilkS))
  (gr_text 14 (at 39.3954 25.3746) (layer F.SilkS))
  (gr_text 13 (at 36.4236 25.2984) (layer F.SilkS))
  (gr_text 7 (at 31.9786 41.8846) (layer F.SilkS))
  (gr_text 6 (at 34.1884 41.91) (layer F.SilkS))
  (gr_text 0 (at 49.7332 41.91) (layer F.SilkS))
  (gr_text 8 (at 52.324 41.8846) (layer F.SilkS))
  (gr_text 9 (at 54.7116 41.8846) (layer F.SilkS))
  (gr_text 3 (at 42.1132 41.91) (layer F.SilkS))
  (gr_text 2 (at 44.6278 41.8846) (layer F.SilkS))
  (gr_text 1 (at 47.1424 41.91) (layer F.SilkS))
  (gr_line (start 30.48 20.828) (end 30.48 46.228) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 55.88 20.828) (end 30.48 20.828) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 55.88 46.228) (end 55.88 20.828) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 30.48 46.228) (end 55.88 46.228) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.58 20.93) (xy 55.78 20.93) (xy 55.78 46.13) (xy 30.58 46.13)
      )
    )
  )
  (zone (net 2) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.58 20.93) (xy 55.78 20.93) (xy 55.78 46.13) (xy 30.58 46.13)
      )
    )
  )
)
