(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 82)
    (zones 0)
    (modules 23)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 Earth)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 "Net-(C6-Pad2)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 "Net-(R3-Pad2)")
  (net 11 "Net-(R4-Pad2)")
  (net 12 "Net-(R4-Pad1)")
  (net 13 "Net-(U1-Pad1)")
  (net 14 "Net-(U1-Pad5)")
  (net 15 "Net-(U1-Pad8)")
  (net 16 "Net-(C7-Pad1)")
  (net 17 "Net-(K1-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(K1-Pad10)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad8)")
  )
  (module Steve_Library:AD8055ANZ (layer F.Cu) (tedit 5D6D9EA9)
    (at 129.032 101.6 270)
    (fp_text reference U1 (at -3.81 -3.81 270) (layer F.SilkS))
    (fp_text value AD8055ANZ (at -10.16 -3.048 180) (layer F.SilkS))
    (fp_text user ~ (at 0 0 270) (layer Cmts.User))
    (fp_text user * (at -7.62 -9.144 270) (layer F.SilkS))
    (fp_text user * (at -7.112 -7.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -7.62 -7.62 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 -5.08 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 "Net-(R4-Pad1)"))
    (pad 3 thru_hole circle (at -7.62 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at -7.62 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 5 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "Net-(R4-Pad2)"))
    (pad 7 thru_hole circle (at 0 -5.08 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 8 thru_hole circle (at 0 -7.62 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad8)"))
  )
  (module Steve_Library:RNF14FTD470R (layer F.Cu) (tedit 5D6D9BAC)
    (at 125.5 104.75 180)
    (fp_text reference R4 (at -6.096 0 180) (layer F.SilkS))
    (fp_text value 470 (at -10.25 -2.5 180) (layer F.SilkS))
    (fp_text user ~ (at 0 0 180) (layer F.Fab))
    (fp_text user ~ (at 0 0 180) (layer F.SilkS))
    (fp_text user ~ (at 0 0 180) (layer Cmts.User))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 11 "Net-(R4-Pad2)"))
    (pad 1 thru_hole rect (at -12.192 0 180) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 "Net-(R4-Pad1)"))
  )
  (module Steve_Library:MFP-25BRD52-75R (layer F.Cu) (tedit 5D6D9B68)
    (at 132.5 108.5)
    (fp_text reference R5 (at -5.842 0) (layer F.SilkS))
    (fp_text value 75 (at -5.75 2.5) (layer F.SilkS))
    (fp_text user ~ (at 0 0) (layer Cmts.User))
    (fp_text user ~ (at 0 0) (layer F.SilkS))
    (fp_text user ~ (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at -11.684 0) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 11 "Net-(R4-Pad2)"))
  )
  (module Steve_Library:RNF14FTD470R (layer F.Cu) (tedit 5D6D9B39)
    (at 117.856 78.74 90)
    (fp_text reference R3 (at -6.096 0 90) (layer F.SilkS))
    (fp_text value 470 (at -5.588 2.54 90) (layer F.SilkS))
    (fp_text user ~ (at 0 0 90) (layer Cmts.User))
    (fp_text user ~ (at 0 0 90) (layer F.SilkS))
    (fp_text user ~ (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -12.192 0 90) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "Net-(R3-Pad2)"))
  )
  (module Steve_Library:MFP-25BRD52-100K (layer F.Cu) (tedit 5D6D9B18)
    (at 113.792 90.424 270)
    (fp_text reference R1 (at -5.842 0 270) (layer F.SilkS))
    (fp_text value 100k (at -4.572 2.54 270) (layer F.SilkS))
    (fp_text user ~ (at 0 0 270) (layer Cmts.User))
    (fp_text user ~ (at 0 0 270) (layer F.SilkS))
    (fp_text user ~ (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -11.684 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Steve_Library:MFP-25BRD52-100K (layer F.Cu) (tedit 5D6D9AE2)
    (at 96.52 91.44 180)
    (fp_text reference R2 (at -6.096 0 180) (layer F.SilkS))
    (fp_text value 100k (at -5.588 -2.54 180) (layer F.SilkS))
    (fp_text user ~ (at 0 0 180) (layer F.Fab))
    (fp_text user ~ (at 0 0 180) (layer F.SilkS))
    (fp_text user ~ (at 0 0 180) (layer Cmts.User))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 1 thru_hole rect (at -11.684 0 180) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Steve_Library:MFR-25FBF52-150R (layer F.Cu) (tedit 5D6D9AAC)
    (at 107.696 87.376)
    (fp_text reference R6 (at -5.588 0) (layer F.SilkS))
    (fp_text value 150 (at -5.588 -2.54) (layer F.SilkS))
    (fp_text user ~ (at 0 0) (layer Cmts.User))
    (fp_text user ~ (at 0 0) (layer F.SilkS))
    (fp_text user ~ (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at -11.684 0) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
  )
  (module Steve_Library:Binocular (layer F.Cu) (tedit 5D575AEB)
    (at 98.044 106.68 270)
    (descr "Binocular core 2:1")
    (fp_text reference T1 (at -2 -4 270) (layer F.SilkS))
    (fp_text value 1:1 (at -2 -8 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 5 3 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -8 3 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad2)"))
    (pad 2 thru_hole circle (at 4 -16 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at -8 -16 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 117.856 98.552)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.5 0) (layer F.SilkS))
    (fp_text value ".1 uF" (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 117.856 94.488)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.54 0) (layer F.SilkS))
    (fp_text value "5 pF" (at 0.508 2.032) (layer F.Fab))
    (fp_text user %R (at 3.048 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 116.84 102.108 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.5 0 270) (layer F.SilkS))
    (fp_text value ".22 uF" (at 2.5 2.5 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 107.696 83.82 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value ".1 uF" (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Steve_Library:UVR1H100MDD1TD (layer F.Cu) (tedit 0)
    (at 102.616 79.248 90)
    (fp_text reference C5 (at -1.0033 0 90) (layer F.SilkS))
    (fp_text value "10 uF" (at -1.524 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.0066 0 90) (size 1.2192 1.2192) (drill 0.7112) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.2192 1.2192) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 Earth))
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 81.28 86.36)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 2.54 0) (layer F.SilkS))
    (fp_text value ".22 uF" (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 122.428 89.408 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 5.588 0 90) (layer F.SilkS))
    (fp_text value 1N4740A (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user %R (at 4.064 -2.032 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Steve_Library:Fconnector (layer F.Cu) (tedit 5CBCCC54)
    (at 86.36 97.536)
    (descr "Amphenol Vertical F")
    (tags "Connector F")
    (fp_text reference J1 (at 0 0.5) (layer F.SilkS))
    (fp_text value "F Conn" (at 0 -0.5) (layer F.Fab))
    (pad 2 thru_hole circle (at 4.06 -4.06) (size 5 5) (drill 2.4) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at -4.06 4.06) (size 5 5) (drill 2.4) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at -4.06 -4.06) (size 5 5) (drill 2.4) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at 4.06 4.06) (size 5 5) (drill 2.4) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.4) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
  )
  (module Inductor_THT:L_Axial_L9.5mm_D4.0mm_P12.70mm_Horizontal_Fastron_SMCC (layer F.Cu) (tedit 5AE59B05)
    (at 82.296 116.84)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=9.5*4mm^2, Fastron, SMCC, http://cdn-reichelt.de/documents/datenblatt/B400/DS_SMCC_NEU.pdf, http://cdn-reichelt.de/documents/datenblatt/B400/LEADEDINDUCTORS.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 12.7mm  length 9.5mm diameter 4mm Fastron SMCC")
    (fp_text reference L1 (at 6.096 0.508) (layer F.SilkS))
    (fp_text value "470 uH" (at 6.35 3.12) (layer F.Fab))
    (fp_text user %R (at 6.35 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L9.5mm_D4.0mm_P12.70mm_Horizontal_Fastron_SMCC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L9.5mm_D4.0mm_P12.70mm_Horizontal_Fastron_SMCC (layer F.Cu) (tedit 5AE59B05)
    (at 93.98 80.772 180)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=9.5*4mm^2, Fastron, SMCC, http://cdn-reichelt.de/documents/datenblatt/B400/DS_SMCC_NEU.pdf, http://cdn-reichelt.de/documents/datenblatt/B400/LEADEDINDUCTORS.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 12.7mm  length 9.5mm diameter 4mm Fastron SMCC")
    (fp_text reference L2 (at 6.096 0 180) (layer F.SilkS))
    (fp_text value "470 uH" (at 6.35 3.12 180) (layer F.Fab))
    (fp_text user %R (at 6.35 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L9.5mm_D4.0mm_P12.70mm_Horizontal_Fastron_SMCC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad_Via (layer F.Cu) (tedit 56DDBFD7)
    (at 132.588 115.316)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference J2 (at 3.912 -4.066) (layer F.SilkS))
    (fp_text value Antenna (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad_Via (layer F.Cu) (tedit 56DDBFD7)
    (at 132.588 82.296)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference J3 (at -4.338 -3.796) (layer F.SilkS))
    (fp_text value Ground (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 3 Earth))
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 110.5 116.25 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value ".1 uF" (at 8.5 -0.25 180) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 112 119.5 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 4 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 12 -0.5 180) (layer F.SilkS))
    (fp_text user %R (at 4.11 0 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.Fab))
    (fp_text user K (at 0 -1.8 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_THT:Relay_SPDT_Omron_G5V-1 (layer F.Cu) (tedit 5A57D9C3)
    (at 115.75 118.5 90)
    (descr "Relay Omron G5V-1, see http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v_1.pdf")
    (tags "Relay Omron G5V-1")
    (fp_text reference G5V-1 (at 7.5 4) (layer F.SilkS))
    (fp_text value G5V-1 (at 2.5 12.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 6.35 90) (layer F.Fab))
    (pad 10 thru_hole circle (at 5.08 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(K1-Pad10)"))
    (pad 9 thru_hole circle (at 5.08 2.54 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (pad 6 thru_hole circle (at 5.08 10.16 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_Omron_G5V-1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 5T (at 114 104.5) (layer F.SilkS))
  (gr_text 5T (at 95 104.75) (layer F.SilkS))
  (gr_text "VE6WZ HI-Z Pre-amp\n(Circuit design by W1FV)" (at 104.5 100.75) (layer B.SilkS))
  (gr_text "VE6WZ HI-Z Pre-amp\n(Circuit by W1FV)" (at 87.5 107.75) (layer F.SilkS))
  (gr_text ".22 uF" (at 119.25 105 90) (layer F.SilkS))
  (gr_text "5 pF" (at 121.412 91.948) (layer F.SilkS))
  (gr_text ".1 uF" (at 120.396 101.092) (layer F.SilkS))
  (gr_text Antenna (at 132.588 120.396) (layer F.SilkS))
  (gr_text Ground (at 132.588 87.376) (layer F.SilkS))
  (gr_text 1N4740A (at 124.968 84.836 90) (layer F.SilkS))
  (gr_text ".1 uF" (at 110.236 81.28 90) (layer F.SilkS))
  (gr_text "10 uF" (at 97.536 79.248) (layer F.SilkS))
  (gr_text 1:1 (at 102.75 114) (layer F.SilkS))
  (gr_text "470 uH" (at 87.376 119.888) (layer F.SilkS))
  (gr_text "470 uH" (at 87.376 77.724) (layer F.SilkS))
  (gr_text ".22 uF" (at 83.82 88.9) (layer F.SilkS))
  (gr_line (start 139.7 121.92) (end 139.7 76.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 78.232 121.92) (end 139.7 121.92) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 78.232 76.2) (end 78.232 121.92) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.7 76.2) (end 78.232 76.2) (layer Edge.Cuts) (width 0.1))
  (zone (net 3) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.74 76.708) (xy 139.192 76.708) (xy 139.192 121.412) (xy 78.74 121.412)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.353912 94.488) (xy 112.609912 94.488) (xy 112.776 114.808) (xy 96.353912 114.808)
      )
    )
  )
)
