(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 101)
    (zones 0)
    (modules 17)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 BTN_L)
  (net 2 GND)
  (net 3 BTN_M)
  (net 4 BTN_R)
  (net 5 BTN_DPI)
  (net 6 BTN_SCROLL)
  (net 7 LED_L)
  (net 8 LED_M)
  (net 9 LED_R)
  (net 10 LED_DPI)
  (net 11 LED_SCROLL)
  (net 12 "Net-(J11-Pad8)")
  (net 13 "Net-(J11-Pad7)")
  (net 14 /YELLOW)
  (net 15 "Net-(J11-Pad3)")
  (net 16 "Net-(U1-Pad20)")
  (net 17 "Net-(U1-Pad14)")
  (net 18 "Net-(U1-Pad26)")
  (net 19 "Net-(U1-Pad27)")
  (net 20 "Net-(U1-Pad28)")
  (net 21 "Net-(U1-Pad29)")
  (net 22 "Net-(U1-Pad30)")
  (net 23 "Net-(U1-Pad31)")
  (net 24 "Net-(U1-Pad32)")
  (net 25 "Net-(U1-Pad13)")
  (net 26 "Net-(U1-Pad3)")
  (net 27 "Net-(U1-Pad2)")
  (net 28 VIN)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /YELLOW)
    (add_net BTN_DPI)
    (add_net BTN_L)
    (add_net BTN_M)
    (add_net BTN_R)
    (add_net BTN_SCROLL)
    (add_net GND)
    (add_net LED_DPI)
    (add_net LED_L)
    (add_net LED_M)
    (add_net LED_R)
    (add_net LED_SCROLL)
    (add_net "Net-(J11-Pad3)")
    (add_net "Net-(J11-Pad7)")
    (add_net "Net-(J11-Pad8)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net VIN)
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5BECCDD7)
    (at 102.5 42.5 90)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048 90) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5BECCDD7)
    (at 87.5 57 90)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048 90) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5BECCDD7)
    (at 72 103 90)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048 90) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5BECCB98)
    (at 102.87 91.44 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J1 (at 1.25 -3.5 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 1.25 4.5 270) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 BTN_L))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5BECCB9B)
    (at 95.25 91.44 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J2 (at 1.25 -3.5 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 1.25 4.5 270) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 3 BTN_M))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5BECCB9E)
    (at 87.63 91.44 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J3 (at 1.25 -3.5 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 1.25 4.5 270) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 4 BTN_R))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5BECCBA2)
    (at 80.01 91.44 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J4 (at 1.25 -3.5 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 1.25 4.5 270) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 5 BTN_DPI))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5BECCBA7)
    (at 72.39 91.44 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J5 (at 1.25 -3.5 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 1.25 4.5 270) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 6 BTN_SCROLL))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5BECCB83)
    (at 101.854 85.09 90)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J6 (at 1.25 -3.5 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 1.25 4.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 7 LED_L))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5BECCB8A)
    (at 94.234 85.09 90)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J7 (at 1.25 -3.5 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 1.25 4.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 8 LED_M))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5BECCB8E)
    (at 86.614 85.09 90)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J8 (at 1.25 -3.5 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 1.25 4.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 9 LED_R))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5BECCB92)
    (at 78.994 85.09 90)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J9 (at 1.25 -3.5 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 1.25 4.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 10 LED_DPI))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5BECCB95)
    (at 71.374 85.09 90)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J10 (at 1.25 -3.5 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 1.25 4.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 11 LED_SCROLL))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 69.596 46.736)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Trackball (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J11-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J11-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 VIN))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /YELLOW))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J11-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 VIN))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x08_Pitch2.54mm.wrl
      (offset (xyz 0 -8.889999866485596 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module TeensyMod:Teensy30_31_32_LC_NoCenterPads (layer F.Cu) (tedit 5BA19769)
    (at 87.63 56.5 270)
    (fp_text reference U1 (at 0 -10.16 270) (layer F.SilkS))
    (fp_text value Teensy3.2 (at 0 10.16 270) (layer F.Fab))
    (pad 20 thru_hole circle (at 16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad20)"))
    (pad 14 thru_hole circle (at 16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U1-Pad14)"))
    (pad 21 thru_hole circle (at 13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 LED_L))
    (pad 22 thru_hole circle (at 11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 LED_M))
    (pad 23 thru_hole circle (at 8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 LED_R))
    (pad 24 thru_hole circle (at 6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 LED_DPI))
    (pad 25 thru_hole circle (at 3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 LED_SCROLL))
    (pad 26 thru_hole circle (at 1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U1-Pad26)"))
    (pad 27 thru_hole circle (at -1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U1-Pad27)"))
    (pad 28 thru_hole circle (at -3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U1-Pad28)"))
    (pad 29 thru_hole circle (at -6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U1-Pad29)"))
    (pad 30 thru_hole circle (at -8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U1-Pad30)"))
    (pad 31 thru_hole circle (at -11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U1-Pad31)"))
    (pad 32 thru_hole circle (at -13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U1-Pad32)"))
    (pad 33 thru_hole circle (at -16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 28 VIN))
    (pad 13 thru_hole circle (at 13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U1-Pad13)"))
    (pad 12 thru_hole circle (at 11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 BTN_SCROLL))
    (pad 11 thru_hole circle (at 8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 BTN_DPI))
    (pad 10 thru_hole circle (at 6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 BTN_R))
    (pad 9 thru_hole circle (at 3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 BTN_M))
    (pad 8 thru_hole circle (at 1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 BTN_L))
    (pad 7 thru_hole circle (at -1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J11-Pad8)"))
    (pad 6 thru_hole circle (at -3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J11-Pad7)"))
    (pad 5 thru_hole circle (at -6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 /YELLOW))
    (pad 4 thru_hole circle (at -8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J11-Pad3)"))
    (pad 3 thru_hole circle (at -11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U1-Pad3)"))
    (pad 2 thru_hole circle (at -13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U1-Pad2)"))
    (pad 1 thru_hole rect (at -16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5BECCDD7)
    (at 102.5 103 90)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048 90) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Logos:logo_MLlabs_small (layer B.Cu) (tedit 0)
    (at 87.5 68.5 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text "MANIACAL LABS" (at 87.5 77) (layer B.SilkS))
  (gr_text "Arcade\nTrackball \nMouse Adapter" (at 102 62.5 90) (layer F.SilkS))
  (gr_line (start 67.5 106.5) (end 108 106.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.5 38.5) (end 67.5 106.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108 38.5) (end 67.5 38.5) (layer Edge.Cuts) (width 0.15))
  (gr_text TRACKBALL (at 71.5 67.5) (layer F.SilkS))
  (gr_text BLACK (at 73.75 46.75) (layer F.SilkS))
  (gr_text "RED\n" (at 71.75 49.25) (layer F.SilkS))
  (gr_text PURPLE (at 71.75 64.5) (layer F.SilkS))
  (gr_text BLUE (at 71.75 62) (layer F.SilkS))
  (gr_text RED (at 71.75 59.5) (layer F.SilkS))
  (gr_text BLACK (at 71.75 57) (layer F.SilkS))
  (gr_text GREEN (at 71.75 54.25) (layer F.SilkS))
  (gr_text YELLOW (at 71.75 51.75) (layer F.SilkS))
  (gr_line (start 108 38.5) (end 108 106.5) (layer Edge.Cuts) (width 0.2))
  (gr_text SCROLL (at 72.136 98.044) (layer F.SilkS))
  (gr_text DPI (at 79.756 98.044) (layer F.SilkS))
  (gr_text R (at 87.376 98.044) (layer F.SilkS))
  (gr_text M (at 94.996 98.044) (layer F.SilkS))
  (gr_text L (at 102.616 98.044) (layer F.SilkS))
  (gr_text BTN (at 106.68 92.964 90) (layer F.SilkS))
  (gr_text LED (at 106.68 83.82 90) (layer F.SilkS))
)
