<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="52.05" y2="0" width="0" layer="20"/>
<wire x1="52.05" y1="0" x2="52.05" y2="47.93" width="0" layer="20"/>
<wire x1="52.05" y1="47.93" x2="0" y2="47.93" width="0" layer="20"/>
<wire x1="0" y1="47.93" x2="0" y2="0" width="0" layer="20"/>
<hole x="49.53" y="44.45" drill="3.556"/>
<hole x="49.53" y="2.54" drill="3.556"/>
<hole x="2.54" y="30.48" drill="3.556"/>
</plain>
<libraries>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE15">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
<package name="FE05-1">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_12MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 12mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-5050)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA04-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74ttl-din">
<description>&lt;b&gt;TTL Devices with DIN Symbols&lt;/b&gt;&lt;p&gt;
CadSoft and the author do not warrant that this library is free from error
or will meet your specific requirements.&lt;p&gt;
&lt;author&gt;Created by Holger Bettenbühl, hol.bet.@rhein-main.net&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="buzzer">
<description>&lt;b&gt;Speakers and Buzzers&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;Distributors:
&lt;li&gt;Buerklin
&lt;li&gt;Spoerle
&lt;li&gt;Schukat
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F/CM12P">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ARDUINO_L" library="con-lsta" package="FE15" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="ARDUINO_R" library="con-lsta" package="FE15" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="JOYSTICK" library="con-lsta" package="FE05-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="LCD" library="pinhead" package="1X16" value=""/>
<element name="LCD_L" library="pinhead" package="1X02" value=""/>
<element name="LCD_R" library="pinhead" package="1X02" value=""/>
<element name="SHOOT" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_12MM" value="MOMENTARY-SWITCH-SPST-PTH-12MM">
<attribute name="PROD_ID" value="SWCH-09185"/>
<attribute name="SF_SKU" value="COM-09190"/>
</element>
<element name="TRANSCEIVER" library="con-lstb" package="MA04-2" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="TUR_L" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_12MM" value="MOMENTARY-SWITCH-SPST-PTH-12MM">
<attribute name="PROD_ID" value="SWCH-09185"/>
<attribute name="SF_SKU" value="COM-09190"/>
</element>
<element name="TUR_R" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_12MM" value="MOMENTARY-SWITCH-SPST-PTH-12MM">
<attribute name="PROD_ID" value="SWCH-09185"/>
<attribute name="SF_SKU" value="COM-09190"/>
</element>
<element name="V1" library="74ttl-din" package="DIL14" value="7404N"/>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="AXIAL-0.3" value="1.2k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="AXIAL-0.3" value="1.2k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="AXIAL-0.3" value="1.2k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-12182"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="AXIAL-0.3" value="1.2k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value="1.2k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.3" value="560">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.3" value="560">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="AXIAL-0.3" value="560">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="AXIAL-0.3" value="560">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="AXIAL-0.3" value="1.2k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="BATTERY" library="pinhead" package="1X02" value=""/>
<element name="SG1" library="buzzer" package="F/CM12P" value="F/CM12P">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="PIN4" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="PIN5" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="PIN1" library="SparkFun-Connectors" package="1X02" value=""/>
</elements>
<signals>
<signal name="D13">
<contactref element="ARDUINO_R" pad="1"/>
<contactref element="TRANSCEIVER" pad="5"/>
</signal>
<signal name="3V3">
<contactref element="ARDUINO_R" pad="2"/>
<contactref element="TRANSCEIVER" pad="2"/>
</signal>
<signal name="A0">
<contactref element="ARDUINO_R" pad="4"/>
<contactref element="JOYSTICK" pad="4"/>
</signal>
<signal name="A1">
<contactref element="ARDUINO_R" pad="5"/>
<contactref element="JOYSTICK" pad="3"/>
</signal>
<signal name="A2">
<contactref element="ARDUINO_R" pad="6"/>
<contactref element="LCD" pad="11"/>
</signal>
<signal name="A3">
<contactref element="ARDUINO_R" pad="7"/>
<contactref element="LCD" pad="12"/>
</signal>
<signal name="A4">
<contactref element="ARDUINO_R" pad="8"/>
<contactref element="LCD" pad="13"/>
</signal>
<signal name="A5">
<contactref element="ARDUINO_R" pad="9"/>
<contactref element="LCD" pad="14"/>
</signal>
<signal name="A6">
<contactref element="ARDUINO_R" pad="10"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="5V">
<contactref element="ARDUINO_R" pad="12"/>
<contactref element="JOYSTICK" pad="2"/>
<contactref element="V1" pad="14"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R4" pad="P$1"/>
<contactref element="R5" pad="P$1"/>
<contactref element="LCD" pad="2"/>
<contactref element="LCD" pad="15"/>
</signal>
<signal name="RST">
<contactref element="ARDUINO_R" pad="13"/>
<contactref element="ARDUINO_L" pad="3"/>
</signal>
<signal name="GND">
<contactref element="ARDUINO_R" pad="14"/>
<contactref element="TRANSCEIVER" pad="1"/>
<contactref element="JOYSTICK" pad="1"/>
<contactref element="ARDUINO_L" pad="4"/>
<contactref element="TUR_L" pad="1"/>
<contactref element="TUR_R" pad="1"/>
<contactref element="SHOOT" pad="1"/>
<contactref element="LCD_L" pad="1"/>
<contactref element="LCD_R" pad="1"/>
<contactref element="V1" pad="7"/>
<contactref element="LCD" pad="1"/>
<contactref element="LCD" pad="3"/>
<contactref element="LCD" pad="16"/>
<contactref element="LCD" pad="5"/>
<contactref element="R15" pad="P$2"/>
<contactref element="BATTERY" pad="2"/>
<contactref element="SG1" pad="-"/>
<contactref element="PIN4" pad="1"/>
<contactref element="PIN5" pad="1"/>
<contactref element="PIN1" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="ARDUINO_R" pad="15"/>
<contactref element="BATTERY" pad="1"/>
</signal>
<signal name="D2">
<contactref element="ARDUINO_L" pad="5"/>
<contactref element="JOYSTICK" pad="5"/>
</signal>
<signal name="D3">
<contactref element="ARDUINO_L" pad="6"/>
<contactref element="PIN1" pad="2"/>
</signal>
<signal name="D4">
<contactref element="ARDUINO_L" pad="7"/>
<contactref element="PIN4" pad="2"/>
</signal>
<signal name="D5">
<contactref element="ARDUINO_L" pad="8"/>
<contactref element="PIN5" pad="2"/>
</signal>
<signal name="D6">
<contactref element="ARDUINO_L" pad="9"/>
<contactref element="SG1" pad="+"/>
</signal>
<signal name="D12">
<contactref element="ARDUINO_L" pad="15"/>
<contactref element="TRANSCEIVER" pad="7"/>
</signal>
<signal name="D11">
<contactref element="ARDUINO_L" pad="14"/>
<contactref element="TRANSCEIVER" pad="6"/>
</signal>
<signal name="D10">
<contactref element="ARDUINO_L" pad="13"/>
<contactref element="LCD" pad="6"/>
</signal>
<signal name="D9">
<contactref element="ARDUINO_L" pad="12"/>
<contactref element="LCD" pad="4"/>
</signal>
<signal name="D8">
<contactref element="ARDUINO_L" pad="11"/>
<contactref element="TRANSCEIVER" pad="4"/>
</signal>
<signal name="D7">
<contactref element="ARDUINO_L" pad="10"/>
<contactref element="TRANSCEIVER" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="LCD_R" pad="2"/>
<contactref element="V1" pad="3"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="TUR_L" pad="3"/>
<contactref element="V1" pad="13"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="TUR_R" pad="3"/>
<contactref element="V1" pad="11"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="SHOOT" pad="3"/>
<contactref element="V1" pad="9"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="LCD_L" pad="2"/>
<contactref element="V1" pad="1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$12">
<contactref element="V1" pad="10"/>
<contactref element="R9" pad="P$1"/>
</signal>
<signal name="N$18">
<contactref element="V1" pad="2"/>
<contactref element="R11" pad="P$1"/>
</signal>
<signal name="N$19">
<contactref element="V1" pad="8"/>
<contactref element="R10" pad="P$1"/>
</signal>
<signal name="N$20">
<contactref element="V1" pad="4"/>
<contactref element="R12" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="V1" pad="12"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="R9" pad="P$2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R8" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="R10" pad="P$2"/>
<contactref element="R8" pad="P$2"/>
<contactref element="R13" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="R11" pad="P$2"/>
<contactref element="R13" pad="P$2"/>
<contactref element="R14" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="R12" pad="P$2"/>
<contactref element="R14" pad="P$2"/>
<contactref element="R15" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
