(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 204)
    (zones 0)
    (modules 15)
    (nets 18)
  )
  (page A)
  (title_block
    (title "Beetje 32U4 Blok")
    (date 2018-08-10)
    (rev 0.0)
    (company www.MakersBox.us)
    (comment 1 648.ken@gmail.com)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.5 3.500001)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 /RESET)
  (net 4 /LED_HB)
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 /LED_ERR)
  (net 8 /LED_PMODE)
  (net 9 "Net-(D3-Pad1)")
  (net 10 /MISO)
  (net 11 /SCK)
  (net 12 /MOSI)
  (net 13 /RST)
  (net 14 "Net-(U2-Pad9)")
  (net 15 "Net-(U2-Pad10)")
  (net 16 "Net-(D4-Pad1)")
  (net 17 "Net-(F1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /LED_ERR)
    (add_net /LED_HB)
    (add_net /LED_PMODE)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /RST)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad9)")
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 638D4183)
    (at 31 -2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D2 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value ERR (at 0 1.75 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /LED_ERR))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 35.5 -4 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:MEC8-113-CARD_2 locked (layer F.Cu) (tedit 637EA67F)
    (at 0 -0.1 90)
    (fp_text reference X0 (at 4.375 -1.25 90) (layer F.Fab))
    (fp_text value "Card Edge" (at 10.9 -1 90) (layer F.Fab))
    (fp_line (start 21 50.5) (end 21 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 19 51.5) (end 20 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 0 51.5) (end 1 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start -1 50.5) (end -1 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 19 6.5) (end 20 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 0 6.5) (end 1 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 17 0) (end 11.3 0) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 3 0) (end 7.9 0) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 9.4 6.5) (end 9.8 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 10.8 5.5) (end 10.8 0.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 8.4 0.5) (end 8.4 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 2.5 0.5) (end 2.5 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 17.5 0.5) (end 17.5 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 18.5 6.5) (end 19 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 1 6.5) (end 1.5 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 8.5 51.5) (end 1 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 11.5 51.5) (end 19 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 21 7.5) (end 21 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start -1 47.5) (end -1 7.5) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 3 0.5) (end 3 0) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 17 0.5) (end 17.5 0.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 11.3 0.5) (end 11.3 0) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 7.9 0.5) (end 8.4 0.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 9.8 5.5) (end 9.8 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 9.4 5.5) (end 8.4 5.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 1.5 5.5) (end 1.5 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 18.5 5.5) (end 17.5 5.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 20 7.5) (end 21 7.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 0 7.5) (end 0 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 0 50.5) (end -1 50.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 20 50.5) (end 20 51.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 10 51.5) (end 11.5 51.5) (angle -180) (layer Edge.Cuts) (width 0.12))
    (pad 13 smd rect (at 16.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(F1-Pad1)"))
    (pad 26 smd rect (at 16.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 15.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask))
    (pad 25 smd rect (at 15.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 14.8 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /RESET))
    (pad 24 smd rect (at 14.8 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 14 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /SCK))
    (pad 23 smd rect (at 14 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 13.2 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 12 /MOSI))
    (pad 22 smd rect (at 13.2 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 12.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 10 /MISO))
    (pad 21 smd rect (at 12.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 11.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd rect (at 11.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_PMODE))
    (pad 6 smd rect (at 7.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd rect (at 7.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 6.8 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd rect (at 6.8 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd rect (at 6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 5.2 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 7 /LED_ERR))
    (pad 16 smd rect (at 5.2 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 4.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /LED_HB))
    (pad 15 smd rect (at 4.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 3.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 13 /RST))
    (pad 14 smd rect (at 3.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 25.95 -9)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.68) (layer F.SilkS) hide)
    (fp_text value 10uF (at -3.45 0) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RESET))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 26.5 -4.08 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 22 -4 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D4-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 22 -2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D4 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value D13/D2 (at 0 1.75 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 26.5 -2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D1 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value HEART (at 0 1.75 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /LED_HB))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 35.5 -2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D3 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value PRG (at 0 1.75 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_PMODE))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 31 -4.08 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 10 -11.5 90)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 168/328 (at 3.5 35.75 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 16.51 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /RST))
    (pad 15 thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /MOSI))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /MISO))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /SCK))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 21 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(U2-Pad9)"))
    (pad 23 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U2-Pad10)"))
    (pad 24 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/3D/ED281DT--3DModel-STEP-56544.STEP
      (offset (xyz 3.5 -16.5 -3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module footprints:Resonator_SMD_CTSC_1.3mmx3.2mm (layer F.Cu) (tedit 636FC12A)
    (at 30 -9 180)
    (descr "SMD Resomator/Filter Murata TPSKA, http://cdn-reichelt.de/documents/datenblatt/B400/SFECV-107.pdf, hand-soldering, 7.9x3.8mm^2 package")
    (tags "SMD SMT ceramic resonator filter filter hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at -0.127 -1.27) (layer F.SilkS) hide)
    (fp_text value 16Mhz (at -3.5 0) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.2 0 180) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad10)"))
    (pad 2 smd rect (at 0 0 180) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.2 0 180) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U2-Pad9)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Resonator_SMD_muRata_TPSKA-3pin_7.9x3.8mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/3D/resontator_CSTNE16M0V530000R0.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 10 -1 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 25/45/85 (at 3.81 -2.5 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /RST))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /MOSI))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /MISO))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /SCK))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KIPRJMOD}/3D/c-1-2199298-2-a-3d.stp
      (offset (xyz 4 -4 4.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 40.5 -7.04)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value ISP (at 5 2.54 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /MISO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /RST))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0805_2012Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 7.5 -15.6875 270)
    (descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags fuse)
    (attr smd)
    (fp_text reference F1 (at -0.0625 1.5 90) (layer F.SilkS))
    (fp_text value 54mA (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(F1-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 4.5 (width 0.15) (layer Dwgs.User)
    (gr_text "4.500 mm" (at 33.25 2.05) (layer Dwgs.User))
    (feature1 (pts (xy 35.5 -2) (xy 35.5 1.336421)))
    (feature2 (pts (xy 31 -2) (xy 31 1.336421)))
    (crossbar (pts (xy 31 0.75) (xy 35.5 0.75)))
    (arrow1a (pts (xy 35.5 0.75) (xy 34.373496 1.336421)))
    (arrow1b (pts (xy 35.5 0.75) (xy 34.373496 0.163579)))
    (arrow2a (pts (xy 31 0.75) (xy 32.126504 1.336421)))
    (arrow2b (pts (xy 31 0.75) (xy 32.126504 0.163579)))
  )
  (dimension 4.5 (width 0.15) (layer Dwgs.User)
    (gr_text "4.500 mm" (at 28.75 2.05) (layer Dwgs.User))
    (feature1 (pts (xy 31 -2) (xy 31 1.336421)))
    (feature2 (pts (xy 26.5 -2) (xy 26.5 1.336421)))
    (crossbar (pts (xy 26.5 0.75) (xy 31 0.75)))
    (arrow1a (pts (xy 31 0.75) (xy 29.873496 1.336421)))
    (arrow1b (pts (xy 31 0.75) (xy 29.873496 0.163579)))
    (arrow2a (pts (xy 26.5 0.75) (xy 27.626504 1.336421)))
    (arrow2b (pts (xy 26.5 0.75) (xy 27.626504 0.163579)))
  )
  (dimension 4.5 (width 0.15) (layer Dwgs.User)
    (gr_text "4.500 mm" (at 24.25 2.05) (layer Dwgs.User))
    (feature1 (pts (xy 26.5 -2) (xy 26.5 1.336421)))
    (feature2 (pts (xy 22 -2) (xy 22 1.336421)))
    (crossbar (pts (xy 22 0.75) (xy 26.5 0.75)))
    (arrow1a (pts (xy 26.5 0.75) (xy 25.373496 1.336421)))
    (arrow1b (pts (xy 26.5 0.75) (xy 25.373496 0.163579)))
    (arrow2a (pts (xy 22 0.75) (xy 23.126504 1.336421)))
    (arrow2b (pts (xy 22 0.75) (xy 23.126504 0.163579)))
  )
  (gr_text https://www.digikey.com/en/products/detail/on-shore-technology-inc/ED281DT/4147600 (at 30.75 3.5) (layer Dwgs.User))
  (gr_text "- Remove card prior to programming base (dissables reset).\n- [File]->[Examples]->[ArduinoISP]\n- [Tools]->[Progammer]->[Arduino as ISP]\n- Insert card in X1 slot.\n\n- [Tools]->[Burn Bootloader] for Attiny to set clock speed." (at 48.25 -13.5) (layer B.SilkS))
  (gr_text "-     +" (at 45.25 -4.5 90) (layer F.SilkS))
  (gr_text "Rev 0.0\nNov 2022" (at 50 -1.9) (layer B.SilkS))
  (gr_text github.com/aspro648/RPB (at 27.75 -1.5) (layer B.SilkS))
  (gr_text ArduinoISP (at 29.75 -6.5) (layer F.SilkS))
  (gr_text "Rapid Prototyping Card" (at 27.75 -3) (layer B.SilkS))
)
