(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 0.1016)
    (drawings 18)
    (tracks 11)
    (zones 0)
    (modules 4)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.3048)
    (user_via 0.6858 0.3302)
    (user_via 0.8128 0.4064)
    (user_via 1.2192 0.6096)
    (user_via 1.4224 0.8128)
    (blind_buried_vias_allowed yes)
    (uvia_size 0.3)
    (uvia_drill 0.1016)
    (uvias_allowed yes)
    (uvia_min_size 0.2032)
    (uvia_min_drill 0.1016)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.8 3.8)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7EFEF77F)
    (pcbplotparams
      (layerselection 0x01000_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad7)")
  (net 3 /signal)
  (net 4 /bias)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1016)
    (add_net /bias)
    (add_net /signal)
    (add_net GND)
    (add_net "Net-(J1-Pad7)")
  )
  (module gerber:bot_hatched (layer F.Cu) (tedit 0)
    (at 1.27 0)
    (fp_text reference G*** (at 0 0) (layer B.Cu) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.Cu) hide)
  )
  (module gerber:top_hatched (layer F.Cu) (tedit 0)
    (at 1.27 0)
    (fp_text reference G*** (at 0 0) (layer F.Cu) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Cu) hide)
  )
  (module MSAG_Misc:Omnetics_A115061-001 (layer F.Cu) (tedit 61A933C1)
    (at -101.6 0 90)
    (descr "Through hole righ angle nano strip conn, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference JSSD1 (at 3.7338 12.2936 180) (layer F.SilkS))
    (fp_text value "Omnetics A115061-001" (at 0.381 2.032 90) (layer F.Fab))
    (fp_text user %R (at -0.595 0.02 90) (layer F.Fab))
    (pad 10 thru_hole oval (at -5.675 4.1275) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at -4.445 6.6675) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at -3.135 4.1275) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at -1.905 6.6675) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at -0.595 4.1275) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0.675 6.6675) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 1.945 4.1275) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 /signal))
    (pad 3 thru_hole oval (at 3.215 6.6675) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 4.485 4.1275) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 /bias))
    (pad 1 thru_hole rect (at 5.755 6.6675) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model "${MSAG}/MSAG_KiCad3d/Omnetics A115061-001 REV 2.STEP"
      (offset (xyz 0 0 0.8890000000000001))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module MSAG_Misc:TMS-110-01-S-S-RA (layer F.Cu) (tedit 61AA46C4)
    (at 101.6 0 270)
    (fp_text reference J1 (at -6.4262 2.2606 180) (layer F.SilkS))
    (fp_text value TMS-110-01-S-S-RA (at 7.89 2.135 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.715 0 270) (size 1.01 1.01) (drill 0.66) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -4.445 0 270) (size 1.01 1.01) (drill 0.66) (layers *.Cu *.Mask)
      (net 4 /bias))
    (pad 3 thru_hole circle (at -3.175 0 270) (size 1.01 1.01) (drill 0.66) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -1.905 0 270) (size 1.01 1.01) (drill 0.66) (layers *.Cu *.Mask)
      (net 3 /signal))
    (pad 5 thru_hole circle (at -0.635 0 270) (size 1.01 1.01) (drill 0.66) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 0.635 0 270) (size 1.01 1.01) (drill 0.66) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 1.905 0 270) (size 1.01 1.01) (drill 0.66) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 3.175 0 270) (size 1.01 1.01) (drill 0.66) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 4.445 0 270) (size 1.01 1.01) (drill 0.66) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 5.715 0 270) (size 1.01 1.01) (drill 0.66) (layers *.Cu *.Mask))
    (model ${MSAG}/MSAG_KiCad3d/TMS-110-01-S-S-RA.stp
      (offset (xyz 0 1.524 1.27))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 105.664 8.0264) (end 96.7486 8.0264) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 96.7486 6.7564) (end 95.4786 6.7564) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 94.2086 6.7564) (end 95.4786 6.7564) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 94.2086 -6.7564) (end 95.4786 -6.7564) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.664 -8.0264) (end 96.7486 -8.0264) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 96.7486 -6.7564) (end 95.4786 -6.7564) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 -5.4864) (end 94.2086 -5.4864) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 5.4864) (end 94.2086 5.4864) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -92.5068 6.7564) (end -91.2368 6.7564) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -89.9668 6.7564) (end -91.2368 6.7564) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 5.4864) (end -89.9668 5.4864) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -103.124 8.0264) (end -92.5068 8.0264) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 -5.4864) (end -89.9668 -5.4864) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -89.9668 -6.7564) (end -91.2368 -6.7564) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -92.5068 -6.7564) (end -91.2368 -6.7564) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -103.124 -8.0264) (end -92.5068 -8.0264) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -103.124 -8.0264) (end -103.124 8.0264) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.664 -8.0264) (end 105.664 8.0264) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name "Net-(J1-Pad7)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy 100.2235 2.0066) (xy 100.416582 2.017545) (xy 100.572709 2.047253) (xy 100.70112 2.091034) (xy 100.811054 2.144196)
        (xy 100.91175 2.20205) (xy 101.012445 2.259903) (xy 101.122379 2.313065) (xy 101.25079 2.356846) (xy 101.406917 2.386554)
        (xy 101.6 2.3975) (xy 101.84625 1.905) (xy 101.6 1.4125) (xy 101.406917 1.423445) (xy 101.25079 1.453153)
        (xy 101.122379 1.496934) (xy 101.012445 1.550096) (xy 100.91175 1.60795) (xy 100.811054 1.665803) (xy 100.70112 1.718965)
        (xy 100.572709 1.762746) (xy 100.416582 1.792454) (xy 100.2235 1.8034)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad7)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy -93.5425 1.8034) (xy -93.737584 1.792244) (xy -93.895279 1.761966) (xy -94.024931 1.717345) (xy -94.135889 1.663163)
        (xy -94.2375 1.6042) (xy -94.33911 1.545236) (xy -94.450068 1.491054) (xy -94.57972 1.446433) (xy -94.737415 1.416155)
        (xy -94.9325 1.405) (xy -95.1825 1.905) (xy -94.9325 2.405) (xy -94.737415 2.393844) (xy -94.57972 2.363566)
        (xy -94.450068 2.318945) (xy -94.33911 2.264763) (xy -94.2375 2.2058) (xy -94.135889 2.146836) (xy -94.024931 2.092654)
        (xy -93.895279 2.048033) (xy -93.737584 2.017755) (xy -93.5425 2.0066)
      )
    )
  )
  (zone (net 3) (net_name /signal) (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy 100.2235 -1.8034) (xy 100.416582 -1.792454) (xy 100.572709 -1.762746) (xy 100.70112 -1.718965) (xy 100.811054 -1.665803)
        (xy 100.91175 -1.60795) (xy 101.012445 -1.550096) (xy 101.122379 -1.496934) (xy 101.25079 -1.453153) (xy 101.406917 -1.423445)
        (xy 101.6 -1.4125) (xy 101.84625 -1.905) (xy 101.6 -2.3975) (xy 101.406917 -2.386554) (xy 101.25079 -2.356846)
        (xy 101.122379 -2.313065) (xy 101.012445 -2.259903) (xy 100.91175 -2.20205) (xy 100.811054 -2.144196) (xy 100.70112 -2.091034)
        (xy 100.572709 -2.047253) (xy 100.416582 -2.017545) (xy 100.2235 -2.0066)
      )
    )
  )
  (zone (net 3) (net_name /signal) (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy -96.0825 -2.0466) (xy -96.277584 -2.057755) (xy -96.435279 -2.088033) (xy -96.564931 -2.132654) (xy -96.675889 -2.186836)
        (xy -96.7775 -2.2458) (xy -96.87911 -2.304763) (xy -96.990068 -2.358945) (xy -97.11972 -2.403566) (xy -97.277415 -2.433844)
        (xy -97.4725 -2.445) (xy -97.7225 -1.945) (xy -97.4725 -1.445) (xy -97.277415 -1.456155) (xy -97.11972 -1.486433)
        (xy -96.990068 -1.531054) (xy -96.87911 -1.585236) (xy -96.7775 -1.6442) (xy -96.675889 -1.703163) (xy -96.564931 -1.757345)
        (xy -96.435279 -1.801966) (xy -96.277584 -1.832244) (xy -96.0825 -1.8434)
      )
    )
  )
  (zone (net 4) (net_name /bias) (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy 100.2235 -4.3434) (xy 100.416582 -4.332454) (xy 100.572709 -4.302746) (xy 100.70112 -4.258965) (xy 100.811054 -4.205803)
        (xy 100.91175 -4.14795) (xy 101.012445 -4.090096) (xy 101.122379 -4.036934) (xy 101.25079 -3.993153) (xy 101.406917 -3.963445)
        (xy 101.6 -3.9525) (xy 101.84625 -4.445) (xy 101.6 -4.9375) (xy 101.406917 -4.926554) (xy 101.25079 -4.896846)
        (xy 101.122379 -4.853065) (xy 101.012445 -4.799903) (xy 100.91175 -4.74205) (xy 100.811054 -4.684196) (xy 100.70112 -4.631034)
        (xy 100.572709 -4.587253) (xy 100.416582 -4.557545) (xy 100.2235 -4.5466)
      )
    )
  )
  (zone (net 4) (net_name /bias) (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy -96.0825 -4.5866) (xy -96.277584 -4.597755) (xy -96.435279 -4.628033) (xy -96.564931 -4.672654) (xy -96.675889 -4.726836)
        (xy -96.7775 -4.7858) (xy -96.87911 -4.844763) (xy -96.990068 -4.898945) (xy -97.11972 -4.943566) (xy -97.277415 -4.973844)
        (xy -97.4725 -4.985) (xy -97.7225 -4.485) (xy -97.4725 -3.985) (xy -97.277415 -3.996155) (xy -97.11972 -4.026433)
        (xy -96.990068 -4.071054) (xy -96.87911 -4.125236) (xy -96.7775 -4.1842) (xy -96.675889 -4.243163) (xy -96.564931 -4.297345)
        (xy -96.435279 -4.341966) (xy -96.277584 -4.372244) (xy -96.0825 -4.3834)
      )
    )
  )
)
