(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 103)
    (tracks 1563)
    (zones 0)
    (modules 203)
    (nets 226)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu power hide)
    (2 In2.Cu mixed)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.127)
    (user_trace_width 0.1778)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.016)
    (trace_clearance 0.127)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.254)
    (via_min_drill 0.254)
    (user_via 0.4572 0.254)
    (user_via 0.5588 0.254)
    (uvia_size 0.4572)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.254)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.27 0.27)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 42.48666 41.59788)
    (visible_elements 7EFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C4-Pad2)")
  (net 3 "Net-(C5-Pad1)")
  (net 4 "Net-(C7-Pad1)")
  (net 5 "Net-(C8-Pad2)")
  (net 6 +5V)
  (net 7 "Net-(C11-Pad2)")
  (net 8 "Net-(C11-Pad1)")
  (net 9 "Net-(C12-Pad1)")
  (net 10 "Net-(C14-Pad2)")
  (net 11 "Net-(C14-Pad1)")
  (net 12 "Net-(F1-Pad2)")
  (net 13 "/Connectors, IO/CW_TARG4")
  (net 14 "/Connectors, IO/CW_TARG3")
  (net 15 "/Connectors, IO/CW_TARG2")
  (net 16 "/Connectors, IO/CW_TARG1")
  (net 17 "/Connectors, IO/CW_HS2")
  (net 18 "/Connectors, IO/CW_HS1")
  (net 19 "/Connectors, IO/CW_PDID")
  (net 20 "/Connectors, IO/CW_PDIC")
  (net 21 "/Connectors, IO/CW_SCK")
  (net 22 "/Connectors, IO/CW_MOSI")
  (net 23 "/Connectors, IO/CW_MISO")
  (net 24 +1V0)
  (net 25 "Net-(JP2-Pad2)")
  (net 26 JA1)
  (net 27 "Net-(J2-Pad1)")
  (net 28 JA3)
  (net 29 "Net-(J2-Pad3)")
  (net 30 JA2)
  (net 31 "Net-(J2-Pad2)")
  (net 32 JA4)
  (net 33 "Net-(J2-Pad4)")
  (net 34 "Net-(J2-Pad8)")
  (net 35 JA8)
  (net 36 "Net-(J2-Pad10)")
  (net 37 JA10)
  (net 38 "Net-(J2-Pad7)")
  (net 39 JA7)
  (net 40 "Net-(J2-Pad9)")
  (net 41 JA9)
  (net 42 "Net-(R25-Pad1)")
  (net 43 "Net-(R27-Pad2)")
  (net 44 "Net-(R28-Pad2)")
  (net 45 PGOOD)
  (net 46 "Net-(Q3-Pad3)")
  (net 47 "Net-(R41-Pad1)")
  (net 48 "Net-(R42-Pad2)")
  (net 49 ON_OFF)
  (net 50 "Net-(J7-Pad14)")
  (net 51 "Net-(J7-Pad12)")
  (net 52 VCORE_CURRENT_GAIN_1)
  (net 53 VCORE_CURRENT_GAIN_0)
  (net 54 VCORE_CURRENT)
  (net 55 "Net-(U9-Pad14)")
  (net 56 "Net-(U9-Pad13)")
  (net 57 "Net-(U9-Pad12)")
  (net 58 "Net-(U9-Pad11)")
  (net 59 "Net-(U9-Pad6)")
  (net 60 "Net-(U9-Pad5)")
  (net 61 "Net-(U9-Pad4)")
  (net 62 "Net-(U9-Pad3)")
  (net 63 "/Connectors, IO/CW_RST")
  (net 64 "Net-(U1-PadV7)")
  (net 65 "Net-(U1-PadV6)")
  (net 66 "Net-(U1-PadU7)")
  (net 67 "Net-(U1-PadU6)")
  (net 68 "Net-(U1-PadU4)")
  (net 69 "Net-(U1-PadU2)")
  (net 70 "Net-(U1-PadT3)")
  (net 71 "Net-(U1-PadT2)")
  (net 72 "Net-(U1-PadP18)")
  (net 73 "Net-(U1-PadN18)")
  (net 74 "Net-(U1-PadN17)")
  (net 75 "Net-(U1-PadN3)")
  (net 76 "Net-(U1-PadL3)")
  (net 77 "Net-(U1-PadL2)")
  (net 78 "Net-(U1-PadK3)")
  (net 79 "Net-(U1-PadK2)")
  (net 80 "Net-(U1-PadH18)")
  (net 81 "Net-(U1-PadH17)")
  (net 82 "Net-(U1-PadH2)")
  (net 83 "Net-(U1-PadG17)")
  (net 84 "Net-(U1-PadE18)")
  (net 85 "Net-(U1-PadC17)")
  (net 86 "Net-(U1-PadC16)")
  (net 87 "Net-(U1-PadB17)")
  (net 88 "Net-(U1-PadB16)")
  (net 89 "Net-(U1-PadB15)")
  (net 90 "Net-(U1-PadB10)")
  (net 91 "Net-(U1-PadA17)")
  (net 92 "Net-(U1-PadA10)")
  (net 93 FC_3V3)
  (net 94 FC_5V)
  (net 95 FC_RST)
  (net 96 FC_IO)
  (net 97 FD_TF)
  (net 98 FD2C_CLK)
  (net 99 FC2D_CLK)
  (net 100 FC_DIO0)
  (net 101 FC_DIO1)
  (net 102 FC_DIO2)
  (net 103 FC_DIO3)
  (net 104 SW_DONE)
  (net 105 SW_DIN)
  (net 106 SW_INIT_B)
  (net 107 SW_CLK)
  (net 108 SW_PROGRAM_B)
  (net 109 FC2D_HS)
  (net 110 FD2C_HS)
  (net 111 FC_PROG)
  (net 112 FC_DIO1_MUX)
  (net 113 FC_DIO2_MUX)
  (net 114 FC_DIO3_MUX)
  (net 115 FC_DIO0_MUX)
  (net 116 "Net-(R52-Pad1)")
  (net 117 "Net-(R56-Pad2)")
  (net 118 "Net-(Q4-Pad3)")
  (net 119 "Net-(Q5-Pad3)")
  (net 120 "Net-(Q6-Pad3)")
  (net 121 "Net-(R63-Pad2)")
  (net 122 "Net-(R65-Pad2)")
  (net 123 "Net-(S4-Pad4)")
  (net 124 "Net-(S4-Pad2)")
  (net 125 "Net-(S5-Pad4)")
  (net 126 "Net-(S5-Pad2)")
  (net 127 +3V3)
  (net 128 +1V8)
  (net 129 VCCINT)
  (net 130 "Net-(Q7-Pad3)")
  (net 131 "Net-(J5-Pad1)")
  (net 132 "Net-(U1-PadL18)")
  (net 133 USER_LED_1)
  (net 134 USER_LED_2)
  (net 135 USER_LED_4)
  (net 136 USER_LED_3)
  (net 137 USER_BTN_1)
  (net 138 USER_BTN_2)
  (net 139 "Net-(U1-PadU9)")
  (net 140 "Net-(D6-Pad1)")
  (net 141 "Net-(U1-PadV4)")
  (net 142 "Net-(J10-Pad3)")
  (net 143 "Net-(U1-PadW15)")
  (net 144 "Net-(U1-PadW7)")
  (net 145 "Net-(U1-PadW4)")
  (net 146 "Net-(U1-PadW3)")
  (net 147 "Net-(U1-PadW2)")
  (net 148 "Net-(U1-PadV17)")
  (net 149 "Net-(U1-PadV16)")
  (net 150 "Net-(U1-PadV14)")
  (net 151 "Net-(U1-PadV9)")
  (net 152 "Net-(U1-PadV3)")
  (net 153 "Net-(U1-PadU18)")
  (net 154 "Net-(U1-PadU17)")
  (net 155 "Net-(U1-PadU16)")
  (net 156 "Net-(U1-PadU14)")
  (net 157 "Net-(U1-PadU8)")
  (net 158 "Net-(U1-PadU3)")
  (net 159 "Net-(U1-PadT18)")
  (net 160 "Net-(U1-PadT17)")
  (net 161 "Net-(U1-PadP17)")
  (net 162 "Net-(U1-PadP3)")
  (net 163 "Net-(U1-PadP2)")
  (net 164 "Net-(U1-PadN2)")
  (net 165 "Net-(U1-PadM19)")
  (net 166 "Net-(U1-PadL19)")
  (net 167 "Net-(U1-PadL17)")
  (net 168 "Net-(U1-PadJ17)")
  (net 169 "Net-(U1-PadH19)")
  (net 170 "Net-(U1-PadH3)")
  (net 171 "Net-(U1-PadG18)")
  (net 172 "Net-(U1-PadG3)")
  (net 173 "Net-(U1-PadG2)")
  (net 174 "Net-(U1-PadF19)")
  (net 175 "Net-(U1-PadD2)")
  (net 176 "Net-(U1-PadD1)")
  (net 177 "Net-(U1-PadC15)")
  (net 178 "Net-(U1-PadB18)")
  (net 179 "Net-(U1-PadB8)")
  (net 180 "Net-(U1-PadB2)")
  (net 181 "Net-(U1-PadA18)")
  (net 182 "Net-(U1-PadA16)")
  (net 183 "Net-(U1-PadA8)")
  (net 184 "Net-(U1-PadA2)")
  (net 185 "Net-(R73-Pad2)")
  (net 186 "Net-(S2-Pad4)")
  (net 187 "Net-(S2-Pad2)")
  (net 188 "Net-(S3-Pad3)")
  (net 189 "Net-(S3-Pad1)")
  (net 190 "/FPGA Programming/MODE_1")
  (net 191 "Net-(D1-Pad1)")
  (net 192 "Net-(D2-Pad1)")
  (net 193 "Net-(D3-Pad1)")
  (net 194 "Net-(D4-Pad1)")
  (net 195 "Net-(D5-Pad1)")
  (net 196 "/FPGA Programming/TDI")
  (net 197 "/FPGA Programming/TCK")
  (net 198 "/FPGA Programming/TMS")
  (net 199 "/FPGA 1/FCS")
  (net 200 "/FPGA 1/MOSI")
  (net 201 "/FPGA 1/DIN")
  (net 202 "/FPGA Programming/MODE_2")
  (net 203 "/FPGA Programming/CCLK")
  (net 204 "/FPGA 1/PUDC")
  (net 205 "Net-(SW2-Pad2)")
  (net 206 "Net-(SW2-Pad1)")
  (net 207 "Net-(Q2-Pad3)")
  (net 208 "Net-(Q2-Pad1)")
  (net 209 /Power/pre1V8)
  (net 210 /Power/pre3V3)
  (net 211 /Power/EN2)
  (net 212 /Power/EN3)
  (net 213 /Power/MODE)
  (net 214 /Power/FB1)
  (net 215 /Power/FB2)
  (net 216 /Power/FB3)
  (net 217 /Power/SW1)
  (net 218 /Power/SW2)
  (net 219 /Power/SW3)
  (net 220 "Net-(S1-Pad6)")
  (net 221 "Net-(S1-Pad5)")
  (net 222 "Net-(S1-Pad4)")
  (net 223 TDO)
  (net 224 MODE_0)
  (net 225 "Net-(U1-PadP19)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.4572)
    (uvia_drill 0.254)
    (add_net +1V0)
    (add_net +1V8)
    (add_net +3V3)
    (add_net +5V)
    (add_net "/Connectors, IO/CW_HS1")
    (add_net "/Connectors, IO/CW_HS2")
    (add_net "/Connectors, IO/CW_MISO")
    (add_net "/Connectors, IO/CW_MOSI")
    (add_net "/Connectors, IO/CW_PDIC")
    (add_net "/Connectors, IO/CW_PDID")
    (add_net "/Connectors, IO/CW_RST")
    (add_net "/Connectors, IO/CW_SCK")
    (add_net "/Connectors, IO/CW_TARG1")
    (add_net "/Connectors, IO/CW_TARG2")
    (add_net "/Connectors, IO/CW_TARG3")
    (add_net "/Connectors, IO/CW_TARG4")
    (add_net "/FPGA 1/DIN")
    (add_net "/FPGA 1/FCS")
    (add_net "/FPGA 1/MOSI")
    (add_net "/FPGA 1/PUDC")
    (add_net "/FPGA Programming/CCLK")
    (add_net "/FPGA Programming/MODE_1")
    (add_net "/FPGA Programming/MODE_2")
    (add_net "/FPGA Programming/TCK")
    (add_net "/FPGA Programming/TDI")
    (add_net "/FPGA Programming/TMS")
    (add_net /Power/EN2)
    (add_net /Power/EN3)
    (add_net /Power/FB1)
    (add_net /Power/FB2)
    (add_net /Power/FB3)
    (add_net /Power/MODE)
    (add_net /Power/SW1)
    (add_net /Power/SW2)
    (add_net /Power/SW3)
    (add_net /Power/pre1V8)
    (add_net /Power/pre3V3)
    (add_net FC2D_CLK)
    (add_net FC2D_HS)
    (add_net FC_3V3)
    (add_net FC_5V)
    (add_net FC_DIO0)
    (add_net FC_DIO0_MUX)
    (add_net FC_DIO1)
    (add_net FC_DIO1_MUX)
    (add_net FC_DIO2)
    (add_net FC_DIO2_MUX)
    (add_net FC_DIO3)
    (add_net FC_DIO3_MUX)
    (add_net FC_IO)
    (add_net FC_PROG)
    (add_net FC_RST)
    (add_net FD2C_CLK)
    (add_net FD2C_HS)
    (add_net FD_TF)
    (add_net GND)
    (add_net JA1)
    (add_net JA10)
    (add_net JA2)
    (add_net JA3)
    (add_net JA4)
    (add_net JA7)
    (add_net JA8)
    (add_net JA9)
    (add_net MODE_0)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J10-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J7-Pad12)")
    (add_net "Net-(J7-Pad14)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q4-Pad3)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q6-Pad3)")
    (add_net "Net-(Q7-Pad3)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R41-Pad1)")
    (add_net "Net-(R42-Pad2)")
    (add_net "Net-(R52-Pad1)")
    (add_net "Net-(R56-Pad2)")
    (add_net "Net-(R63-Pad2)")
    (add_net "Net-(R65-Pad2)")
    (add_net "Net-(R73-Pad2)")
    (add_net "Net-(S1-Pad4)")
    (add_net "Net-(S1-Pad5)")
    (add_net "Net-(S1-Pad6)")
    (add_net "Net-(S2-Pad2)")
    (add_net "Net-(S2-Pad4)")
    (add_net "Net-(S3-Pad1)")
    (add_net "Net-(S3-Pad3)")
    (add_net "Net-(S4-Pad2)")
    (add_net "Net-(S4-Pad4)")
    (add_net "Net-(S5-Pad2)")
    (add_net "Net-(S5-Pad4)")
    (add_net "Net-(SW2-Pad1)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(U1-PadA10)")
    (add_net "Net-(U1-PadA16)")
    (add_net "Net-(U1-PadA17)")
    (add_net "Net-(U1-PadA18)")
    (add_net "Net-(U1-PadA2)")
    (add_net "Net-(U1-PadA8)")
    (add_net "Net-(U1-PadB10)")
    (add_net "Net-(U1-PadB15)")
    (add_net "Net-(U1-PadB16)")
    (add_net "Net-(U1-PadB17)")
    (add_net "Net-(U1-PadB18)")
    (add_net "Net-(U1-PadB2)")
    (add_net "Net-(U1-PadB8)")
    (add_net "Net-(U1-PadC15)")
    (add_net "Net-(U1-PadC16)")
    (add_net "Net-(U1-PadC17)")
    (add_net "Net-(U1-PadD1)")
    (add_net "Net-(U1-PadD2)")
    (add_net "Net-(U1-PadE18)")
    (add_net "Net-(U1-PadF19)")
    (add_net "Net-(U1-PadG17)")
    (add_net "Net-(U1-PadG18)")
    (add_net "Net-(U1-PadG2)")
    (add_net "Net-(U1-PadG3)")
    (add_net "Net-(U1-PadH17)")
    (add_net "Net-(U1-PadH18)")
    (add_net "Net-(U1-PadH19)")
    (add_net "Net-(U1-PadH2)")
    (add_net "Net-(U1-PadH3)")
    (add_net "Net-(U1-PadJ17)")
    (add_net "Net-(U1-PadK2)")
    (add_net "Net-(U1-PadK3)")
    (add_net "Net-(U1-PadL17)")
    (add_net "Net-(U1-PadL18)")
    (add_net "Net-(U1-PadL19)")
    (add_net "Net-(U1-PadL2)")
    (add_net "Net-(U1-PadL3)")
    (add_net "Net-(U1-PadM19)")
    (add_net "Net-(U1-PadN17)")
    (add_net "Net-(U1-PadN18)")
    (add_net "Net-(U1-PadN2)")
    (add_net "Net-(U1-PadN3)")
    (add_net "Net-(U1-PadP17)")
    (add_net "Net-(U1-PadP18)")
    (add_net "Net-(U1-PadP19)")
    (add_net "Net-(U1-PadP2)")
    (add_net "Net-(U1-PadP3)")
    (add_net "Net-(U1-PadT17)")
    (add_net "Net-(U1-PadT18)")
    (add_net "Net-(U1-PadT2)")
    (add_net "Net-(U1-PadT3)")
    (add_net "Net-(U1-PadU14)")
    (add_net "Net-(U1-PadU16)")
    (add_net "Net-(U1-PadU17)")
    (add_net "Net-(U1-PadU18)")
    (add_net "Net-(U1-PadU2)")
    (add_net "Net-(U1-PadU3)")
    (add_net "Net-(U1-PadU4)")
    (add_net "Net-(U1-PadU6)")
    (add_net "Net-(U1-PadU7)")
    (add_net "Net-(U1-PadU8)")
    (add_net "Net-(U1-PadU9)")
    (add_net "Net-(U1-PadV14)")
    (add_net "Net-(U1-PadV16)")
    (add_net "Net-(U1-PadV17)")
    (add_net "Net-(U1-PadV3)")
    (add_net "Net-(U1-PadV4)")
    (add_net "Net-(U1-PadV6)")
    (add_net "Net-(U1-PadV7)")
    (add_net "Net-(U1-PadV9)")
    (add_net "Net-(U1-PadW15)")
    (add_net "Net-(U1-PadW2)")
    (add_net "Net-(U1-PadW3)")
    (add_net "Net-(U1-PadW4)")
    (add_net "Net-(U1-PadW7)")
    (add_net "Net-(U9-Pad11)")
    (add_net "Net-(U9-Pad12)")
    (add_net "Net-(U9-Pad13)")
    (add_net "Net-(U9-Pad14)")
    (add_net "Net-(U9-Pad3)")
    (add_net "Net-(U9-Pad4)")
    (add_net "Net-(U9-Pad5)")
    (add_net "Net-(U9-Pad6)")
    (add_net ON_OFF)
    (add_net PGOOD)
    (add_net SW_CLK)
    (add_net SW_DIN)
    (add_net SW_DONE)
    (add_net SW_INIT_B)
    (add_net SW_PROGRAM_B)
    (add_net TDO)
    (add_net USER_BTN_1)
    (add_net USER_BTN_2)
    (add_net USER_LED_1)
    (add_net USER_LED_2)
    (add_net USER_LED_3)
    (add_net USER_LED_4)
    (add_net VCCINT)
    (add_net VCORE_CURRENT)
    (add_net VCORE_CURRENT_GAIN_0)
    (add_net VCORE_CURRENT_GAIN_1)
  )
  (module cerg:TSSOP-16-1EP_W4.40mm (layer F.Cu) (tedit 621854B4)
    (at 76.74066 36.68388)
    (attr smd)
    (fp_text reference U8 (at 0.29 -4.484) (layer F.SilkS))
    (fp_text value LTC3569EFE#PBF (at 0 5.4) (layer F.Fab))
    (fp_text user REF** (at 0.2 0) (layer F.Fab))
    (pad 17 thru_hole circle (at 0.8 0.8) (size 0.38 0.38) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.7 0.8) (size 0.38 0.38) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.8 -0.7) (size 0.38 0.38) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.7 -0.7) (size 0.38 0.38) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 0 0 180) (size 2.74 2.74) (layers F.Cu)
      (net 1 GND))
    (pad 15 smd rect (at -1.625 -2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 215 /Power/FB2) (solder_mask_margin 0.07))
    (pad 14 smd rect (at -0.975 -2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V) (solder_mask_margin 0.07))
    (pad 13 smd rect (at -0.325 -2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 213 /Power/MODE) (solder_mask_margin 0.07))
    (pad 12 smd rect (at 0.325 -2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 45 PGOOD) (solder_mask_margin 0.07))
    (pad 11 smd rect (at 0.975 -2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 1.625 -2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 218 /Power/SW2) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 2.275 -2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 217 /Power/SW1) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 2.275 2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 1.625 2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 219 /Power/SW3) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 0.975 2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 49 ON_OFF) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 0.325 2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 211 /Power/EN2) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -0.325 2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 212 /Power/EN3) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -0.975 2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.625 2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V) (solder_mask_margin 0.07))
    (pad 16 smd rect (at -2.275 -2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 214 /Power/FB1) (solder_mask_margin 0.07))
    (pad 17 smd rect (at 0 0) (size 2.31 2.46) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0001))
    (pad 1 smd rect (at -2.275 2.8) (size 0.3 1.05) (layers F.Cu F.Paste F.Mask)
      (net 216 /Power/FB3) (solder_mask_margin 0.07))
    (model ${KIPRJMOD}/cerg_3d_models/TSSOP-16_FEBA_LIT.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module cerg:Switch_Slide_JS202011SCQN (layer F.Cu) (tedit 621853AF)
    (at 84.65866 11.61788 270)
    (attr smd)
    (fp_text reference S1 (at -4.064 -3.302 180) (layer F.SilkS))
    (fp_text value JS202011SCQN (at 0.1 5.575 270) (layer F.Fab))
    (fp_text user %R (at -0.025 -0.05 270) (layer F.Fab))
    (pad 6 smd rect (at 2.5 -2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(S1-Pad6)"))
    (pad 5 smd rect (at 0 -2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(S1-Pad5)"))
    (pad 4 smd rect (at -2.5 -2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(S1-Pad4)"))
    (pad 1 smd rect (at -2.5 2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R42-Pad2)"))
    (pad 2 smd rect (at 0 2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 49 ON_OFF))
    (pad 3 smd rect (at 2.5 2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R41-Pad1)"))
    (model ${KIPRJMOD}/cerg_3d_models/JS202011SCQN.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Symbol:Symbol_Barrel_Polarity (layer F.Cu) (tedit 5765E9A7)
    (at 75.25266 13.53088)
    (descr "Barrel connector polarity indicator")
    (tags "barrel polarity")
    (attr virtual)
    (fp_text reference REF** (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Symbol_Barrel_Polarity (at 0 2) (layer F.Fab))
  )
  (module cerg:cerg_logo (layer F.Cu) (tedit 5F1F4B39)
    (at 47.18566 26.61188)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module cerg:PinHeader_2x7_P2mm_SMD (layer F.Cu) (tedit 5FF2B815)
    (at 21.98666 0.28588 180)
    (descr http://www.molex.com/pdm_docs/sd/878322620_sd.pdf)
    (attr smd)
    (fp_text reference J7 (at -9.652 2.892) (layer F.SilkS))
    (fp_text value 0878321420 (at 0 5.04) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5 0 180) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad 2 smd rect (at -6 -2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad 1 smd rect (at -6 2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4 -2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 198 "/FPGA Programming/TMS"))
    (pad 3 smd rect (at -4 2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2 -2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 197 "/FPGA Programming/TCK"))
    (pad 5 smd rect (at -2 2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0 -2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 223 TDO))
    (pad 7 smd rect (at 0 2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2 -2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 196 "/FPGA Programming/TDI"))
    (pad 9 smd rect (at 2 2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 4 -2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J7-Pad12)"))
    (pad 11 smd rect (at 4 2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 6 -2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J7-Pad14)"))
    (pad 13 smd rect (at 6 2.13 180) (size 1 2.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at -5 0 180) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/3d models/87832-1420_stp/878321420.stp"
      (offset (xyz 0 0 4.3815))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:SMA-JOHNSON-142-0701-801 (layer F.Cu) (tedit 5F1F56CA)
    (at 2.48166 15.56288 90)
    (fp_text reference J6 (at 7.239 0.127 180) (layer F.SilkS))
    (fp_text value Measure (at 0 -3.6 90) (layer F.Fab))
    (pad 2 smd rect (at 4.4 0 90) (size 2.4 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.4 0 90) (size 2.4 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.4 0 90) (size 2.4 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.4 0 90) (size 2.4 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 90) (size 2.3 5.08) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C14-Pad1)"))
    (model ${KIPRJMOD}/cerg_3d_models/SMA_Board_Edge_Molex_732511150.step
      (offset (xyz 0 2.54 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model ${KIPRJMOD}/cerg_3d_models/SMA_Board_Edge_Molex_732511150.wrl
      (offset (xyz 0 2.54 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module cerg:SMA-JOHNSON-142-0701-201 (layer F.Cu) (tedit 60BC4306)
    (at 32.32666 16.19788 90)
    (fp_text reference J4 (at 4.826 0 180) (layer F.SilkS))
    (fp_text value Glitch (at 0 -0.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.54 2.54) (drill 1.7018) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.54 2.54) (drill 1.7018) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.54 2.54) (drill 1.7018) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.54 2.54) (drill 1.7018) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.54 2.54) (drill 1.5748) (layers *.Cu *.Mask)
      (net 129 VCCINT))
    (model "${KIPRJMOD}/3d models/BELFUSE_1420701201/142-0701-201.stp"
      (offset (xyz 0 0 9.651999999999999))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Package_BGA:Xilinx_CPG238 (layer F.Cu) (tedit 61EB2CA1)
    (at 46.98666 37.09788 180)
    (descr "Artix-7 BGA, 19x19 grid, 10x10mm package, 0.5mm pitch; https://www.xilinx.com/support/documentation/user_guides/ug475_7Series_Pkg_Pinout.pdf#page=267, NSMD pad definition Appendix A")
    (tags "BGA 238 0.5 CPG238")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference U1 (at 0 -6 180) (layer F.SilkS))
    (fp_text value XC7A12T-CPG238 (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad A1 smd circle (at -4.5 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A2 smd circle (at -4 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(U1-PadA2)"))
    (pad A3 smd circle (at -3.5 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A4 smd circle (at -3 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A5 smd circle (at -2.5 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A6 smd circle (at -2 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A7 smd circle (at -1.5 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A8 smd circle (at -1 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(U1-PadA8)"))
    (pad A9 smd circle (at -0.5 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A10 smd circle (at 0 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U1-PadA10)"))
    (pad A11 smd circle (at 0.5 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A12 smd circle (at 1 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A13 smd circle (at 1.5 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A14 smd circle (at 2 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 133 USER_LED_1))
    (pad A15 smd circle (at 2.5 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 137 USER_BTN_1))
    (pad A16 smd circle (at 3 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(U1-PadA16)"))
    (pad A17 smd circle (at 3.5 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U1-PadA17)"))
    (pad A18 smd circle (at 4 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(U1-PadA18)"))
    (pad A19 smd circle (at 4.5 -4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B1 smd circle (at -4.5 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B2 smd circle (at -4 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(U1-PadB2)"))
    (pad B3 smd circle (at -3.5 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd circle (at -3 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B5 smd circle (at -2.5 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B6 smd circle (at -2 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B7 smd circle (at -1.5 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B8 smd circle (at -1 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U1-PadB8)"))
    (pad B9 smd circle (at -0.5 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B10 smd circle (at 0 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U1-PadB10)"))
    (pad B11 smd circle (at 0.5 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B12 smd circle (at 1 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B13 smd circle (at 1.5 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B14 smd circle (at 2 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B15 smd circle (at 2.5 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U1-PadB15)"))
    (pad B16 smd circle (at 3 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U1-PadB16)"))
    (pad B17 smd circle (at 3.5 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U1-PadB17)"))
    (pad B18 smd circle (at 4 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(U1-PadB18)"))
    (pad B19 smd circle (at 4.5 -4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad C1 smd circle (at -4.5 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C2 smd circle (at -4 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C3 smd circle (at -3.5 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C4 smd circle (at -3 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C5 smd circle (at -2.5 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C6 smd circle (at -2 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C7 smd circle (at -1.5 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C8 smd circle (at -1 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 197 "/FPGA Programming/TCK"))
    (pad C9 smd circle (at -0.5 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C10 smd circle (at 0 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C11 smd circle (at 0.5 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 203 "/FPGA Programming/CCLK"))
    (pad C12 smd circle (at 1 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C13 smd circle (at 1.5 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 128 +1V8))
    (pad C14 smd circle (at 2 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad C15 smd circle (at 2.5 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U1-PadC15)"))
    (pad C16 smd circle (at 3 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U1-PadC16)"))
    (pad C17 smd circle (at 3.5 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U1-PadC17)"))
    (pad C18 smd circle (at 4 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad C19 smd circle (at 4.5 -3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad D1 smd circle (at -4.5 -3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(U1-PadD1)"))
    (pad D2 smd circle (at -4 -3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(U1-PadD2)"))
    (pad D3 smd circle (at -3.5 -3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad D17 smd circle (at 3.5 -3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 200 "/FPGA 1/MOSI"))
    (pad D18 smd circle (at 4 -3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 200 "/FPGA 1/MOSI"))
    (pad D19 smd circle (at 4.5 -3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 201 "/FPGA 1/DIN"))
    (pad E1 smd circle (at -4.5 -2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E2 smd circle (at -4 -2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E3 smd circle (at -3.5 -2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E17 smd circle (at 3.5 -2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 204 "/FPGA 1/PUDC"))
    (pad E18 smd circle (at 4 -2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U1-PadE18)"))
    (pad E19 smd circle (at 4.5 -2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 95 FC_RST))
    (pad F1 smd circle (at -4.5 -2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad F2 smd circle (at -4 -2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad F3 smd circle (at -3.5 -2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad F17 smd circle (at 3.5 -2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad F18 smd circle (at 4 -2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad F19 smd circle (at 4.5 -2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(U1-PadF19)"))
    (pad G1 smd circle (at -4.5 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 134 USER_LED_2))
    (pad G2 smd circle (at -4 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(U1-PadG2)"))
    (pad G3 smd circle (at -3.5 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(U1-PadG3)"))
    (pad G7 smd circle (at -1.5 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad G8 smd circle (at -1 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad G9 smd circle (at -0.5 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad G10 smd circle (at 0 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 129 VCCINT))
    (pad G11 smd circle (at 0.5 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad G12 smd circle (at 1 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad G13 smd circle (at 1.5 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad G17 smd circle (at 3.5 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U1-PadG17)"))
    (pad G18 smd circle (at 4 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(U1-PadG18)"))
    (pad G19 smd circle (at 4.5 -1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 199 "/FPGA 1/FCS"))
    (pad H1 smd circle (at -4.5 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 138 USER_BTN_2))
    (pad H2 smd circle (at -4 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U1-PadH2)"))
    (pad H3 smd circle (at -3.5 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(U1-PadH3)"))
    (pad H7 smd circle (at -1.5 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad H8 smd circle (at -1 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad H9 smd circle (at -0.5 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad H10 smd circle (at 0 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 129 VCCINT))
    (pad H11 smd circle (at 0.5 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad H12 smd circle (at 1 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad H13 smd circle (at 1.5 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 128 +1V8))
    (pad H17 smd circle (at 3.5 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U1-PadH17)"))
    (pad H18 smd circle (at 4 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U1-PadH18)"))
    (pad H19 smd circle (at 4.5 -1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(U1-PadH19)"))
    (pad J1 smd circle (at -4.5 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 136 USER_LED_3))
    (pad J2 smd circle (at -4 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad J3 smd circle (at -3.5 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad J7 smd circle (at -1.5 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad J8 smd circle (at -1 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad J9 smd circle (at -0.5 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad J10 smd circle (at 0 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 129 VCCINT))
    (pad J11 smd circle (at 0.5 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad J12 smd circle (at 1 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad J13 smd circle (at 1.5 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 128 +1V8))
    (pad J17 smd circle (at 3.5 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(U1-PadJ17)"))
    (pad J18 smd circle (at 4 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad J19 smd circle (at 4.5 -0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad K1 smd circle (at -4.5 0 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 135 USER_LED_4))
    (pad K2 smd circle (at -4 0 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U1-PadK2)"))
    (pad K3 smd circle (at -3.5 0 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U1-PadK3)"))
    (pad K7 smd circle (at -1.5 0 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad K8 smd circle (at -1 0 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad K12 smd circle (at 1 0 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad K13 smd circle (at 1.5 0 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad K17 smd circle (at 3.5 0 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 98 FD2C_CLK))
    (pad K18 smd circle (at 4 0 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 98 FD2C_CLK))
    (pad K19 smd circle (at 4.5 0 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 98 FD2C_CLK))
    (pad L1 smd circle (at -4.5 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 37 JA10))
    (pad L2 smd circle (at -4 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U1-PadL2)"))
    (pad L3 smd circle (at -3.5 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U1-PadL3)"))
    (pad L7 smd circle (at -1.5 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad L8 smd circle (at -1 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad L9 smd circle (at -0.5 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad L10 smd circle (at 0 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 129 VCCINT))
    (pad L11 smd circle (at 0.5 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad L12 smd circle (at 1 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad L13 smd circle (at 1.5 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad L17 smd circle (at 3.5 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(U1-PadL17)"))
    (pad L18 smd circle (at 4 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(U1-PadL18)"))
    (pad L19 smd circle (at 4.5 0.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(U1-PadL19)"))
    (pad M1 smd circle (at -4.5 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 32 JA4))
    (pad M2 smd circle (at -4 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad M3 smd circle (at -3.5 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad M7 smd circle (at -1.5 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad M8 smd circle (at -1 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad M9 smd circle (at -0.5 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad M10 smd circle (at 0 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 129 VCCINT))
    (pad M11 smd circle (at 0.5 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 129 VCCINT))
    (pad M12 smd circle (at 1 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad M13 smd circle (at 1.5 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad M17 smd circle (at 3.5 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad M18 smd circle (at 4 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad M19 smd circle (at 4.5 1 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(U1-PadM19)"))
    (pad N1 smd circle (at -4.5 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 41 JA9))
    (pad N2 smd circle (at -4 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(U1-PadN2)"))
    (pad N3 smd circle (at -3.5 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U1-PadN3)"))
    (pad N7 smd circle (at -1.5 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad N8 smd circle (at -1 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad N9 smd circle (at -0.5 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad N10 smd circle (at 0 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 129 VCCINT))
    (pad N11 smd circle (at 0.5 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 129 VCCINT))
    (pad N12 smd circle (at 1 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad N13 smd circle (at 1.5 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad N17 smd circle (at 3.5 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U1-PadN17)"))
    (pad N18 smd circle (at 4 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U1-PadN18)"))
    (pad N19 smd circle (at 4.5 1.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 99 FC2D_CLK))
    (pad P1 smd circle (at -4.5 2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 28 JA3))
    (pad P2 smd circle (at -4 2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(U1-PadP2)"))
    (pad P3 smd circle (at -3.5 2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(U1-PadP3)"))
    (pad P17 smd circle (at 3.5 2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(U1-PadP17)"))
    (pad P18 smd circle (at 4 2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-PadP18)"))
    (pad P19 smd circle (at 4.5 2 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(U1-PadP19)"))
    (pad R1 smd circle (at -4.5 2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 35 JA8))
    (pad R2 smd circle (at -4 2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad R3 smd circle (at -3.5 2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad R17 smd circle (at 3.5 2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad R18 smd circle (at 4 2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad R19 smd circle (at 4.5 2.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 96 FC_IO))
    (pad T1 smd circle (at -4.5 3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 30 JA2))
    (pad T2 smd circle (at -4 3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U1-PadT2)"))
    (pad T3 smd circle (at -3.5 3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U1-PadT3)"))
    (pad T17 smd circle (at 3.5 3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(U1-PadT17)"))
    (pad T18 smd circle (at 4 3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(U1-PadT18)"))
    (pad T19 smd circle (at 4.5 3 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 115 FC_DIO0_MUX))
    (pad U1 smd circle (at -4.5 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 39 JA7))
    (pad U2 smd circle (at -4 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U1-PadU2)"))
    (pad U3 smd circle (at -3.5 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(U1-PadU3)"))
    (pad U4 smd circle (at -3 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U1-PadU4)"))
    (pad U5 smd circle (at -2.5 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad U6 smd circle (at -2 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U1-PadU6)"))
    (pad U7 smd circle (at -1.5 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U1-PadU7)"))
    (pad U8 smd circle (at -1 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(U1-PadU8)"))
    (pad U9 smd circle (at -0.5 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(U1-PadU9)"))
    (pad U10 smd circle (at 0 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 108 SW_PROGRAM_B))
    (pad U11 smd circle (at 0.5 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 104 SW_DONE))
    (pad U12 smd circle (at 1 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad U13 smd circle (at 1.5 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 202 "/FPGA Programming/MODE_2"))
    (pad U14 smd circle (at 2 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(U1-PadU14)"))
    (pad U15 smd circle (at 2.5 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad U16 smd circle (at 3 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(U1-PadU16)"))
    (pad U17 smd circle (at 3.5 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(U1-PadU17)"))
    (pad U18 smd circle (at 4 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(U1-PadU18)"))
    (pad U19 smd circle (at 4.5 3.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 112 FC_DIO1_MUX))
    (pad V1 smd circle (at -4.5 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 26 JA1))
    (pad V2 smd circle (at -4 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad V3 smd circle (at -3.5 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(U1-PadV3)"))
    (pad V4 smd circle (at -3 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(U1-PadV4)"))
    (pad V5 smd circle (at -2.5 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad V6 smd circle (at -2 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U1-PadV6)"))
    (pad V7 smd circle (at -1.5 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U1-PadV7)"))
    (pad V8 smd circle (at -1 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad V9 smd circle (at -0.5 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(U1-PadV9)"))
    (pad V10 smd circle (at 0 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 223 TDO))
    (pad V11 smd circle (at 0.5 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 127 +3V3))
    (pad V12 smd circle (at 1 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad V13 smd circle (at 1.5 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 224 MODE_0))
    (pad V14 smd circle (at 2 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(U1-PadV14)"))
    (pad V15 smd circle (at 2.5 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad V16 smd circle (at 3 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(U1-PadV16)"))
    (pad V17 smd circle (at 3.5 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(U1-PadV17)"))
    (pad V18 smd circle (at 4 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad V19 smd circle (at 4.5 4 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 113 FC_DIO2_MUX))
    (pad W1 smd circle (at -4.5 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad W2 smd circle (at -4 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(U1-PadW2)"))
    (pad W3 smd circle (at -3.5 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(U1-PadW3)"))
    (pad W4 smd circle (at -3 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(U1-PadW4)"))
    (pad W5 smd circle (at -2.5 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 52 VCORE_CURRENT_GAIN_1))
    (pad W6 smd circle (at -2 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 53 VCORE_CURRENT_GAIN_0))
    (pad W7 smd circle (at -1.5 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(U1-PadW7)"))
    (pad W8 smd circle (at -1 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad W9 smd circle (at -0.5 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 223 TDO))
    (pad W10 smd circle (at 0 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 198 "/FPGA Programming/TMS"))
    (pad W11 smd circle (at 0.5 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 196 "/FPGA Programming/TDI"))
    (pad W12 smd circle (at 1 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 106 SW_INIT_B))
    (pad W13 smd circle (at 1.5 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 190 "/FPGA Programming/MODE_1"))
    (pad W14 smd circle (at 2 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 224 MODE_0))
    (pad W15 smd circle (at 2.5 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(U1-PadW15)"))
    (pad W16 smd circle (at 3 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 110 FD2C_HS))
    (pad W17 smd circle (at 3.5 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 109 FC2D_HS))
    (pad W18 smd circle (at 4 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 114 FC_DIO3_MUX))
    (pad W19 smd circle (at 4.5 4.5 180) (size 0.27 0.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_BGA.3dshapes/Xilinx_CPG238.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3d models/XA7A25T-1CPG238Q.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-10_3x3mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 65.35466 48.95588 180)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U11 (at -3.81 0 90) (layer F.SilkS))
    (fp_text value SP3003-04ATG (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 10 smd rect (at 2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 JA10))
    (pad 9 smd rect (at 2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 JA4))
    (pad 8 smd rect (at 2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 JA9))
    (pad 6 smd rect (at 2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 JA3))
    (pad 5 smd rect (at -2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 JA3))
    (pad 4 smd rect (at -2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 JA9))
    (pad 3 smd rect (at -2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 FC_3V3))
    (pad 2 smd rect (at -2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 JA4))
    (pad 1 smd rect (at -2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 JA10))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-10_3x3mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 65.35466 45.14588 180)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U10 (at -3.81 -0.254 90) (layer F.SilkS))
    (fp_text value SP3003-04ATG (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 10 smd rect (at 2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 JA8))
    (pad 9 smd rect (at 2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 JA2))
    (pad 8 smd rect (at 2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 JA7))
    (pad 6 smd rect (at 2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 JA1))
    (pad 5 smd rect (at -2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 JA1))
    (pad 4 smd rect (at -2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 JA7))
    (pad 3 smd rect (at -2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 FC_3V3))
    (pad 2 smd rect (at -2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 JA2))
    (pad 1 smd rect (at -2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 JA8))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 65.35466 51.74988)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C58 (at 2.794 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 65.35466 42.35188)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C57 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 65.84666 34.98588 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at 2.524 0 90) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 211 /Power/EN2))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 69.40266 34.98588 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -0.016 2.54) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(Q2-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fobos-shield:PinSocket_2x06_P2.54mm_Horizontal_FLipped (layer F.Cu) (tedit 60BFCF20)
    (at 77.54666 48.70188)
    (descr "Through hole angled socket strip, 2x06, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 2x06 2.54mm double row")
    (fp_text reference J2 (at 4.564 -2.532) (layer F.SilkS))
    (fp_text value "Pmod 2x6" (at 0 16.51) (layer F.Fab))
    (fp_text user %R (at 8.315 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 FC_3V3))
    (pad 7 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 FC_3V3))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Horizontal.wrl
      (offset (xyz 0 -12.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module cerg:SMA-JOHNSON-142-0701-801 (layer F.Cu) (tedit 5F1F56CA)
    (at 41.021 -0.82812)
    (fp_text reference J9 (at 6.55366 -1.778) (layer F.SilkS))
    (fp_text value Measure (at 0 -3.6) (layer F.Fab))
    (pad 2 smd rect (at 4.4 0) (size 2.4 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.4 0) (size 2.4 5.08) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.4 0) (size 2.4 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.4 0) (size 2.4 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 2.3 5.08) (layers F.Cu F.Paste F.Mask)
      (net 54 VCORE_CURRENT))
    (model ${KIPRJMOD}/cerg_3d_models/SMA_Board_Edge_Molex_732511150.step
      (offset (xyz 0 2.54 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model ${KIPRJMOD}/cerg_3d_models/SMA_Board_Edge_Molex_732511150.wrl
      (offset (xyz 0 2.54 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module cerg:5281 (layer F.Cu) (tedit 5FF275B6)
    (at 87.19866 37.27188 270)
    (fp_text reference TP7 (at -2.032 0 180) (layer F.SilkS))
    (fp_text value 5281 (at 0 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.6162 2.6162) (drill 1.6002) (layers *.Cu *.Mask)
      (net 127 +3V3))
    (model C:/Users/Maxwell/Downloads/keystone-PN5281.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:5281 (layer F.Cu) (tedit 5FF275B6)
    (at 65.10066 27.36588)
    (fp_text reference TP6 (at 0 -2.032) (layer F.SilkS))
    (fp_text value 5281 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6162 2.6162) (drill 1.6002) (layers *.Cu *.Mask)
      (net 128 +1V8))
    (model C:/Users/Maxwell/Downloads/keystone-PN5281.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:5281 (layer F.Cu) (tedit 5FF275B6)
    (at 87.19866 44.38388 270)
    (fp_text reference TP9 (at 1.786 2.294 180) (layer F.SilkS))
    (fp_text value 5281 (at 0 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.6162 2.6162) (drill 1.6002) (layers *.Cu *.Mask)
      (net 210 /Power/pre3V3))
    (model C:/Users/Maxwell/Downloads/keystone-PN5281.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:5281 (layer F.Cu) (tedit 5FF275B6)
    (at 72.21266 27.36588)
    (fp_text reference TP8 (at 0 -2.032) (layer F.SilkS))
    (fp_text value 5281 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6162 2.6162) (drill 1.6002) (layers *.Cu *.Mask)
      (net 209 /Power/pre1V8))
    (model C:/Users/Maxwell/Downloads/keystone-PN5281.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:Switch_Tactile_THT_6x6mm (layer F.Cu) (tedit 6006874C)
    (at 14.04666 54.10788)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1825910&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference S3 (at 2.944 6.604) (layer F.SilkS))
    (fp_text value 1825910-6 (at 3.6322 7.0866) (layer F.Fab))
    (fp_text user %R (at 3.3782 2.286) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 4.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 188 "Net-(S3-Pad3)"))
    (pad 4 thru_hole circle (at 6.5 4.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 6.5 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 108 SW_PROGRAM_B))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 189 "Net-(S3-Pad1)"))
    (model "${KIPRJMOD}/3d models/ENG_CVM_CVM_1825910-6_C.3d_stp/c-1825910-6-c-3d.stp"
      (offset (xyz 3.2512 -2.2352 5.105400000000001))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module cerg:Switch_Tactile_THT_6x6mm (layer F.Cu) (tedit 6006874C)
    (at 14.15066 64.95788)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1825910&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference S2 (at 2.436 6.858) (layer F.SilkS))
    (fp_text value 1825910-6 (at 3.6322 7.0866) (layer F.Fab))
    (fp_text user %R (at 3.3782 2.286) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 4.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 185 "Net-(R73-Pad2)"))
    (pad 4 thru_hole circle (at 6.5 4.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 186 "Net-(S2-Pad4)"))
    (pad 2 thru_hole circle (at 6.5 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 187 "Net-(S2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 93 FC_3V3))
    (model "${KIPRJMOD}/3d models/ENG_CVM_CVM_1825910-6_C.3d_stp/c-1825910-6-c-3d.stp"
      (offset (xyz 3.2512 -2.2352 5.105400000000001))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 30.988 44.70088 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R78 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 204 "/FPGA 1/PUDC"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 30.988 41.58988 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R77 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 204 "/FPGA 1/PUDC"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 87.19866 40.82788 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R76 (at -1.913 -1.786 90) (layer F.SilkS))
    (fp_text value 0.1R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 127 +3V3))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 210 /Power/pre3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 68.67266 27.36588 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R75 (at 0 1.524) (layer F.SilkS))
    (fp_text value 0.1R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 128 +1V8))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 209 /Power/pre1V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 11.76066 65.21188 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R74 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 FC_RST))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 185 "Net-(R73-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 11.76066 69.02188 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R73 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 185 "Net-(R73-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 26.23066 30.73088 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R55 (at -0.072 -1.397 90) (layer F.SilkS))
    (fp_text value 4.7KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 SW_INIT_B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 28.77866 49.46388 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R53 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 200R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 SW_DONE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5F68FEF0)
    (at 56.69316 16.44388)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 0.0255 1.27) (layer F.SilkS))
    (fp_text value 1k/500mA (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C5-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 50.10666 29.09238 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C56 (at 4.7665 0.889 90) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 129 VCCINT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 54.42466 28.49038 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C55 (at 4.1645 1.524 90) (layer B.SilkS))
    (fp_text value 47uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 129 VCCINT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 54.87316 38.29588)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C53 (at 2.9805 0.254) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 54.93266 33.59688)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C52 (at 3.04 -0.246) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 54.87316 37.27988)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C51 (at 2.9805 0) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 54.87316 35.24788)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C50 (at 3.04 -0.508) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 54.93266 32.58088)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C49 (at 3.04 -0.5) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 54.87316 36.26388)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C48 (at 3.04 -0.254) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 47.59316 27.75488 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C47 (at 3.0745 0) (layer B.SilkS))
    (fp_text value 47uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 129 VCCINT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 51.12266 29.09238 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C46 (at 4.7665 1.143 90) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 129 VCCINT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 55.69466 40.26838 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C45 (at -2.5995 0 90) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 128 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 52.13866 29.09238 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C44 (at 4.7665 1.397 90) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 129 VCCINT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 54.67866 40.26838 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C43 (at -2.5995 -0.254 90) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 128 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 47.56266 38.61338)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C42 (at -0.008 2.4765) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 129 VCCINT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 53.15466 29.09238 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C41 (at 4.7665 1.524 90) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 129 VCCINT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 56.71066 40.26838 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C40 (at -2.5995 0.254 90) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 128 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 60.52066 40.07388)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C39 (at 0 1.778) (layer B.SilkS))
    (fp_text value 47uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 128 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 48.70966 24.41438 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C38 (at -0.0385 -3.048 90) (layer B.SilkS))
    (fp_text value 100uF (at 0 -2.3 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.5625 0 90) (size 1.325 2.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5625 0 90) (size 1.325 2.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.188679)
      (net 129 VCCINT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 51.38466 45.14588 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C37 (at 3.564 0.008 270) (layer B.SilkS))
    (fp_text value 47uF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 48.33666 45.14588 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C36 (at 3.564 0.008 90) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 38.93866 36.13688 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C35 (at 3.818 0.246) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 42.74866 45.14588 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C34 (at 3.564 0.516 90) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 38.93866 37.15288 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C33 (at 3.818 -0.262) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 38.93066 38.16888 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C32 (at 3.818 -0.77) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 46.81266 45.14588 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C31 (at 3.564 0.008 90) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 49.86066 45.14588 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C30 (at 3.564 0.008 90) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 38.93066 39.18488 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C29 (at 3.818 -1.278) (layer B.SilkS))
    (fp_text value .47uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 45.28866 45.14588 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C28 (at 3.564 0.008 90) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 38.93066 40.20088 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C27 (at 3.818 -1.786) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 44.01866 45.14588 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C26 (at 3.564 0.262 90) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.16 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer B.Cu) (tedit 5F6BB22C)
    (at 38.93866 41.21688 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C25 (at 3.818 -2.294) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.16) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 41.98666 17.71388 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 5.08 270) (layer F.SilkS))
    (fp_text value Shunt1R (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 129 VCCINT))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x10_P2.54mm_Horizontal (layer F.Cu) (tedit 5EAC9A08)
    (at 5.588 52.25788 180)
    (descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole horizontal IDC box header THT 2x10 2.54mm double row")
    (fp_text reference J1 (at -2.29066 -2.28388) (layer F.SilkS))
    (fp_text value Target (at 6.215 28.96) (layer F.Fab))
    (fp_text user %R (at 8.83 11.43 90) (layer F.Fab))
    (pad 20 thru_hole circle (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 FC_5V))
    (pad 18 thru_hole circle (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 FC_3V3))
    (pad 16 thru_hole circle (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/Connectors, IO/CW_TARG4"))
    (pad 14 thru_hole circle (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/Connectors, IO/CW_TARG3"))
    (pad 12 thru_hole circle (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/Connectors, IO/CW_TARG2"))
    (pad 10 thru_hole circle (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/Connectors, IO/CW_TARG1"))
    (pad 8 thru_hole circle (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 FC_3V3))
    (pad 6 thru_hole circle (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/Connectors, IO/CW_HS2"))
    (pad 4 thru_hole circle (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/Connectors, IO/CW_HS1"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole circle (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/Connectors, IO/CW_PDID"))
    (pad 13 thru_hole circle (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/Connectors, IO/CW_PDIC"))
    (pad 11 thru_hole circle (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/Connectors, IO/CW_SCK"))
    (pad 9 thru_hole circle (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/Connectors, IO/CW_MOSI"))
    (pad 7 thru_hole circle (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/Connectors, IO/CW_MISO"))
    (pad 5 thru_hole circle (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "/Connectors, IO/CW_RST"))
    (pad 3 thru_hole circle (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 FC_3V3))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 94 FC_5V))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:DS04-254-2-03BK-SMT (layer F.Cu) (tedit 5FE90085)
    (at 16.58866 13.06988 180)
    (fp_text reference SW2 (at 4.318 6.31 180) (layer F.SilkS))
    (fp_text value SW_DIP_x03 (at 5 2.5) (layer F.Fab))
    (pad 6 smd rect (at 8.9 5 270) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 93 FC_3V3))
    (pad 5 smd rect (at 0 5 270) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 53 VCORE_CURRENT_GAIN_0))
    (pad 4 smd rect (at 8.9 2.5 270) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 93 FC_3V3))
    (pad 3 smd rect (at 0 2.5 270) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 52 VCORE_CURRENT_GAIN_1))
    (pad 2 smd rect (at 8.9 0 90) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(SW2-Pad2)"))
    (pad 1 smd rect (at 0 0 90) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(SW2-Pad1)"))
    (model ${KIPRJMOD}/cerg_3d_models/CUI_DEVICES_DS04-254-2-03BK-SMT-TR.step
      (offset (xyz -4.4958 -6.5278 0.9906))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 58.98866 55.81388 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q7 (at 0.016 2.54 180) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(Q7-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 136 USER_LED_3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-10_3x3mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 18.61866 35.74788 180)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U2 (at -2.54 -2.54) (layer F.SilkS))
    (fp_text value SP3003-04ATG (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 10 smd rect (at 2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 102 FC_DIO2))
    (pad 9 smd rect (at 2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 FD2C_HS))
    (pad 8 smd rect (at 2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 103 FC_DIO3))
    (pad 6 smd rect (at 2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 FC_PROG))
    (pad 5 smd rect (at -2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 FC_PROG))
    (pad 4 smd rect (at -2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 103 FC_DIO3))
    (pad 3 smd rect (at -2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 FC_3V3))
    (pad 2 smd rect (at -2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 FD2C_HS))
    (pad 1 smd rect (at -2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 102 FC_DIO2))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-10_3x3mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 18.61866 47.93988 180)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U4 (at -2.54 -2.54) (layer F.SilkS))
    (fp_text value SP3003-04ATG (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0.14 -0.01) (layer F.Fab))
    (pad 10 smd rect (at 2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 98 FD2C_CLK))
    (pad 9 smd rect (at 2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 95 FC_RST))
    (pad 8 smd rect (at 2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 99 FC2D_CLK))
    (pad 6 smd rect (at 2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 96 FC_IO))
    (pad 5 smd rect (at -2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 96 FC_IO))
    (pad 4 smd rect (at -2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 99 FC2D_CLK))
    (pad 3 smd rect (at -2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 FC_3V3))
    (pad 2 smd rect (at -2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 95 FC_RST))
    (pad 1 smd rect (at -2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 98 FD2C_CLK))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:SSOP-16_4.0x5.0mm_P0.635mm (layer F.Cu) (tedit 6028A075)
    (at 27.92266 35.43038)
    (descr "SSOP16: plastic shrink small outline package; 16 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot519-1_po.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U7 (at 0.094 3.6195) (layer F.SilkS))
    (fp_text value TS3A5018DBQR (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -2.2225) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 111 FC_PROG))
    (pad 2 smd rect (at -2.7 -1.5875) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 114 FC_DIO3_MUX))
    (pad 3 smd rect (at -2.7 -0.9525) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 106 SW_INIT_B))
    (pad 4 smd rect (at -2.7 -0.3175) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 103 FC_DIO3))
    (pad 5 smd rect (at -2.7 0.3175) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 113 FC_DIO2_MUX))
    (pad 6 smd rect (at -2.7 0.9525) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 108 SW_PROGRAM_B))
    (pad 7 smd rect (at -2.7 1.5875) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 102 FC_DIO2))
    (pad 8 smd rect (at -2.7 2.2225) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.7 2.2225) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 100 FC_DIO0))
    (pad 10 smd rect (at 2.7 1.5875) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 107 SW_CLK))
    (pad 11 smd rect (at 2.7 0.9525) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 115 FC_DIO0_MUX))
    (pad 12 smd rect (at 2.7 0.3175) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 101 FC_DIO1))
    (pad 13 smd rect (at 2.7 -0.3175) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 105 SW_DIN))
    (pad 14 smd rect (at 2.7 -0.9525) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 112 FC_DIO1_MUX))
    (pad 15 smd rect (at 2.7 -1.5875) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 2.7 -2.2225) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 93 FC_3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-16_3.9x4.9mm_P0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/cerg_3d_models/User Library-SSOP16.step"
      (offset (xyz 0 0 0.6))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 25.78566 26.10388 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R32 (at -3.62 0 180) (layer F.SilkS))
    (fp_text value 4.7KR (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 190 "/FPGA Programming/MODE_1"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 25.78566 24.32588 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R31 (at -3.747 0 180) (layer F.SilkS))
    (fp_text value 4.7KR (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 224 MODE_0))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 25.78566 27.88188 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R33 (at -3.62 0 180) (layer F.SilkS))
    (fp_text value 4.7KR (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 202 "/FPGA Programming/MODE_2"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:BarrelJack_CUI_PJ-102AH_Horizontal (layer F.Cu) (tedit 5F1F5C2A)
    (at 75.26066 10.34788 180)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J10 (at 6.35 -0.254) (layer F.SilkS))
    (fp_text value Barrel_Jack_Switch (at -5.5 6.2 90) (layer F.Fab))
    (fp_text user %R (at 0 6.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 94 FC_5V))
    (pad 2 thru_hole circle (at 0 6 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 4.7 3 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 142 "Net-(J10-Pad3)"))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-102AH_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/cerg_3d_models/CUI_PJ-102AH.step
      (offset (xyz 0 -13.6 6))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Fuse:Fuse_1206_3216Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 62.05266 17.72188 90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags fuse)
    (attr smd)
    (fp_text reference F1 (at -3.302 0.119) (layer F.SilkS))
    (fp_text value MF-MSMF050-2 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(F1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:Switch_Tactile_THT_6x6mm (layer F.Cu) (tedit 6006874C)
    (at 60.02066 64.90288)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1825910&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference S5 (at 3.302 6.604) (layer F.SilkS))
    (fp_text value 1825910-6 (at 3.6322 7.0866) (layer F.Fab))
    (fp_text user %R (at 3.3782 2.286) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 4.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 122 "Net-(R65-Pad2)"))
    (pad 4 thru_hole circle (at 6.5 4.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 125 "Net-(S5-Pad4)"))
    (pad 2 thru_hole circle (at 6.5 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 126 "Net-(S5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 93 FC_3V3))
    (model "${KIPRJMOD}/3d models/ENG_CVM_CVM_1825910-6_C.3d_stp/c-1825910-6-c-3d.stp"
      (offset (xyz 3.2512 -2.2352 5.105400000000001))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module cerg:Switch_Tactile_THT_6x6mm (layer F.Cu) (tedit 6006874C)
    (at 47.32066 64.90288)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1825910&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference S4 (at 3.302 6.604) (layer F.SilkS))
    (fp_text value 1825910-6 (at 3.6322 7.0866) (layer F.Fab))
    (fp_text user %R (at 3.3782 2.286) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 4.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 121 "Net-(R63-Pad2)"))
    (pad 4 thru_hole circle (at 6.5 4.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 123 "Net-(S4-Pad4)"))
    (pad 2 thru_hole circle (at 6.5 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 124 "Net-(S4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 93 FC_3V3))
    (model "${KIPRJMOD}/3d models/ENG_CVM_CVM_1825910-6_C.3d_stp/c-1825910-6-c-3d.stp"
      (offset (xyz 3.2512 -2.2352 5.105400000000001))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 24.96866 50.22588 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D6 (at 0 1.524) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 84.42066 22.28588)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -0.016 2.54) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(Q3-Pad3)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 PGOOD))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 66.39616 60.38588)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D5 (at -2.54 -0.00212) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 195 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 60.30016 60.38588)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D4 (at -2.5655 -0.00212) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 194 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 53.67066 60.38588)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D3 (at -2.54 0) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 193 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 47.57466 60.38588)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D2 (at -2.54 0) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 192 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 84.65866 19.49188 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D1 (at 2.032 0 90) (layer F.SilkS))
    (fp_text value LG_L29K-G2J1-24-Z (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 191 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 8.96666 61.14788 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP4 (at 0 4.826 180) (layer F.SilkS))
    (fp_text value FC3V3_3V3_SHUNT (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 127 +3V3))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 FC_3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 27.25466 49.46388 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R72 (at 2.794 0 90) (layer F.SilkS))
    (fp_text value 200R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 SW_DONE))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:DS04-254-2-03BK-SMT (layer F.Cu) (tedit 5FE90085)
    (at 13.78466 24.40588)
    (fp_text reference SW1 (at -1.016 -1.604 -180) (layer F.SilkS))
    (fp_text value SW_DIP_x03 (at 5 2.5) (layer F.Fab))
    (pad 6 smd rect (at 8.9 5 90) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 202 "/FPGA Programming/MODE_2"))
    (pad 5 smd rect (at 0 5 90) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 8.9 2.5 90) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 190 "/FPGA Programming/MODE_1"))
    (pad 3 smd rect (at 0 2.5 90) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 8.9 0 270) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 224 MODE_0))
    (pad 1 smd rect (at 0 0 270) (size 1.1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/cerg_3d_models/CUI_DEVICES_DS04-254-2-03BK-SMT-TR.step
      (offset (xyz -4.50088 -6.499860000000001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.922 45.65388)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.581129 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 FC_IO))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "/Connectors, IO/CW_MISO"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5EA53D3B)
    (at 58.42466 8.88788)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (fp_text reference J5 (at -2.794 2.54) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.27 4.08) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 131 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 65.08466 55.81388 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 2.54) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(Q6-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 135 USER_LED_4))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 52.40066 55.74788 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 2.474 180) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(Q5-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 134 USER_LED_2))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 46.28866 55.81388 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -0.27 2.54) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(Q4-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 133 USER_LED_1))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 34.86666 8.89488 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R71 (at 0.063 1.397 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 VCORE_CURRENT_GAIN_1))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 36.64466 8.13388 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R70 (at -1.334 -1.651 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 VCORE_CURRENT_GAIN_0))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 64.78366 58.60788 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R69 (at -2.985 0.00212) (layer F.SilkS))
    (fp_text value 470R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 120 "Net-(Q6-Pad3)"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 195 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 67.89466 55.75088 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R68 (at -2.477 0.00212 180) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 135 USER_LED_4))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 24.384 42.35188)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R67 (at 0.06866 -1.516) (layer F.SilkS))
    (fp_text value 0R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 SW_DONE))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 FD_TF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 39.116 63.17988 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 0R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 203 "/FPGA Programming/CCLK"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 SW_CLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 57.73466 65.27488 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R66 (at 0.00466 -1.524 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 USER_BTN_2))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 "Net-(R65-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 57.73466 69.21288 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R65 (at 0.00466 -1.524 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 "Net-(R65-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 45.03466 65.27488 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R64 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 137 USER_BTN_1))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 121 "Net-(R63-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 45.03466 69.21288 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R63 (at -0.00466 -1.524 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 121 "Net-(R63-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 61.79866 55.81388 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R62 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 136 USER_LED_3))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 55.19466 55.81388 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R61 (at -2.54 0.00212 180) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 USER_LED_2))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 49.09866 55.87688 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R60 (at -2.603 0 180) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 USER_LED_1))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:MH_4-40 (layer F.Cu) (tedit 600FA2BD)
    (at 83.89666 1.45788)
    (fp_text reference H4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.604 6.604) (drill 3.048) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/3d models/91772A106_18-8 SS PAN HEAD PHILLIPS MACHINE SCREW.STEP"
      (offset (xyz 0 0 -6.3246))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3d models/91780A537_ALUM FEM THRDED HEX STANDOFF.STEP"
      (offset (xyz 0 0 -14.4272))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:MH_4-40 (layer F.Cu) (tedit 600FA2BD)
    (at 83.89666 67.49788)
    (fp_text reference H3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.604 6.604) (drill 3.048) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/3d models/91772A106_18-8 SS PAN HEAD PHILLIPS MACHINE SCREW.STEP"
      (offset (xyz 0 0 -6.3246))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3d models/91780A537_ALUM FEM THRDED HEX STANDOFF.STEP"
      (offset (xyz 0 0 -14.4272))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:MH_4-40 (layer F.Cu) (tedit 600FA2BD)
    (at 5.15666 1.45788)
    (fp_text reference H2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.604 6.604) (drill 3.048) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/3d models/91772A106_18-8 SS PAN HEAD PHILLIPS MACHINE SCREW.STEP"
      (offset (xyz 0 0 -6.3246))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3d models/91780A537_ALUM FEM THRDED HEX STANDOFF.STEP"
      (offset (xyz 0 0 -14.4272))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:MH_4-40 (layer F.Cu) (tedit 600FA2BD)
    (at 5.08 67.49788)
    (fp_text reference H1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.604 6.604) (drill 3.048) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/3d models/91772A106_18-8 SS PAN HEAD PHILLIPS MACHINE SCREW.STEP"
      (offset (xyz 0 0 -6.3246))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3d models/91780A537_ALUM FEM THRDED HEX STANDOFF.STEP"
      (offset (xyz 0 0 -14.4272))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:L_SRN2012 (layer F.Cu) (tedit 600F969C)
    (at 78.37266 42.42388)
    (fp_text reference L5 (at 0.762 2.032) (layer F.SilkS))
    (fp_text value 2.2uH (at 0 -0.5) (layer F.Fab))
    (pad 2 smd rect (at 1.5748 0) (size 0.7874 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 210 /Power/pre3V3))
    (pad 1 smd rect (at 0 0) (size 0.7874 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 219 /Power/SW3))
    (model "${KIPRJMOD}/3d models/SRN2012 series.stp"
      (offset (xyz -0.4572 -0.9906 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:L_BRC2012 (layer F.Cu) (tedit 600F98B9)
    (at 77.29266 29.90588 180)
    (fp_text reference L4 (at 0.254 1.90288) (layer F.SilkS))
    (fp_text value 3.3uH (at 0 -0.5) (layer F.Fab))
    (pad 2 smd rect (at 1.6 0 180) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 209 /Power/pre1V8))
    (pad 1 smd rect (at 0 0 180) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 218 /Power/SW2))
    (model "${KIPRJMOD}/3d models/BRC2012T3R3MD.STEP"
      (offset (xyz 0.79 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:L_SRN2012 (layer F.Cu) (tedit 600F969C)
    (at 80.78778 32.06534 90)
    (fp_text reference L3 (at 0.88146 -1.85212 90) (layer F.SilkS))
    (fp_text value 1.5uH (at 0 -0.5 90) (layer F.Fab))
    (pad 2 smd rect (at 1.5748 0 90) (size 0.7874 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 24 +1V0))
    (pad 1 smd rect (at 0 0 90) (size 0.7874 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 217 /Power/SW1))
    (model "${KIPRJMOD}/3d models/SRN2012 series.stp"
      (offset (xyz -0.4572 -0.9906 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 58.68766 58.60788 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R59 (at -2.985 0.00212) (layer F.SilkS))
    (fp_text value 470R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 "Net-(Q7-Pad3)"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 194 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 52.08366 58.60788 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R58 (at -2.985 0) (layer F.SilkS))
    (fp_text value 470R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 "Net-(Q5-Pad3)"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 193 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 45.98766 58.60788 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R57 (at -2.985 0) (layer F.SilkS))
    (fp_text value 470R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 118 "Net-(Q4-Pad3)"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 192 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:575-8 (layer F.Cu) (tedit 600E533B)
    (at 53.85266 1.52188)
    (fp_text reference J8 (at 4.318 -4.064) (layer F.SilkS))
    (fp_text value 575-8 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 9.144 9.144) (drill 5.334) (layers *.Cu *.Mask)
      (net 131 "Net-(J5-Pad1)"))
    (model "${KIPRJMOD}/3d models/keystone-PN575-8.STEP"
      (offset (xyz 0 0 -8.864599999999998))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:575-8 (layer F.Cu) (tedit 600E533B)
    (at 65.53666 1.524)
    (fp_text reference J3 (at 4.064 -4.06612) (layer F.SilkS))
    (fp_text value 575-8 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 9.144 9.144) (drill 5.334) (layers *.Cu *.Mask)
      (net 1 GND))
    (model "${KIPRJMOD}/3d models/keystone-PN575-8.STEP"
      (offset (xyz 0 0 -8.864599999999998))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 39.116 66.48188 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R56 (at -0.063 -1.524 90) (layer F.SilkS))
    (fp_text value 33R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 117 "Net-(R56-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 SW_CLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 28.26266 30.73088 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R54 (at 0.063 1.524 90) (layer F.SilkS))
    (fp_text value 4.7KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 SW_PROGRAM_B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 36.39866 54.79788 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R52 (at 0.127 1.524) (layer F.SilkS))
    (fp_text value 4.7KR (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 116 "Net-(R52-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 30.30266 54.03588)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 0.127 -1.397) (layer F.SilkS))
    (fp_text value 4.7KR (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 199 "/FPGA 1/FCS"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 23.19066 32.38288 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R51 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 FC_PROG))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 31.18366 30.73088 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C54 (at 3.035 0.254 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 49.60666 17.71388 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at -2.54 1.27) (layer F.SilkS))
    (fp_text value CurProbe (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(JP2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cerg:5281 (layer F.Cu) (tedit 5FF275B6)
    (at 74.24466 45.14588)
    (fp_text reference TP1 (at 2.794 -0.5) (layer F.SilkS))
    (fp_text value 5281 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6162 2.6162) (drill 1.6002) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model C:/Users/Maxwell/Downloads/keystone-PN5281.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:5281 (layer F.Cu) (tedit 5FF275B6)
    (at 65.10066 23.04788)
    (fp_text reference TP5 (at -2.032 0 90) (layer F.SilkS))
    (fp_text value 5281 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6162 2.6162) (drill 1.6002) (layers *.Cu *.Mask)
      (net 24 +1V0))
    (model C:/Users/Maxwell/Downloads/keystone-PN5281.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:5281 (layer F.Cu) (tedit 5FF275B6)
    (at 8.96666 21.77788)
    (fp_text reference TP4 (at -0.0715 -2.405) (layer F.SilkS))
    (fp_text value 5281 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6162 2.6162) (drill 1.6002) (layers *.Cu *.Mask)
      (net 1 GND))
    (model C:/Users/Maxwell/Downloads/keystone-PN5281.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:5281 (layer F.Cu) (tedit 5FF275B6)
    (at 8.96666 27.61988)
    (fp_text reference TP3 (at 0.0555 -2.278) (layer F.SilkS))
    (fp_text value 5281 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6162 2.6162) (drill 1.6002) (layers *.Cu *.Mask)
      (net 94 FC_5V))
    (model C:/Users/Maxwell/Downloads/keystone-PN5281.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module cerg:5281 (layer F.Cu) (tedit 5FF275B6)
    (at 8.96666 30.92188)
    (fp_text reference TP2 (at 2.9765 0.389) (layer F.SilkS))
    (fp_text value 5281 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6162 2.6162) (drill 1.6002) (layers *.Cu *.Mask)
      (net 93 FC_3V3))
    (model C:/Users/Maxwell/Downloads/keystone-PN5281.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 32.58866 61.90988 270)
    (descr "SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U9 (at -4.818 -6.596 180) (layer F.SilkS))
    (fp_text value IS25LP256D-JMLE (at 0 6.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd roundrect (at 4.65 -4.445 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 117 "Net-(R56-Pad2)"))
    (pad 15 smd roundrect (at 4.65 -3.175 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(R27-Pad2)"))
    (pad 14 smd roundrect (at 4.65 -1.905 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(U9-Pad14)"))
    (pad 13 smd roundrect (at 4.65 -0.635 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(U9-Pad13)"))
    (pad 12 smd roundrect (at 4.65 0.635 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(U9-Pad12)"))
    (pad 11 smd roundrect (at 4.65 1.905 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(U9-Pad11)"))
    (pad 10 smd roundrect (at 4.65 3.175 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at 4.65 4.445 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(R25-Pad1)"))
    (pad 8 smd roundrect (at -4.65 4.445 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(R28-Pad2)"))
    (pad 7 smd roundrect (at -4.65 3.175 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 199 "/FPGA 1/FCS"))
    (pad 6 smd roundrect (at -4.65 1.905 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(U9-Pad6)"))
    (pad 5 smd roundrect (at -4.65 0.635 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(U9-Pad5)"))
    (pad 4 smd roundrect (at -4.65 -0.635 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(U9-Pad4)"))
    (pad 3 smd roundrect (at -4.65 -1.905 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(U9-Pad3)"))
    (pad 2 smd roundrect (at -4.65 -3.175 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (pad 1 smd roundrect (at -4.65 -4.445 270) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 116 "Net-(R52-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 45.03466 10.08088 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 86.94466 22.09488 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R50 (at 2.993 0.008 90) (layer F.SilkS))
    (fp_text value 800R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(Q3-Pad3)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 191 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 81.86466 22.09488 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R49 (at 0.191 1.27 90) (layer F.SilkS))
    (fp_text value 100KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 PGOOD))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 84.72266 38.10588 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R48 (at 2.476 -0.055) (layer F.SilkS))
    (fp_text value 57.6KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 216 /Power/FB3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 71.19666 30.66788 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R47 (at 0.508 -4.064 90) (layer F.SilkS))
    (fp_text value 120KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 215 /Power/FB2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 86.50066 31.25254 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R46 (at 3.05266 -0.064 90) (layer F.SilkS))
    (fp_text value 120KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 214 /Power/FB1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.23666 38.10588 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R45 (at 2.476 1.38 180) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 210 /Power/pre3V3))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 216 /Power/FB3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 72.72066 30.66788 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R44 (at 0.508 -4.318 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 209 /Power/pre1V8))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 215 /Power/FB2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 82.94466 31.24788 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R43 (at 3.048 0.19 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +1V0))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 214 /Power/FB1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 87.96066 18.28488 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R42 (at -3.628 0.373 270) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(R42-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 81.10266 18.22188 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R41 (at -0.246 1.532 270) (layer F.SilkS))
    (fp_text value 4.7KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(R41-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 65.67166 37.52588)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R40 (at 0 1.524) (layer F.SilkS))
    (fp_text value 100KR (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 211 /Power/EN2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 69.22766 37.52588 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R39 (at 0.063 -1.524) (layer F.SilkS))
    (fp_text value 100KR (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 207 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 64.91866 32.12788)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R38 (at -2.104 0.318 90) (layer F.SilkS))
    (fp_text value 100KR (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 213 /Power/MODE))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 64.91866 30.34988 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R37 (at 2.104 0.952 90) (layer F.SilkS))
    (fp_text value 0R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 213 /Power/MODE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 71.95866 35.30288 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R36 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value 1KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 208 "Net-(Q2-Pad1)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +1V0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 71.38766 42.35188)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R35 (at -2.985 0) (layer F.SilkS))
    (fp_text value 10KR (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 212 /Power/EN3))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 71.38766 40.82788 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R34 (at 2.985 0) (layer F.SilkS))
    (fp_text value 3.48KR (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 +1V8))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 212 /Power/EN3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 82.81766 42.42388)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 2.032) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 210 /Power/pre3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 75.00666 26.92388 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0.828 2.54 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 209 /Power/pre1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 81.35666 27.68588 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 2.352 0 180) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +1V0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 81.04178 38.11054 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 3.05266 -0.07412 90) (layer F.SilkS))
    (fp_text value 20pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 216 /Power/FB3))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 210 /Power/pre3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.24466 30.65488 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at -0.495 4.572 90) (layer F.SilkS))
    (fp_text value 20pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 215 /Power/FB2))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 209 /Power/pre1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 84.72266 31.24788 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at -3.048 0 90) (layer F.SilkS))
    (fp_text value 20pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 214 /Power/FB1))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +1V0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 83.48666 35.59788)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at -0.106 -2.001) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 5A02FF57)
    (at 19.88066 16.84788)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference U6 (at -2.794 -1.158) (layer F.SilkS))
    (fp_text value BGA2801 (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 0 -270) (layer F.Fab))
    (pad 6 smd rect (at 0.95 -0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 4 smd rect (at 0.95 0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.95 0) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.95 0) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.95 0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at -0.95 -0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-8_3x3mm_P0.65mm (layer F.Cu) (tedit 5E509FDD)
    (at 40.71666 10.09388 180)
    (descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (attr smd)
    (fp_text reference U5 (at -2.54 -2.54) (layer F.SilkS))
    (fp_text value INA225 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.1125 -0.975 180) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 VCCINT))
    (pad 7 smd roundrect (at 2.1125 -0.325 180) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 2.1125 0.325 180) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 VCORE_CURRENT_GAIN_1))
    (pad 5 smd roundrect (at 2.1125 0.975 180) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 VCORE_CURRENT_GAIN_0))
    (pad 4 smd roundrect (at -2.1125 0.975 180) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 VCORE_CURRENT))
    (pad 3 smd roundrect (at -2.1125 0.325 180) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 2 smd roundrect (at -2.1125 -0.325 180) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.1125 -0.975 180) (size 1.625 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-10_3x3mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 18.61866 41.84388 180)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U3 (at -2.54 -2.54) (layer F.SilkS))
    (fp_text value SP3003-04ATG (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 10 smd rect (at 2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 100 FC_DIO0))
    (pad 9 smd rect (at 2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 97 FD_TF))
    (pad 8 smd rect (at 2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 101 FC_DIO1))
    (pad 6 smd rect (at 2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 109 FC2D_HS))
    (pad 5 smd rect (at -2.2 1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 109 FC2D_HS))
    (pad 4 smd rect (at -2.2 0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 101 FC_DIO1))
    (pad 3 smd rect (at -2.2 0 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 FC_3V3))
    (pad 2 smd rect (at -2.2 -0.5 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 97 FD_TF))
    (pad 1 smd rect (at -2.2 -1 180) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 100 FC_DIO0))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 26.23866 55.55988 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at 0.19 1.524 270) (layer F.SilkS))
    (fp_text value 0R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 201 "/FPGA 1/DIN"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 SW_DIN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 26.23866 58.86188 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at -0.064 1.524 90) (layer F.SilkS))
    (fp_text value 33R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(R28-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 201 "/FPGA 1/DIN"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 39.116 59.87788 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 0.064 -1.651 90) (layer F.SilkS))
    (fp_text value 33R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(R27-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 200 "/FPGA 1/MOSI"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 25.98466 66.22788 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 4.7KR (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(R25-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 26.29466 16.19788)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0 1.524) (layer F.SilkS))
    (fp_text value 49R9 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 VCCINT))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 40.71666 14.66588)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 0R1 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 25 "Net-(JP2-Pad2)"))
    (pad 1 smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 129 VCCINT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 69.67266 19.42888 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0.063 -1.524 90) (layer F.SilkS))
    (fp_text value 100R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 69.67266 16.12688 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0.063 1.524 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.18166 55.55988)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -2.97134 -0.06612) (layer F.SilkS))
    (fp_text value 200R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(J2-Pad9)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 JA9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.18166 49.46388)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -2.97134 -0.06612) (layer F.SilkS))
    (fp_text value 200R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(J2-Pad7)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 JA7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.93566 34.98588 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -3.04366 -0.008) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "/Connectors, IO/CW_TARG4"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 FC_DIO3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.93566 38.03388 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at -3.04366 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "/Connectors, IO/CW_TARG3"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 FC_DIO2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.92666 41.08188 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at -3.05266 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "/Connectors, IO/CW_TARG2"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 FC_DIO1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.92666 44.12988 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -3.05266 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "/Connectors, IO/CW_TARG1"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 FC_DIO0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.92666 47.17788 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -3.05266 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "/Connectors, IO/CW_HS2"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 FC2D_CLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.92666 50.22588 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -3.05266 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "/Connectors, IO/CW_HS1"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 FD2C_CLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.18166 58.60788)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -2.97134 -0.06612) (layer F.SilkS))
    (fp_text value 200R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(J2-Pad10)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 JA10))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.18166 52.51188)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -2.97134 -0.06612) (layer F.SilkS))
    (fp_text value 200R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(J2-Pad8)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 JA8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.18166 57.08388 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 2.985 0.00212) (layer F.SilkS))
    (fp_text value 200R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 JA4))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.18166 50.98788 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.477 0) (layer F.SilkS))
    (fp_text value 200R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 JA2))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.18166 54.03588 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 2.477 0) (layer F.SilkS))
    (fp_text value 200R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 JA3))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.18166 47.93988 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 2.477 0.00212) (layer F.SilkS))
    (fp_text value 200R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 JA1))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.93566 33.46188)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 2.567469 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 FC_PROG))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "/Connectors, IO/CW_PDID"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.93566 36.50988)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 2.567469 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 FD2C_HS))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "/Connectors, IO/CW_PDIC"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.92666 39.55788)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 2.576469 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 FC2D_HS))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "/Connectors, IO/CW_SCK"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.92666 42.60588)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.576469 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 FD_TF))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "/Connectors, IO/CW_MOSI"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 10.92666 48.70188)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.576469 -0.00212) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 FC_RST))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "/Connectors, IO/CW_RST"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 73.35566 20.69688 270)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference Q1 (at -2.983 -3.429 270) (layer F.SilkS))
    (fp_text value FDS9435A (at 0 3.4 270) (layer F.Fab))
    (fp_text user %R (at 0.169998 -0.059001 270) (layer B.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (pad 7 smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (pad 6 smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (pad 5 smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (pad 4 smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C4-Pad2)"))
    (pad 3 smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 FC_5V))
    (pad 2 smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 FC_5V))
    (pad 1 smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 FC_5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5F68FEF0)
    (at 19.85516 9.33988 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at -0.0255 1.524) (layer F.SilkS))
    (fp_text value 1k/500mA (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C12-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 65.10066 17.71388 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.794) (layer F.SilkS))
    (fp_text value Source (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 +1V0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 25.98466 62.41788 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0.013 1.651 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 19.88066 11.11788)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 3.236 0 180) (layer F.SilkS))
    (fp_text value 2u2 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 16.57866 17.46788)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0.267 1.524) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C14-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 19.88066 12.89588)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 3.035 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C12-Pad1)"))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 19.88066 14.41988)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 3.048 0) (layer F.SilkS))
    (fp_text value 4n7 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 23.16966 16.19788)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 1.524) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C11-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 77.29266 20.94988 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 1.778 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 53.16266 19.98688 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -3.035 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 69.67266 22.78088 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.013 -1.524 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C8-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 55.19466 19.81188 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.86 0.762 90) (layer F.SilkS))
    (fp_text value 47uF6.3V (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 57.98866 19.81188 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.86 -1.016 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 60.02066 20.01288 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -3.061 -0.254 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 72.22566 15.68188 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.045 1.778) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 FC_5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 18.61866 44.89188)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 18.61866 38.79588)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 18.61866 32.69988)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -3.1195 -0.0555 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 FC_3V3))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Only \nclose\nif J1\nempty" (at 4.39466 59.62388) (layer F.SilkS))
  (gr_text V_CORE (at 57.22666 14.15788) (layer F.SilkS))
  (gr_text OFF (at 84.40466 6.02988) (layer F.SilkS))
  (gr_text Power (at 84.65866 17.45988) (layer F.SilkS))
  (gr_text cryptography.gmu.edu (at 32.08066 70.54588) (layer F.SilkS))
  (gr_text "not Done" (at 24.96866 51.74988) (layer F.SilkS))
  (gr_text Program (at 17.34866 51.74988) (layer F.SilkS))
  (gr_text Reset (at 17.09466 62.92588) (layer F.SilkS))
  (gr_text + (at 78.30066 13.56288) (layer F.SilkS))
  (gr_text - (at 72.29466 13.56288) (layer F.SilkS))
  (gr_text 5V (at 75.25266 15.59488) (layer F.SilkS))
  (gr_text +20db (at 23.18266 19.49988) (layer F.SilkS))
  (gr_text Target (at 7.95066 40.82788 90) (layer F.SilkS))
  (gr_text "Pin 1" (at 53.18666 42.29788 -45) (layer F.SilkS))
  (gr_text LED_4 (at 66.37066 62.16388) (layer F.SilkS))
  (gr_text LED_3 (at 60.27466 62.16388) (layer F.SilkS))
  (gr_text LED_2 (at 53.67066 62.16388) (layer F.SilkS))
  (gr_text LED_1 (at 47.57466 62.16388) (layer F.SilkS))
  (gr_text CURRENT (at 40.97066 4.50588) (layer F.SilkS))
  (gr_text GND (at 65.79066 7.61788) (layer F.SilkS))
  (gr_text +1V0 (at 50.62266 7.80788) (layer F.SilkS))
  (gr_text "+5V\nFC_3V3\nFC_5V\nGND\n+1V0\n+1V8\n+3V3" (at 74.30866 66.29988 90) (layer F.SilkS))
  (gr_text "TP1\nTP2\nTP3\nTP4\nTP5\nTP6\nTP7" (at 74.30866 70.61788 90) (layer F.SilkS))
  (gr_text 20 (at 3.05266 27.42988) (layer F.SilkS))
  (gr_text 19 (at 5.59266 27.42988) (layer F.SilkS))
  (gr_text 2 (at 3.05266 54.35388) (layer F.SilkS))
  (gr_text 1 (at 5.59266 54.35388) (layer F.SilkS))
  (gr_text 12 (at 81.35666 63.94188) (layer F.SilkS))
  (gr_text 6 (at 75.76866 61.40188) (layer F.SilkS))
  (gr_text 7 (at 80.07866 46.16188) (layer F.SilkS))
  (gr_text 1 (at 76.78466 46.16188) (layer F.SilkS))
  (gr_text "FOBOS DUT-ARTIX7-A12 rev1" (at 47.32066 50.47988) (layer F.SilkS))
  (gr_text "MEASURE VCORE" (at 41.22466 2.98188) (layer F.SilkS))
  (dimension 76.2 (width 0.15) (layer Dwgs.User)
    (gr_text "3.0000 in" (at 97.38066 34.48588 270) (layer Dwgs.User))
    (feature1 (pts (xy 88.84166 72.58588) (xy 96.667081 72.58588)))
    (feature2 (pts (xy 88.84166 -3.61412) (xy 96.667081 -3.61412)))
    (crossbar (pts (xy 96.08066 -3.61412) (xy 96.08066 72.58588)))
    (arrow1a (pts (xy 96.08066 72.58588) (xy 95.494239 71.459376)))
    (arrow1b (pts (xy 96.08066 72.58588) (xy 96.667081 71.459376)))
    (arrow2a (pts (xy 96.08066 -3.61412) (xy 95.494239 -2.487616)))
    (arrow2b (pts (xy 96.08066 -3.61412) (xy 96.667081 -2.487616)))
  )
  (dimension 88.9 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5000 in" (at 44.45 -9.682) (layer Dwgs.User))
    (feature1 (pts (xy 88.9 0) (xy 88.9 -8.968421)))
    (feature2 (pts (xy 0 0) (xy 0 -8.968421)))
    (crossbar (pts (xy 0 -8.382) (xy 88.9 -8.382)))
    (arrow1a (pts (xy 88.9 -8.382) (xy 87.773496 -7.795579)))
    (arrow1b (pts (xy 88.9 -8.382) (xy 87.773496 -8.968421)))
    (arrow2a (pts (xy 0 -8.382) (xy 1.126504 -7.795579)))
    (arrow2b (pts (xy 0 -8.382) (xy 1.126504 -8.968421)))
  )
  (gr_line (start 0 -3.62212) (end 0 72.57788) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.9 -3.62212) (end 0 -3.62212) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.9 72.57788) (end 88.9 -3.62212) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 72.57788) (end 88.9 72.57788) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.65066 72.33188) (xy 0.25866 72.33188) (xy 0.33066 -3.36812) (xy 88.65066 -3.36812)
      )
    )
  )
  (zone (net 210) (net_name /Power/pre3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.65866 40.89988) (xy 80.65866 38.35988) (xy 83.70666 38.35988) (xy 83.70666 40.89988) (xy 82.43666 40.89988)
        (xy 82.43666 46.59788) (xy 79.64266 46.59788) (xy 79.64266 40.89988)
      )
    )
  )
  (zone (net 217) (net_name /Power/SW1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.67466 31.75588) (xy 81.67466 34.54988) (xy 78.88066 34.54988) (xy 78.88066 31.75588)
      )
    )
  )
  (zone (net 24) (net_name +1V0) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.23066 28.19988) (xy 85.23066 30.99388) (xy 79.89666 30.99388) (xy 79.89666 28.19988)
      )
    )
  )
  (zone (net 218) (net_name /Power/SW2) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.57586 29.14388) (xy 78.57586 34.54988) (xy 78.11866 34.54988) (xy 78.11866 31.50188) (xy 77.35666 30.99388)
        (xy 76.78466 30.99388) (xy 76.78466 29.14388)
      )
    )
  )
  (zone (net 209) (net_name /Power/pre1V8) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.065839 27.11188) (xy 76.065839 30.41388) (xy 71.95866 30.41388) (xy 71.95866 27.11188)
      )
    )
  )
  (zone (net 94) (net_name FC_5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.03866 18.72988) (xy 72.46666 18.72988) (xy 72.46666 9.07788) (xy 77.03866 9.07788)
      )
    )
  )
  (zone (net 6) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.55466 24.57188) (xy 68.91066 24.57188) (xy 68.91066 23.04788) (xy 70.68866 23.04788) (xy 70.68866 21.26988)
        (xy 78.55466 21.26988)
      )
    )
  )
  (zone (net 2) (net_name "Net-(C4-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.95866 19.23788) (xy 68.91066 19.23788) (xy 68.91066 16.44388) (xy 70.68866 16.44388) (xy 70.68866 14.91988)
        (xy 71.95866 14.91988)
      )
    )
  )
  (zone (net 12) (net_name "Net-(F1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.11666 16.18988) (xy 63.32266 16.18988) (xy 63.32266 16.95988) (xy 61.03666 16.95988) (xy 61.03666 14.15788)
        (xy 66.11666 14.15788)
      )
    )
  )
  (zone (net 131) (net_name "Net-(J5-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.51266 11.61788) (xy 66.11666 11.61788) (xy 66.11666 13.64988) (xy 57.48066 13.64988) (xy 57.48066 6.28388)
        (xy 49.09866 6.28388) (xy 49.09866 -3.11412) (xy 59.25866 -3.11412)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C5-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.48866 18.22988) (xy 63.06066 18.22988) (xy 63.06066 19.75388) (xy 57.21866 19.75388) (xy 57.21866 15.68988)
        (xy 58.48866 15.68988)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C7-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.45666 19.75388) (xy 48.58266 19.75388) (xy 48.58266 16.70588) (xy 50.86866 16.70588) (xy 50.86866 18.22988)
        (xy 55.18666 18.22988) (xy 55.18666 15.68988) (xy 56.45666 15.68988)
      )
    )
  )
  (zone (net 25) (net_name "Net-(JP2-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47.82066 18.99188) (xy 40.96266 18.99188) (xy 40.96266 15.94388) (xy 41.47066 15.43588) (xy 41.72466 15.43588)
        (xy 41.72466 13.65788) (xy 47.82066 13.65788)
      )
    )
  )
  (zone (net 129) (net_name VCCINT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.69266 15.94388) (xy 40.20066 15.94388) (xy 40.20066 18.99188) (xy 26.73866 18.99188) (xy 26.73866 14.92788)
        (xy 36.39066 14.92788) (xy 36.39066 13.40388) (xy 39.69266 13.40388)
      )
    )
  )
  (zone (net 219) (net_name /Power/SW3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.48666 40.59788) (xy 78.73666 41.09788) (xy 78.73666 43.34788) (xy 77.48666 43.34788) (xy 77.48666 41.09788)
        (xy 78.23666 40.34788) (xy 78.23666 39.09788) (xy 78.48666 39.09788)
      )
    )
  )
  (zone (net 210) (net_name /Power/pre3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.98666 46.59788) (xy 82.23666 46.59788) (xy 82.23666 43.59788) (xy 86.48666 43.59788) (xy 86.48666 41.34788)
        (xy 87.98666 41.34788)
      )
    )
  )
  (zone (net 127) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.98666 40.34788) (xy 86.48666 40.34788) (xy 86.48666 36.84788) (xy 87.98666 36.84788)
      )
    )
  )
  (zone (net 6) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.23666 36.34788) (xy 79.98666 36.34788) (xy 79.98666 40.09788) (xy 78.98666 40.09788) (xy 78.98666 38.34788)
        (xy 78.48666 38.34788) (xy 78.48666 34.84788) (xy 81.98666 34.84788) (xy 81.98666 33.59788) (xy 83.23666 33.59788)
      )
    )
  )
  (zone (net 129) (net_name VCCINT) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.18666 23.56388) (xy 55.18666 31.43788) (xy 52.64666 31.43788) (xy 52.64666 35.75588) (xy 48.58266 35.75588)
        (xy 48.58266 39.56588) (xy 46.04266 39.56588) (xy 46.16966 26.86588) (xy 30.29466 26.86588) (xy 30.29466 14.67388)
        (xy 40.70866 14.67388) (xy 40.70866 21.53188) (xy 51.88466 21.53188) (xy 51.88466 23.56388)
      )
    )
  )
  (zone (net 6) (net_name +5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.71466 34.86688) (xy 75.88766 34.99388) (xy 72.83966 37.78788) (xy 67.25166 37.78788) (xy 67.25166 31.05688)
        (xy 62.17166 31.05688) (xy 62.17166 29.78688) (xy 67.25166 29.78688) (xy 67.25166 21.78588) (xy 88.71466 21.78588)
      )
    )
  )
  (zone (net 93) (net_name FC_3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.71466 72.45888) (xy 0.06866 72.45888) (xy 0.06866 60.39388) (xy 16.83266 60.39388) (xy 16.83266 66.99788)
        (xy 46.29666 66.99788) (xy 46.29666 59.37788) (xy 66.74366 59.37788) (xy 66.61666 42.10588) (xy 88.71466 42.10588)
      )
    )
  )
  (zone (net 24) (net_name +1V0) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.09466 20.38888) (xy 85.15866 24.83388) (xy 85.15866 32.45388) (xy 73.09366 32.45388) (xy 73.09366 34.23188)
        (xy 71.31566 34.23188) (xy 71.31566 32.45388) (xy 66.74366 28.64388) (xy 66.74366 24.96088) (xy 63.44166 24.96088)
        (xy 63.44166 16.45188) (xy 81.09466 16.45188)
      )
    )
  )
  (zone (net 93) (net_name FC_3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47.56666 14.16588) (xy 29.78666 14.16588) (xy 29.78666 21.27788) (xy 29.78666 27.37388) (xy 33.08866 27.37388)
        (xy 33.08866 39.05788) (xy 24.57966 39.05788) (xy 24.57966 48.58288) (xy 20.26166 48.58288) (xy 20.26166 32.45388)
        (xy 28.26266 32.45388) (xy 28.26266 22.80188) (xy 24.19866 22.80188) (xy 24.19866 17.97588) (xy 21.27766 14.67388)
        (xy 21.27766 8.83188) (xy 47.56666 8.83188)
      )
    )
  )
  (zone (net 94) (net_name FC_5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.71466 21.02388) (xy 67.12466 21.02388) (xy 67.12466 13.91188) (xy 48.07466 13.91188) (xy 48.07466 8.32388)
        (xy 29.65966 8.32388) (xy 29.65966 3.24388) (xy 13.53066 3.24388) (xy 13.53066 21.27788) (xy 13.53066 51.50388)
        (xy 12.00666 51.50388) (xy 12.00666 54.17088) (xy 0.57666 54.17088) (xy 0.44966 -3.48712) (xy 88.71466 -3.48712)
      )
    )
  )
  (zone (net 128) (net_name +1V8) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45.78866 37.53388) (xy 45.78866 39.81988) (xy 53.15466 39.81988) (xy 53.15466 42.86788) (xy 50.86866 42.86788)
        (xy 50.86866 41.85188) (xy 45.02666 41.85188) (xy 45.02666 38.54988) (xy 44.77266 38.54988) (xy 44.26466 38.04188)
        (xy 44.26466 37.53388)
      )
    )
  )
  (zone (net 127) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29.15166 8.45088) (xy 21.02366 8.45088) (xy 21.02366 14.80088) (xy 23.94466 18.10288) (xy 23.94466 23.30988)
        (xy 28.00866 23.30988) (xy 28.00866 32.19988) (xy 19.88066 32.19988) (xy 19.88066 48.83688) (xy 24.83366 48.83688)
        (xy 24.89716 39.81988) (xy 33.34266 39.81988) (xy 33.34266 27.37388) (xy 45.78866 27.37388) (xy 45.78866 37.27988)
        (xy 44.01066 37.27988) (xy 44.01066 38.04188) (xy 44.77266 38.80388) (xy 44.77266 42.48688) (xy 50.23366 42.48688)
        (xy 50.23366 43.12188) (xy 53.40866 43.12188) (xy 53.40866 38.80388) (xy 48.83666 38.80388) (xy 48.83666 36.00988)
        (xy 49.59866 36.00988) (xy 52.90066 36.00988) (xy 52.90066 31.69188) (xy 66.74366 31.69188) (xy 66.74366 38.16888)
        (xy 73.22066 38.16888) (xy 76.26866 35.37488) (xy 88.71466 35.37488) (xy 88.71466 41.85188) (xy 65.98166 41.85188)
        (xy 65.98166 58.61588) (xy 45.53466 58.61588) (xy 45.53466 66.48988) (xy 17.34066 66.48988) (xy 17.34066 59.88588)
        (xy 7.94266 59.88588) (xy 7.94266 55.82188) (xy 14.03866 55.82188) (xy 14.03866 3.75188) (xy 29.15166 3.75188)
      )
    )
  )
  (zone (net 127) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.80566 32.19988) (xy 54.80566 38.80388) (xy 52.39266 38.80388) (xy 50.86866 40.29788) (xy 41.97866 40.32788)
        (xy 41.97866 41.59788) (xy 39.05766 41.59788) (xy 39.05766 35.75588) (xy 44.77266 35.75588) (xy 45.28066 36.26388)
        (xy 48.58266 36.26388) (xy 48.90016 35.75588) (xy 48.90016 34.04138) (xy 48.13816 33.21588) (xy 47.05866 33.21588)
        (xy 46.55066 33.72388) (xy 46.55066 34.48588) (xy 45.78866 34.48588) (xy 45.78866 33.46988) (xy 46.80466 32.45388)
        (xy 46.80466 32.19988) (xy 49.59866 32.19988)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.93166 13.02288) (xy 35.50166 13.02288) (xy 35.50166 14.29288) (xy 25.97666 14.29288) (xy 25.97666 21.91288)
        (xy -0.05834 21.91288) (xy -0.05834 6.03788) (xy 46.93166 6.03788)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47.56666 21.91288) (xy 25.34166 21.91288) (xy 25.34166 19.37288) (xy 47.56666 19.37288)
      )
    )
  )
  (zone (net 128) (net_name +1V8) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.36266 28.89788) (xy 60.52066 28.89788) (xy 60.52066 42.86788) (xy 51.75766 42.86788) (xy 51.75766 41.97888)
        (xy 52.64666 41.97888) (xy 52.64666 39.81988) (xy 57.72666 39.81988) (xy 57.72666 25.84988) (xy 66.36266 25.84988)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.71066 38.80388) (xy 55.05966 38.80388) (xy 55.05966 32.19988) (xy 56.71066 32.19988)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.80366 41.59788) (xy 36.77166 41.59788) (xy 36.77166 35.75588) (xy 38.80366 35.75588)
      )
    )
  )
  (zone (net 129) (net_name VCCINT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51.24966 29.15188) (xy 53.66266 29.15188) (xy 53.66266 28.38988) (xy 55.18666 28.38988) (xy 55.18666 31.43788)
        (xy 46.04266 31.43788) (xy 46.04266 24.57988) (xy 51.24966 24.57988)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.61666 29.15188) (xy 55.69466 29.15188) (xy 55.69466 23.05588) (xy 52.39266 23.05588) (xy 52.39266 21.02388)
        (xy 41.21666 21.02388) (xy 41.21666 14.67388) (xy 66.61666 14.67388)
      )
    )
  )
)
