(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 84)
    (no_connects 0)
    (area 49.949999 42.949999 152.850001 129.950001)
    (thickness 1.6)
    (drawings 104)
    (tracks 310)
    (zones 0)
    (modules 50)
    (nets 41)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.75)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 50 43)
    (grid_origin 50 43)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Fabricate/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C3-Pad2)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(D4-Pad1)")
  (net 7 "Net-(D5-Pad1)")
  (net 8 "Net-(C1-Pad2)")
  (net 9 "Net-(C2-Pad2)")
  (net 10 "Net-(D1-Pad1)")
  (net 11 "Net-(D6-Pad2)")
  (net 12 "Net-(D8-Pad1)")
  (net 13 "Net-(F1-Pad1)")
  (net 14 "Net-(K2-Pad1)")
  (net 15 "Net-(SSR5-Pad5)")
  (net 16 "Net-(U2-Pad10)")
  (net 17 "Net-(U2-Pad11)")
  (net 18 "Net-(D7-Pad1)")
  (net 19 "Net-(K3-Pad1)")
  (net 20 "Net-(K3-Pad2)")
  (net 21 "Net-(K4-Pad3)")
  (net 22 "Net-(D1-Pad2)")
  (net 23 "Net-(D2-Pad2)")
  (net 24 "Net-(D3-Pad2)")
  (net 25 "Net-(D4-Pad2)")
  (net 26 "Net-(D5-Pad2)")
  (net 27 "Net-(C4-Pad1)")
  (net 28 "Net-(D9-Pad2)")
  (net 29 "Net-(D9-Pad1)")
  (net 30 "Net-(R6-Pad1)")
  (net 31 "Net-(JP1-Pad2)")
  (net 32 +15V)
  (net 33 "Net-(JP2-Pad1)")
  (net 34 "Net-(JP2-Pad3)")
  (net 35 "Net-(JP3-Pad1)")
  (net 36 "Net-(JP3-Pad3)")
  (net 37 "Net-(JP4-Pad1)")
  (net 38 "Net-(JP4-Pad3)")
  (net 39 "Net-(JP5-Pad1)")
  (net 40 "Net-(JP5-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP2-Pad3)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(JP3-Pad3)")
    (add_net "Net-(JP4-Pad1)")
    (add_net "Net-(JP4-Pad3)")
    (add_net "Net-(JP5-Pad1)")
    (add_net "Net-(JP5-Pad3)")
    (add_net "Net-(K2-Pad1)")
    (add_net "Net-(K3-Pad1)")
    (add_net "Net-(K3-Pad2)")
    (add_net "Net-(K4-Pad3)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(SSR5-Pad5)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 598480EC)
    (at 147.905 48.65)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value 3.2mm/M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 598480EC)
    (at 54.895 48.65)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value 3.2mm/M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module w_logo:Logo_silk_high_voltage_10x8.5mm (layer B.Cu) (tedit 0)
    (at 101.25 49 180)
    (descr "High voltage logo, 10x8.5mm")
    (fp_text reference G*** (at 0 -4.43738 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 4.43738 180) (layer B.SilkS) hide)
  )
  (module w_logo:Logo_silk_high_voltage_10x8.5mm (layer F.Cu) (tedit 0)
    (at 101.25 49)
    (descr "High voltage logo, 10x8.5mm")
    (fp_text reference G*** (at 0 4.43738) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -4.43738) (layer F.SilkS) hide)
  )
  (module "0 My SSRs:G3MC" (layer F.Cu) (tedit 59807593)
    (at 59 84)
    (fp_text reference SSR1 (at -1.27 -13.97) (layer F.SilkS))
    (fp_text value G3MC-202P-VD (at -2.69 -1.36 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -11.43) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(K3-Pad2)"))
    (pad 2 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C1-Pad2)"))
    (pad 3 thru_hole circle (at 0 6.35) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 32 +15V))
    (pad 4 thru_hole circle (at 0 8.89) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(D1-Pad2)"))
  )
  (module "0 My SSRs:G3MC" (layer F.Cu) (tedit 5980759D)
    (at 83 84)
    (fp_text reference SSR2 (at -1.27 -13.97) (layer F.SilkS))
    (fp_text value G3MC-202P-VD (at -2.63 -1.36 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -11.43) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(K3-Pad2)"))
    (pad 2 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(C2-Pad2)"))
    (pad 3 thru_hole circle (at 0 6.35) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 32 +15V))
    (pad 4 thru_hole circle (at 0 8.89) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(D2-Pad2)"))
  )
  (module "0 My SSRs:G3MC" (layer F.Cu) (tedit 598075A5)
    (at 107 84)
    (fp_text reference SSR3 (at -1.27 -13.97) (layer F.SilkS))
    (fp_text value G3MC-202P-VD (at -2.57 -1.36 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -11.43) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(K3-Pad2)"))
    (pad 2 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 3 thru_hole circle (at 0 6.35) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 32 +15V))
    (pad 4 thru_hole circle (at 0 8.89) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(D3-Pad2)"))
  )
  (module "0 My SSRs:G3MC" (layer F.Cu) (tedit 598075AD)
    (at 131 84)
    (fp_text reference SSR4 (at -1.27 -13.97) (layer F.SilkS))
    (fp_text value G3MC-202P-VD (at -2.51 -1.36 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -11.43) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(K3-Pad2)"))
    (pad 2 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 0 6.35) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 32 +15V))
    (pad 4 thru_hole circle (at 0 8.89) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(D4-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L32.0mm_W15.0mm_P27.00mm (layer F.Cu) (tedit 5981EEF7)
    (at 70 62 270)
    (descr "C, Rect series, Radial, pin pitch=27.00mm, , length*width=32*15mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 27.00mm  length 32mm width 15mm Capacitor")
    (fp_text reference C1 (at 13.5 -8.25 270) (layer F.SilkS))
    (fp_text value C* (at 13.5 8.81 270) (layer F.Fab))
    (fp_text user %R (at 13.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 27 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L32.0mm_W15.0mm_P27.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L32.0mm_W15.0mm_P27.00mm (layer F.Cu) (tedit 5981EEFC)
    (at 94 62 270)
    (descr "C, Rect series, Radial, pin pitch=27.00mm, , length*width=32*15mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 27.00mm  length 32mm width 15mm Capacitor")
    (fp_text reference C2 (at 13.5 -8.25 270) (layer F.SilkS))
    (fp_text value C* (at 13.5 8.81 270) (layer F.Fab))
    (fp_text user %R (at 13.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 27 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L32.0mm_W15.0mm_P27.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5981F0A5)
    (at 142.71 110.31)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value JUMPER (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 +15V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 58CC8E33)
    (at 137 93 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference SSR5 (at 3.81 -2.39 90) (layer F.SilkS))
    (fp_text value AQH3213 (at 3.81 10.01 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(D5-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(SSR5-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 +15V))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(K4-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(D5-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(D5-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(K3-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-18_W7.62mm (layer F.Cu) (tedit 5981EF36)
    (at 108 110 90)
    (descr "18-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.39 90) (layer F.SilkS) hide)
    (fp_text value LM3914 (at 3.81 22.71 90) (layer F.Fab))
    (fp_text user %R (at 3.81 10.16 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(JP2-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U2-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(JP1-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(JP5-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(JP5-Pad3)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(D9-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(JP4-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D8-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(JP4-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R6-Pad1)"))
    (pad 16 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(JP3-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(JP3-Pad3)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(JP1-Pad2)"))
    (pad 18 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(JP2-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-18_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_logo:Logo_silk_CC-BY-NC-SA_10x3.6mm (layer F.Cu) (tedit 0)
    (at 118.1355 96.594)
    (descr "CC BY-NC-SA logo, 10x3.6mm")
    (fp_text reference G*** (at 0.3 -1.4) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.3 0.5) (layer F.SilkS) hide)
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 63.25 53.25)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Capacitors_ThroughHole:C_Rect_L32.0mm_W15.0mm_P27.00mm (layer F.Cu) (tedit 5981EEFF)
    (at 118 62 270)
    (descr "C, Rect series, Radial, pin pitch=27.00mm, , length*width=32*15mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 27.00mm  length 32mm width 15mm Capacitor")
    (fp_text reference C3 (at 13.5 -8.25 270) (layer F.SilkS))
    (fp_text value C* (at 13.5 8.81 270) (layer F.Fab))
    (fp_text user %R (at 13.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 27 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L32.0mm_W15.0mm_P27.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Varistors:RV_Disc_D21.5_W6.1_P7.5 (layer F.Cu) (tedit 5980E300)
    (at 138 66 270)
    (descr varistor)
    (tags "varistor SIOV")
    (fp_text reference VAR1 (at 15.5 1 360) (layer F.SilkS))
    (fp_text value TMOV20RP200E (at 3.75 -2.6 270) (layer F.Fab))
    (fp_text user %R (at 3.81 5.715 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 2.9 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(K3-Pad2)"))
  )
  (module Varistors:RV_Disc_D21.5_W6.1_P7.5 (layer F.Cu) (tedit 5980E309)
    (at 146 66 270)
    (descr varistor)
    (tags "varistor SIOV")
    (fp_text reference VAR2 (at 15.5 1.5 360) (layer F.SilkS))
    (fp_text value TMOV20RP200E (at 3.75 -2.6 270) (layer F.Fab))
    (fp_text user %R (at 3.81 5.715 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(K4-Pad3)"))
    (pad 2 thru_hole circle (at 7.5 2.9 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(K3-Pad2)"))
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_03x5.08mm_Vertical (layer F.Cu) (tedit 5980E239)
    (at 80.3 124.25 180)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 03; pin pitch: 5.08mm; Vertical || order number: 1755749 12A || order number: 1924318 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x03_G_5.08mm")
    (fp_text reference K1 (at -5.7 -1.75 180) (layer F.SilkS))
    (fp_text value CONN_3 (at 5.08 4.8 180) (layer F.Fab))
    (fp_text user %R (at 5.08 -3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 28 "Net-(D9-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 13 "Net-(F1-Pad1)"))
    (pad 3 thru_hole oval (at 10.16 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_03x5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical (layer F.Cu) (tedit 5980E321)
    (at 58.001 61.923 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 3 -2 270) (layer F.SilkS))
    (fp_text value 1M (at 2.54 2.66 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical (layer F.Cu) (tedit 5980E315)
    (at 82.004 61.923 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 3 -2 270) (layer F.SilkS))
    (fp_text value 1M (at 2.54 2.66 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical (layer F.Cu) (tedit 5980E325)
    (at 106.007 61.923 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R3 (at 3 -2 270) (layer F.SilkS))
    (fp_text value 1M (at 2.54 2.66 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_06x5.08mm_Vertical (layer F.Cu) (tedit 5980E236)
    (at 137.75 124.25 180)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 06; pin pitch: 5.08mm; Vertical || order number: 1755778 12A || order number: 1924347 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x06_G_5.08mm")
    (fp_text reference K2 (at -6.15 -1.8 180) (layer F.SilkS))
    (fp_text value CONN_6 (at 12.7 4.8 180) (layer F.Fab))
    (fp_text user %R (at 12.7 -3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 14 "Net-(K2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (pad 3 thru_hole oval (at 10.16 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 4 thru_hole oval (at 15.24 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 5 thru_hole oval (at 20.32 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad1)"))
    (pad 6 thru_hole oval (at 25.4 0 180) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_06x5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_02x5.08mm_Vertical (layer F.Cu) (tedit 59808834)
    (at 75.2 48.7)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 02; pin pitch: 5.08mm; Vertical || order number: 1755736 12A || order number: 1924305 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x02_G_5.08mm")
    (fp_text reference K3 (at 10.8 -3.7) (layer F.SilkS))
    (fp_text value CONN_2 (at 2.54 4.8) (layer F.Fab))
    (fp_text user %R (at 3.54 -3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 19 "Net-(K3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 20 "Net-(K3-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_02x5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_03x5.08mm_Vertical (layer F.Cu) (tedit 5980883C)
    (at 122.5 48.7)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 03; pin pitch: 5.08mm; Vertical || order number: 1755749 12A || order number: 1924318 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x03_G_5.08mm")
    (fp_text reference K4 (at 15.5 -3.7) (layer F.SilkS))
    (fp_text value CONN_3 (at 5.08 4.8) (layer F.Fab))
    (fp_text user %R (at 5.08 -3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 19 "Net-(K3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 10.16 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 21 "Net-(K4-Pad3)"))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_03x5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 61.557 97.61 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 85.56 97.61 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 109.436 97.61 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 133.566 97.61 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 142.71 97.61 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5980E26D)
    (at 74.25 105.25 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D7 (at 5 0 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 64 108 180)
    (descr "TO-220, Vertical, RM 2.54mm")
    (tags "TO-220 Vertical RM 2.54mm")
    (fp_text reference U1 (at 2.54 -3.62 180) (layer F.SilkS))
    (fp_text value R-78E15-0.5 (at 2.54 3.92 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(C4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 32 +15V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D8.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5980E284)
    (at 87 113 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=8*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 8mm width 2.5mm Capacitor")
    (fp_text reference F1 (at 2.5 3 90) (layer F.SilkS))
    (fp_text value MF-R050 (at 2.5 2.56 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D8.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 72.987 110.437 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C4 (at 1.25 -4.46 270) (layer F.SilkS))
    (fp_text value 47uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5981EE2C)
    (at 72.987 96.975 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C5 (at -3.75 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 +15V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5981EE27)
    (at 66 97 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C6 (at -2.5 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.56 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 +15V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical (layer F.Cu) (tedit 5980E2EF)
    (at 146.52 97.61 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R4 (at 3 -2 270) (layer F.SilkS))
    (fp_text value 680 (at 2.54 2.66 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(K2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical (layer F.Cu) (tedit 5980E2D9)
    (at 137.63 112.85 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R5 (at 3 -2 180) (layer F.SilkS))
    (fp_text value 4.7K (at 2.54 2.66 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(JP1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical (layer F.Cu) (tedit 5980E2ED)
    (at 133.185 105.23)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R6 (at 3 -2) (layer F.SilkS))
    (fp_text value 820 (at 2.54 2.66) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R6-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical (layer F.Cu) (tedit 5980E273)
    (at 85 103 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R10 (at 3 -2 180) (layer F.SilkS))
    (fp_text value 4.7K (at 2.54 2.66 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(D7-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-41_SOD81_P5.08mm_Vertical_KathodeUp (layer F.Cu) (tedit 5921392F)
    (at 81 108 270)
    (descr "D, DO-41_SOD81 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Vertical pin pitch 5.08mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D6 (at 2.54 -2.690635 270) (layer F.SilkS))
    (fp_text value 1N4001 (at 2.54 2.690635 270) (layer F.Fab))
    (fp_text user K (at -1.8 0 270) (layer F.Fab))
    (fp_text user %R (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 "Net-(C4-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P5.08mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P5.08mm_Vertical_KathodeUp (layer F.Cu) (tedit 5980E2E5)
    (at 128.74 113.485 180)
    (descr "D, DO-35_SOD27 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Vertical pin pitch 5.08mm  length 4mm diameter 2mm")
    (fp_text reference D8 (at 2.5 2 180) (layer F.SilkS))
    (fp_text value 10V (at 2.54 2.266371 180) (layer F.Fab))
    (fp_text user K (at -1.5 0 180) (layer F.Fab))
    (fp_text user %R (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D8-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P5.08mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P5.08mm_Vertical_AnodeUp (layer F.Cu) (tedit 5921392F)
    (at 99.53 113.104 180)
    (descr "D, DO-35_SOD27 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Vertical pin pitch 5.08mm  length 4mm diameter 2mm")
    (fp_text reference D9 (at 2.54 -2.266371 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 2.54 2.266371 180) (layer F.Fab))
    (fp_text user K (at -1.966371 0 180) (layer F.Fab))
    (fp_text user %R (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(D9-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P5.08mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 59847F15)
    (at 147.905 124.25)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59847F94)
    (at 54.784 124.25)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value 3.2mm/M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical (layer F.Cu) (tedit 59A5B2DF)
    (at 110.5 113.5 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R7 (at 3 -2 180) (layer F.SilkS))
    (fp_text value 10K (at 2.54 2.66 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(D9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:GS3 (layer B.Cu) (tedit 58613494)
    (at 101.435 105.738 180)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP2 (at -1.7 0 450) (layer B.SilkS))
    (fp_text value JUMPER3 (at 1.8 0 450) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 0 0 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at 0 -1.27 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(JP2-Pad3)"))
  )
  (module Connect:GS3 (layer B.Cu) (tedit 58613494)
    (at 111.849 105.23 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP3 (at -1.7 0 360) (layer B.SilkS))
    (fp_text value JUMPER3 (at 1.8 0 360) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(JP3-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 3 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(JP3-Pad3)"))
  )
  (module Connect:GS3 (layer B.Cu) (tedit 58613494)
    (at 116.8655 99.4515 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP4 (at -1.7 0 360) (layer B.SilkS))
    (fp_text value JUMPER3 (at 1.8 0 360) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(JP4-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 3 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(JP4-Pad3)"))
  )
  (module Connect:GS3 (layer B.Cu) (tedit 59A5D377)
    (at 122.009 99.4515 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP5 (at -1.7 0 360) (layer B.SilkS))
    (fp_text value JUMPER3 (at 1.8 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(JP5-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (pad 3 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(JP5-Pad3)"))
  )
  (gr_text "AC Fan\nController" (at 97.117 98.753) (layer F.SilkS))
  (gr_text by (at 96.609 106.119) (layer F.SilkS))
  (gr_text "BUD DMB-4773 Enclosure" (at 150.5 101 90) (layer F.SilkS))
  (gr_text "0-10 EN" (at 145.631 111.58 90) (layer F.SilkS))
  (gr_text REV (at 133 54.5) (layer F.SilkS))
  (gr_text +24VDC (at 75 118) (layer F.SilkS))
  (gr_text 0-10VDC (at 82.25 118) (layer F.SilkS))
  (gr_text G (at 70 118) (layer F.SilkS))
  (dimension 103 (width 0.3) (layer Cmts.User)
    (gr_text "102.8 mm" (at 101.5 137.35) (layer Cmts.User))
    (feature1 (pts (xy 153 131) (xy 153 138.7)))
    (feature2 (pts (xy 50 131) (xy 50 138.7)))
    (crossbar (pts (xy 50 136) (xy 153 136)))
    (arrow1a (pts (xy 153 136) (xy 151.873496 136.586421)))
    (arrow1b (pts (xy 153 136) (xy 151.873496 135.413579)))
    (arrow2a (pts (xy 50 136) (xy 51.126504 136.586421)))
    (arrow2b (pts (xy 50 136) (xy 51.126504 135.413579)))
  )
  (dimension 87 (width 0.3) (layer Cmts.User)
    (gr_text "86.9 mm" (at 160.35 86.5 270) (layer Cmts.User))
    (feature1 (pts (xy 154 130) (xy 161.7 130)))
    (feature2 (pts (xy 154 43) (xy 161.7 43)))
    (crossbar (pts (xy 159 43) (xy 159 130)))
    (arrow1a (pts (xy 159 130) (xy 158.413579 128.873496)))
    (arrow1b (pts (xy 159 130) (xy 159.586421 128.873496)))
    (arrow2a (pts (xy 159 43) (xy 158.413579 44.126504)))
    (arrow2b (pts (xy 159 43) (xy 159.586421 44.126504)))
  )
  (gr_text "Pull To\nGround" (at 104.6 124.5) (layer F.SilkS))
  (gr_text PWR (at 76.5 105.25 90) (layer F.SilkS))
  (gr_text "LINE VOLTAGE!" (at 101.75 55.5) (layer B.SilkS))
  (gr_text "LINE VOLTAGE!" (at 101.75 55.5) (layer F.SilkS))
  (gr_text v2 (at 96.609 103.198) (layer F.SilkS))
  (gr_text jeditekunum (at 96.609 108.405) (layer F.SilkS))
  (gr_text LINE (at 80.75 54.5) (layer F.SilkS))
  (gr_text FAN (at 127.5 54.5) (layer F.SilkS))
  (gr_text N (at 122 54.5) (layer F.SilkS))
  (gr_text N (at 75 54.5) (layer F.SilkS))
  (gr_text 3 (at 118 76.5) (layer F.SilkS))
  (gr_text 2 (at 94 76.5) (layer F.SilkS))
  (gr_text 1 (at 70 76.5) (layer F.SilkS))
  (gr_text REV (at 138 118) (layer F.SilkS))
  (gr_text 4 (at 132.5 118) (layer F.SilkS))
  (gr_text 3 (at 127.5 118) (layer F.SilkS))
  (gr_text 2 (at 122.5 118) (layer F.SilkS))
  (gr_text 1 (at 117.5 118) (layer F.SilkS))
  (gr_text G (at 112.25 118) (layer F.SilkS))
  (gr_line (start 50 43) (end 152.8 43) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.8 43) (end 152.8 129.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50 129.9) (end 152.8 129.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50 43) (end 50 129.9) (angle 90) (layer Edge.Cuts) (width 0.1))
)
