<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="46.66" y2="0" width="0.1524" layer="20"/>
<wire x1="46.66" y1="0" x2="46.66" y2="69.84" width="0.1524" layer="20"/>
<wire x1="46.66" y1="69.84" x2="0" y2="69.84" width="0.1524" layer="20"/>
<wire x1="0" y1="69.84" x2="0" y2="0" width="0.1524" layer="20"/>
<text>Ext.</text>
<text>Int.</text>
<text> Remote Pot.</text>
<text>5A Max</text>
<text>+ Input1 -    + Input2 -</text>
<text>+ Rem Input -</text>
<text> PWM
Activity</text>
<text>Trigger</text>
<text>Mode</text>
<text>RV-Project.Com</text>
<text>Linc PWM Channel 
High Side Adapter</text>
<text>PWM Adjust</text>
<text>+12V In</text>
<text>LOAD</text>
<text>GND</text>
<text>LHPB-1A  RevC</text>
<text>+12V In</text>
<text>LOAD</text>
<text>GND</text>
<text>2/20/2018 Made in USA</text>
<text>Reset</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="GENERIC_0100_DEVICE_150_SPACING">
<description>&lt;h3&gt;Ceramic Capacitor&lt;/h3&gt;
Commonly used for small ceramic capacitors 0150 spacing.</description>
</package>
<package name="RADIAL_ELECTROLYTIC_100MIL(5MM)">
<description>Generic Electrolytic Capacitor 0.100 spacing 0.200 diameter.</description>
</package>
<package name="D041-3.5MIL">
</package>
<package name="3544-2">
</package>
<package name="WAFER2PINVERTICAL">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="TO-220-HEATSINK-JAMECO-PCH">
</package>
<package name="1/4W_AXIAL_RESISTOR_3.5MIL(V2)">
<description>Axial 1/4Watt Resistor&lt;p&gt;0.35" (tiny) footprint</description>
</package>
<package name="BOURNS3362_P">
<description>Standard Bourns Cermet Trimmer
&lt;p&gt;&lt;a href="http://www.mouser.com/ds/2/54/3362-55248.pdf"&gt;Data Sheet&lt;/a&gt;</description>
</package>
<package name="DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="TO-220-REGULATOR">
</package>
<package name="WAFER3PINVERTICAL">
</package>
<package name="WAFER4PINVERTICAL">
</package>
<package name="DIODE-1N4148(NEW)">
</package>
<package name="BIGFOOT_MEDIUM">
</package>
<package name="KF7.62CONNECTOR3">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="TACTILE-PTH-EZ">
</package>
<package name="CREATIVECOMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LONGPADS">
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="a-lib" package="GENERIC_0100_DEVICE_150_SPACING" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="a-lib" package="GENERIC_0100_DEVICE_150_SPACING" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="a-lib" package="RADIAL_ELECTROLYTIC_100MIL(5MM)" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="D3" library="a-lib" package="D041-3.5MIL" value="TVS-SD041">
<attribute name="NAME"/>
</element>
<element name="F1" library="a-lib" package="3544-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X03_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="OK1" library="optocoupler" package="DIL06" value="4N35">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="4N35"/>
<attribute name="OC_FARNELL" value="1328375"/>
<attribute name="OC_NEWARK" value="72K9946"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="a-lib" package="TO-220-HEATSINK-JAMECO-PCH" value="IRF520">
<attribute name="NAME"/>
</element>
<element name="R2" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="R1" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE" value="1.5k"/>
</element>
<element name="R4" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE" value="22k"/>
</element>
<element name="R5" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE" value="33k"/>
</element>
<element name="R3" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="R6" library="a-lib" package="BOURNS3362_P" value="10k">
<attribute name="MARKING" value="103"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="S1" library="a-lib" package="DIL04" value="DIPSWITCH-2"/>
<element name="U1" library="a-lib" package="DIP08" value="TINY85-20-DIP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09445"/>
</element>
<element name="U2" library="a-lib" package="TO-220-REGULATOR" value="78XX">
<attribute name="NAME"/>
<attribute name="VALUE" value="78XX"/>
</element>
<element name="J2" library="a-lib" package="WAFER2PINVERTICAL" value="WAFER2PVERTICAL"/>
<element name="J3" library="a-lib" package="WAFER3PINVERTICAL" value="WAFER3PVERTICAL"/>
<element name="J1" library="a-lib" package="WAFER4PINVERTICAL" value="WAFER4PVERTICAL"/>
<element name="C2" library="a-lib" package="GENERIC_0100_DEVICE_150_SPACING" value="0.33uF">
<attribute name="NAME"/>
</element>
<element name="D4" library="a-lib" package="D041-3.5MIL" value="TVS-SD041">
<attribute name="NAME"/>
</element>
<element name="D1" library="a-lib" package="DIODE-1N4148(NEW)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="a-lib" package="DIODE-1N4148(NEW)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="a-lib" package="BIGFOOT_MEDIUM" value="Bigfoot Medium"/>
<element name="D5" library="a-lib" package="D041-3.5MIL" value="TVS-SD041">
<attribute name="NAME"/>
</element>
<element name="J4" library="a-lib" package="KF7.62CONNECTOR3" value="KF762-3CONNECTOR"/>
<element name="R10" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="a-lib" package="TO-92" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08447"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="a-lib" package="TACTILE-PTH-EZ" value="SWITCH-MOMENTARY-2PTH_EZ"/>
<element name="U$1" library="a-lib" package="CREATIVECOMMONS" value=""/>
</elements>
<signals>
<signal name="5V">
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="OUT"/>
<contactref element="J3" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="OK1" pad="4"/>
<contactref element="R6" pad="3"/>
<contactref element="LED2" pad="K"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="GND"/>
<contactref element="C4" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="J3" pad="P$1"/>
<contactref element="J2" pad="P$1"/>
<contactref element="C2" pad="2"/>
<contactref element="D4" pad="A"/>
<contactref element="D5" pad="A"/>
<contactref element="J4" pad="3"/>
<contactref element="Q1" pad="1"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="OK1" pad="5"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$13">
<contactref element="OK1" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="LED1" pad="K"/>
<contactref element="J1" pad="P$1"/>
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="N$15">
<contactref element="R2" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="R1" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$16">
<contactref element="R2" pad="2"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="6"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="12V">
<contactref element="U2" pad="IN"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="D4" pad="C"/>
<contactref element="F1" pad="P$1-1"/>
<contactref element="F1" pad="P$1-2"/>
<contactref element="R10" pad="2"/>
<contactref element="Q2" pad="S"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="3"/>
<contactref element="R8" pad="2"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R6" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="LED2" pad="A"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="R5" pad="1"/>
<contactref element="J2" pad="P$2"/>
</signal>
<signal name="N$21">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$5">
</signal>
<signal name="N$9">
</signal>
<signal name="N$17">
</signal>
<signal name="N$20">
<contactref element="J3" pad="P$3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$10">
</signal>
<signal name="N$14">
<contactref element="J1" pad="P$4"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$23">
</signal>
<signal name="N$6">
</signal>
<signal name="N$27">
</signal>
<signal name="N$26">
</signal>
<signal name="N$24">
<contactref element="D2" pad="A"/>
<contactref element="J1" pad="P$2"/>
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$31">
</signal>
<signal name="N$32">
<contactref element="R11" pad="1"/>
<contactref element="D5" pad="C"/>
<contactref element="J4" pad="2"/>
<contactref element="Q2" pad="D"/>
</signal>
<signal name="N$22">
<contactref element="F1" pad="P$2-1"/>
<contactref element="F1" pad="P$2-2"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="Q1" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="R10" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="G"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
