(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 210)
    (no_connects 0)
    (area 141.775 97.475 168.325 124.025)
    (thickness 0.8)
    (drawings 134)
    (tracks 811)
    (zones 0)
    (modules 88)
    (nets 83)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.155)
    (user_trace_width 0.16)
    (user_trace_width 0.2)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (trace_clearance 0.15)
    (zone_clearance 0.05)
    (zone_45_only yes)
    (trace_min 0.155)
    (segment_width 0.02)
    (edge_width 0.04)
    (via_size 0.4)
    (via_drill 0.25)
    (via_min_size 0.36)
    (via_min_drill 0.25)
    (user_via 0.38 0.25)
    (user_via 0.4 0.25)
    (user_via 0.45 0.25)
    (user_via 0.55 0.35)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.3 1.3)
    (pad_drill 1.3)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance_ratio -0.05)
    (aux_axis_origin 0 0)
    (grid_origin 155 117.9)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00010_00000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /MicroESC1S3mosfets1/M_A)
  (net 4 /MicroESC1S3mosfets1/M_B)
  (net 5 /MicroESC1S3mosfets1/M_C)
  (net 6 /MicroESC1S3mosfets2/M_A)
  (net 7 /MicroESC1S3mosfets2/M_B)
  (net 8 /MicroESC1S3mosfets2/M_C)
  (net 9 /MicroESC1S3mosfets3/M_A)
  (net 10 /MicroESC1S3mosfets3/M_B)
  (net 11 /MicroESC1S3mosfets3/M_C)
  (net 12 "Net-(Q1-Pad5)")
  (net 13 "Net-(Q1-Pad2)")
  (net 14 "Net-(Q2-Pad5)")
  (net 15 "Net-(Q2-Pad2)")
  (net 16 "Net-(Q3-Pad5)")
  (net 17 "Net-(Q3-Pad2)")
  (net 18 "Net-(Q4-Pad5)")
  (net 19 "Net-(Q4-Pad2)")
  (net 20 "Net-(Q5-Pad5)")
  (net 21 "Net-(Q5-Pad2)")
  (net 22 "Net-(Q6-Pad5)")
  (net 23 "Net-(Q6-Pad2)")
  (net 24 "Net-(Q7-Pad5)")
  (net 25 "Net-(Q7-Pad2)")
  (net 26 "Net-(Q8-Pad5)")
  (net 27 "Net-(Q8-Pad2)")
  (net 28 "Net-(Q9-Pad5)")
  (net 29 "Net-(Q9-Pad2)")
  (net 30 /MicroESC1S3mosfets1/C2CK)
  (net 31 "Net-(R2-Pad1)")
  (net 32 "Net-(R3-Pad2)")
  (net 33 "Net-(R5-Pad2)")
  (net 34 "Net-(R7-Pad2)")
  (net 35 /MicroESC1S3mosfets2/C2CK)
  (net 36 "Net-(R11-Pad1)")
  (net 37 "Net-(R10-Pad2)")
  (net 38 "Net-(R12-Pad2)")
  (net 39 "Net-(R14-Pad2)")
  (net 40 /MicroESC1S3mosfets3/C2CK)
  (net 41 "Net-(R16-Pad1)")
  (net 42 "Net-(R17-Pad2)")
  (net 43 "Net-(R19-Pad2)")
  (net 44 "Net-(R21-Pad2)")
  (net 45 "Net-(U1-Pad16)")
  (net 46 "Net-(U1-Pad15)")
  (net 47 "Net-(U1-Pad18)")
  (net 48 /MicroESC1S3mosfets1/RC)
  (net 49 /MicroESC1S3mosfets1/C2D)
  (net 50 "Net-(U1-Pad7)")
  (net 51 "Net-(U2-Pad16)")
  (net 52 "Net-(U2-Pad15)")
  (net 53 "Net-(U2-Pad18)")
  (net 54 /MicroESC1S3mosfets2/RC)
  (net 55 /MicroESC1S3mosfets2/C2D)
  (net 56 "Net-(U2-Pad7)")
  (net 57 "Net-(U3-Pad16)")
  (net 58 "Net-(U3-Pad15)")
  (net 59 "Net-(U3-Pad18)")
  (net 60 /MicroESC1S3mosfets3/RC)
  (net 61 /MicroESC1S3mosfets3/C2D)
  (net 62 "Net-(U3-Pad7)")
  (net 63 /MicroESC1S3mosfets4/M_A)
  (net 64 /MicroESC1S3mosfets4/M_B)
  (net 65 /MicroESC1S3mosfets4/M_C)
  (net 66 "Net-(Q10-Pad5)")
  (net 67 "Net-(Q10-Pad2)")
  (net 68 "Net-(Q11-Pad5)")
  (net 69 "Net-(Q11-Pad2)")
  (net 70 "Net-(Q12-Pad5)")
  (net 71 "Net-(Q12-Pad2)")
  (net 72 /MicroESC1S3mosfets4/C2CK)
  (net 73 "Net-(R23-Pad1)")
  (net 74 "Net-(R24-Pad2)")
  (net 75 "Net-(R26-Pad2)")
  (net 76 "Net-(R28-Pad2)")
  (net 77 "Net-(U4-Pad16)")
  (net 78 "Net-(U4-Pad15)")
  (net 79 "Net-(U4-Pad18)")
  (net 80 /MicroESC1S3mosfets4/RC)
  (net 81 /MicroESC1S3mosfets4/C2D)
  (net 82 "Net-(U4-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.155)
    (via_dia 0.4)
    (via_drill 0.25)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /MicroESC1S3mosfets1/C2CK)
    (add_net /MicroESC1S3mosfets1/C2D)
    (add_net /MicroESC1S3mosfets1/M_A)
    (add_net /MicroESC1S3mosfets1/M_B)
    (add_net /MicroESC1S3mosfets1/M_C)
    (add_net /MicroESC1S3mosfets1/RC)
    (add_net /MicroESC1S3mosfets2/C2CK)
    (add_net /MicroESC1S3mosfets2/C2D)
    (add_net /MicroESC1S3mosfets2/M_A)
    (add_net /MicroESC1S3mosfets2/M_B)
    (add_net /MicroESC1S3mosfets2/M_C)
    (add_net /MicroESC1S3mosfets2/RC)
    (add_net /MicroESC1S3mosfets3/C2CK)
    (add_net /MicroESC1S3mosfets3/C2D)
    (add_net /MicroESC1S3mosfets3/M_A)
    (add_net /MicroESC1S3mosfets3/M_B)
    (add_net /MicroESC1S3mosfets3/M_C)
    (add_net /MicroESC1S3mosfets3/RC)
    (add_net /MicroESC1S3mosfets4/C2CK)
    (add_net /MicroESC1S3mosfets4/C2D)
    (add_net /MicroESC1S3mosfets4/M_A)
    (add_net /MicroESC1S3mosfets4/M_B)
    (add_net /MicroESC1S3mosfets4/M_C)
    (add_net /MicroESC1S3mosfets4/RC)
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad5)")
    (add_net "Net-(Q10-Pad2)")
    (add_net "Net-(Q10-Pad5)")
    (add_net "Net-(Q11-Pad2)")
    (add_net "Net-(Q11-Pad5)")
    (add_net "Net-(Q12-Pad2)")
    (add_net "Net-(Q12-Pad5)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q2-Pad5)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q3-Pad5)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(Q4-Pad5)")
    (add_net "Net-(Q5-Pad2)")
    (add_net "Net-(Q5-Pad5)")
    (add_net "Net-(Q6-Pad2)")
    (add_net "Net-(Q6-Pad5)")
    (add_net "Net-(Q7-Pad2)")
    (add_net "Net-(Q7-Pad5)")
    (add_net "Net-(Q8-Pad2)")
    (add_net "Net-(Q8-Pad5)")
    (add_net "Net-(Q9-Pad2)")
    (add_net "Net-(Q9-Pad5)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad18)")
    (add_net "Net-(U4-Pad7)")
  )
  (net_class POWER ""
    (clearance 0.15)
    (trace_width 1.2)
    (via_dia 0.55)
    (via_drill 0.35)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 151.7 104 270)
    (fp_text reference Q1 (at -0.1 6.6 270) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 270) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /MicroESC1S3mosfets1/M_A) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /MicroESC1S3mosfets1/M_A) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 3 /MicroESC1S3mosfets1/M_A))
    (pad 5 smd rect (at 0 -0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q1-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 3 /MicroESC1S3mosfets1/M_A))
    (pad 2 smd rect (at 0 0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Test_PAD_0.6X0.4 (layer F.Cu) (tedit 5A2A47F5)
    (at 151.85 106.37)
    (fp_text reference J23 (at 0 2) (layer F.SilkS) hide)
    (fp_text value C (at 0.1 -2) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0) (size 0.4 0.6) (layers F.Cu F.Mask)
      (net 72 /MicroESC1S3mosfets4/C2CK))
  )
  (module QFN20_small (layer F.Cu) (tedit 5A2A4786)
    (at 152.6 108.3 180)
    (fp_text reference U4 (at -0.127 3.302 180) (layer F.SilkS) hide)
    (fp_text value EFM8BB21 (at -0.1 4.9 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.4 1.4 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(R28-Pad2)"))
    (pad 16 smd rect (at -1.4 -1.4 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U4-Pad16)"))
    (pad 21 smd rect (at 0 0 180) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.15))
    (pad 20 smd rect (at -1.4 0.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(R24-Pad2)"))
    (pad 14 smd rect (at -0.25 -1.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(Q10-Pad2)"))
    (pad 15 smd rect (at -0.75 -1.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U4-Pad15)"))
    (pad 13 smd rect (at 0.25 -1.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(Q10-Pad5)"))
    (pad 19 smd rect (at -1.4 0.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R23-Pad1)"))
    (pad 18 smd rect (at -1.4 -0.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U4-Pad18)"))
    (pad 17 smd rect (at -1.4 -0.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 80 /MicroESC1S3mosfets4/RC))
    (pad 12 smd rect (at 0.75 -1.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.4 -1.4 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(Q11-Pad2)"))
    (pad 10 smd rect (at 1.4 -0.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(Q11-Pad5)"))
    (pad 6 smd rect (at 1.4 1.4 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 81 /MicroESC1S3mosfets4/C2D))
    (pad 7 smd rect (at 1.4 0.75 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U4-Pad7)"))
    (pad 9 smd rect (at 1.4 -0.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q12-Pad2)"))
    (pad 8 smd rect (at 1.4 0.25 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(Q12-Pad5)"))
    (pad 5 smd rect (at 0.75 1.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 /MicroESC1S3mosfets4/C2CK))
    (pad 4 smd rect (at 0.25 1.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -0.25 1.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.75 1.4 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(R26-Pad2)"))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59F9CBD6)
    (at 160.98 104.7)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value hole (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.02 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59FC1E64)
    (at 151.74 103.59 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59FAE068)
    (at 156.55 108.31 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value 10uf (at 0 -1.27 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59FAE072)
    (at 157.39 108.31 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.27 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59FAE2AE)
    (at 158.31 103.59 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59FC413B)
    (at 157.3 113.09)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 1.27) (layer B.SilkS) hide)
    (fp_text value 10uf (at 0 -1.27) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59FC4134)
    (at 157.3 112.25)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 1.27) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.27) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59FC41A1)
    (at 147.87 114.05)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59FC3FCF)
    (at 152.6 113 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0 1.27 270) (layer B.SilkS) hide)
    (fp_text value 10uf (at 0 -1.27 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59FC3FCD)
    (at 153.44 113 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 0 1.27 270) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.27 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE06B)
    (at 158.75 107.99 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 1.2 90) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 /MicroESC1S3mosfets1/C2CK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE040)
    (at 153.81 105.25 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 1.2 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /MicroESC1S3mosfets1/M_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE044)
    (at 155.16 106.79 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 1.2 270) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /MicroESC1S3mosfets1/M_A))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE060)
    (at 155.49 105.47 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 1.2 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /MicroESC1S3mosfets1/M_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE05B)
    (at 156.61 106.46)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.2) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /MicroESC1S3mosfets1/M_B))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE410)
    (at 157.18 105.42)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 1.2) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /MicroESC1S3mosfets1/M_C))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE056)
    (at 158.52 105.77 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 1.2 270) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /MicroESC1S3mosfets1/M_C))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE2B6)
    (at 157.79 114.5)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 1.2) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 35 /MicroESC1S3mosfets2/C2CK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE2AA)
    (at 160.45 109.47 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 0 1.2 90) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 /MicroESC1S3mosfets2/M_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FC446C)
    (at 158.92 110.86 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 0 1.2 180) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 /MicroESC1S3mosfets2/M_A))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE06E)
    (at 160.24 111.14 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 0 1.2 90) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 /MicroESC1S3mosfets2/M_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FC444A)
    (at 159.18 112.32 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at 0 1.2 270) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 /MicroESC1S3mosfets2/M_B))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE2B1)
    (at 160.3 112.84 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at 0 1.2 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 /MicroESC1S3mosfets2/M_C))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FC4416)
    (at 159.92 114.17 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at 0 1.2 180) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 /MicroESC1S3mosfets2/M_C))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(R14-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FC3F5F)
    (at 151.2 113.45 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 0 1.2 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 40 /MicroESC1S3mosfets3/C2CK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FC3EFC)
    (at 156.31 116.17)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at 0 1.2) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 /MicroESC1S3mosfets3/M_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FC4303)
    (at 154.88 114.63 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R17 (at 0 1.2 90) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 /MicroESC1S3mosfets3/M_A))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FC41CB)
    (at 154.6 115.9)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at 0 1.2) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 /MicroESC1S3mosfets3/M_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FC42C9)
    (at 153.37 114.89 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R19 (at 0 1.2 180) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 /MicroESC1S3mosfets3/M_B))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FC41FE)
    (at 152.83 115.98 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R20 (at 0 1.2 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 /MicroESC1S3mosfets3/M_C))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FC4238)
    (at 151.53 115.59 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R21 (at 0 1.2 90) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 /MicroESC1S3mosfets3/M_C))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59FC1CD9)
    (at 147.82 107.4)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59FAE02B)
    (at 152.6 108.32 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at 0 1.27 180) (layer B.SilkS) hide)
    (fp_text value 10uf (at 0 -1.27 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59FAE025)
    (at 152.6 109.15 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0 1.27 180) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.27 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59F9D2E8)
    (at 161.8 116.7)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value hole (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -0.8 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module KiCadCustomLibs:MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59F9CB4E)
    (at 148.98 116.1)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value hole (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.02 0.6) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module KiCadCustomLibs:MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59F9CA6F)
    (at 148.98 104.7)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value hole (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.02 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE01C)
    (at 152.25 106.9 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R22 (at 0 1.2 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 72 /MicroESC1S3mosfets4/C2CK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE078)
    (at 149.55 111.9 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R23 (at 0 1.2 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(R23-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 63 /MicroESC1S3mosfets4/M_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE07B)
    (at 151.06 110.53)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R24 (at 0 1.2) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 63 /MicroESC1S3mosfets4/M_A))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(R24-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE034)
    (at 149.71 110.25 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R25 (at 0 1.2 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(R23-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 64 /MicroESC1S3mosfets4/M_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE02F)
    (at 150.71 109.05 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R26 (at 0 1.2 90) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 64 /MicroESC1S3mosfets4/M_B))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(R26-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE03A)
    (at 149.66 108.6 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R27 (at 0 1.2 90) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.25 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(R23-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 65 /MicroESC1S3mosfets4/M_C))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59FAE020)
    (at 150.06 107.25)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R28 (at 0 1.2) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 65 /MicroESC1S3mosfets4/M_C))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R28-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59FC6FC8)
    (at 151.68 117.82 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59FC6FCC)
    (at 162.13 114.01)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59FC6FCF)
    (at 162.12 107.4)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59FC6FD1)
    (at 158.34 117.83 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value 47uf (at 0 -1.5 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:PAD_1.2X0.6_Round (layer F.Cu) (tedit 59FC6F12)
    (at 156.43 110.69)
    (fp_text reference J13 (at 0.6 1.1) (layer F.SilkS) hide)
    (fp_text value RC1 (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /MicroESC1S3mosfets1/RC))
  )
  (module KiCadCustomLibs:PAD_1.2X0.6_Round (layer F.Cu) (tedit 59FC6F12)
    (at 155.03 112.09 90)
    (fp_text reference J14 (at 0.6 1.1 90) (layer F.SilkS) hide)
    (fp_text value RC1 (at 0 -1.1 90) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 /MicroESC1S3mosfets2/RC))
  )
  (module KiCadCustomLibs:PAD_1.2X0.6_Round (layer F.Cu) (tedit 59FC6F12)
    (at 153.63 110.69)
    (fp_text reference J15 (at 0.6 1.1) (layer F.SilkS) hide)
    (fp_text value RC1 (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 /MicroESC1S3mosfets3/RC))
  )
  (module KiCadCustomLibs:PAD_1.2X0.6_Round (layer F.Cu) (tedit 59FC6F12)
    (at 155.03 109.39 90)
    (fp_text reference J16 (at 0.6 1.1 90) (layer F.SilkS) hide)
    (fp_text value RC1 (at 0 -1.1 90) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 80 /MicroESC1S3mosfets4/RC))
  )
  (module KiCadCustomLibs:Test_PAD_0.6X0.4 (layer F.Cu) (tedit 5A2A47F5)
    (at 150.92 106.9 90)
    (fp_text reference J24 (at 0 2 90) (layer F.SilkS) hide)
    (fp_text value D (at 0.1 -2 90) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0 90) (size 0.4 0.6) (layers F.Cu F.Mask)
      (net 81 /MicroESC1S3mosfets4/C2D))
  )
  (module KiCadCustomLibs:QFN20_small (layer F.Cu) (tedit 5A2A4786)
    (at 157.4 108.3 90)
    (fp_text reference U1 (at -0.127 3.302 90) (layer F.SilkS) hide)
    (fp_text value EFM8BB21 (at -0.1 4.9 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.4 1.4 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R7-Pad2)"))
    (pad 16 smd rect (at -1.4 -1.4 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad16)"))
    (pad 21 smd rect (at 0 0 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.15))
    (pad 20 smd rect (at -1.4 0.75 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R3-Pad2)"))
    (pad 14 smd rect (at -0.25 -1.4 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad2)"))
    (pad 15 smd rect (at -0.75 -1.4 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad15)"))
    (pad 13 smd rect (at 0.25 -1.4 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q1-Pad5)"))
    (pad 19 smd rect (at -1.4 0.25 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R2-Pad1)"))
    (pad 18 smd rect (at -1.4 -0.25 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad18)"))
    (pad 17 smd rect (at -1.4 -0.75 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /MicroESC1S3mosfets1/RC))
    (pad 12 smd rect (at 0.75 -1.4 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.4 -1.4 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q2-Pad2)"))
    (pad 10 smd rect (at 1.4 -0.75 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q2-Pad5)"))
    (pad 6 smd rect (at 1.4 1.4 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 /MicroESC1S3mosfets1/C2D))
    (pad 7 smd rect (at 1.4 0.75 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad7)"))
    (pad 9 smd rect (at 1.4 -0.25 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q3-Pad2)"))
    (pad 8 smd rect (at 1.4 0.25 180) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q3-Pad5)"))
    (pad 5 smd rect (at 0.75 1.4 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /MicroESC1S3mosfets1/C2CK))
    (pad 4 smd rect (at 0.25 1.4 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -0.25 1.4 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.75 1.4 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R5-Pad2)"))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:Test_PAD_0.6X0.4 (layer F.Cu) (tedit 5A2A47F5)
    (at 159.33 107.55 90)
    (fp_text reference J17 (at 0 2 90) (layer F.SilkS) hide)
    (fp_text value C (at 0.1 -2 90) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0 90) (size 0.4 0.6) (layers F.Cu F.Mask)
      (net 30 /MicroESC1S3mosfets1/C2CK))
  )
  (module KiCadCustomLibs:Test_PAD_0.6X0.4 (layer F.Cu) (tedit 5A2A47F5)
    (at 158.79 106.67)
    (fp_text reference J18 (at 0 2) (layer F.SilkS) hide)
    (fp_text value D (at 0.1 -2) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0) (size 0.4 0.6) (layers F.Cu F.Mask)
      (net 49 /MicroESC1S3mosfets1/C2D))
  )
  (module KiCadCustomLibs:QFN20_small (layer F.Cu) (tedit 5A2A4786)
    (at 157.4 113.1)
    (fp_text reference U2 (at -0.127 3.302) (layer F.SilkS) hide)
    (fp_text value EFM8BB21 (at -0.1 4.9) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.4 1.4) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R14-Pad2)"))
    (pad 16 smd rect (at -1.4 -1.4) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U2-Pad16)"))
    (pad 21 smd rect (at 0 0) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.15))
    (pad 20 smd rect (at -1.4 0.75 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R10-Pad2)"))
    (pad 14 smd rect (at -0.25 -1.4) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q4-Pad2)"))
    (pad 15 smd rect (at -0.75 -1.4) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U2-Pad15)"))
    (pad 13 smd rect (at 0.25 -1.4) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q4-Pad5)"))
    (pad 19 smd rect (at -1.4 0.25 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R11-Pad1)"))
    (pad 18 smd rect (at -1.4 -0.25 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U2-Pad18)"))
    (pad 17 smd rect (at -1.4 -0.75 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 /MicroESC1S3mosfets2/RC))
    (pad 12 smd rect (at 0.75 -1.4) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.4 -1.4) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(Q5-Pad2)"))
    (pad 10 smd rect (at 1.4 -0.75 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(Q5-Pad5)"))
    (pad 6 smd rect (at 1.4 1.4) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 /MicroESC1S3mosfets2/C2D))
    (pad 7 smd rect (at 1.4 0.75 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U2-Pad7)"))
    (pad 9 smd rect (at 1.4 -0.25 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q6-Pad2)"))
    (pad 8 smd rect (at 1.4 0.25 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q6-Pad5)"))
    (pad 5 smd rect (at 0.75 1.4) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /MicroESC1S3mosfets2/C2CK))
    (pad 4 smd rect (at 0.25 1.4) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -0.25 1.4) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.75 1.4) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R12-Pad2)"))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:Test_PAD_0.6X0.4 (layer F.Cu) (tedit 5A2A47F5)
    (at 159.03 114.5 90)
    (fp_text reference J20 (at 0 2 90) (layer F.SilkS) hide)
    (fp_text value D (at 0.1 -2 90) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0 90) (size 0.4 0.6) (layers F.Cu F.Mask)
      (net 55 /MicroESC1S3mosfets2/C2D))
  )
  (module KiCadCustomLibs:Test_PAD_0.6X0.4 (layer F.Cu) (tedit 5A2A47F5)
    (at 158.15 115.03)
    (fp_text reference J19 (at 0 2) (layer F.SilkS) hide)
    (fp_text value C (at 0.1 -2) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0) (size 0.4 0.6) (layers F.Cu F.Mask)
      (net 35 /MicroESC1S3mosfets2/C2CK))
  )
  (module KiCadCustomLibs:QFN20_small (layer F.Cu) (tedit 5A2A4786)
    (at 152.6 113.1 270)
    (fp_text reference U3 (at -0.127 3.302 270) (layer F.SilkS) hide)
    (fp_text value EFM8BB21 (at -0.1 4.9 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.4 1.4 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R21-Pad2)"))
    (pad 16 smd rect (at -1.4 -1.4 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U3-Pad16)"))
    (pad 21 smd rect (at 0 0 270) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.15))
    (pad 20 smd rect (at -1.4 0.75) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R17-Pad2)"))
    (pad 14 smd rect (at -0.25 -1.4 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(Q7-Pad2)"))
    (pad 15 smd rect (at -0.75 -1.4 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U3-Pad15)"))
    (pad 13 smd rect (at 0.25 -1.4 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(Q7-Pad5)"))
    (pad 19 smd rect (at -1.4 0.25) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R16-Pad1)"))
    (pad 18 smd rect (at -1.4 -0.25) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U3-Pad18)"))
    (pad 17 smd rect (at -1.4 -0.75) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 /MicroESC1S3mosfets3/RC))
    (pad 12 smd rect (at 0.75 -1.4 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.4 -1.4 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(Q8-Pad2)"))
    (pad 10 smd rect (at 1.4 -0.75) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(Q8-Pad5)"))
    (pad 6 smd rect (at 1.4 1.4 270) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 /MicroESC1S3mosfets3/C2D))
    (pad 7 smd rect (at 1.4 0.75) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U3-Pad7)"))
    (pad 9 smd rect (at 1.4 -0.25) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q9-Pad2)"))
    (pad 8 smd rect (at 1.4 0.25) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Q9-Pad5)"))
    (pad 5 smd rect (at 0.75 1.4 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /MicroESC1S3mosfets3/C2CK))
    (pad 4 smd rect (at 0.25 1.4 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -0.25 1.4 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.75 1.4 270) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R19-Pad2)"))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:Test_PAD_0.6X0.4 (layer F.Cu) (tedit 5A2A47F5)
    (at 151.2 114.72)
    (fp_text reference J22 (at 0 2) (layer F.SilkS) hide)
    (fp_text value D (at 0.1 -2) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0) (size 0.4 0.6) (layers F.Cu F.Mask)
      (net 61 /MicroESC1S3mosfets3/C2D))
  )
  (module KiCadCustomLibs:Test_PAD_0.6X0.4 (layer F.Cu) (tedit 5A2A47F5)
    (at 150.67 113.85 90)
    (fp_text reference J21 (at 0 2 90) (layer F.SilkS) hide)
    (fp_text value C (at 0.1 -2 90) (layer F.Fab) hide)
    (pad 1 smd oval (at 0 0 90) (size 0.4 0.6) (layers F.Cu F.Mask)
      (net 40 /MicroESC1S3mosfets3/C2CK))
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 151.7 117.4 90)
    (fp_text reference Q9 (at -0.1 6.6 90) (layer F.SilkS) hide)
    (fp_text value "DUAL_NP 2x2mm" (at 0.4 -9 90) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /MicroESC1S3mosfets3/M_C) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /MicroESC1S3mosfets3/M_C) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 11 /MicroESC1S3mosfets3/M_C))
    (pad 5 smd rect (at 0 -0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Q9-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 11 /MicroESC1S3mosfets3/M_C))
    (pad 2 smd rect (at 0 0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q9-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 155 117.4 90)
    (fp_text reference Q8 (at -0.1 6.6 90) (layer F.SilkS) hide)
    (fp_text value "DUAL_NP 2x2mm" (at 0.4 -9 90) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /MicroESC1S3mosfets3/M_B) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /MicroESC1S3mosfets3/M_B) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 10 /MicroESC1S3mosfets3/M_B))
    (pad 5 smd rect (at 0 -0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(Q8-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 10 /MicroESC1S3mosfets3/M_B))
    (pad 2 smd rect (at 0 0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(Q8-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 158.3 117.4 90)
    (fp_text reference Q7 (at -0.1 6.6 90) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 90) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /MicroESC1S3mosfets3/M_A) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /MicroESC1S3mosfets3/M_A) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 9 /MicroESC1S3mosfets3/M_A))
    (pad 5 smd rect (at 0 -0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(Q7-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 9 /MicroESC1S3mosfets3/M_A))
    (pad 2 smd rect (at 0 0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(Q7-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915 90) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 161.7 114 180)
    (fp_text reference Q6 (at -0.1 6.6 180) (layer F.SilkS) hide)
    (fp_text value "DUAL_NP 2x2mm" (at 0.4 -9 180) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /MicroESC1S3mosfets2/M_C) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /MicroESC1S3mosfets2/M_C) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 8 /MicroESC1S3mosfets2/M_C))
    (pad 5 smd rect (at 0 -0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q6-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 8 /MicroESC1S3mosfets2/M_C))
    (pad 2 smd rect (at 0 0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q6-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 161.7 110.7 180)
    (fp_text reference Q5 (at -0.1 6.6 180) (layer F.SilkS) hide)
    (fp_text value "DUAL_NP 2x2mm" (at 0.4 -9 180) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /MicroESC1S3mosfets2/M_B) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /MicroESC1S3mosfets2/M_B) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 7 /MicroESC1S3mosfets2/M_B))
    (pad 5 smd rect (at 0 -0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(Q5-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 7 /MicroESC1S3mosfets2/M_B))
    (pad 2 smd rect (at 0 0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(Q5-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 161.7 107.4 180)
    (fp_text reference Q4 (at -0.1 6.6 180) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9 180) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /MicroESC1S3mosfets2/M_A) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /MicroESC1S3mosfets2/M_A) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 6 /MicroESC1S3mosfets2/M_A))
    (pad 5 smd rect (at 0 -0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q4-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 6 /MicroESC1S3mosfets2/M_A))
    (pad 2 smd rect (at 0 0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q4-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915 180) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 158.3 104 270)
    (fp_text reference Q3 (at -0.1 6.6 270) (layer F.SilkS) hide)
    (fp_text value "DUAL_NP 2x2mm" (at 0.4 -9 270) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /MicroESC1S3mosfets1/M_C) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /MicroESC1S3mosfets1/M_C) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 5 /MicroESC1S3mosfets1/M_C))
    (pad 5 smd rect (at 0 -0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q3-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 5 /MicroESC1S3mosfets1/M_C))
    (pad 2 smd rect (at 0 0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q3-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 155 104 270)
    (fp_text reference Q2 (at -0.1 6.6 270) (layer F.SilkS) hide)
    (fp_text value "DUAL_NP 2x2mm" (at 0.4 -9 270) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /MicroESC1S3mosfets1/M_B) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /MicroESC1S3mosfets1/M_B) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 /MicroESC1S3mosfets1/M_B))
    (pad 5 smd rect (at 0 -0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q2-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 /MicroESC1S3mosfets1/M_B))
    (pad 2 smd rect (at 0 0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915 270) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 148.3 107.4)
    (fp_text reference Q12 (at -0.1 6.6) (layer F.SilkS) hide)
    (fp_text value "DUAL_NP 2x2mm" (at 0.4 -9) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 65 /MicroESC1S3mosfets4/M_C) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 65 /MicroESC1S3mosfets4/M_C) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 65 /MicroESC1S3mosfets4/M_C))
    (pad 5 smd rect (at 0 -0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(Q12-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 65 /MicroESC1S3mosfets4/M_C))
    (pad 2 smd rect (at 0 0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q12-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 148.3 110.7)
    (fp_text reference Q11 (at -0.1 6.6) (layer F.SilkS) hide)
    (fp_text value "DUAL_NP 2x2mm" (at 0.4 -9) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 64 /MicroESC1S3mosfets4/M_B) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 64 /MicroESC1S3mosfets4/M_B) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 64 /MicroESC1S3mosfets4/M_B))
    (pad 5 smd rect (at 0 -0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(Q11-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 64 /MicroESC1S3mosfets4/M_B))
    (pad 2 smd rect (at 0 0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(Q11-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:MicroFet-2.0 (layer F.Cu) (tedit 5A2A493E)
    (at 148.3 114)
    (fp_text reference Q10 (at -0.1 6.6) (layer F.SilkS) hide)
    (fp_text value DUAL_NP (at 0.4 -9) (layer F.Fab) hide)
    (pad 3 smd rect (at 0.5 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 63 /MicroESC1S3mosfets4/M_A) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.5 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 63 /MicroESC1S3mosfets4/M_A) (solder_paste_margin_ratio -0.15))
    (pad 6 smd rect (at -0.65 -0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 63 /MicroESC1S3mosfets4/M_A))
    (pad 5 smd rect (at 0 -0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(Q10-Pad5)"))
    (pad 4 smd rect (at 0.65 -0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0.65 0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 63 /MicroESC1S3mosfets4/M_A))
    (pad 2 smd rect (at 0 0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(Q10-Pad2)"))
    (pad 1 smd rect (at -0.65 0.915) (size 0.42 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 151.7 102.5 180)
    (fp_text reference J1 (at 0 1.6 180) (layer F.SilkS) hide)
    (fp_text value M1A (at -0.1 -1.6 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 3 /MicroESC1S3mosfets1/M_A))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 163.2 114 90)
    (fp_text reference J6 (at 0 1.6 90) (layer F.SilkS) hide)
    (fp_text value M2C (at -0.1 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 8 /MicroESC1S3mosfets2/M_C))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 163.2 107.4 90)
    (fp_text reference J4 (at 0 1.6 90) (layer F.SilkS) hide)
    (fp_text value M2A (at -0.1 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 6 /MicroESC1S3mosfets2/M_A))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 163.2 110.7 90)
    (fp_text reference J5 (at 0 1.6 90) (layer F.SilkS) hide)
    (fp_text value M2B (at -0.1 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 7 /MicroESC1S3mosfets2/M_B))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 151.7 118.9)
    (fp_text reference J9 (at 0 1.6) (layer F.SilkS) hide)
    (fp_text value M3C (at -0.1 -1.6) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 11 /MicroESC1S3mosfets3/M_C))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 158.33 118.89)
    (fp_text reference J7 (at 0 1.6) (layer F.SilkS) hide)
    (fp_text value M3A (at -0.1 -1.6) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 9 /MicroESC1S3mosfets3/M_A))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 155 118.9)
    (fp_text reference J8 (at 0 1.6) (layer F.SilkS) hide)
    (fp_text value M3B (at -0.1 -1.6) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 10 /MicroESC1S3mosfets3/M_B))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 146.8 107.4 90)
    (fp_text reference J12 (at 0 1.6 90) (layer F.SilkS) hide)
    (fp_text value M4C (at -0.1 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 65 /MicroESC1S3mosfets4/M_C))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 146.8 114 90)
    (fp_text reference J10 (at 0 1.6 90) (layer F.SilkS) hide)
    (fp_text value M4A (at -0.1 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 63 /MicroESC1S3mosfets4/M_A))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 146.8 110.7 90)
    (fp_text reference J11 (at 0 1.6 90) (layer F.SilkS) hide)
    (fp_text value M4B (at -0.1 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 64 /MicroESC1S3mosfets4/M_B))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 158.3 102.5 180)
    (fp_text reference J3 (at 0 1.6 180) (layer F.SilkS) hide)
    (fp_text value M1C (at -0.1 -1.6 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 5 /MicroESC1S3mosfets1/M_C))
  )
  (module KiCadCustomLibs:PAD_0.6X1.2 (layer F.Cu) (tedit 5A2A4A1C)
    (at 155 102.5 180)
    (fp_text reference J2 (at 0 1.6 180) (layer F.SilkS) hide)
    (fp_text value M1B (at -0.1 -1.6 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 1.2 0.6) (layers F.Cu F.Mask)
      (net 4 /MicroESC1S3mosfets1/M_B))
  )
  (gr_text + (at 155 117.1) (layer B.SilkS))
  (gr_text - (at 155 118.5) (layer B.SilkS))
  (gr_text - (at 162.8 110.7 90) (layer B.SilkS))
  (gr_text + (at 161.4 110.7 90) (layer B.SilkS))
  (gr_text + (at 148.5 110.7 90) (layer B.SilkS))
  (gr_text - (at 147.1 110.7 90) (layer B.SilkS))
  (gr_text - (at 155 102.8) (layer B.SilkS))
  (gr_text + (at 155 104.2) (layer B.SilkS))
  (gr_text 4A (at 155.06 113.02) (layer B.SilkS))
  (gr_text 1S (at 154.99 108.86) (layer B.SilkS))
  (gr_text 4in1 (at 155.1 111.69) (layer B.SilkS))
  (gr_text uESC (at 154.94 110.32) (layer B.SilkS))
  (gr_text + (at 149.53 103.29) (layer B.SilkS))
  (gr_text + (at 147.73 105.19) (layer B.SilkS))
  (gr_text D (at 162.9 115.76 180) (layer F.SilkS))
  (gr_text "C\n" (at 160.23 102.75 270) (layer F.SilkS))
  (gr_text B (at 149.89 118.65 90) (layer F.SilkS))
  (gr_text A (at 147.06 105.57) (layer F.SilkS))
  (gr_text C (at 157.93 110.69 270) (layer F.SilkS))
  (gr_text D (at 155.03 113.69 180) (layer F.SilkS))
  (gr_text B (at 152.13 110.69 90) (layer F.SilkS))
  (gr_text A (at 155.03 107.99) (layer F.SilkS))
  (gr_text - (at 148.13 103.8 45) (layer F.SilkS))
  (gr_line (start 149 102.5) (end 149.3 102.2) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 147.5 102.5) (end 149 102.5) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 146.8 104.7) (end 146.8 103.2) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_arc (start 147.5 103.2) (end 146.8 103.2) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 146.8 116.7) (end 146.5 116.4) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 146.87 116.79) (end 146.8 116.7) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 146.88 116.86) (end 146.87 116.79) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 146.9 117.03) (end 146.88 116.86) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 146.93 117.19) (end 146.9 117.03) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 146.99 117.4) (end 146.93 117.19) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 147.07 117.59) (end 146.99 117.4) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 147.15 117.75) (end 147.07 117.59) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 147.24 117.89) (end 147.15 117.75) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 147.34 118.03) (end 147.24 117.89) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 147.43 118.14) (end 147.34 118.03) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 147.54 118.26) (end 147.43 118.14) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 147.67 118.36) (end 147.54 118.26) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 147.8 118.46) (end 147.67 118.36) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 147.95 118.55) (end 147.8 118.46) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 148.15 118.65) (end 147.95 118.55) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 148.28 118.7) (end 148.15 118.65) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 148.42 118.75) (end 148.28 118.7) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 148.6 118.79) (end 148.42 118.75) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 148.77 118.82) (end 148.6 118.79) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 148.91 118.83) (end 148.77 118.82) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 148.98 118.88) (end 148.91 118.83) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 149.3 119.2) (end 148.98 118.88) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161 118.9) (end 160.71 119.2) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161.17 118.82) (end 161 118.9) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161.29 118.81) (end 161.17 118.82) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161.45 118.78) (end 161.29 118.81) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161.6 118.74) (end 161.45 118.78) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161.73 118.7) (end 161.6 118.74) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161.9 118.63) (end 161.73 118.7) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.05 118.55) (end 161.9 118.63) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.18 118.47) (end 162.05 118.55) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.33 118.36) (end 162.18 118.47) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.52 118.19) (end 162.33 118.36) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.63 118.07) (end 162.52 118.19) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.75 117.91) (end 162.63 118.07) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.84 117.77) (end 162.75 117.91) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.91 117.63) (end 162.84 117.77) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.98 117.48) (end 162.91 117.63) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.01 117.39) (end 162.98 117.48) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.05 117.27) (end 163.01 117.39) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.08 117.15) (end 163.05 117.27) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.11 116.98) (end 163.08 117.15) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.13 116.77) (end 163.11 116.98) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.5 116.4) (end 163.13 116.77) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.21 104.71) (end 163.5 105) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.13 104.62) (end 163.21 104.71) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.12 104.49) (end 163.13 104.62) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.08 104.25) (end 163.12 104.49) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.02 104.03) (end 163.08 104.25) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.95 103.85) (end 163.02 104.03) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.83 103.62) (end 162.95 103.85) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.7 103.42) (end 162.83 103.62) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.56 103.25) (end 162.7 103.42) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.39 103.09) (end 162.56 103.25) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.23 102.96) (end 162.39 103.09) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 162.04 102.84) (end 162.23 102.96) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161.79 102.72) (end 162.04 102.84) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161.52 102.64) (end 161.79 102.72) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161.28 102.59) (end 161.52 102.64) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 161.08 102.57) (end 161.28 102.59) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 160.71 102.2) (end 161.08 102.57) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 146.5 105) (end 146.8 104.7) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 163.5 116.4) (end 163.5 105) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 149.3 119.2) (end 160.71 119.2) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 146.5 105) (end 146.5 116.4) (angle 90) (layer Edge.Cuts) (width 0.04))
  (gr_line (start 149.3 102.2) (end 160.71 102.2) (angle 90) (layer Edge.Cuts) (width 0.04))
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.04))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 149 103.15) (xy 148.86 103.15) (xy 148.72 103.17) (xy 148.62 103.19) (xy 148.5 103.23)
        (xy 148.32 103.3) (xy 148.21 103.36) (xy 148.09 103.44) (xy 148 103.51) (xy 147.91 103.59)
        (xy 147.84 103.66) (xy 147.77 103.75) (xy 147.68 103.87) (xy 147.61 104) (xy 147.55 104.13)
        (xy 147.48 104.38) (xy 147.45 104.56) (xy 147.45 104.7) (xy 146.7 104.7) (xy 146.7 102.5)
        (xy 149 102.5)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.04))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 148.599206 102.50034) (xy 148.6 102.5) (xy 148.694441 102.566664) (xy 150.217059 103.627059) (xy 150.2445 103.6545)
        (xy 150.240351 103.657895) (xy 150.241379 103.658621) (xy 150.245 103.655) (xy 150.28 103.69) (xy 159.73 103.69)
        (xy 160.33 104.29) (xy 160.866707 104.841616) (xy 160.816883 104.903896) (xy 161.006148 105.072131) (xy 161.002915 104.981607)
        (xy 162.03 106.037222) (xy 162.03 115.39) (xy 161.22 116.2) (xy 160.9 116.2) (xy 160.9 116.52)
        (xy 159.68 117.74) (xy 150.28 117.74) (xy 147.98 115.44) (xy 147.98 105.99) (xy 147.952 105.948)
        (xy 147.957143 105.942857) (xy 146.8 104.4) (xy 145.85 103.6) (xy 147.45 101.7)
      )
    )
    (polygon
      (pts        (xy 151.3 105.3) (xy 149.5 107.1) (xy 149.5 114.1) (xy 151.5 116.1) (xy 158.542857 116.1)
        (xy 158.8 115.8) (xy 160.5 114.1) (xy 160.5 107.3) (xy 158.5 105.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.04))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 149 103.15) (xy 148.89 103.15) (xy 148.68 103.18) (xy 148.42 103.26) (xy 148.28 103.32)
        (xy 148.19 103.37) (xy 148.04 103.48) (xy 147.9 103.6) (xy 147.7 103.85) (xy 147.64 103.94)
        (xy 147.56 104.11) (xy 147.5 104.28) (xy 147.47 104.42) (xy 147.45 104.56) (xy 147.44 104.66)
        (xy 147.442222 104.7) (xy 146.7 104.7) (xy 146.7 102.5) (xy 149 102.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 150.264 103.5) (xy 149.942951 103.263935) (xy 150.331765 103.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 164.1 120.3) (xy 145.5 120.1) (xy 145.305714 116.7) (xy 145.3 116.7) (xy 145.3 104.8)
        (xy 146.887692 104.8) (xy 147.8 105.986) (xy 147.8 115.5) (xy 150.2 117.9) (xy 159.8 117.9)
        (xy 162.2 115.5) (xy 162.2 105.9) (xy 159.8 103.5) (xy 150.3585 103.5) (xy 149.2 102.641852)
        (xy 149.2 101.466667) (xy 149.358 101.098) (xy 149.363158 101) (xy 164.1 101)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.04))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 151.1 102) (xy 151.1 103.5) (xy 150.2 103.5) (xy 147.9 105.9) (xy 147.8 106.1)
        (xy 147.8 106.8) (xy 146.1 106.8) (xy 146.1 102)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.5 119) (xy 153.5 119) (xy 153.5 118) (xy 154.5 118)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.5 117.7) (xy 155.5 117.7) (xy 155.5 116.7) (xy 156.5 116.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.3 112.2) (xy 162.3 112.2) (xy 162.3 111.2) (xy 163.3 111.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162 110.2) (xy 161 110.2) (xy 161 109.2) (xy 162 109.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.5 103.4) (xy 155.5 103.4) (xy 155.5 102.4) (xy 156.5 102.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.5 104.7) (xy 153.5 104.7) (xy 153.5 103.7) (xy 154.5 103.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.7 110.2) (xy 146.7 110.2) (xy 146.7 109.2) (xy 147.7 109.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149 112.2) (xy 148 112.2) (xy 148 111.2) (xy 149 111.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Paste) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.16 102.95) (xy 147.76 102.95) (xy 147.76 103.55) (xy 147.18 103.55) (xy 147.18 103.54)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Paste) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.06 102.89) (xy 147.06 103.53) (xy 147.69 103.53) (xy 147.69 102.87) (xy 147.09 102.87)
        (xy 147.09 102.86)
      )
    )
  )
)
