<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>Mezzanine Template</text>
<text>Mezzanine Template</text>
</plain>
<libraries>
<library name="mezza">
<description>Generated from &lt;b&gt;mezza.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="55510-140LF">
</package>
<package name="61083-063402LF">
</package>
<package name="DRAGONBOARD410C">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PCB1" library="mezza" package="DRAGONBOARD410C" value="DB410C-PCB-FOOTPRINT"/>
<element name="J1" library="mezza" package="55510-140LF" value="55510-140LF">
<attribute name="NAME"/>
</element>
<element name="J2" library="mezza" package="61083-063402LF" value="61083-063402LF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="PCB1" pad="G$1"/>
<contactref element="J1" pad="P$1"/>
<contactref element="J1" pad="P$39"/>
<contactref element="J1" pad="P$2"/>
<contactref element="J1" pad="P$40"/>
<contactref element="PCB1" pad="G$4"/>
<contactref element="PCB1" pad="G$2"/>
<contactref element="PCB1" pad="G$3"/>
<contactref element="J2" pad="P$13"/>
<contactref element="J2" pad="P$19"/>
<contactref element="J2" pad="P$25"/>
<contactref element="J2" pad="P$31"/>
<contactref element="J2" pad="P$37"/>
<contactref element="J2" pad="P$43"/>
<contactref element="J2" pad="P$49"/>
<contactref element="J2" pad="P$55"/>
<contactref element="J2" pad="P$6"/>
<contactref element="J2" pad="P$12"/>
<contactref element="J2" pad="P$18"/>
<contactref element="J2" pad="P$24"/>
<contactref element="J2" pad="P$30"/>
<contactref element="J2" pad="P$40"/>
<contactref element="J2" pad="P$46"/>
<contactref element="J2" pad="P$52"/>
<contactref element="J2" pad="P$58"/>
</signal>
<signal name="UART0_CTS">
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="UART0_TXD">
<contactref element="J1" pad="P$5"/>
</signal>
<signal name="UART0_RXD">
<contactref element="J1" pad="P$7"/>
</signal>
<signal name="UART0_RTS">
<contactref element="J1" pad="P$9"/>
</signal>
<signal name="UART1_TXD">
<contactref element="J1" pad="P$11"/>
</signal>
<signal name="UART1_RXD">
<contactref element="J1" pad="P$13"/>
</signal>
<signal name="I2C0_SCL">
<contactref element="J1" pad="P$15"/>
</signal>
<signal name="I2C0_SDA">
<contactref element="J1" pad="P$17"/>
</signal>
<signal name="I2C1_SCL">
<contactref element="J1" pad="P$19"/>
</signal>
<signal name="I2C1_SDA">
<contactref element="J1" pad="P$21"/>
</signal>
<signal name="GPIO-A">
<contactref element="J1" pad="P$23"/>
</signal>
<signal name="GPIO-C">
<contactref element="J1" pad="P$25"/>
</signal>
<signal name="GPIO-G">
<contactref element="J1" pad="P$29"/>
</signal>
<signal name="GPIO-K">
<contactref element="J1" pad="P$33"/>
</signal>
<signal name="GPIO-E">
<contactref element="J1" pad="P$27"/>
</signal>
<signal name="GPIO-I">
<contactref element="J1" pad="P$31"/>
</signal>
<signal name="+1V8">
<contactref element="J1" pad="P$35"/>
</signal>
<signal name="PWR_BTN_N">
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="RST_BTN_N">
<contactref element="J1" pad="P$6"/>
</signal>
<signal name="SPI0_SCLK">
<contactref element="J1" pad="P$8"/>
</signal>
<signal name="SPI0_DIN">
<contactref element="J1" pad="P$10"/>
</signal>
<signal name="SPI0_CS">
<contactref element="J1" pad="P$12"/>
</signal>
<signal name="SPI0_DOUT">
<contactref element="J1" pad="P$14"/>
</signal>
<signal name="PCM_FS">
<contactref element="J1" pad="P$16"/>
</signal>
<signal name="PCM_CLK">
<contactref element="J1" pad="P$18"/>
</signal>
<signal name="PCM_DO">
<contactref element="J1" pad="P$20"/>
</signal>
<signal name="GPIO-B">
<contactref element="J1" pad="P$24"/>
</signal>
<signal name="GPIO-D">
<contactref element="J1" pad="P$26"/>
</signal>
<signal name="GPIO-F">
<contactref element="J1" pad="P$28"/>
</signal>
<signal name="GPIO-H">
<contactref element="J1" pad="P$30"/>
</signal>
<signal name="GPIO-J">
<contactref element="J1" pad="P$32"/>
</signal>
<signal name="GPIO-L">
<contactref element="J1" pad="P$34"/>
</signal>
<signal name="SD_DAT0/SPI1_DOUT">
<contactref element="J2" pad="P$1"/>
</signal>
<signal name="SD_DAT3/SPI1_CS">
<contactref element="J2" pad="P$7"/>
</signal>
<signal name="SD_SCLK/SPI1_SCLK">
<contactref element="J2" pad="P$9"/>
</signal>
<signal name="SD_CMD/SPI1_DIN">
<contactref element="J2" pad="P$11"/>
</signal>
<signal name="CLK0/CSI0_MCLK">
<contactref element="J2" pad="P$15"/>
</signal>
<signal name="CLK1/CSI1_MCLK">
<contactref element="J2" pad="P$17"/>
</signal>
<signal name="DSI_CLK+">
<contactref element="J2" pad="P$21"/>
</signal>
<signal name="DSI_CLK-">
<contactref element="J2" pad="P$23"/>
</signal>
<signal name="DSI_D0+">
<contactref element="J2" pad="P$27"/>
</signal>
<signal name="DSI_D0-">
<contactref element="J2" pad="P$29"/>
</signal>
<signal name="DSI_D1+">
<contactref element="J2" pad="P$33"/>
</signal>
<signal name="DSI_D1-">
<contactref element="J2" pad="P$35"/>
</signal>
<signal name="DSI_D2+">
<contactref element="J2" pad="P$39"/>
</signal>
<signal name="DSI_D2-">
<contactref element="J2" pad="P$41"/>
</signal>
<signal name="DSI_D3+">
<contactref element="J2" pad="P$45"/>
</signal>
<signal name="DSI_D3-">
<contactref element="J2" pad="P$47"/>
</signal>
<signal name="USB_D+">
<contactref element="J2" pad="P$51"/>
</signal>
<signal name="USB_D-">
<contactref element="J2" pad="P$53"/>
</signal>
<signal name="CSI0_C+">
<contactref element="J2" pad="P$2"/>
</signal>
<signal name="CSI0_C-">
<contactref element="J2" pad="P$4"/>
</signal>
<signal name="CSI0_D0+">
<contactref element="J2" pad="P$8"/>
</signal>
<signal name="CSI0_D0-">
<contactref element="J2" pad="P$10"/>
</signal>
<signal name="CSI0_D1+">
<contactref element="J2" pad="P$14"/>
</signal>
<signal name="CSI0_D2+">
<contactref element="J2" pad="P$20"/>
</signal>
<signal name="CSI0_D2-">
<contactref element="J2" pad="P$22"/>
</signal>
<signal name="CSI0_D3+">
<contactref element="J2" pad="P$26"/>
</signal>
<signal name="CSI0_D3-">
<contactref element="J2" pad="P$28"/>
</signal>
<signal name="I2C2_SCL">
<contactref element="J2" pad="P$32"/>
</signal>
<signal name="I2C2_SDA">
<contactref element="J2" pad="P$34"/>
</signal>
<signal name="I2C3_SCL">
<contactref element="J2" pad="P$36"/>
</signal>
<signal name="I2C3_SDA">
<contactref element="J2" pad="P$38"/>
</signal>
<signal name="CSI1_D0+">
<contactref element="J2" pad="P$42"/>
</signal>
<signal name="CSI1_D0-">
<contactref element="J2" pad="P$44"/>
</signal>
<signal name="CSI1_D1+">
<contactref element="J2" pad="P$48"/>
</signal>
<signal name="CSI1_D1-">
<contactref element="J2" pad="P$50"/>
</signal>
<signal name="CSI1_C+">
<contactref element="J2" pad="P$54"/>
</signal>
<signal name="CSI1_C-">
<contactref element="J2" pad="P$56"/>
</signal>
<signal name="CSI0_D1-">
<contactref element="J2" pad="P$16"/>
</signal>
<signal name="SYS_DCIN">
<contactref element="J1" pad="P$36"/>
<contactref element="J1" pad="P$38"/>
</signal>
<signal name="SD_DAT1">
<contactref element="J2" pad="P$3"/>
</signal>
<signal name="SD_DAT2">
<contactref element="J2" pad="P$5"/>
</signal>
<signal name="RESERVED">
<contactref element="J2" pad="P$60"/>
</signal>
<signal name="HSIC_STR">
<contactref element="J2" pad="P$57"/>
</signal>
<signal name="HSIC_DATA">
<contactref element="J2" pad="P$59"/>
</signal>
<signal name="+5V">
<contactref element="J1" pad="P$37"/>
</signal>
<signal name="PCM_DI">
<contactref element="J1" pad="P$22"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
