(kicad_pcb (version 20171130) (host pcbnew 5.1.4-e60b266~84~ubuntu19.04.1)
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 2)
    (zones 0)
    (modules 6)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
  )
  (module afterdark:osh-park-text-cu-mask (layer B.Cu) (tedit 5DEE72F0)
    (at 121.92 52.2605 180)
    (descr "Imported from OSHPARK.svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference OSH_small (at 0 3.81 180) (layer B.Cu) hide)
    (fp_text value G*** (at 0 -2.54 180) (layer B.Cu) hide)
  )
  (module Symbol:KiCad-Logo_5mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 122.174 59.8805)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo_5mm_SilkScreen (at 0 3.81) (layer F.Fab) hide)
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 5DEE5A23)
    (at 122.428 53.721)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module touch:TestPoint_Pad_4.0x4.0mm (layer F.Cu) (tedit 5DEE53EA)
    (at 134.65556 55.86476)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 -2.898) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 -2.9) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 10 10) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5DED2E95)
    (at 113.16716 55.81142)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference J1 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.77) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5DED2F5D)
    (at 107.8357 55.81142)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference J2 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.77) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 106.4895 61.214) (end 106.4895 60.833) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.4895 60.833) (end 106.9975 60.833) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.4895 61.595) (end 106.9975 61.595) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.4895 61.214) (end 106.1085 61.214) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.9975 61.214) (end 107.3785 61.214) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.9975 61.214) (end 106.9975 61.595) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.299 50.4825) (end 105.918 50.4825) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.299 50.4825) (end 106.299 50.1015) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.299 50.1015) (end 106.807 50.1015) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.299 50.8635) (end 106.807 50.8635) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.807 50.4825) (end 106.807 50.8635) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.807 50.4825) (end 107.188 50.4825) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.954 50.546) (end 140.335 50.546) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.446 50.546) (end 139.446 50.165) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.446 50.927) (end 139.954 50.927) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.446 50.546) (end 139.065 50.546) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.954 50.546) (end 139.954 50.927) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.446 50.165) (end 139.954 50.165) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.446 61.849) (end 139.954 61.849) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.446 61.087) (end 139.954 61.087) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.954 61.468) (end 139.954 61.849) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.954 61.468) (end 140.335 61.468) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.446 61.468) (end 139.065 61.468) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.446 61.468) (end 139.446 61.087) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.41 50.165) (end 105.41 60.96) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.97 61.595) (end 140.97 50.8) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 140.335 61.595) (end 140.335 62.23) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.335 62.23) (end 106.68 62.23) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.68 60.96) (end 105.41 60.96) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.045 49.53) (end 139.7 49.53) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.045 50.165) (end 106.045 49.53) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 139.7 50.8) (end 140.97 50.8) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "Flex Touch Test with Teardrop\n2019-12-09\nDrew Fustini + @HelenLeigh\nhttps://github.com/pdp7/flextouch" (at 122.682 56.642) (layer B.SilkS))
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.606023 55.55742) (xy 114.573031 55.557041) (xy 114.540402 55.555904) (xy 114.508137 55.55401) (xy 114.476234 55.551358)
        (xy 114.444695 55.547948) (xy 114.413518 55.54378) (xy 114.382705 55.538854) (xy 114.352254 55.533171) (xy 114.322167 55.52673)
        (xy 114.292442 55.519531) (xy 114.263081 55.511574) (xy 114.234082 55.50286) (xy 114.205447 55.493388) (xy 114.177174 55.483158)
        (xy 114.149265 55.47217) (xy 114.121718 55.460424) (xy 114.094534 55.447921) (xy 114.067714 55.43466) (xy 114.041256 55.420641)
        (xy 114.015162 55.405864) (xy 113.98943 55.39033) (xy 113.964061 55.374038) (xy 113.939056 55.356988) (xy 113.914413 55.33918)
        (xy 113.890134 55.320614) (xy 113.866217 55.301291) (xy 113.842663 55.28121) (xy 113.819473 55.260371) (xy 113.796645 55.238774)
        (xy 113.774181 55.21642) (xy 112.74216 55.81142) (xy 113.774181 56.40642) (xy 113.796645 56.384065) (xy 113.819473 56.362468)
        (xy 113.842663 56.341629) (xy 113.866217 56.321548) (xy 113.890134 56.302225) (xy 113.914413 56.283659) (xy 113.939056 56.265851)
        (xy 113.964061 56.248801) (xy 113.98943 56.232509) (xy 114.015162 56.216975) (xy 114.041256 56.202198) (xy 114.067714 56.188179)
        (xy 114.094534 56.174918) (xy 114.121718 56.162415) (xy 114.149265 56.150669) (xy 114.177174 56.139681) (xy 114.205447 56.129451)
        (xy 114.234082 56.119979) (xy 114.263081 56.111265) (xy 114.292442 56.103308) (xy 114.322167 56.096109) (xy 114.352254 56.089668)
        (xy 114.382705 56.083985) (xy 114.413518 56.079059) (xy 114.444695 56.074891) (xy 114.476234 56.071481) (xy 114.508137 56.068829)
        (xy 114.540402 56.066935) (xy 114.573031 56.065798) (xy 114.606023 56.06542)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.144427 56.06542) (xy 123.459921 56.072523) (xy 123.771911 56.086721) (xy 124.080397 56.108014) (xy 124.385379 56.136402)
        (xy 124.686856 56.171884) (xy 124.984828 56.214462) (xy 125.279296 56.264134) (xy 125.57026 56.320901) (xy 125.857719 56.384762)
        (xy 126.141674 56.455719) (xy 126.422125 56.53377) (xy 126.699071 56.618917) (xy 126.972513 56.711158) (xy 127.24245 56.810493)
        (xy 127.508883 56.916924) (xy 127.771811 57.030449) (xy 128.031235 57.15107) (xy 128.287155 57.278785) (xy 128.53957 57.413594)
        (xy 128.788481 57.555499) (xy 129.033887 57.704498) (xy 129.275789 57.860593) (xy 129.514187 58.023782) (xy 129.74908 58.194066)
        (xy 129.980468 58.371444) (xy 130.208353 58.555918) (xy 130.432732 58.747486) (xy 130.653608 58.946149) (xy 130.870979 59.151907)
        (xy 131.084846 59.36476) (xy 137.15556 55.86476) (xy 131.084846 52.36476) (xy 130.870979 52.577494) (xy 130.653608 52.782896)
        (xy 130.432732 52.980966) (xy 130.208353 53.171705) (xy 129.980468 53.355111) (xy 129.74908 53.531186) (xy 129.514187 53.699929)
        (xy 129.275789 53.86134) (xy 129.033887 54.015419) (xy 128.788481 54.162167) (xy 128.53957 54.301582) (xy 128.287155 54.433666)
        (xy 128.031235 54.558417) (xy 127.771811 54.675837) (xy 127.508883 54.785925) (xy 127.24245 54.888681) (xy 126.972513 54.984105)
        (xy 126.699071 55.072198) (xy 126.422125 55.152958) (xy 126.141674 55.226387) (xy 125.857719 55.292483) (xy 125.57026 55.351248)
        (xy 125.279296 55.402681) (xy 124.984828 55.446782) (xy 124.686856 55.483551) (xy 124.385379 55.512989) (xy 124.080397 55.535094)
        (xy 123.771911 55.549868) (xy 123.459921 55.55731) (xy 123.144427 55.55742)
      )
    )
  )
)
