(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 27)
    (tracks 57)
    (zones 0)
    (modules 8)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.8 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 Tach1)
  (net 4 "Net-(J1-Pad4)")
  (net 5 Tach2)
  (net 6 Tach3)
  (net 7 "Net-(J4-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J4-Pad4)")
    (add_net Tach1)
    (add_net Tach2)
    (add_net Tach3)
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 152.4 128.27)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.5) (layer Cmts.User))
    (fp_text value MountingHole (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 114.3 128.27)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.5) (layer Cmts.User))
    (fp_text value MountingHole (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Connector_Molex:4_pin_fan_header.-.Molex-470531000 (layer F.Cu) (tedit 5FAC016D)
    (at 143.51 116.84)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (fp_text reference J1 (at -2.54 -0.508 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 3 Tach1))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad "" thru_hole circle (at 5.08 -2.54) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:4_pin_fan_header.-.Molex-470531000 (layer F.Cu) (tedit 5FAC016D)
    (at 129.54 116.84)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (fp_text reference J2 (at -2.54 -0.508 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad "" thru_hole circle (at 5.08 -2.54) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 5 Tach2))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:4_pin_fan_header.-.Molex-470531000 (layer F.Cu) (tedit 5FAC016D)
    (at 115.57 116.84)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-04A example for new part number: 22-27-2041, 4 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (fp_text reference J3 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 3.81 4.08) (layer F.Fab))
    (fp_text user %R (at 3.81 -2.22) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 6 Tach3))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad "" thru_hole circle (at 5.08 -2.54) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-04A_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Mate-N-Lok:641737-1 (layer F.Cu) (tedit 0)
    (at 125.73 128.27)
    (fp_text reference J4 (at 7.62 0) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 7.62 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at 10.16 0) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 4 thru_hole circle (at 15.24 0) (size 2.286 2.286) (drill 1.524) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad4)"))
    (pad 5 thru_hole circle (at -2.54 2.54) (size 2.794 2.794) (drill 2.54) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 17.78 2.54) (size 2.794 2.794) (drill 2.54) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 2.54 10.16) (size 4.572 4.572) (drill 4.064) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 12.7 10.16) (size 4.572 4.572) (drill 4.064) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 149.86 138.43 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Tach1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 116.84 138.43 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Tach1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 Tach2))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 Tach3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 2020 (at 132.461 124.079) (layer B.SilkS))
  (gr_text "Project: OVERKILL" (at 132.08 120.396) (layer B.SilkS))
  (gr_text R (at 140.97 131.064) (layer F.SilkS))
  (gr_text BK (at 135.89 131.064) (layer F.SilkS))
  (gr_text BK (at 130.81 131.064) (layer F.SilkS))
  (gr_text Y (at 125.73 131.064) (layer F.SilkS))
  (gr_line (start 154.813 124.079) (end 154.813 113.03) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.607 126.873) (end 154.813 124.079) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 111.76 124.206) (end 111.76 113.03) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.093 126.873) (end 111.76 124.206) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.813 113.03) (end 133.985 113.03) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.607 141.351) (end 157.607 126.873) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.093 141.351) (end 157.607 141.351) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.093 126.873) (end 109.093 141.351) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.985 113.03) (end 111.76 113.03) (layer Edge.Cuts) (width 0.05))
  (gr_text RPM3 (at 111.887 134.366 90) (layer F.SilkS))
  (gr_text RPM2 (at 114.3 134.366 90) (layer F.SilkS))
  (gr_text RPM1 (at 116.84 134.366 90) (layer F.SilkS))
  (gr_text PWM (at 152.654 134.62 270) (layer F.SilkS))
  (gr_text RPM (at 149.606 134.366 270) (layer F.SilkS))
  (gr_text "Fan 3" (at 119.126 121.158) (layer F.SilkS))
  (gr_text "Fan 2" (at 133.096 121.158) (layer F.SilkS))
  (gr_text "Fan 1" (at 146.812 121.158) (layer F.SilkS))
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer B.Cu) (hatch full 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 137.414 129.794) (xy 129.286 129.794) (xy 129.286 126.746) (xy 137.414 126.746)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer B.Cu) (hatch full 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 147.32 124.968) (xy 144.78 124.968) (xy 144.78 115.316) (xy 147.32 115.316)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer B.Cu) (hatch full 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 133.35 123.698) (xy 130.81 123.698) (xy 130.81 115.57) (xy 133.35 115.57)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer B.Cu) (hatch full 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 119.38 124.46) (xy 116.84 124.46) (xy 116.84 115.316) (xy 119.38 115.316)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer B.Cu) (hatch full 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 147.32 125.984) (xy 128.016 125.984) (xy 127.254 126.746) (xy 127.254 128.778) (xy 126.238 130.302)
        (xy 125.222 130.302) (xy 123.952 128.778) (xy 123.952 127.254) (xy 122.936 126.238) (xy 118.618 126.238)
        (xy 116.84 124.714) (xy 116.84 122.174) (xy 147.32 122.174)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer B.Cu) (hatch full 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 120.396 122.174) (xy 129.794 122.174) (xy 130.81 121.158) (xy 133.35 121.158) (xy 134.62 122.174)
        (xy 143.764 122.174) (xy 144.78 121.158) (xy 146.812 121.158) (xy 146.812 124.46) (xy 117.602 124.46)
        (xy 117.602 121.158) (xy 119.38 121.158)
      )
    )
  )
)
