(kicad_pcb (version 4) (host pcbnew "(2014-10-14 BZR 5188)-product")
  (general
    (links 174)
    (no_connects 0)
    (area 89.809499 83.809499 112.690501 96.190501)
    (thickness 1.6002)
    (drawings 20)
    (tracks 718)
    (zones 0)
    (modules 62)
    (nets 64)
  )
  (page A4)
  (title_block
    (date "28 jun 2014")
  )
  (layers
    (0 C1F signal)
    (1 C2 signal)
    (2 C3 signal)
    (31 C4B signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.2286)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.127)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2032)
    (edge_width 0.381)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (user_via 0.7874 0.4064)
    (user_via 0.9398 0.508)
    (user_via 1.0668 0.635)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.1905)
    (pcb_text_size 0.762 1.016)
    (mod_edge_width 0.2032)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 0.74 0.7)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0762)
    (pad_to_paste_clearance_ratio -0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 /DC)
  (net 2 /DD)
  (net 3 /RESET_N)
  (net 4 /SHIELD)
  (net 5 /USBDM_DN2)
  (net 6 /USBDP_DN2)
  (net 7 /VBUS)
  (net 8 3V3)
  (net 9 GND)
  (net 10 "Net-(C1-Pad2)")
  (net 11 "Net-(C6-Pad2)")
  (net 12 "Net-(C6-Pad1)")
  (net 13 "Net-(C7-Pad1)")
  (net 14 "Net-(C10-Pad1)")
  (net 15 "Net-(C11-Pad1)")
  (net 16 "Net-(C15-Pad2)")
  (net 17 "Net-(C16-Pad2)")
  (net 18 "Net-(C21-Pad1)")
  (net 19 "Net-(C26-Pad1)")
  (net 20 "Net-(FB1-Pad2)")
  (net 21 "Net-(J1-Pad2)")
  (net 22 "Net-(J1-Pad3)")
  (net 23 "Net-(R2-Pad1)")
  (net 24 "Net-(R4-Pad1)")
  (net 25 "Net-(R9-Pad1)")
  (net 26 "Net-(R10-Pad2)")
  (net 27 "Net-(R11-Pad2)")
  (net 28 "Net-(R14-Pad1)")
  (net 29 "Net-(R15-Pad1)")
  (net 30 "Net-(T1-Pad3)")
  (net 31 "Net-(T1-Pad4)")
  (net 32 "Net-(R17-Pad1)")
  (net 33 "Net-(R17-Pad2)")
  (net 34 "Net-(U3-Pad7)")
  (net 35 "Net-(U3-Pad8)")
  (net 36 "Net-(R5-Pad1)")
  (net 37 "Net-(U1-Pad1)")
  (net 38 "Net-(U1-Pad5)")
  (net 39 "Net-(U1-Pad6)")
  (net 40 "Net-(U1-Pad7)")
  (net 41 "Net-(U1-Pad8)")
  (net 42 "Net-(U1-Pad9)")
  (net 43 "Net-(U1-Pad13)")
  (net 44 "Net-(U1-Pad14)")
  (net 45 "Net-(U1-Pad17)")
  (net 46 "Net-(U1-Pad18)")
  (net 47 "Net-(U1-Pad32)")
  (net 48 "Net-(U1-Pad33)")
  (net 49 "Net-(U1-Pad34)")
  (net 50 "Net-(U1-Pad35)")
  (net 51 "Net-(U1-Pad36)")
  (net 52 "Net-(U3-Pad5)")
  (net 53 "Net-(U3-Pad6)")
  (net 54 "Net-(U3-Pad9)")
  (net 55 "Net-(U3-Pad11)")
  (net 56 "Net-(U3-Pad12)")
  (net 57 "Net-(U3-Pad25)")
  (net 58 "Net-(U4-Pad6)")
  (net 59 "Net-(U5-Pad1)")
  (net 60 "Net-(U5-Pad3)")
  (net 61 "Net-(R5-Pad2)")
  (net 62 "Net-(D1-Pad1)")
  (net 63 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /DC)
    (add_net /DD)
    (add_net /RESET_N)
    (add_net /SHIELD)
    (add_net /USBDM_DN2)
    (add_net /USBDP_DN2)
    (add_net /VBUS)
    (add_net 3V3)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(FB1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(T1-Pad3)")
    (add_net "Net-(T1-Pad4)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad25)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad9)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad3)")
  )
  (module cc1111-legacy:GSG-SOT553 (layer C1F) (tedit 54C7D34C)
    (at 97.45 85.11 270)
    (fp_text reference U5 (at 0.21 -0.03 270) (layer F.SilkS))
    (fp_text value AH1806 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.50038 0.8509 270) (size 0.32004 0.50038) (layers C1F F.Paste F.Mask)
      (net 59 "Net-(U5-Pad1)") (die_length 0.08382))
    (pad 2 smd rect (at 0 0.8509 270) (size 0.32004 0.50038) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648))
    (pad 3 smd rect (at 0.50038 0.8509 270) (size 0.32004 0.50038) (layers C1F F.Paste F.Mask)
      (net 60 "Net-(U5-Pad3)") (die_length -2147.483648))
    (pad 4 smd rect (at 0.50038 -0.8509 270) (size 0.32004 0.50038) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (die_length -2147.483648))
    (pad 5 smd rect (at -0.50038 -0.8509 270) (size 0.32004 0.50038) (layers C1F F.Paste F.Mask)
      (net 1 /DC) (die_length 0.1651))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D0A7)
    (at 97.49 86.51 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C28 (at 0 -0.03 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D112)
    (at 105.3 85.2 270)
    (solder_mask_margin 0.1016)
    (fp_text reference C1 (at -0.01 -0.02 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 0.0508 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 10 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D115)
    (at 106.4 85.2 90)
    (solder_mask_margin 0.1016)
    (fp_text reference C2 (at 0 0.02 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D0FE)
    (at 99.91 88.15)
    (solder_mask_margin 0.1016)
    (fp_text reference C3 (at 0 0.02) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D21F)
    (at 109.6 89.2 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C4 (at 0 -0.02 180) (layer B.SilkS))
    (fp_text value 220pF (at 0 0.0508 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 8 3V3) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D222)
    (at 109.42 88.4 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C5 (at -0.01 -0.02 180) (layer B.SilkS))
    (fp_text value 10nF (at 0 0.0508 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 8 3V3) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D135)
    (at 110 87.5 270)
    (solder_mask_margin 0.1016)
    (fp_text reference C6 (at 0 -0.02 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 0.0508 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 11 "Net-(C6-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 12 "Net-(C6-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D130)
    (at 109.1 87.5 90)
    (solder_mask_margin 0.1016)
    (fp_text reference C7 (at 0 0.03 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 13 "Net-(C7-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D154)
    (at 107.7 94.1)
    (solder_mask_margin 0.1016)
    (fp_text reference C8 (at 0 0.02) (layer F.SilkS))
    (fp_text value 10nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D149)
    (at 109.6 90.7 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C9 (at 0 -0.02 180) (layer F.SilkS))
    (fp_text value 2p2 (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D158)
    (at 108.4 94.9 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C10 (at 0 -0.03 180) (layer F.SilkS))
    (fp_text value 22pF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 14 "Net-(C10-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D14D)
    (at 109.6 91.5)
    (solder_mask_margin 0.1016)
    (fp_text reference C11 (at 0 0.01) (layer F.SilkS))
    (fp_text value 22pF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 15 "Net-(C11-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D22B)
    (at 104.7 94.6 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C12 (at 0 -0.02 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 8 3V3) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D1B9)
    (at 99.7 85.2 270)
    (solder_mask_margin 0.1016)
    (fp_text reference C13 (at 0 -0.02 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 0.0508 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 7 /VBUS) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D20B)
    (at 104.15 84.7)
    (solder_mask_margin 0.1016)
    (fp_text reference C14 (at 0 0.03) (layer B.SilkS))
    (fp_text value 4u7 (at 0 0.0508) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 8 3V3) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D1AC)
    (at 96.3 87.5 90)
    (solder_mask_margin 0.1016)
    (fp_text reference C15 (at 0 0.02 90) (layer B.SilkS))
    (fp_text value 18pF (at 0 0.0508 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 16 "Net-(C15-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D1EF)
    (at 99.7 87.5 270)
    (solder_mask_margin 0.1016)
    (fp_text reference C16 (at 0 -0.02 270) (layer B.SilkS))
    (fp_text value 18pF (at 0 0.0508 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 17 "Net-(C16-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D196)
    (at 91.6 92.8 90)
    (solder_mask_margin 0.1016)
    (fp_text reference C17 (at 0 0.02 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 0.0508 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 4 /SHIELD) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D0F9)
    (at 98.47 88.97)
    (solder_mask_margin 0.1016)
    (fp_text reference C18 (at 0 0.02) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D1A6)
    (at 91 86.8 90)
    (solder_mask_margin 0.1016)
    (fp_text reference C19 (at 0.01 0.02 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 0.0508 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 7 /VBUS) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D0C3)
    (at 96.7 90)
    (solder_mask_margin 0.1016)
    (fp_text reference C20 (at 0 0.02) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D0B9)
    (at 96.7 92.7)
    (solder_mask_margin 0.1016)
    (fp_text reference C21 (at 0 0.02) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 18 "Net-(C21-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D165)
    (at 100.73 93.13 270)
    (solder_mask_margin 0.1016)
    (fp_text reference C22 (at 0 -0.02 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D0B0)
    (at 96.8 94.9 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C23 (at 0 -0.02 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D160)
    (at 99.73 95.3)
    (solder_mask_margin 0.1016)
    (fp_text reference C24 (at 0 0.02) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D22F)
    (at 104.9 92.7)
    (solder_mask_margin 0.1016)
    (fp_text reference C25 (at 0 0.02) (layer B.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 7 /VBUS) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D21A)
    (at 107.4 89.8 90)
    (solder_mask_margin 0.1016)
    (fp_text reference C26 (at 0 0.02 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 0.0508 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 19 "Net-(C26-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0805 (layer C4B) (tedit 50998367)
    (at 109.5 92.3 270)
    (solder_mask_margin 0.1016)
    (fp_text reference C27 (at 0 0 270) (layer B.SilkS))
    (fp_text value 47uF (at 0 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 1.016 0 270) (size 1.15062 1.44018) (layers C4B B.Paste B.Mask)
      (net 9 GND) (die_length 0.08128) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -1.016 0 270) (size 1.15062 1.44018) (layers C4B B.Paste B.Mask)
      (net 19 "Net-(C26-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module cc1111-legacy:GSG-0805 (layer C4B) (tedit 50998367)
    (at 91.3 89.8 270)
    (solder_mask_margin 0.1016)
    (fp_text reference FB1 (at 0 0 270) (layer B.SilkS))
    (fp_text value FILTER (at 0 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 1.016 0 270) (size 1.15062 1.44018) (layers C4B B.Paste B.Mask)
      (net 20 "Net-(FB1-Pad2)") (die_length 0.08128) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -1.016 0 270) (size 1.15062 1.44018) (layers C4B B.Paste B.Mask)
      (net 7 /VBUS) (die_length -2147.483648) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module cc1111-legacy:GSG-USB-A-1001-010-01001-SHIELD (layer C1F) (tedit 54C7D338)
    (at 90 90 270)
    (fp_text reference J1 (at 0.05 -2.9 270) (layer F.SilkS))
    (fp_text value USB-DEVICE-SHIELD (at 0 -2.99974 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.50012 -5.00126 270) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(FB1-Pad2)"))
    (pad 2 thru_hole circle (at 1.00076 -5.00126 270) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -1.00076 -5.00126 270) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -3.50012 -5.00126 270) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad "" thru_hole circle (at 2.30124 -2.90068 270) (size 1.30048 1.30048) (drill 1.30048) (layers *.Cu *.Mask)
      (clearance -0.09906))
    (pad "" thru_hole circle (at -2.30124 -2.90068 270) (size 1.30048 1.30048) (drill 1.30048) (layers *.Cu *.Mask)
      (clearance -0.09906))
    (pad 5 thru_hole circle (at 5.69976 -2.90068 270) (size 3.50012 3.50012) (drill 2.49936) (layers *.Cu *.Mask)
      (net 4 /SHIELD))
    (pad 5 thru_hole circle (at -5.69976 -2.90068 270) (size 3.50012 3.50012) (drill 2.49936) (layers *.Cu *.Mask)
      (net 4 /SHIELD))
  )
  (module cc1111-legacy:GSG-50MIL-HEADER-1x1-TH (layer C1F) (tedit 54C7D36B)
    (at 109.4 85.8)
    (fp_text reference P1 (at -0.05 0.08) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 12 "Net-(C6-Pad1)") (die_length 0.04318))
  )
  (module cc1111-legacy:GSG-TESTPOINT-50MIL (layer C4B) (tedit 53AA93E1)
    (at 104.74 86.25)
    (fp_text reference P2 (at 0 0) (layer B.SilkS))
    (fp_text value RESET_N (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 3 /RESET_N) (die_length 0.1651))
  )
  (module cc1111-legacy:GSG-TESTPOINT-50MIL (layer C4B) (tedit 53AA93E1)
    (at 106.3 94.7)
    (fp_text reference P3 (at 0 0) (layer B.SilkS))
    (fp_text value DD (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 2 /DD) (die_length 0.1651))
  )
  (module cc1111-legacy:GSG-TESTPOINT-50MIL (layer C4B) (tedit 53AA93E1)
    (at 98 85)
    (fp_text reference P4 (at 0 0) (layer B.SilkS))
    (fp_text value DC (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 1 /DC) (die_length 0.1651))
  )
  (module cc1111-legacy:GSG-TESTPOINT-50MIL (layer C4B) (tedit 53AA93E1)
    (at 107.55 86.25)
    (fp_text reference P5 (at 0 0) (layer B.SilkS))
    (fp_text value 3V3 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 8 3V3) (die_length 0.1651))
  )
  (module cc1111-legacy:GSG-TESTPOINT-50MIL (layer C4B) (tedit 53AA93E1)
    (at 95.5 85)
    (fp_text reference P6 (at 0 0) (layer B.SilkS))
    (fp_text value GND (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 9 GND) (die_length 0.1651))
  )
  (module cc1111-legacy:GSG-50MIL-HEADER-1x5-TH (layer C1F) (tedit 54C7D370)
    (at 111.8 90 270)
    (fp_text reference P7 (at 0 0.18 270) (layer F.SilkS))
    (fp_text value CABLE (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0.635 270) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 /USBDM_DN2))
    (pad 2 thru_hole circle (at -1.27 0.635 270) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 6 /USBDP_DN2))
    (pad 3 thru_hole circle (at 0 0.635 270) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 4 thru_hole circle (at 1.27 0.635 270) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 19 "Net-(C26-Pad1)"))
    (pad 5 thru_hole circle (at 2.54 0.635 270) (size 1.0668 1.0668) (drill 0.7112) (layers *.Cu *.Mask)
      (net 4 /SHIELD))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D10B)
    (at 104.2 85.2 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R1 (at 0 0.02 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 3 /RESET_N) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D119)
    (at 107.5 85.4 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R2 (at 0 0.02 90) (layer F.SilkS))
    (fp_text value 56k (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 23 "Net-(R2-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D239)
    (at 102.65 93.4 270)
    (solder_mask_margin 0.1016)
    (fp_text reference R4 (at 0 -0.02 270) (layer B.SilkS))
    (fp_text value 33 (at 0 0.0508 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 32 "Net-(R17-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 24 "Net-(R4-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D234)
    (at 103.45 93.4 270)
    (solder_mask_margin 0.1016)
    (fp_text reference R5 (at 0 -0.02 270) (layer B.SilkS))
    (fp_text value 33 (at 0 0.0508 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 61 "Net-(R5-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 36 "Net-(R5-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D105)
    (at 100.3 84.8 180)
    (solder_mask_margin 0.1016)
    (fp_text reference R6 (at 0 -0.02 180) (layer F.SilkS))
    (fp_text value 100k (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 /DC) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 3V3) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D19B)
    (at 90.8 92.8 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R7 (at 0 0.02 90) (layer B.SilkS))
    (fp_text value 330 (at 0 0.0508 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 4 /SHIELD) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D1B0)
    (at 98 86.1)
    (solder_mask_margin 0.1016)
    (fp_text reference R8 (at 0 0.03) (layer B.SilkS))
    (fp_text value 1M (at 0 0.0508) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 17 "Net-(C16-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 16 "Net-(C15-Pad2)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D1F3)
    (at 100.5 87.5 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R9 (at 0 0.02 90) (layer B.SilkS))
    (fp_text value 12k (at 0 0.0508 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 25 "Net-(R9-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D17F)
    (at 93.2 89)
    (solder_mask_margin 0.1016)
    (fp_text reference R10 (at 0 0.01) (layer B.SilkS))
    (fp_text value 100k (at 0 0.0508) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 26 "Net-(R10-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 7 /VBUS) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D0BE)
    (at 96.7 91.9 180)
    (solder_mask_margin 0.1016)
    (fp_text reference R11 (at 0 -0.02 180) (layer F.SilkS))
    (fp_text value 50k (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 27 "Net-(R11-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D184)
    (at 93.2 89.8 180)
    (solder_mask_margin 0.1016)
    (fp_text reference R12 (at 0 -0.02 180) (layer B.SilkS))
    (fp_text value 100k (at 0 0.0508 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 26 "Net-(R10-Pad2)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D188)
    (at 93.2 91.1)
    (solder_mask_margin 0.1016)
    (fp_text reference R13 (at 0 0.02) (layer B.SilkS))
    (fp_text value 100k (at 0 0.0508) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 18 "Net-(C21-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 8 3V3) (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D191)
    (at 93.1 93.4 180)
    (solder_mask_margin 0.1016)
    (fp_text reference R14 (at 0 -0.03 180) (layer B.SilkS))
    (fp_text value 100k (at 0 0.0508 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 28 "Net-(R14-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D0B4)
    (at 96.8 93.7 180)
    (solder_mask_margin 0.1016)
    (fp_text reference R15 (at 0 -0.03 180) (layer F.SilkS))
    (fp_text value 50k (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 29 "Net-(R15-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-B0310J50100AHF (layer C1F) (tedit 54C7D13D)
    (at 109.5 89.5)
    (fp_text reference T1 (at 0 0) (layer F.SilkS))
    (fp_text value BALUN (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.6604 -0.4953) (size 0.40894 0.3302) (layers C1F F.Paste F.Mask)
      (net 11 "Net-(C6-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 0 -0.4953) (size 0.40894 0.3302) (layers C1F F.Paste F.Mask)
      (net 13 "Net-(C7-Pad1)") (die_length -2147.483648))
    (pad 3 smd rect (at -0.6604 -0.4953) (size 0.40894 0.3302) (layers C1F F.Paste F.Mask)
      (net 30 "Net-(T1-Pad3)") (die_length -2147.483648))
    (pad 4 smd rect (at -0.6604 0.4953) (size 0.40894 0.3302) (layers C1F F.Paste F.Mask)
      (net 31 "Net-(T1-Pad4)") (die_length 0.01524))
    (pad 5 smd rect (at 0 0.4953) (size 0.40894 0.3302) (layers C1F F.Paste F.Mask))
    (pad 6 smd rect (at 0.6604 0.4953) (size 0.40894 0.3302) (layers C1F F.Paste F.Mask)
      (die_length 0.08128))
  )
  (module cc1111-legacy:GSG-QFN36 (layer C1F) (tedit 50C67CFC)
    (at 104.5 90)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value CC1111 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd oval (at -2.90068 -1.99898) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 37 "Net-(U1-Pad1)"))
    (pad 2 smd oval (at -2.90068 -1.50114) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 8 3V3))
    (pad 3 smd oval (at -2.90068 -1.00076) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 63 "Net-(R3-Pad1)"))
    (pad 4 smd oval (at -2.90068 -0.50038) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 33 "Net-(R17-Pad2)"))
    (pad 5 smd oval (at -2.90068 0) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 38 "Net-(U1-Pad5)"))
    (pad 6 smd oval (at -2.90068 0.50038) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 39 "Net-(U1-Pad6)"))
    (pad 7 smd oval (at -2.90068 1.00076) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 40 "Net-(U1-Pad7)"))
    (pad 8 smd oval (at -2.90068 1.50114) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 41 "Net-(U1-Pad8)"))
    (pad 9 smd oval (at -2.90068 1.99898) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 42 "Net-(U1-Pad9)"))
    (pad 10 smd oval (at -1.99898 2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 32 "Net-(R17-Pad1)"))
    (pad 11 smd oval (at -1.50114 2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 61 "Net-(R5-Pad2)"))
    (pad 12 smd oval (at -1.00076 2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 8 3V3))
    (pad 13 smd oval (at -0.50038 2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 43 "Net-(U1-Pad13)"))
    (pad 14 smd oval (at 0 2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 44 "Net-(U1-Pad14)"))
    (pad 15 smd oval (at 0.50038 2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 2 /DD))
    (pad 16 smd oval (at 1.00076 2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 1 /DC))
    (pad 17 smd oval (at 1.50114 2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 45 "Net-(U1-Pad17)"))
    (pad 18 smd oval (at 1.99898 2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 46 "Net-(U1-Pad18)"))
    (pad 19 smd oval (at 2.90068 1.99898) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 8 3V3))
    (pad 20 smd oval (at 2.90068 1.50114) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 14 "Net-(C10-Pad1)"))
    (pad 21 smd oval (at 2.90068 1.00076) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 15 "Net-(C11-Pad1)"))
    (pad 22 smd oval (at 2.90068 0.50038) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 8 3V3))
    (pad 23 smd oval (at 2.90068 0) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 31 "Net-(T1-Pad4)"))
    (pad 24 smd oval (at 2.90068 -0.50038) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 30 "Net-(T1-Pad3)"))
    (pad 25 smd oval (at 2.90068 -1.00076) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 8 3V3))
    (pad 26 smd oval (at 2.90068 -1.50114) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 8 3V3))
    (pad 27 smd oval (at 2.90068 -1.99898) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 23 "Net-(R2-Pad1)"))
    (pad 28 smd oval (at 1.99898 -2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 8 3V3))
    (pad 29 smd oval (at 1.50114 -2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 8 3V3))
    (pad 30 smd oval (at 1.00076 -2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 10 "Net-(C1-Pad2)"))
    (pad 31 smd oval (at 0.50038 -2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 3 /RESET_N))
    (pad 32 smd oval (at 0 -2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 47 "Net-(U1-Pad32)"))
    (pad 33 smd oval (at -0.50038 -2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 48 "Net-(U1-Pad33)"))
    (pad 34 smd oval (at -1.00076 -2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 49 "Net-(U1-Pad34)"))
    (pad 35 smd oval (at -1.50114 -2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 50 "Net-(U1-Pad35)"))
    (pad 36 smd oval (at -1.99898 -2.90068 90) (size 1.00076 0.2794) (layers C1F F.Paste F.Mask)
      (net 51 "Net-(U1-Pad36)"))
    (pad 0 smd rect (at 0 0) (size 1.47066 1.47066) (layers C1F F.Paste F.Mask)
      (net 9 GND))
    (pad 0 smd rect (at 1.4605 0) (size 1.47066 1.47066) (layers C1F F.Paste F.Mask)
      (net 9 GND))
    (pad 0 smd rect (at -1.4605 0) (size 1.47066 1.47066) (layers C1F F.Paste F.Mask)
      (net 9 GND))
    (pad 0 smd rect (at 0 -1.4605) (size 1.47066 1.47066) (layers C1F F.Paste F.Mask)
      (net 9 GND))
    (pad 0 smd rect (at 0 1.4605) (size 1.47066 1.47066) (layers C1F F.Paste F.Mask)
      (net 9 GND))
    (pad 0 smd rect (at 1.4605 -1.4605) (size 1.47066 1.47066) (layers C1F F.Paste F.Mask)
      (net 9 GND))
    (pad 0 smd rect (at -1.4605 -1.4605) (size 1.47066 1.47066) (layers C1F F.Paste F.Mask)
      (net 9 GND))
    (pad 0 smd rect (at -1.4605 1.4605) (size 1.47066 1.47066) (layers C1F F.Paste F.Mask)
      (net 9 GND))
    (pad 0 smd rect (at 1.4605 1.4605) (size 1.47066 1.47066) (layers C1F F.Paste F.Mask)
      (net 9 GND))
    (pad 0 thru_hole circle (at 1.4605 -1.4605) (size 0.635 0.635) (drill 0.381) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 0 thru_hole circle (at 0 -1.4605) (size 0.635 0.635) (drill 0.381) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 0 thru_hole circle (at -1.4605 -1.4605) (size 0.635 0.635) (drill 0.381) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 0 thru_hole circle (at -1.4605 0) (size 0.635 0.635) (drill 0.381) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 0 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.381) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 0 thru_hole circle (at 1.4605 0) (size 0.635 0.635) (drill 0.381) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 0 thru_hole circle (at -1.4605 1.4605) (size 0.635 0.635) (drill 0.381) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 0 thru_hole circle (at 0 1.4605) (size 0.635 0.635) (drill 0.381) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 0 thru_hole circle (at 1.4605 1.4605) (size 0.635 0.635) (drill 0.381) (layers *.Cu *.Mask)
      (net 9 GND))
  )
  (module cc1111-legacy:GSG-SOT23-3 (layer C4B) (tedit 54C7D202)
    (at 101.76 85.81 180)
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 0.96 180) (layer B.SilkS))
    (fp_text value AP7313 (at 0 0 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at -0.889 1.016 180) (size 0.9144 0.9144) (layers C4B B.Paste B.Mask)
      (net 8 3V3) (die_length 0.00762))
    (pad 1 smd rect (at 0.889 1.016 180) (size 0.9144 0.9144) (layers C4B B.Paste B.Mask)
      (net 7 /VBUS))
    (pad 3 smd rect (at 0 -1.016 180) (size 0.9144 0.9144) (layers C4B B.Paste B.Mask)
      (net 9 GND) (die_length 0.28194))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module cc1111-legacy:GSG-QFN28 (layer C4B) (tedit 54C7D245)
    (at 99 92 180)
    (fp_text reference U3 (at 0 0 180) (layer B.SilkS))
    (fp_text value USB2412 (at 0 0 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -2.21 1.5 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 6 /USBDP_DN2))
    (pad 2 smd oval (at -2.21 1 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 36 "Net-(R5-Pad1)"))
    (pad 3 smd oval (at -2.21 0.5 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 24 "Net-(R4-Pad1)"))
    (pad 4 smd oval (at -2.21 0 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 8 3V3))
    (pad 5 smd oval (at -2.21 -0.5 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 52 "Net-(U3-Pad5)"))
    (pad 6 smd oval (at -2.21 -1 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 53 "Net-(U3-Pad6)"))
    (pad 7 smd oval (at -2.21 -1.5 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 34 "Net-(U3-Pad7)"))
    (pad 8 smd oval (at -1.5 -2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 35 "Net-(U3-Pad8)"))
    (pad 9 smd oval (at -1 -2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 54 "Net-(U3-Pad9)"))
    (pad 10 smd oval (at -0.5 -2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 8 3V3))
    (pad 11 smd oval (at 0 -2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 55 "Net-(U3-Pad11)"))
    (pad 12 smd oval (at 0.5 -2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 56 "Net-(U3-Pad12)"))
    (pad 13 smd oval (at 1 -2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 29 "Net-(R15-Pad1)"))
    (pad 14 smd oval (at 1.5 -2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 8 3V3))
    (pad 15 smd oval (at 2.21 -1.5 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 9 GND))
    (pad 16 smd oval (at 2.21 -1 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 28 "Net-(R14-Pad1)"))
    (pad 17 smd oval (at 2.21 -0.5 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 18 "Net-(C21-Pad1)"))
    (pad 18 smd oval (at 2.21 0 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 26 "Net-(R10-Pad2)"))
    (pad 19 smd oval (at 2.21 0.5 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 27 "Net-(R11-Pad2)"))
    (pad 20 smd oval (at 2.21 1 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 8 3V3))
    (pad 21 smd oval (at 2.21 1.5 180) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 21 "Net-(J1-Pad2)"))
    (pad 22 smd oval (at 1.5 2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 22 "Net-(J1-Pad3)"))
    (pad 23 smd oval (at 1 2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 16 "Net-(C15-Pad2)"))
    (pad 24 smd oval (at 0.5 2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 17 "Net-(C16-Pad2)"))
    (pad 25 smd oval (at 0 2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 57 "Net-(U3-Pad25)"))
    (pad 26 smd oval (at -0.5 2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 25 "Net-(R9-Pad1)"))
    (pad 27 smd oval (at -1 2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 8 3V3))
    (pad 28 smd oval (at -1.5 2.21 90) (size 0.89 0.28) (layers C4B B.Paste B.Mask)
      (net 5 /USBDM_DN2))
    (pad 0 smd rect (at 0 0 90) (size 3.1 3.1) (layers C4B B.Mask)
      (net 9 GND))
    (pad 0 smd rect (at -1 1 90) (size 1 1) (layers C4B B.Paste)
      (net 9 GND))
    (pad 0 smd rect (at 0 1 90) (size 1 1) (layers C4B B.Paste)
      (net 9 GND))
    (pad 0 smd rect (at 1 1 90) (size 1 1) (layers C4B B.Paste)
      (net 9 GND))
    (pad 0 smd rect (at -1 0 90) (size 1 1) (layers C4B B.Paste)
      (net 9 GND))
    (pad 0 smd rect (at 0 0 90) (size 1 1) (layers C4B B.Paste)
      (net 9 GND))
    (pad 0 smd rect (at 1 0 90) (size 1 1) (layers C4B B.Paste)
      (net 9 GND))
    (pad 0 smd rect (at -1 -1 90) (size 1 1) (layers C4B B.Paste)
      (net 9 GND))
    (pad 0 smd rect (at 0 -1 90) (size 1 1) (layers C4B B.Paste)
      (net 9 GND))
    (pad 0 smd rect (at 1 -1 90) (size 1 1) (layers C4B B.Paste)
      (net 9 GND))
    (pad 0 thru_hole circle (at -1 1 90) (size 0.6 0.6) (drill 0.35) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
    (pad 0 thru_hole circle (at 0 1 90) (size 0.6 0.6) (drill 0.35) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
    (pad 0 thru_hole circle (at 1 1 90) (size 0.6 0.6) (drill 0.35) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
    (pad 0 thru_hole circle (at -1 0 90) (size 0.6 0.6) (drill 0.35) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
    (pad 0 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.35) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
    (pad 0 thru_hole circle (at 1 0 90) (size 0.6 0.6) (drill 0.35) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
    (pad 0 thru_hole circle (at -1 -1 90) (size 0.6 0.6) (drill 0.35) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
    (pad 0 thru_hole circle (at 0 -1 90) (size 0.6 0.6) (drill 0.35) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
    (pad 0 thru_hole circle (at 1 -1 90) (size 0.6 0.6) (drill 0.35) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
  )
  (module cc1111-legacy:GSG-U-DFN2020-6 (layer C4B) (tedit 54C7D214)
    (at 107.5 92 90)
    (fp_text reference U4 (at 0 0 90) (layer B.SilkS))
    (fp_text value AP2511SN-7 (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.65 -0.825 90) (size 0.37 0.45) (layers C4B B.Paste B.Mask)
      (net 7 /VBUS))
    (pad 2 smd rect (at 0 -0.625 90) (size 0.37 0.85) (layers C4B B.Paste B.Mask)
      (net 9 GND))
    (pad 3 smd rect (at 0.65 -0.825 90) (size 0.37 0.45) (layers C4B B.Paste B.Mask)
      (net 34 "Net-(U3-Pad7)"))
    (pad 4 smd rect (at 0.65 0.825 90) (size 0.37 0.45) (layers C4B B.Paste B.Mask)
      (net 35 "Net-(U3-Pad8)"))
    (pad 5 smd rect (at 0 0.825 90) (size 0.37 0.45) (layers C4B B.Paste B.Mask)
      (net 19 "Net-(C26-Pad1)"))
    (pad 6 smd rect (at -0.65 0.825 90) (size 0.37 0.45) (layers C4B B.Paste B.Mask)
      (net 58 "Net-(U4-Pad6)"))
    (pad 2 smd rect (at 0 0 90) (size 1.67 0.88) (layers C4B B.Paste B.Mask)
      (net 9 GND))
  )
  (module cc1111-legacy:GSG-XTAL2.0x1.6mm (layer C1F) (tedit 53AF33DE)
    (at 109.6 93.1 90)
    (fp_text reference X1 (at 0 0 90) (layer F.SilkS))
    (fp_text value GSG-XTAL4PIN (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.68 0.5 90) (size 0.74 0.7) (layers C1F F.Paste F.Mask)
      (net 14 "Net-(C10-Pad1)") (die_length 0.08128))
    (pad 3 smd rect (at 0.68 -0.5 90) (size 0.74 0.7) (layers C1F F.Paste F.Mask)
      (net 15 "Net-(C11-Pad1)") (die_length 0.08382))
    (pad 2 smd rect (at 0.68 0.5 90) (size 0.74 0.7) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648))
    (pad 4 smd rect (at -0.68 -0.5 90) (size 0.74 0.7) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length -2147.483648))
  )
  (module cc1111-legacy:GSG-XTAL2.0x1.6mm (layer C4B) (tedit 53AF33DE)
    (at 97.98 87.51)
    (fp_text reference X2 (at 0 0) (layer B.SilkS))
    (fp_text value GSG-XTAL4PIN (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.68 -0.5) (size 0.74 0.7) (layers C4B B.Paste B.Mask)
      (net 16 "Net-(C15-Pad2)") (die_length 0.08128))
    (pad 3 smd rect (at 0.68 0.5) (size 0.74 0.7) (layers C4B B.Paste B.Mask)
      (net 17 "Net-(C16-Pad2)") (die_length 0.08382))
    (pad 2 smd rect (at 0.68 -0.5) (size 0.74 0.7) (layers C4B B.Paste B.Mask)
      (net 9 GND) (die_length -2147.483648))
    (pad 4 smd rect (at -0.68 0.5) (size 0.74 0.7) (layers C4B B.Paste B.Mask)
      (net 9 GND) (die_length -2147.483648))
  )
  (module cc1111-legacy:GSG-0402 (layer C4B) (tedit 54C7D23E)
    (at 102.52 95.15 180)
    (solder_mask_margin 0.1016)
    (fp_text reference R17 (at 0 -0.03 180) (layer B.SilkS))
    (fp_text value 1.5k (at 0 0.0508 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 33 "Net-(R17-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C4B B.Paste B.Mask)
      (net 32 "Net-(R17-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (module cc1111-legacy:GSG-0603D (layer C1F) (tedit 54C7D0A1)
    (at 97.24 87.74 180)
    (solder_mask_margin 0.1016)
    (fp_text reference D1 (at 2.08 -0.01 180) (layer F.SilkS))
    (fp_text value LED1 (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 9 GND) (die_length 0.04572) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 62 "Net-(D1-Pad1)") (die_length 0.08382) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module cc1111-legacy:GSG-0402 (layer C1F) (tedit 54C7D0C8)
    (at 98.9 89.96 180)
    (solder_mask_margin 0.1016)
    (fp_text reference R3 (at 0 0 180) (layer F.SilkS))
    (fp_text value 330 (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 62 "Net-(D1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 63 "Net-(R3-Pad1)") (die_length -2147.483648) (solder_mask_margin 0.1016))
  )
  (gr_text TURNIPSCHOOL (at 104.65 87.8) (layer B.SilkS))
  (gr_text 2015-01-27 (at 90.85 89.64 90) (layer F.SilkS))
  (gr_line (start 112.5 87.5) (end 112.5 92.5) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 109 84) (end 112.5 87.5) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 90 84) (end 109 84) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 109 96) (end 112.5 92.5) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 90 96) (end 109 96) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 90 84) (end 90 96) (angle 90) (layer Edge.Cuts) (width 0.381))
  (zone (net 9) (net_name GND) (layer C2) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 90 84) (xy 90 95) (xy 108.2 95) (xy 110 93.4) (xy 110 91)
        (xy 112.4 91) (xy 112.4 87.4) (xy 109 84)
      )
    )
  )
  (zone (net 8) (net_name 3V3) (layer C3) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 92.1 87.7) (xy 92.1 92.3) (xy 93.7 92.3) (xy 96.4 95) (xy 104.8 95)
        (xy 105.6 94.2) (xy 105.6 93.1) (xy 106.9 93.1) (xy 106.9 96) (xy 109 96)
        (xy 112.5 92.5) (xy 112.5 87.5) (xy 109 84) (xy 102.5 84) (xy 102.5 85.2)
        (xy 97.9 85.2) (xy 95.4 87.7)
      )
    )
  )
  (zone (net 4) (net_name /SHIELD) (layer C1F) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 90 84) (xy 90 96) (xy 95 96) (xy 95 84)
      )
    )
  )
  (zone (net 4) (net_name /SHIELD) (layer C2) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 90 96) (xy 90 95.3) (xy 108.3 95.3) (xy 110.3 93.5) (xy 110.3 91.3)
        (xy 112.5 91.3) (xy 112.5 92.5) (xy 109 96)
      )
    )
  )
  (zone (net 7) (net_name /VBUS) (layer C4B) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 91.4 88) (xy 92.4 88) (xy 92.4 85.9) (xy 91.4 85.9)
      )
    )
  )
  (zone (net 7) (net_name /VBUS) (layer C3) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 90 84) (xy 102.2 84) (xy 102.2 84.9) (xy 97.7 84.9) (xy 95.2 87.4)
        (xy 91.8 87.4) (xy 91.8 92.6) (xy 93.5 92.6) (xy 96.2 95.3) (xy 105 95.3)
        (xy 105.9 94.4) (xy 105.9 93.4) (xy 106.6 93.4) (xy 106.6 96) (xy 90 96)
      )
    )
  )
  (zone (net 8) (net_name 3V3) (layer C4B) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 103.7 85.4) (xy 103.7 86) (xy 101.6 86) (xy 101.6 85.4)
      )
    )
  )
)
