(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (date "mar. 31 mars 2015")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 100 100)
    (grid_origin 100 100)
    (pcbplotparams
      (layerselection 0x0000030_80000001)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "unconnected-(J7-Pad3)")
  (net 3 "unconnected-(J7-Pad4)")
  (net 4 "unconnected-(J7-Pad5)")
  (net 5 "unconnected-(J7-Pad6)")
  (net 6 "unconnected-(J7-Pad7)")
  (net 7 "unconnected-(J7-Pad8)")
  (net 8 "unconnected-(J7-Pad9)")
  (net 9 "unconnected-(J7-Pad10)")
  (net 10 "/*44")
  (net 11 "/*45")
  (net 12 "/42")
  (net 13 "/43")
  (net 14 "/40")
  (net 15 "/41")
  (net 16 "/38")
  (net 17 "/39")
  (net 18 "/36")
  (net 19 "/37")
  (net 20 "/34")
  (net 21 "/35")
  (net 22 "/32")
  (net 23 "/33")
  (net 24 "/30")
  (net 25 "/31")
  (net 26 "/28")
  (net 27 "/29")
  (net 28 "/26")
  (net 29 "/27")
  (net 30 "/24")
  (net 31 "/25")
  (net 32 "/22")
  (net 33 "/23")
  (net 34 "+5V")
  (net 35 "/IOREF")
  (net 36 "/A0")
  (net 37 "/A1")
  (net 38 "/A2")
  (net 39 "/A3")
  (net 40 "/A4")
  (net 41 "/A5")
  (net 42 "/A6")
  (net 43 "/A7")
  (net 44 "/A8")
  (net 45 "/A9")
  (net 46 "/A10")
  (net 47 "/A11")
  (net 48 "/A12")
  (net 49 "/A13")
  (net 50 "/A14")
  (net 51 "/A15")
  (net 52 "/AREF")
  (net 53 "/*13")
  (net 54 "/*12")
  (net 55 "/*11")
  (net 56 "/*10")
  (net 57 "/*9")
  (net 58 "/*8")
  (net 59 "/*7")
  (net 60 "/*6")
  (net 61 "/*5")
  (net 62 "/*4")
  (net 63 "/*3")
  (net 64 "/*2")
  (net 65 "/TX0{slash}1")
  (net 66 "/RX0{slash}0")
  (net 67 "+3V3")
  (net 68 "/TX3{slash}14")
  (net 69 "/RX3{slash}15")
  (net 70 "/TX2{slash}16")
  (net 71 "/RX2{slash}17")
  (net 72 "/TX1{slash}18")
  (net 73 "/RX1{slash}19")
  (net 74 "/SDA{slash}20")
  (net 75 "/SCL{slash}21")
  (net 76 "VCC")
  (net 77 "/~{RESET}")
  (net 78 "unconnected-(J1-Pad1)")
  (net 79 "unconnected-(U1-Pad2)")
  (net 80 "unconnected-(U1-Pad8)")
  (net 81 "unconnected-(U1-Pad9)")
  (net 82 "unconnected-(U2-Pad2)")
  (net 83 "unconnected-(U2-Pad8)")
  (net 84 "unconnected-(U2-Pad9)")
  (net 85 "Net-(J8-Pad1)")
  (net 86 "Net-(J8-Pad2)")
  (net 87 "Net-(J9-Pad1)")
  (net 88 "Net-(J9-Pad2)")
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x18_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 5A19A42A)
    (at 193.98 92.38 180)
    (descr "Through hole straight socket strip, 2x18, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x18 2.54mm double row")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at -1.27 -2.77) (layer "F.SilkS") hide)
    (fp_text value "Digital" (at -1.27 46.99) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.286 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "unconnected-(J7-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(J7-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(J7-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "unconnected-(J7-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "unconnected-(J7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "unconnected-(J7-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "unconnected-(J7-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "unconnected-(J7-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/*44") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/*45") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/42") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at -2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/43") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/40") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at -2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/41") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval locked (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/38") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval locked (at -2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/39") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval locked (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/36") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval locked (at -2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/37") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval locked (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/34") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval locked (at -2.54 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/35") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval locked (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/32") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval locked (at -2.54 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/33") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval locked (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/30") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval locked (at -2.54 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/31") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval locked (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/28") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval locked (at -2.54 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/29") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval locked (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/26") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval locked (at -2.54 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/27") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval locked (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/24") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval locked (at -2.54 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/25") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole oval locked (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/22") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval locked (at -2.54 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/23") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole oval locked (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "+5V") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval locked (at -2.54 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "+5V") (pinfunction "Pin_36") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x18_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 5A19A420)
    (at 127.94 97.46 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.77 90) (layer "F.SilkS") hide)
    (fp_text value "Power" (at -3.81 8.89 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "unconnected-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/IOREF") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "/~{RESET}") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "+3V3") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "+5V") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "VCC") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 5A19A420)
    (at 150.8 97.46 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77 90) (layer "F.SilkS") hide)
    (fp_text value "Analog" (at -3.81 8.89 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/A0") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/A1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/A2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/A3") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/A4") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/A5") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/A6") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "/A7") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 5A19A420)
    (at 173.66 97.46 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.77 90) (layer "F.SilkS") hide)
    (fp_text value "Analog" (at -3.81 8.89 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/A8") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/A9") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/A10") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/A11") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/A12") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/A13") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "/A14") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "/A15") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x10_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 5A19A425)
    (at 118.796 49.2 90)
    (descr "Through hole straight socket strip, 1x10, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x10 2.54mm single row")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77 90) (layer "F.SilkS") hide)
    (fp_text value "PWM" (at 3.81 11.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "/SCL{slash}21") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "/SDA{slash}20") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "/AREF") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/*13") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/*12") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "/*11") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "/*10") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "/*9") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "/*8") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 5A19A420)
    (at 145.72 49.2 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.77 90) (layer "F.SilkS") hide)
    (fp_text value "PWM" (at 3.81 8.89 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "/*7") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "/*6") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "/*5") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "/*4") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "/*3") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "/*2") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/TX0{slash}1") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "/RX0{slash}0") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 5A19A420)
    (at 168.58 49.2 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 0 -2.77 90) (layer "F.SilkS") hide)
    (fp_text value "Communication" (at 3.81 8.89 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "/TX3{slash}14") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "/RX3{slash}15") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "/TX2{slash}16") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "/RX2{slash}17") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "/TX1{slash}18") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "/RX1{slash}19") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "/SDA{slash}20") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "/SCL{slash}21") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MAX31865:MAX31856" (layer "F.Cu")
    (tedit 61257442)
    (at 179.5 81.5 90)
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 0 -11.684 90) (layer "F.SilkS"))
    (fp_text value "thermo_max31856" (at 0 11.938 90) (layer "F.Fab"))
    (fp_text user "GND" (at -5.08 6.604 90) (layer "F.SilkS"))
    (fp_text user "SCK" (at -2.54 9.906 90) (layer "F.SilkS"))
    (fp_text user "FLT" (at 7.62 9.906 90) (layer "F.SilkS"))
    (fp_text user "-" (at 1.778 -8.89 90) (layer "F.SilkS"))
    (fp_text user "MAX31856" (at 0 0 90) (layer "F.SilkS"))
    (fp_text user "CS" (at 5.08 6.604 90) (layer "F.SilkS"))
    (fp_text user "3Vo" (at -7.62 9.906 90) (layer "F.SilkS"))
    (fp_text user "SDO" (at 0 6.604 90) (layer "F.SilkS"))
    (fp_text user "+" (at -1.778 -8.89 90) (layer "F.SilkS"))
    (fp_text user "VIN" (at -10.16 6.604 90) (layer "F.SilkS"))
    (fp_text user "SDI" (at 2.54 9.906 90) (layer "F.SilkS"))
    (fp_text user "DRDY" (at 10.16 6.604 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -10.16 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 67 "+3V3") (pinfunction "VIN") (pintype "input"))
    (pad "2" thru_hole circle (at -7.62 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 79 "unconnected-(U1-Pad2)") (pinfunction "3vo") (pintype "output"))
    (pad "3" thru_hole circle (at -5.08 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "4" thru_hole circle (at -2.54 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/23") (pinfunction "SCK") (pintype "input"))
    (pad "5" thru_hole circle (at 0 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/25") (pinfunction "SDO") (pintype "output"))
    (pad "6" thru_hole circle (at 2.54 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/27") (pinfunction "SDI") (pintype "input"))
    (pad "7" thru_hole circle (at 5.08 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/29") (pinfunction "CS") (pintype "input"))
    (pad "8" thru_hole circle (at 7.62 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 80 "unconnected-(U1-Pad8)") (pinfunction "FLT") (pintype "output"))
    (pad "9" thru_hole circle (at 10.16 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 81 "unconnected-(U1-Pad9)") (pinfunction "DRDY") (pintype "output"))
    (pad "10" thru_hole circle (at -1.778 -6.985 90) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(J9-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "11" thru_hole circle (at 1.778 -6.985 90) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(J9-Pad2)") (pinfunction "+") (pintype "input"))
  )
  (footprint "Arduino_MountingHole:MountingHole_3.2mm" locked (layer "F.Cu")
    (tedit 60369150)
    (at 196.52 97.46)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MH6" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_6-G-3.5_1x06_P3.50mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED0)
    (at 142.7675 43.1425)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/6-G-3.5; number of pins: 06; pin pitch: 3.50mm; Vertical || order number: 1843648 8A 160V")
    (tags "phoenix_contact connector MCV_01x06_G_3.5mm")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at 8.75 -5.45) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Female" (at 8.75 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.75 -3.55) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.5 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 7 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 10.5 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 14 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 "+5V") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 17.5 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_6-G-3.5_1x06_P3.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MAX31865:MAX31856" (layer "F.Cu")
    (tedit 61257442)
    (at 149.5 81.5 90)
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 -11.684 90) (layer "F.SilkS"))
    (fp_text value "thermo_max31856" (at 0 11.938 90) (layer "F.Fab"))
    (fp_text user "+" (at -1.778 -8.89 90) (layer "F.SilkS"))
    (fp_text user "SCK" (at -2.54 9.906 90) (layer "F.SilkS"))
    (fp_text user "-" (at 1.778 -8.89 90) (layer "F.SilkS"))
    (fp_text user "SDO" (at 0 6.604 90) (layer "F.SilkS"))
    (fp_text user "3Vo" (at -7.62 9.906 90) (layer "F.SilkS"))
    (fp_text user "FLT" (at 7.62 9.906 90) (layer "F.SilkS"))
    (fp_text user "SDI" (at 2.54 9.906 90) (layer "F.SilkS"))
    (fp_text user "MAX31856" (at 0 0 90) (layer "F.SilkS"))
    (fp_text user "CS" (at 5.08 6.604 90) (layer "F.SilkS"))
    (fp_text user "VIN" (at -10.16 6.604 90) (layer "F.SilkS"))
    (fp_text user "GND" (at -5.08 6.604 90) (layer "F.SilkS"))
    (fp_text user "DRDY" (at 10.16 6.604 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -10.16 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 67 "+3V3") (pinfunction "VIN") (pintype "input"))
    (pad "2" thru_hole circle (at -7.62 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 82 "unconnected-(U2-Pad2)") (pinfunction "3vo") (pintype "output"))
    (pad "3" thru_hole circle (at -5.08 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "4" thru_hole circle (at -2.54 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/28") (pinfunction "SCK") (pintype "input"))
    (pad "5" thru_hole circle (at 0 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/26") (pinfunction "SDO") (pintype "output"))
    (pad "6" thru_hole circle (at 2.54 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/24") (pinfunction "SDI") (pintype "input"))
    (pad "7" thru_hole circle (at 5.08 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/22") (pinfunction "CS") (pintype "input"))
    (pad "8" thru_hole circle (at 7.62 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 83 "unconnected-(U2-Pad8)") (pinfunction "FLT") (pintype "output"))
    (pad "9" thru_hole circle (at 10.16 8.255 90) (size 1.778 1.778) (drill 1) (layers *.Cu *.Mask)
      (net 84 "unconnected-(U2-Pad9)") (pinfunction "DRDY") (pintype "output"))
    (pad "10" thru_hole circle (at -1.778 -6.985 90) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(J8-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "11" thru_hole circle (at 1.778 -6.985 90) (size 2.184 2.184) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(J8-Pad2)") (pinfunction "+") (pintype "input"))
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_6-G-3.5_1x06_P3.50mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED0)
    (at 167.7675 43.1425)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/6-G-3.5; number of pins: 06; pin pitch: 3.50mm; Vertical || order number: 1843648 8A 160V")
    (tags "phoenix_contact connector MCV_01x06_G_3.5mm")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J11" (at 8.75 -5.45) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Female" (at 8.75 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.75 -3.55) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 68 "/TX3{slash}14") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.5 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 69 "/RX3{slash}15") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 7 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 10.5 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 14 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 70 "/TX2{slash}16") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 17.5 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 71 "/RX2{slash}17") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_6-G-3.5_1x06_P3.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_2-G-3.5_1x02_P3.50mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED0)
    (at 105.6425 74.7325 90)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-3.5; number of pins: 02; pin pitch: 3.50mm; Vertical || order number: 1843606 8A 160V")
    (tags "phoenix_contact connector MCV_01x02_G_3.5mm")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 1.75 -5.45 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Female" (at 1.75 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 -3.55 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 87 "Net-(J9-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.5 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 88 "Net-(J9-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_2-G-3.5_1x02_P3.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Arduino_MountingHole:MountingHole_3.2mm" locked (layer "F.Cu")
    (tedit 60369150)
    (at 115.24 49.2)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MH1" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_2-G-3.5_1x02_P3.50mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED0)
    (at 105.6425 84.2325 90)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-3.5; number of pins: 02; pin pitch: 3.50mm; Vertical || order number: 1843606 8A 160V")
    (tags "phoenix_contact connector MCV_01x02_G_3.5mm")
    (property "Sheetfile" "HumidityO2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 1.75 -5.45 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Female" (at 1.75 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 -3.55 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 85 "Net-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.5 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 86 "Net-(J8-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_2-G-3.5_1x02_P3.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Arduino_MountingHole:MountingHole_3.2mm" locked (layer "F.Cu")
    (tedit 60369150)
    (at 113.97 97.46)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MH2" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Arduino_MountingHole:MountingHole_3.2mm" locked (layer "F.Cu")
    (tedit 60369150)
    (at 166.04 64.44)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MH3" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Arduino_MountingHole:MountingHole_3.2mm" locked (layer "F.Cu")
    (tedit 60369150)
    (at 166.04 92.38)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MH4" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Arduino_MountingHole:MountingHole_3.2mm" locked (layer "F.Cu")
    (tedit 60369150)
    (at 190.17 49.2)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MH5" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 196.5 37.5) (end 196.5 46.66) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 199.06 59.36) (end 201.6 61.9) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 100 99.238) (end 100 47.422) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 201.6 61.9) (end 201.6 96.19) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 198.298 100) (end 100.762 100) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 100.762 37.5) (end 196.5 37.5) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 100.762 100) (mid 100.223185 99.776815) (end 100 99.238) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 201.6 96.19) (end 199.06 98.73) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 100.762 37.5) (end 100.762 46.66) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 196.5 46.66) (end 199.06 49.2) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 199.06 99.238) (mid 198.836815 99.776815) (end 198.298 100) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 199.06 49.2) (end 199.06 59.36) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 199.06 98.73) (end 199.06 99.238) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 100 47.422) (mid 100.223185 46.883185) (end 100.762 46.66) (layer "Edge.Cuts") (width 0.15))
  (gr_text "ICSP" (at 164.897 72.06 90) (layer "Dwgs.User"))
)
