(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 58)
    (no_connects 0)
    (area 91.874999 59.924999 121.092857 100.005001)
    (thickness 1.6)
    (drawings 5)
    (tracks 186)
    (zones 0)
    (modules 24)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.01)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.2 1.2)
    (mod_edge_width 0.15)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.12)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad5)")
  (net 2 "Net-(U1-Pad6)")
  (net 3 "Net-(U1-Pad8)")
  (net 4 "Net-(U1-Pad10)")
  (net 5 "Net-(U1-Pad14)")
  (net 6 "Net-(U1-Pad18)")
  (net 7 "Net-(U1-Pad19)")
  (net 8 "Net-(U1-Pad20)")
  (net 9 "Net-(U1-Pad21)")
  (net 10 "Net-(U1-Pad22)")
  (net 11 "Net-(U1-Pad23)")
  (net 12 "Net-(U1-Pad24)")
  (net 13 "Net-(U1-Pad32)")
  (net 14 "Net-(P1-Pad4)")
  (net 15 "Net-(P1-Pad1)")
  (net 16 "Net-(P1-Pad7)")
  (net 17 EXT_VCC)
  (net 18 GND)
  (net 19 +3V3)
  (net 20 "Net-(C3-Pad2)")
  (net 21 "Net-(C4-Pad2)")
  (net 22 "Net-(C8-Pad1)")
  (net 23 "Net-(C8-Pad2)")
  (net 24 "Net-(D1-Pad2)")
  (net 25 "Net-(D1-Pad1)")
  (net 26 TXD)
  (net 27 RXD)
  (net 28 BRC)
  (net 29 FLASH_TXD)
  (net 30 FLASH_RXD)
  (net 31 "Net-(R1-Pad2)")
  (net 32 "Net-(R3-Pad1)")
  (net 33 "Net-(R5-Pad1)")
  (net 34 "Net-(R6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net BRC)
    (add_net EXT_VCC)
    (add_net FLASH_RXD)
    (add_net FLASH_TXD)
    (add_net GND)
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
    (add_net RXD)
    (add_net TXD)
  )
  (module Pin_Headers:Pin_Header_Angled_1x03 (layer F.Cu) (tedit 595299CA)
    (at 102.75 67 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -4.6 0 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab))
    (fp_text user Rx (at -2.1 2.5 270) (layer F.SilkS))
    (fp_text user Tx (at -2.1 0 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 FLASH_TXD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 FLASH_RXD))
    (pad 3 thru_hole rect (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Hand (layer F.Cu) (tedit 5952916B)
    (at 106.25 73.75 90)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C2 (at 0 -2 180) (layer F.SilkS))
    (fp_text value 33uF (at 0 2.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 3.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 3.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_2520-4pin_2.5x2.0mm (layer F.Cu) (tedit 59529126)
    (at 104 82.25 270)
    (descr "SMD Crystal SERIES SMD2520/4 http://www.newxtal.com/UploadFiles/Images/2012-11-12-09-29-09-776.pdf, 2.5x2.0mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference X1 (at 0 2.25 360) (layer F.SilkS))
    (fp_text value "40 MHz" (at 0 2.2 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.875 0.7 270) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 0.875 0.7 270) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 3 smd rect (at 0.875 -0.7 270) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C3-Pad2)"))
    (pad 4 smd rect (at -0.875 -0.7 270) (size 1.15 1) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_2520-4pin_2.5x2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-32-1EP_5x5mm_Pitch0.5mm (layer F.Cu) (tedit 58EDC894)
    (at 110 82.75 90)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at -3.75 2.75 180) (layer F.SilkS) hide)
    (fp_text value ESP8285 (at 0 3.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2.4 -1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 2 smd rect (at -2.4 -1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C8-Pad2)"))
    (pad 3 smd rect (at -2.4 -0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 4 smd rect (at -2.4 -0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 5 smd rect (at -2.4 0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -2.4 0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -2.4 1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R3-Pad1)"))
    (pad 8 smd rect (at -2.4 1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -1.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D1-Pad2)"))
    (pad 10 smd rect (at -1.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at -0.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 12 smd rect (at -0.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R1-Pad2)"))
    (pad 13 smd rect (at 0.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 RXD))
    (pad 14 smd rect (at 0.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 1.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R5-Pad1)"))
    (pad 16 smd rect (at 1.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 BRC))
    (pad 17 smd rect (at 2.4 1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 18 smd rect (at 2.4 1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 2.4 0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 2.4 0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 2.4 -0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 2.4 -0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 2.4 -1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 2.4 -1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad24)"))
    (pad 25 smd rect (at 1.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 FLASH_RXD))
    (pad 26 smd rect (at 1.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 FLASH_TXD))
    (pad 27 smd rect (at 0.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C4-Pad2)"))
    (pad 28 smd rect (at 0.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C3-Pad2)"))
    (pad 29 smd rect (at -0.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 30 smd rect (at -0.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 31 smd rect (at -1.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R6-Pad1)"))
    (pad 32 smd rect (at -1.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad32)"))
    (pad 33 smd rect (at 0.8625 0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mini-din_8pin:mini-din_8pin (layer F.Cu) (tedit 58ED56B3)
    (at 110 65.5)
    (fp_text reference P1 (at 4.25 -1.75) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 -0.5) (layer F.Fab))
    (pad 5 thru_hole circle (at -2.5 0.4) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 26 TXD))
    (pad 4 thru_hole circle (at 0.5 0.4) (size 0.85 0.85) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P1-Pad4)"))
    (pad 3 thru_hole circle (at 2.5 0.4) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 27 RXD))
    (pad 8 thru_hole circle (at -2 -1.6) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 18 GND))
    (pad 6 thru_hole circle (at 2 -1.6) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 28 BRC))
    (pad 2 thru_hole circle (at -1 2.4) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 17 EXT_VCC))
    (pad 1 thru_hole circle (at 1 2.4) (size 0.85 0.85) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P1-Pad1)"))
    (pad 7 thru_hole circle (at 0 -1.6) (size 1.5 1.5) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P1-Pad7)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 594FBC20)
    (at 109.5 71.25 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.5 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 EXT_VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 595284DB)
    (at 104.25 85)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.75 0) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 595284D2)
    (at 104.25 79.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.75 0 180) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 594FC740)
    (at 107.25 88.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -2.5 -0.5 360) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 594FDD25)
    (at 111.25 88.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.5 -0.75 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 594FDD2B)
    (at 111.25 86.75 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.5 -0.75 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 594FD531)
    (at 108.75 88.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.5 -0.25 180) (layer F.SilkS))
    (fp_text value 5.6pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 594FDDA4)
    (at 114.5 85.75 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0.75 1.25 180) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module antennas:RFANT8010080A3T (layer F.Cu) (tedit 594FA1F7)
    (at 112.5 94.75)
    (fp_text reference P2 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value ANTENNA (at 0 2.5) (layer F.SilkS))
    (pad 1 smd rect (at -3.75 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 3.75 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 584F28DA)
    (at 116.25 80.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.75 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 TXD))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 584F28E3)
    (at 116.25 82.25)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.75 0) (layer F.SilkS))
    (fp_text value 2k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 594FD701)
    (at 111.5 90.75 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.75 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5850540F)
    (at 116.25 78)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.75 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 RXD))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 594FBBFD)
    (at 109.5 77.25 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.5 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 594FD928)
    (at 105 88.25 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.75 540) (layer F.SilkS))
    (fp_text value 12k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 594FD3DA)
    (at 116.25 84)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.75 0) (layer F.SilkS))
    (fp_text value 20 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module micro_switches:ALPS_SKRELHE010 (layer F.Cu) (tedit 59529A9D)
    (at 118.5 88.75 270)
    (fp_text reference SW1 (at -3.75 -1 360) (layer F.SilkS) hide)
    (fp_text value R (at 0 2.5 450) (layer F.SilkS))
    (pad 1 smd rect (at -1.9 0 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.9 0 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R3-Pad1)"))
  )
  (module micro_switches:ALPS_SKRELHE010 (layer F.Cu) (tedit 59529AAB)
    (at 118.5 65.25 90)
    (fp_text reference SW2 (at -3.75 1 180) (layer F.SilkS) hide)
    (fp_text value F (at 0 -2.5 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.9 0 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.9 0 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R5-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 594FA1C3)
    (at 115.25 72.5)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value TS2940CW-3.3 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 EXT_VCC))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "reksio 1.2" (at 114.5 61.25) (layer F.Mask))
  (gr_line (start 120 100) (end 100 100) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 120 60) (end 120 100) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 100 60) (end 120 60) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 100 100) (end 100 60) (angle 90) (layer Edge.Cuts) (width 0.01))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.75 99.75) (xy 100.25 99.75) (xy 100.25 92) (xy 119.75 92)
      )
    )
  )
  (zone (net 18) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.125)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 119.75 91.75) (xy 100.25 91.75) (xy 100.25 60.25) (xy 119.75 60.25)
      )
    )
  )
)
