<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="-0.0254" y1="4.2418" x2="23.2666" y2="4.2164" width="0" layer="20"/>
<wire x1="23.2666" y1="4.2164" x2="23.2412" y2="31.2066" width="0" layer="20"/>
<wire x1="23.2412" y1="31.2066" x2="-0.0762" y2="31.232" width="0" layer="20"/>
<wire x1="-0.0762" y1="31.232" x2="-0.0254" y2="4.2418" width="0" layer="20"/>
<text>pink
boost
v2</text>
<text>IN</text>
<text>G</text>
<text>+9V</text>
<text>OUT</text>
<text>GND</text>
<text>9V</text>
</plain>
<libraries>
<library name="potentiometers">
<packages>
<package name="16MM_C.MOUNT">
<description>&lt;b&gt;16mm / Right-Angle /  PC Mount / Short Pin&lt;/b&gt;
&lt;p&gt;
For aligning the center of the pot shaft to a specific drill location
&lt;p&gt;
&lt;a href="http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/"&gt;http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="caps-elec">
<packages>
<package name="0632">
<description>0.1" (2.54mm) spacing</description>
</package>
</packages>
</library>
<library name="caps-film">
<packages>
<package name="0.1&quot;">
<description>0.1" (2.54mm) spacing</description>
</package>
<package name="0.2&quot;.SML">
<description>0.2" (5.08mm) spacing
&lt;p&gt;
&lt;b&gt; 
10pf - 180n&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diodes">
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistors-FET">
<packages>
<package name="TO92">
</package>
</packages>
</library>
<library name="resistors">
<packages>
<package name="0.3&quot;.B">
<description>0.3"  (7.62mm) lead spacing, 1/4W (flat)</description>
</package>
</packages>
</library>
<library name="supply pins">
<packages>
<package name="PAD4">
<description>&lt;b&gt;Square (no label) - 76mil Diameter, 39mil Drill&lt;b&gt;</description>
</package>
<package name="PAD2">
<description>&lt;b&gt;Round Pad (no label) - 76mil Diameter, 39mil Drill&lt;b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BOOST" library="potentiometers" package="16MM_C.MOUNT" value="50kC">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="C1" library="caps-elec" package="0632" value="100uF"/>
<element name="C2" library="caps-film" package="0.2&quot;.SML" value="1uF"/>
<element name="C3" library="caps-film" package="0.1&quot;" value="100pF">
<attribute name="NAME"/>
</element>
<element name="C4" library="caps-film" package="0.2&quot;.SML" value="47nF"/>
<element name="C5" library="caps-elec" package="0632" value="22uF"/>
<element name="D1" library="diodes" package="DO41-3" value="1N4002"/>
<element name="Q1" library="transistors-FET" package="TO92" value="2N5952"/>
<element name="R1" library="resistors" package="0.3&quot;.B" value="2M"/>
<element name="R10" library="resistors" package="0.3&quot;.B" value="150k"/>
<element name="R2" library="resistors" package="0.3&quot;.B" value="14k7"/>
<element name="R3" library="resistors" package="0.3&quot;.B" value="2M"/>
<element name="R4" library="resistors" package="0.3&quot;.B" value="12k"/>
<element name="R5" library="resistors" package="0.3&quot;.B" value="14k7"/>
<element name="R6" library="resistors" package="0.3&quot;.B" value="1k"/>
<element name="R8" library="resistors" package="0.3&quot;.B" value="150k"/>
<element name="R9" library="resistors" package="0.3&quot;.B" value="1k"/>
<element name="U$2" library="supply pins" package="PAD4" value="PADS.SQR_NL"/>
<element name="GND" library="supply pins" package="PAD4" value="PADS.SQR_NL"/>
<element name="U$4" library="supply pins" package="PAD2" value="PADS.RND_NL"/>
<element name="U$5" library="supply pins" package="PAD2" value="PADS.RND_NL"/>
<element name="U$6" library="supply pins" package="PAD2" value="PADS.RND_NL"/>
<element name="U$1" library="supply pins" package="PAD4" value="PADS.SQR_NL"/>
</elements>
<signals>
<signal name="GND">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="R8" pad="2"/>
<contactref element="BOOST" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="GND" pad="P$1"/>
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="+"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="3"/>
<contactref element="R5" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="+9V">
<contactref element="R6" pad="1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="R6" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="D1" pad="C"/>
<contactref element="C1" pad="+"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="C4" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="C5" pad="-"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R9" pad="1"/>
<contactref element="BOOST" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="BOOST" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="IN">
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="OUT">
<contactref element="C2" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="U$4" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
