(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "AC1")
	(net 2 "AC2")
	(net 3 "Out+")
	(net 4 "Out-")
	(footprint "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-PMxx"
		(layer "F.Cu")
		(at 137.92 97)
		(descr "ACDC-Converter, 3W, Hi-Link, HLK-PMxx, THT (Script generated with StandardBox.py) (https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%973W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%913W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf)")
		(tags "ACDC-Converter 3W THT Hi-Link board mount module")
		(property "Reference" "PS1"
			(at -1.66 -9.79 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HLK-PMxxx"
			(at 14.58 -3.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Converter_ACDC:Converter_ACDC_Hi-Link_HLK-PMxx"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://h.hlktech.com/download/ACDC%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%973W%E7%B3%BB%E5%88%97/1/%E6%B5%B7%E5%87%8C%E7%A7%913W%E7%B3%BB%E5%88%97%E7%94%B5%E6%BA%90%E6%A8%A1%E5%9D%97%E8%A7%84%E6%A0%BC%E4%B9%A6V2.8.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Compact AC/DC board mount power module 3W 5V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "AC1")
			(pinfunction "AC/L")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "AC2")
			(pinfunction "AC/N")
			(pintype "power_in")
		)
		(pad "3" thru_hole circle
			(at 29.08 10)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Out+")
			(pinfunction "-Vout")
			(pintype "power_out")
		)
		(pad "4" thru_hole circle
			(at 29.08 -5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Out-")
			(pinfunction "+Vout")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_Hi-Link_HLK-PMxx.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 127.5 104.5)
		(property "Reference" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "AC1")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 177 107)
		(property "Reference" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "3" thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Out+")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 177 92)
		(property "Reference" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "4" thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Out-")
		)
	)
	(footprint "Connector_Pin:Pin_D1.0mm_L10.0mm"
		(layer "F.Cu")
		(at 127.5 94.5)
		(descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
		(tags "solder Pin_ press fit")
		(property "Reference" "AC2"
			(at 0 2.25 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 -2.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_Pin:Pin_D1.0mm_L10.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "2" thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "AC2")
		)
	)
	(gr_line
		(start 185.5 85.5)
		(end 185.5 114.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.5 114.5)
		(end 119.5 85.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 120.5 115.5)
		(mid 119.792893 115.207107)
		(end 119.5 114.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.5 115.5)
		(end 120.5 115.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119.5 85.5)
		(mid 119.792893 84.792893)
		(end 120.5 84.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.5 114.5)
		(mid 185.207107 115.207107)
		(end 184.5 115.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 184.499999 84.500001)
		(mid 185.207106 84.792894)
		(end 185.499999 85.500001)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.5 84.5)
		(end 120.5 84.5)
		(layer "Edge.Cuts")
	)
	(gr_text "In\n"
		(at 127.5 100.5 0)
		(layer "B.SilkS")
	)
	(gr_text "Out"
		(at 177.5 100.5 0)
		(layer "B.SilkS")
	)
	(gr_text "~"
		(at 128 103 0)
		(layer "B.SilkS")
	)
	(gr_text "~"
		(at 128 98 0)
		(layer "B.SilkS")
	)
	(gr_text "+"
		(at 176 105 0)
		(layer "B.SilkS")
	)
	(gr_text "-"
		(at 176 96 0)
		(layer "B.SilkS")
	)
	(gr_text "Install Module\non This Side"
		(at 152.5 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "In\n"
		(at 127.5 100.5 0)
		(layer "F.SilkS")
	)
	(gr_text "~"
		(at 126.5 103 0)
		(layer "F.SilkS")
	)
	(gr_text "Out"
		(at 177.5 100.5 0)
		(layer "F.SilkS")
	)
	(gr_text "~"
		(at 126.5 98 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 176 96 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 176 105 0)
		(layer "F.SilkS")
	)
)