(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~65~ubuntu17.10.1)
  (general
    (thickness 1.6)
    (drawings 1259)
    (tracks 1286)
    (zones 0)
    (modules 91)
    (nets 86)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (1 In1.Cu mixed)
    (2 In2.Cu power)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.13)
    (user_trace_width 0.2)
    (user_trace_width 0.4)
    (trace_clearance 0.13)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.13)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.45)
    (via_drill 0.26)
    (via_min_size 0.45)
    (via_min_drill 0.26)
    (user_via 0.45 0.26)
    (user_via 0.5 0.4)
    (uvia_size 0.36)
    (uvia_drill 0.26)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x20000_7ffffff8)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "SVG/"))
  )
  (net 0 "")
  (net 1 2V8)
  (net 2 GND)
  (net 3 "Net-(C5-Pad1)")
  (net 4 "Net-(C6-Pad1)")
  (net 5 /VDD_IO)
  (net 6 /VAA)
  (net 7 "Net-(C15-Pad1)")
  (net 8 /135_VDD)
  (net 9 /VDD_PLL)
  (net 10 /SDATA)
  (net 11 /SCLK)
  (net 12 /VSYNC)
  (net 13 /FLASH)
  (net 14 /HSYNC)
  (net 15 /DCMI_D1)
  (net 16 /DCMI_D4)
  (net 17 /DCMI_D0)
  (net 18 /DCMI_D5)
  (net 19 /DCMI_D6)
  (net 20 /DCMI_D2)
  (net 21 /DCMI_D3)
  (net 22 /DCMI_D7)
  (net 23 /EXTCLK)
  (net 24 /PIXCLK)
  (net 25 "Net-(R2-Pad2)")
  (net 26 "Net-(R3-Pad2)")
  (net 27 "Net-(R4-Pad2)")
  (net 28 "Net-(R5-Pad2)")
  (net 29 "Net-(R6-Pad2)")
  (net 30 "Net-(R7-Pad2)")
  (net 31 "Net-(R8-Pad2)")
  (net 32 "Net-(R9-Pad2)")
  (net 33 "Net-(R10-Pad2)")
  (net 34 "Net-(R11-Pad2)")
  (net 35 /STANDBY)
  (net 36 /CH_GND)
  (net 37 "Net-(L1-Pad2)")
  (net 38 "Net-(L2-Pad2)")
  (net 39 "Net-(R25-Pad2)")
  (net 40 /STANDBY2)
  (net 41 "Net-(R19-Pad1)")
  (net 42 "Net-(R20-Pad1)")
  (net 43 "Net-(R21-Pad1)")
  (net 44 "Net-(R21-Pad2)")
  (net 45 /VSYNC1)
  (net 46 /VSYNC2)
  (net 47 /HSYNC1)
  (net 48 /HSYNC2)
  (net 49 "Net-(R24-Pad1)")
  (net 50 "Net-(R28-Pad1)")
  (net 51 /LASER)
  (net 52 "Net-(C4-Pad1)")
  (net 53 "Net-(C7-Pad1)")
  (net 54 "Net-(C8-Pad1)")
  (net 55 "Net-(C40-Pad1)")
  (net 56 "Net-(C41-Pad1)")
  (net 57 /DCMI_D6R)
  (net 58 /DCMI_D6L)
  (net 59 /DCMI_D7R)
  (net 60 /DCMI_D7L)
  (net 61 /DCMI_D1R)
  (net 62 /DCMI_D1L)
  (net 63 /DCMI_D0R)
  (net 64 /DCMI_D0L)
  (net 65 /DCMI_D4R)
  (net 66 /DCMI_D5R)
  (net 67 /DCMI_D2R)
  (net 68 /DCMI_D3R)
  (net 69 "Net-(U10-Pad8)")
  (net 70 /DCMI_D4L)
  (net 71 /DCMI_D5L)
  (net 72 /DCMI_D2L)
  (net 73 /DCMI_D3L)
  (net 74 "Net-(U10-Pad11)")
  (net 75 /VAAL)
  (net 76 /VDD_IOL)
  (net 77 /VDD_PLL_L)
  (net 78 /IM_RSTR)
  (net 79 /IM_RSTL)
  (net 80 /TRIGGER_L)
  (net 81 /TRIGGER_R)
  (net 82 "Net-(R31-Pad1)")
  (net 83 /OER)
  (net 84 /OEL)
  (net 85 "Net-(R32-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.13)
    (trace_width 0.13)
    (via_dia 0.45)
    (via_drill 0.26)
    (uvia_dia 0.36)
    (uvia_drill 0.26)
    (add_net /135_VDD)
    (add_net /CH_GND)
    (add_net /DCMI_D0)
    (add_net /DCMI_D0L)
    (add_net /DCMI_D0R)
    (add_net /DCMI_D1)
    (add_net /DCMI_D1L)
    (add_net /DCMI_D1R)
    (add_net /DCMI_D2)
    (add_net /DCMI_D2L)
    (add_net /DCMI_D2R)
    (add_net /DCMI_D3)
    (add_net /DCMI_D3L)
    (add_net /DCMI_D3R)
    (add_net /DCMI_D4)
    (add_net /DCMI_D4L)
    (add_net /DCMI_D4R)
    (add_net /DCMI_D5)
    (add_net /DCMI_D5L)
    (add_net /DCMI_D5R)
    (add_net /DCMI_D6)
    (add_net /DCMI_D6L)
    (add_net /DCMI_D6R)
    (add_net /DCMI_D7)
    (add_net /DCMI_D7L)
    (add_net /DCMI_D7R)
    (add_net /EXTCLK)
    (add_net /FLASH)
    (add_net /HSYNC)
    (add_net /HSYNC1)
    (add_net /HSYNC2)
    (add_net /IM_RSTL)
    (add_net /IM_RSTR)
    (add_net /LASER)
    (add_net /OEL)
    (add_net /OER)
    (add_net /PIXCLK)
    (add_net /SCLK)
    (add_net /SDATA)
    (add_net /STANDBY)
    (add_net /STANDBY2)
    (add_net /TRIGGER_L)
    (add_net /TRIGGER_R)
    (add_net /VAA)
    (add_net /VAAL)
    (add_net /VDD_IO)
    (add_net /VDD_IOL)
    (add_net /VDD_PLL)
    (add_net /VDD_PLL_L)
    (add_net /VSYNC)
    (add_net /VSYNC1)
    (add_net /VSYNC2)
    (add_net 2V8)
    (add_net GND)
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C40-Pad1)")
    (add_net "Net-(C41-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(L2-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R24-Pad1)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R28-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R31-Pad1)")
    (add_net "Net-(R32-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U10-Pad11)")
    (add_net "Net-(U10-Pad8)")
  )
  (module CustomParts:SAMTEC_FT5-15-01-K-RA-TR (layer F.Cu) (tedit 5CA6D872)
    (at 111.7 122.383 180)
    (attr smd)
    (fp_text reference J9 (at -4.96 -4.035 180) (layer F.SilkS) hide)
    (fp_text value FT5-30 (at 8.5 -3.6 180) (layer F.SilkS) hide)
    (pad P4 thru_hole circle (at 6.5 -1.02) (size 1.1 1.1) (drill 0.71) (layers *.Cu *.Mask))
    (pad P2 thru_hole circle (at -6.5 1.23 180) (size 1.1 1.1) (drill 0.71) (layers *.Cu *.Mask))
    (pad P3 thru_hole circle (at 6.5 1.23) (size 1.1 1.1) (drill 0.71) (layers *.Cu *.Mask))
    (pad P1 thru_hole circle (at -6.5 -1.02 180) (size 1.1 1.1) (drill 0.71) (layers *.Cu *.Mask))
    (pad Hole np_thru_hole circle (at 7.75 0.1 180) (size 1.45 1.45) (drill 1.45) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at -7.75 0.1 180) (size 1.45 1.45) (drill 1.45) (layers *.Cu *.Mask F.SilkS))
    (pad 30 smd rect (at 3.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 29 smd rect (at 3.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 28 smd rect (at 3 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 23 /EXTCLK))
    (pad 27 smd rect (at 3 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 24 /PIXCLK))
    (pad 26 smd rect (at 2.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 2.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 14 /HSYNC))
    (pad 24 smd rect (at 2 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /DCMI_D0))
    (pad 23 smd rect (at 2 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 12 /VSYNC))
    (pad 22 smd rect (at 1.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 15 /DCMI_D1))
    (pad 21 smd rect (at 1.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 1 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 22 /DCMI_D7))
    (pad 19 smd rect (at 1 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 13 /FLASH))
    (pad 18 smd rect (at 0.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /DCMI_D6))
    (pad 17 smd rect (at 0.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 51 /LASER))
    (pad 16 smd rect (at 0 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /DCMI_D4))
    (pad 15 smd rect (at 0 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 78 /IM_RSTR))
    (pad 14 smd rect (at -0.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /DCMI_D2))
    (pad 13 smd rect (at -0.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 79 /IM_RSTL))
    (pad 12 smd rect (at -1 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /DCMI_D3))
    (pad 11 smd rect (at -1 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -1.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /DCMI_D5))
    (pad 9 smd rect (at -1.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 80 /TRIGGER_L))
    (pad 8 smd rect (at -2 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -2 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 81 /TRIGGER_R))
    (pad 6 smd rect (at -2.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /SDATA))
    (pad 5 smd rect (at -2.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 83 /OER))
    (pad 4 smd rect (at -3 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCLK))
    (pad 3 smd rect (at -3 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 84 /OEL))
    (pad 2 smd rect (at -3.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 1 smd rect (at -3.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/FT5-15-01-L-RA-K-TR.stp
      (offset (xyz 0 6.21 0.38))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C902ECB)
    (at 56.45 111.35 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /VAA))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomParts:LensM12_Alum (layer B.Cu) (tedit 5CACECC9)
    (at 62.5 112.233 270)
    (fp_text reference U3 (at -7.5 8.4 270) (layer B.SilkS) hide)
    (fp_text value LensM12 (at -6.7 10 270) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at -11 0 270) (size 3.8 3.8) (drill 2.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 11 0 270) (size 3.8 3.8) (drill 2.1) (layers *.Cu *.Mask)
      (net 2 GND) (clearance 0.1))
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/CameraHousing.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/CameraHousingScrew.step
      (offset (xyz 11 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/CameraHousingScrew.step
      (offset (xyz -11 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CA29DFB)
    (at 91.5 102.733)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J11 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 -4.283) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 52 "Net-(C4-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CA29DF8)
    (at 78 114.35)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J12 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 54 "Net-(C8-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CA29E01)
    (at 127 114.35)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J13 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 53 "Net-(C7-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CA29DFE)
    (at 113.5 102.733)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J14 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 2.3 -4.333) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 36 /CH_GND))
  )
  (module CustomParts:IBGA63_9x9 (layer B.Cu) (tedit 5ADE0811)
    (at 62.5 112.233 180)
    (fp_text reference U5 (at -1.9 5.5 180) (layer B.SilkS) hide)
    (fp_text value AR0135 (at 4.8 2.5 180) (layer B.Fab) hide)
    (pad 64 smd circle (at 3.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 78 /IM_RSTR))
    (pad 63 smd circle (at 2.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD_IO))
    (pad 62 smd circle (at 1.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD_IO))
    (pad 2 smd circle (at -2.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd circle (at -1.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd circle (at -0.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd circle (at 0.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd circle (at 1.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 7 smd circle (at 2.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 8 smd circle (at 3.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 35 /STANDBY))
    (pad 9 smd circle (at -3.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 9 /VDD_PLL))
    (pad 10 smd circle (at -2.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd circle (at -1.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd circle (at -0.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd circle (at 0.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd circle (at 1.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 15 smd circle (at 2.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /VAA))
    (pad 16 smd circle (at 3.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /VAA))
    (pad 17 smd circle (at -3.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 23 /EXTCLK))
    (pad 18 smd circle (at -2.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd circle (at -1.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd circle (at -0.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd circle (at 0.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 22 smd circle (at 1.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 23 smd circle (at 2.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 24 smd circle (at 3.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 25 smd circle (at -3.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(R11-Pad2)"))
    (pad 26 smd circle (at -2.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 11 /SCLK))
    (pad 27 smd circle (at -1.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 10 /SDATA))
    (pad 28 smd circle (at -0.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 29 smd circle (at 0.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 30 smd circle (at 1.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 31 smd circle (at 2.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /VAA))
    (pad 32 smd circle (at 3.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /VAA))
    (pad 33 smd circle (at -3.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 47 /HSYNC1))
    (pad 34 smd circle (at -2.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 45 /VSYNC1))
    (pad 35 smd circle (at -1.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R28-Pad1)"))
    (pad 36 smd circle (at -0.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(R32-Pad1)"))
    (pad 37 smd circle (at 0.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 38 smd circle (at 1.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD_IO))
    (pad 39 smd circle (at 2.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 40 smd circle (at 3.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 41 smd circle (at -3.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 65 /DCMI_D4R))
    (pad 42 smd circle (at -2.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 66 /DCMI_D5R))
    (pad 43 smd circle (at -1.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 57 /DCMI_D6R))
    (pad 44 smd circle (at -0.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 59 /DCMI_D7R))
    (pad 45 smd circle (at 0.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 46 smd circle (at 1.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD_IO))
    (pad 47 smd circle (at 2.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 48 smd circle (at 3.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 49 smd circle (at -3.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 63 /DCMI_D0R))
    (pad 50 smd circle (at -2.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 61 /DCMI_D1R))
    (pad 51 smd circle (at -1.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 67 /DCMI_D2R))
    (pad 52 smd circle (at -0.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 68 /DCMI_D3R))
    (pad 53 smd circle (at 0.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 54 smd circle (at 1.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD_IO))
    (pad 55 smd circle (at 2.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 81 /TRIGGER_R))
    (pad 56 smd circle (at 3.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(U10-Pad8)"))
    (pad 57 smd circle (at -3.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 58 smd circle (at -2.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 59 smd circle (at -1.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 60 smd circle (at -0.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 61 smd circle (at 0.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C9032B8)
    (at 100.2 106.55 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 3.5 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.85 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C9032C9)
    (at 101.75 107.3 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.5 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C902F12)
    (at 97.65 110.8 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0.65 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C9032BD)
    (at 102.8 107.35 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10000pF (at 0.8 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C9032CD)
    (at 99.6 108.9 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.2 0.85 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C90333D)
    (at 61 117.683 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0.067 -1.2 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /VDD_IO))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C902EE0)
    (at 55.875 109.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /VAA))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C902EE3)
    (at 55.9 108.05 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /VAA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C903340)
    (at 60 117.683 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.517 -0.15 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /VDD_IO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C902EBB)
    (at 52.9 112.433)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 22uF (at -2.3 -0.283 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.85 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C15-Pad1)"))
    (pad 2 smd roundrect (at 0.85 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C9032B3)
    (at 61 106.783 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.433 0.15 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /135_VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C902EC9)
    (at 56.9 115.3 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at 0 -1.65 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at -0.25 -1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.85 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 /VAA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C9032AB)
    (at 60 106.783 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.733 -0.15 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /135_VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C902EBE)
    (at 52.95 106.433 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at 0 -1.65 180) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.85 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /135_VDD))
    (pad 2 smd roundrect (at 0.85 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C90334A)
    (at 66 107.65 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.3 0.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /VDD_PLL))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C903350)
    (at 64.5 107.1 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 3.5 -0.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.85 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 /VDD_PLL))
    (pad 2 smd roundrect (at 0.85 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C902ED2)
    (at 58.45 118.75 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C39 (at 0 -1.65 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0.2 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.85 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 /VDD_IO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C902EC1)
    (at 55.35 114.483 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.667 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032D2)
    (at 97.75 112.533)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 1.65 -0.033 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032D6)
    (at 97.75 113.533)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 1.65 -0.033 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C903304)
    (at 103.117 116.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.7 -0.017 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C903323)
    (at 105.117 116.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 0.983 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032E5)
    (at 101.117 116.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.65 0.033 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032DC)
    (at 97.8 115.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.667 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032DF)
    (at 97.8 116.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.667 0.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(R8-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C90331F)
    (at 104.117 116.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.35 0.033 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(R9-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032E9)
    (at 102.117 116.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.7 -0.017 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C90333B)
    (at 64.2 110.95)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C90334D)
    (at 107.85 102.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value 1M (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /CH_GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C902ECE)
    (at 53.95 116.55 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value 4.7 (at 2.1 -0.15 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(L1-Pad2)"))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /VDD_IO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C902EB8)
    (at 52.05 114.45 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10 (at 0 1.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C15-Pad1)"))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C902EC4)
    (at 55.85 112.983)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 4.7 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /VAA))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C903344)
    (at 114.55 118.95)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1.5k (at 2.5 -0.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /SDATA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C903347)
    (at 115.2 120 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 1.5k (at -2.55 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /SCLK))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032B1)
    (at 58.95 106.8 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.55 0.15) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /STANDBY))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LGA:LGA-24L_3x3.5mm_P0.43mm (layer F.Cu) (tedit 5C9032C0)
    (at 102.5 112.233)
    (descr "LGA 24L 3x3.5mm Pitch 0.43mm")
    (tags "LGA 24L 3x3.5mm Pitch 0.43mm")
    (attr smd)
    (fp_text reference U1 (at 0 -2.7) (layer F.SilkS) hide)
    (fp_text value LSM9DS1 (at 1.05 1.167) (layer F.Fab))
    (fp_text user %R (at 0 -2.7) (layer F.Fab))
    (pad 1 smd rect (at -1.505 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 2 smd rect (at -1.475 -0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCLK))
    (pad 17 smd rect (at 1.475 -0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.475 -0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 16 smd rect (at 1.475 -0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -1.475 0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 10 /SDATA))
    (pad 15 smd rect (at 1.475 0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.475 0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R2-Pad2)"))
    (pad 14 smd rect (at 1.475 0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at -1.075 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 23 smd rect (at -0.645 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 22 smd rect (at -0.215 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 21 smd rect (at 0.215 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 20 smd rect (at 0.645 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 1.075 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at 1.505 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1.505 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R3-Pad2)"))
    (pad 7 smd rect (at -1.075 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R7-Pad2)"))
    (pad 8 smd rect (at -0.645 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R8-Pad2)"))
    (pad 9 smd rect (at -0.215 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R6-Pad2)"))
    (pad 10 smd rect (at 0.215 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R10-Pad2)"))
    (pad 11 smd rect (at 0.645 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad2)"))
    (pad 12 smd rect (at 1.075 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R9-Pad2)"))
    (pad 13 smd rect (at 1.505 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-24L_3x3.5mm_P0.43mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 52.75 109.433 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at -3 0 270) (layer F.SilkS) hide)
    (fp_text value MCP1700-1802 (at 3 -3 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /135_VDD))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5CCC5D9F)
    (at 55.375 111.358 270)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value Ferrite_Bead (at -0.208 0.575 90) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /VDD_PLL))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C9E48E4)
    (at 96.95 102.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value .1uF (at -0.1 -1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(C4-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C9E48EC)
    (at 131.45 113.6 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C9E48E1)
    (at 82.55 113.6 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(C8-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C9E48E8)
    (at 109.15 102.6 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 -1.43 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at -3.05 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /CH_GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5CAD0F98)
    (at 120.9 106.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.5 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5CACF526)
    (at 100.3 109.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value .1uF (at 2.65 0 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5CACF54D)
    (at 135.2 107.8 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 -1.65 180) (layer F.SilkS) hide)
    (fp_text value 10uF (at 3.6 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.85 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 75 /VAAL))
    (pad 2 smd roundrect (at 0.85 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5CAD0FA5)
    (at 142.6 118.4 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 -1.65 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 -1.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.85 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 76 /VDD_IOL))
    (pad 2 smd roundrect (at 0.85 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5CAD0F95)
    (at 139.9 106.75 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.4 -0.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /135_VDD))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5CAD0F9C)
    (at 141 106.75 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.4 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /135_VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5CAD0F9E)
    (at 148 109.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.55 -0.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 /VDD_PLL_L))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5CAD0F8C)
    (at 139.95 117.8 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.4 0.3 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 /VDD_IOL))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5CAD0FA9)
    (at 142.9 105.9 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.85 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /135_VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5CACF51A)
    (at 148.8 111.35)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 10uF (at 3.5 0.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.85 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 77 /VDD_PLL_L))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5CAD0FA1)
    (at 137.05 111.75 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.5 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /VAAL))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5CACF517)
    (at 136.95 109.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 2.4 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /VAAL))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5CACF51D)
    (at 57 123.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C40 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(C40-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5CACF50A)
    (at 147.75 122 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C41 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(C41-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CACF4FF)
    (at 52 122)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 55 "Net-(C40-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CACF537)
    (at 153 122)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J5 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 56 "Net-(C41-Pad1)"))
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5CACF54A)
    (at 147.55 108.15 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value Ferrite_Bead (at 5.6 -0.05 270) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 /VDD_PLL_L))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(L2-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5CAD0FAD)
    (at 149.2 107.65 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.55 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(L2-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5CAD0F92)
    (at 148.7 113.5 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.7 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(R25-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5CACF521)
    (at 147.65 113.5 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.65 0.05 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(R25-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5CAD0F8F)
    (at 138.7 106.7 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value 0 (at -1.5 0) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /STANDBY2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomParts:IBGA63_9x9 (layer B.Cu) (tedit 5ADE0811)
    (at 142.5 112.233 180)
    (fp_text reference U6 (at -1.9 5.5 180) (layer B.SilkS) hide)
    (fp_text value AR0135 (at 4.8 2.5 180) (layer B.Fab) hide)
    (pad 64 smd circle (at 3.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 79 /IM_RSTL))
    (pad 63 smd circle (at 2.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 76 /VDD_IOL))
    (pad 62 smd circle (at 1.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 76 /VDD_IOL))
    (pad 2 smd circle (at -2.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd circle (at -1.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd circle (at -0.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd circle (at 0.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd circle (at 1.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 7 smd circle (at 2.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 8 smd circle (at 3.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 40 /STANDBY2))
    (pad 9 smd circle (at -3.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 77 /VDD_PLL_L))
    (pad 10 smd circle (at -2.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd circle (at -1.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd circle (at -0.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd circle (at 0.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd circle (at 1.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 15 smd circle (at 2.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 75 /VAAL))
    (pad 16 smd circle (at 3.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 75 /VAAL))
    (pad 17 smd circle (at -3.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 23 /EXTCLK))
    (pad 18 smd circle (at -2.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd circle (at -1.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd circle (at -0.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd circle (at 0.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 22 smd circle (at 1.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 23 smd circle (at 2.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 24 smd circle (at 3.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 25 smd circle (at -3.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(R25-Pad2)"))
    (pad 26 smd circle (at -2.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 11 /SCLK))
    (pad 27 smd circle (at -1.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 10 /SDATA))
    (pad 28 smd circle (at -0.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 29 smd circle (at 0.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 30 smd circle (at 1.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 31 smd circle (at 2.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 75 /VAAL))
    (pad 32 smd circle (at 3.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 75 /VAAL))
    (pad 33 smd circle (at -3.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 48 /HSYNC2))
    (pad 34 smd circle (at -2.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 46 /VSYNC2))
    (pad 35 smd circle (at -1.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R24-Pad1)"))
    (pad 36 smd circle (at -0.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(R31-Pad1)"))
    (pad 37 smd circle (at 0.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 38 smd circle (at 1.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 76 /VDD_IOL))
    (pad 39 smd circle (at 2.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 40 smd circle (at 3.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 41 smd circle (at -3.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 70 /DCMI_D4L))
    (pad 42 smd circle (at -2.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 71 /DCMI_D5L))
    (pad 43 smd circle (at -1.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 58 /DCMI_D6L))
    (pad 44 smd circle (at -0.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 60 /DCMI_D7L))
    (pad 45 smd circle (at 0.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 46 smd circle (at 1.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 76 /VDD_IOL))
    (pad 47 smd circle (at 2.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 48 smd circle (at 3.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 49 smd circle (at -3.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 64 /DCMI_D0L))
    (pad 50 smd circle (at -2.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 62 /DCMI_D1L))
    (pad 51 smd circle (at -1.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 72 /DCMI_D2L))
    (pad 52 smd circle (at -0.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 73 /DCMI_D3L))
    (pad 53 smd circle (at 0.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 54 smd circle (at 1.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 76 /VDD_IOL))
    (pad 55 smd circle (at 2.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 80 /TRIGGER_L))
    (pad 56 smd circle (at 3.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(U10-Pad11)"))
    (pad 57 smd circle (at -3.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 58 smd circle (at -2.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 59 smd circle (at -1.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 60 smd circle (at -0.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 61 smd circle (at 0.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module CustomParts:LensM12_Alum (layer B.Cu) (tedit 5CACECC9)
    (at 142.5 112.233 90)
    (fp_text reference U7 (at -7.5 8.4 90) (layer B.SilkS) hide)
    (fp_text value LensM12 (at -6.7 10 90) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 11 0 90) (size 3.8 3.8) (drill 2.1) (layers *.Cu *.Mask)
      (net 2 GND) (clearance 0.1))
    (pad 1 thru_hole circle (at -11 0 90) (size 3.8 3.8) (drill 2.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/CameraHousing.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/CameraHousingScrew.step
      (offset (xyz 11 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/CameraHousingScrew.step
      (offset (xyz -11 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5CAFBE79)
    (at 103.108234 108.128237)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at -1.6 0 -90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(R19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5CAFBE69)
    (at 103.108234 107.128237 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 1.6 0 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(R20-Pad1)"))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(R19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5CAFBE7E)
    (at 103.108234 106.078237)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at -1.6 0 -90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(R21-Pad1)"))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5CAFBE6F)
    (at 103.108234 105.078237 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 1.6 0 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(R21-Pad1)"))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5CAFBE63)
    (at 117.7 111.6)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -5.375) (layer F.SilkS) hide)
    (fp_text value 74LS32 (at 0.05 -2.85 -180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 /DCMI_D6R))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 /DCMI_D6L))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /DCMI_D6))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 /DCMI_D7R))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 /DCMI_D7L))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /DCMI_D7))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /DCMI_D1))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 /DCMI_D1R))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 /DCMI_D1L))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /DCMI_D0))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 /DCMI_D0R))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 /DCMI_D0L))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-363_SC-70-6 (layer B.Cu) (tedit 5CAFBE66)
    (at 106.608234 106.728237 180)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference U8 (at 0 2 180) (layer B.SilkS) hide)
    (fp_text value 74LVC2G14 (at -2.575001 1.925001) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0.65 180) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 47 /HSYNC1))
    (pad 3 smd rect (at -0.95 -0.65 180) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 48 /HSYNC2))
    (pad 5 smd rect (at 0.95 0 180) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 2V8))
    (pad 2 smd rect (at -0.95 0 180) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.95 -0.65 180) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R20-Pad1)"))
    (pad 6 smd rect (at 0.95 0.65 180) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5CAFC0B9)
    (at 106.4 118.8 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 0 (at -0.05 -1.2) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /PIXCLK))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(R24-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5CAFC0BC)
    (at 64.95 113.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(R28-Pad1)"))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /PIXCLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 5CB0CEC8)
    (at 95 109.66 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 -7.41 180) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 90) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 2V8))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 5CB0BE2B)
    (at 110 109.66 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 -7.41 180) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 2V8))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /LASER))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer B.Cu) (tedit 5CED78B0)
    (at 115.7 113.6)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U9 (at 0 5.375) (layer B.SilkS) hide)
    (fp_text value 74LS32 (at 0 -5.375) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 /DCMI_D5R))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 71 /DCMI_D5L))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 18 /DCMI_D5))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 /DCMI_D3R))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 73 /DCMI_D3L))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 21 /DCMI_D3))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 20 /DCMI_D2))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 /DCMI_D2R))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 72 /DCMI_D2L))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 16 /DCMI_D4))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 65 /DCMI_D4R))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 70 /DCMI_D4L))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer B.Cu) (tedit 5CED7312)
    (at 104.6 113.8 180)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U10 (at 0 5.375 180) (layer B.SilkS) hide)
    (fp_text value 74LS32 (at 0 -5.375 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 14 smd rect (at 2.7 3.81 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 2V8))
    (pad 13 smd rect (at 2.7 2.54 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(R19-Pad1)"))
    (pad 12 smd rect (at 2.7 1.27 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 84 /OEL))
    (pad 11 smd rect (at 2.7 0 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(U10-Pad11)"))
    (pad 10 smd rect (at 2.7 -1.27 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(R21-Pad1)"))
    (pad 9 smd rect (at 2.7 -2.54 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 83 /OER))
    (pad 8 smd rect (at 2.7 -3.81 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(U10-Pad8)"))
    (pad 7 smd rect (at -2.7 -3.81 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.7 -2.54 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 /VSYNC))
    (pad 5 smd rect (at -2.7 -1.27 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 45 /VSYNC1))
    (pad 4 smd rect (at -2.7 0 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 46 /VSYNC2))
    (pad 3 smd rect (at -2.7 1.27 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 /HSYNC))
    (pad 2 smd rect (at -2.7 2.54 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 47 /HSYNC1))
    (pad 1 smd rect (at -2.7 3.81 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 48 /HSYNC2))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5CF6AA0E)
    (at 119.1 119.1 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value .1uF (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5CF6AABE)
    (at 141 117.8 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 /VDD_IOL))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5CF6AB3F)
    (at 145 117.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 4.7 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 /VDD_IOL))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(L2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5CF6AB65)
    (at 136 105.8 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value 4.7 (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(L2-Pad2)"))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /VAAL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5CF6AADE)
    (at 136.4 113.2 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R31 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(R31-Pad1)"))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /FLASH))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5CF6AD1F)
    (at 64.9 118.3 315)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R32 (at 0 -1.17 315) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 315) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(R32-Pad1)"))
    (pad 2 smd roundrect (at 0.48 0 315) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /FLASH))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 49.25 124.75) (end 48.5 124.75) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 155.75 124.75) (end 155.75 125.5) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 140.5 124.75) (end 139.75 124.75) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 64.5 124.75) (end 64.5 125.5) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 84.25 123.75) (end 83.5 123.75) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 120.75 123.75) (end 120.75 124.5) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.75 99.75) (end 111.25 99.75) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 91.500001 102.999999) (end 93.75 99.75) (angle -69.39030706) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.75 99.75) (end 140.25 99.75) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 113.499999 102.999999) (end 115.749998 99.75) (angle -69.39030706) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.75 99.75) (end 151.5 99.75) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 142.499999 103) (end 144.749998 99.750001) (angle -69.39030706) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 62.5 103) (end 64.749999 99.750001) (angle -69.39030706) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.75 99.75) (end 89.25 99.75) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 122.25 122.5) (end 122.25 121.75) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 82.75 122.5) (end 83.5 122.5) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 66 122.5) (end 66 121.75) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 139 122.5) (end 139.75 122.5) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.75 125.5) (end 140.5 125.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.75 124.75) (end 139.75 122.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.5 124.75) (end 156.5 121.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 65.25 124.75) (end 65.25 122.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5 125.5) (end 49.25 125.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5 124.75) (end 48.5 121.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.75 121.75) (end 66 121.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.5 123.75) (end 83.5 122.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.75 124.5) (end 84.25 124.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.5 122.5) (end 121.5 123.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.5 121.75) (end 122.25 121.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139 121.75) (end 122.5 121.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.5 104.75) (end 156.5 121.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.5 99.75) (end 156.5 104.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.5 99.75) (end 60.25 99.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5 104.75) (end 53.5 99.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5 121.75) (end 48.5 104.75) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 48.45 101.683) (xy 46.45 101.683) (xy 46.45 99.683) (xy 156.5 99.75) (xy 156.5 124.75)
        (xy 48.45 124.683)
      )
    )
  )
  (zone (net 1) (net_name 2V8) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.45 104.683) (xy 46.45 104.683) (xy 46.45 102.683) (xy 48.45 102.683) (xy 48.45 99.683)
        (xy 156.5 99.75) (xy 156.5 124.75) (xy 48.45 124.683)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.45 107.683) (xy 46.45 107.683) (xy 46.45 105.683) (xy 48.45 105.683) (xy 48.45 99.683)
        (xy 156.5 99.75) (xy 156.5 124.75) (xy 48.45 124.683)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.45 110.683) (xy 46.45 110.683) (xy 46.45 108.683) (xy 48.45 108.683) (xy 48.45 99.683)
        (xy 156.5 99.75) (xy 156.5 124.75) (xy 48.45 124.683)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.35)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 104.45 113) (xy 103.8 113) (xy 103.8 111.783) (xy 103.8 111.483) (xy 103 111.483)
        (xy 103 110.65) (xy 104.45 110.65)
      )
    )
  )
)
