<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="71.12" y2="0" width="0" layer="20"/>
<wire x1="71.12" y1="0" x2="71.12" y2="54.6" width="0" layer="20"/>
<wire x1="71.12" y1="54.6" x2="0" y2="54.6" width="0" layer="20"/>
<wire x1="0" y1="54.6" x2="0" y2="0" width="0" layer="20"/>
<text>POWER</text>
<text>+</text>
<text>-</text>
<text>SPEAKER</text>
<text>+</text>
<text>-</text>
<text>VPP</text>
<text>VDD</text>
<text>GND</text>
<text>DAT</text>
<text>CLK</text>
<text>PGM</text>
<text>ICSP</text>
<text>U1</text>
<text>U2</text>
<text>U3</text>
<text>U4</text>
<text>USB</text>
<text>C14</text>
<text>C16</text>
<text>C15</text>
<text>C2</text>
<text>C1</text>
<text>C3</text>
<text>C7</text>
<text>R4</text>
<text>R3</text>
<text>C6</text>
<text>C13</text>
<text>C11</text>
<text>C12</text>
<text>R5</text>
<text>R6</text>
<text>R1</text>
<text>C5</text>
<text>R2</text>
<text>C4</text>
<text>C8</text>
<text>R9</text>
<text>R10</text>
<text>C9</text>
<text>R7</text>
<text>C10</text>
<text>R8</text>
<text>STATUS</text>
<text>PLAY</text>
<text>PUSH
TO
PLAY</text>
<text>picWAVE</text>
<text>J3</text>
<text>J4</text>
<text>J2</text>
<text>J1</text>
<text>S1</text>
<text>3.6-16V</text>
<text>Ryan Clarke</text>
<text>28 Dec 2016</text>
</plain>
<libraries>
<library name="kj6msg">
<description>&lt;b&gt;KJ6MSG Eagle Library&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Ryan Clarke&lt;br&gt;
kj6msg@arrl.net</description>
<packages>
<package name="1206">
<description>SparkFun</description>
</package>
<package name="1206@1">
</package>
<package name="NL1GS">
<description>&lt;b&gt;UWT Aluminum Electrolytic Capacitors&lt;/b&gt;
&lt;br&gt;
8 x 10
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="22-05-3021">
<description>&lt;b&gt;Molex 22-05-3021&lt;/b&gt;
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="1X06">
<description>&lt;b&gt;6-pin, 0.1" header&lt;/b&gt;</description>
</package>
<package name="XM7D-0512">
<description>&lt;b&gt;Omron XM7D-0512&lt;/b&gt;
&lt;br&gt;
USB 2.0 USB mini-B Receptacle
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="LED-1206">
<description>SparkFun</description>
</package>
<package name="KS-00Q-01">
<description>&lt;b&gt;E-Switch SPST Pushbutton&lt;/b&gt;
&lt;br&gt;
SPST-NO push button switch
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="SOIJ-8">
<description>&lt;b&gt;8-pin Plastic Small Outline - Medium&lt;/b&gt;
&lt;br&gt;
5.28mm body
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="SSOP-16">
<description>&lt;b&gt;16-pin Plastic Shrink Small Outline&lt;/b&gt;
&lt;br&gt;
3.90mm body
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="SOT-23-5">
<description>&lt;b&gt;5-pin Small Outline Transistor&lt;/b&gt;
&lt;br&gt;
1.60mm body
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
<package name="SOIC-20-W">
<description>&lt;b&gt;20-pin Small Outline Integrated Circuit - Wide&lt;/b&gt;
&lt;br&gt;
7.50mm body
&lt;br&gt;
Ryan Clarke, KJ6MSG</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="kj6msg" package="1206" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C10" library="kj6msg" package="1206@1" value="47p">
<attribute name="VALUE"/>
</element>
<element name="C11" library="kj6msg" package="1206@1" value="4.7u">
<attribute name="VALUE"/>
</element>
<element name="C12" library="kj6msg" package="1206@1" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C13" library="kj6msg" package="1206@1" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C14" library="kj6msg" package="1206" value="1u">
<attribute name="VALUE"/>
</element>
<element name="C15" library="kj6msg" package="1206" value="2.2u">
<attribute name="VALUE"/>
</element>
<element name="C16" library="kj6msg" package="1206" value="10n">
<attribute name="VALUE"/>
</element>
<element name="C2" library="kj6msg" package="1206" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C3" library="kj6msg" package="NL1GS" value="470u"/>
<element name="C4" library="kj6msg" package="1206" value="3300p">
<attribute name="VALUE"/>
</element>
<element name="C5" library="kj6msg" package="1206" value="3900p">
<attribute name="VALUE"/>
</element>
<element name="C6" library="kj6msg" package="1206" value="3300p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="kj6msg" package="1206@1" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="C9" library="kj6msg" package="1206@1" value="47p"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="VERSION" value="v01"/>
<attribute name="DESIGNER" value="Nobody"/>
</element>
<element name="J1" library="kj6msg" package="22-05-3021" value="BATTERY">
<attribute name="VALUE"/>
<attribute name="PART-NO" value="0022053021"/>
<attribute name="MANUFACTURER" value="Molex"/>
<attribute name="DIGI-KEY" value="WM4300-ND"/>
</element>
<element name="J2" library="kj6msg" package="22-05-3021" value="SPEAKER">
<attribute name="VALUE"/>
<attribute name="PART-NO" value="0022053021"/>
<attribute name="MANUFACTURER" value="Molex"/>
<attribute name="DIGI-KEY" value="WM4300-ND"/>
</element>
<element name="J3" library="kj6msg" package="1X06" value="ICSP">
<attribute name="VALUE"/>
</element>
<element name="J4" library="kj6msg" package="XM7D-0512" value="USB-MINI-B">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="kj6msg" package="LED-1206" value="LED-1206">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="kj6msg" package="LED-1206" value="LED-1206">
<attribute name="VALUE"/>
</element>
<element name="R1" library="kj6msg" package="1206" value="2k2">
<attribute name="VALUE"/>
</element>
<element name="R10" library="kj6msg" package="1206" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R2" library="kj6msg" package="1206" value="2k2">
<attribute name="VALUE"/>
</element>
<element name="R3" library="kj6msg" package="1206" value="931">
<attribute name="VALUE"/>
</element>
<element name="R4" library="kj6msg" package="1206" value="931">
<attribute name="VALUE"/>
</element>
<element name="R5" library="kj6msg" package="1206" value="130">
<attribute name="VALUE"/>
</element>
<element name="R6" library="kj6msg" package="1206" value="130">
<attribute name="VALUE"/>
</element>
<element name="R7" library="kj6msg" package="1206" value="27">
<attribute name="VALUE"/>
</element>
<element name="R8" library="kj6msg" package="1206" value="27">
<attribute name="VALUE"/>
</element>
<element name="R9" library="kj6msg" package="1206" value="4k7">
<attribute name="VALUE"/>
</element>
<element name="S1" library="kj6msg" package="KS-00Q-01" value="SWITCH-SPST-ESWITCH">
<attribute name="PART-NO" value="KS-00Q-01"/>
<attribute name="MANUFACTURER" value="E-Switch"/>
<attribute name="DIGI-KEY" value="EG4788-ND"/>
</element>
<element name="U2" library="kj6msg" package="SOIJ-8" value="25AA1024-I/SM">
<attribute name="VALUE"/>
</element>
<element name="U3" library="kj6msg" package="SSOP-16" value="FT230XS">
<attribute name="VALUE"/>
</element>
<element name="U4" library="kj6msg" package="SOT-23-5" value="LP2985-33DBVR"/>
<element name="U1" library="kj6msg" package="SOIC-20-W" value="PIC16F1708-I/SO">
<attribute name="VALUE"/>
</element>
<element name="C7" library="kj6msg" package="1206" value=".022u">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ICSPDAT">
<contactref element="J3" pad="4"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="ICSPCLK">
<contactref element="J3" pad="5"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="N$3">
<contactref element="C5" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="OPA1+">
<contactref element="C4" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="OPA1">
<contactref element="C5" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="!BTN!">
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="4"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="OPA2+">
<contactref element="C6" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="OPA2">
<contactref element="U1" pad="7"/>
<contactref element="C7" pad="2"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="DAC1">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="VPP">
<contactref element="J3" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="SCLK">
<contactref element="U2" pad="6"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="3"/>
<contactref element="C15" pad="1"/>
<contactref element="U4" pad="5"/>
<contactref element="U3" pad="12"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J3" pad="3"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="13"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="J4" pad="5"/>
<contactref element="U2" pad="4"/>
<contactref element="J2" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="LED1">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="RX">
<contactref element="U3" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="VBUS">
<contactref element="R9" pad="2"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="C8" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="10"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="N$11">
<contactref element="R8" pad="1"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="D+">
<contactref element="R7" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="D-">
<contactref element="R8" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R10" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="U3" pad="16"/>
</signal>
<signal name="!RTS!">
<contactref element="U3" pad="2"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="LED2">
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="N$14">
<contactref element="R6" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="R5" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="!SS!">
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="TX">
<contactref element="U3" pad="4"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="VBATT">
<contactref element="C14" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U4" pad="4"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U3" pad="8"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="J2" pad="1"/>
<contactref element="C3" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
