(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~65~ubuntu17.10.1)
  (general
    (thickness 1.6)
    (drawings 51)
    (tracks 3)
    (zones 0)
    (modules 5)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B88D7F3)
    (at 18.73 27.73)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_02x02_Counter_Clockwise (at 1.27 4.87) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm_Clear (layer F.Cu) (tedit 5B88CB70)
    (at 25.255115 10.622036 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96 180) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 3.96 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5B88CBE3)
    (at 7.909315 20.29643 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.37 90) (layer F.SilkS) hide)
    (fp_text value R (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:ART_OSHWA_CIRCLES (layer F.Cu) (tedit 0)
    (at 15.98 19.77)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value ART_OSHWA_CIRCLES (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 15.46 6.043297 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (gr_line (start 11.86 36.69) (end 28.34 36.69) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 26.54 38.15) (end 28.09 36.76) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 24.13 39.42) (end 26.54 38.15) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 22.21 39.99) (end 24.13 39.42) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 19.71 40.23) (end 22.21 39.99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 17.42 39.87) (end 19.71 40.23) (layer Edge.Cuts) (width 0.15))
  (gr_text D (at 26 12.73 90) (layer B.SilkS))
  (gr_text L (at 22.13 12.59 90) (layer B.SilkS))
  (gr_text E (at 24.09 12.64 90) (layer B.SilkS))
  (gr_text "DC26 SAO" (at 16.36 29 90) (layer B.SilkS))
  (gr_text "Andrew Sowa\nOSHWA Summit\n2018 MIT" (at 27 29 90) (layer B.SilkS))
  (gr_text - (at 25.255115 8.35) (layer B.SilkS))
  (gr_text + (at 22.715115 8.35) (layer B.SilkS))
  (gr_text Resistor (at 5.42 16.8 90) (layer B.SilkS))
  (gr_text GND (at 18.73 34.07 90) (layer B.SilkS))
  (gr_text VCC (at 18.73 23.93 90) (layer B.SilkS))
  (gr_arc (start 23.985115 10.622036) (end 18.447872 11.611768) (angle -191.9669199) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 7.909315 16.69643) (end 16.291355 18.445091) (angle -40.85140938) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 23.985115 10.622036) (end 25.779354 5.29087) (angle -43.9669199) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 15.094944 6.043297) (end 15.393359 12.536443) (angle -28.42191916) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 7.909315 16.69643) (end 8.962815 8.198987) (angle -197.8514094) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 15.094944 6.043297) (end 21.575378 5.539341) (angle -194.9219192) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 29.209635 5.068208) (end 29.196802 8.505684) (angle -273.9278235) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 20 29) (end 9.511423 25.107711) (angle -309.7195676) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name "Net-(D1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.814791 41.107139) (xy 33.745209 41.107139) (xy 32.855209 -0.862861) (xy -1.814791 -0.802861)
      )
    )
  )
)
