(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 234)
    (tracks 87)
    (zones 0)
    (modules 15)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.762 0.762)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 /NRST)
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(D4-Pad2)")
  (net 8 "Net-(J1-Pad6)")
  (net 9 /SWCLK)
  (net 10 /SWDIO)
  (net 11 /RED_LED1)
  (net 12 /RED_LED2)
  (net 13 /BLUE_LED)
  (net 14 /WHT_LED)
  (net 15 "Net-(U1-Pad3)")
  (net 16 "Net-(U1-Pad2)")
  (net 17 "Net-(U1-Pad8)")
  (net 18 "Net-(U1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.254)
    (diff_pair_width 0.1524)
    (add_net +BATT)
    (add_net /BLUE_LED)
    (add_net /NRST)
    (add_net /RED_LED1)
    (add_net /RED_LED2)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /WHT_LED)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
  )
  (net_class BATT ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.635)
    (via_drill 0.3048)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.254)
    (diff_pair_width 0.1524)
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 5BD3D222)
    (at 136.4 142 354)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45 354) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 0 1.55 354) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 354) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0 354) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connect:Tag-Connect_TC2030-IDC-NL (layer B.Cu) (tedit 58A4CF26)
    (at 147.486661 138.708893 39)
    (descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf")
    (tags "tag connect programming header pogo pins")
    (attr virtual)
    (fp_text reference J1 (at 0 -2.7 39) (layer B.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 0 2.3 39) (layer B.Fab))
    (fp_text user %R (at 0 0 39) (layer B.Fab))
    (pad 6 connect circle (at 1.27 0.635 39) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "Net-(J1-Pad6)"))
    (pad 5 connect circle (at 1.27 -0.635 39) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 4 connect circle (at -0.000001 0.635 39) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 /SWCLK))
    (pad 3 connect circle (at 0.000001 -0.635 39) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 3 /NRST))
    (pad 2 connect circle (at -1.27 0.635 39) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 /SWDIO))
    (pad 1 connect circle (at -1.27 -0.635 39) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 +BATT))
    (pad "" np_thru_hole circle (at -2.54 0 39) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -1.015999 39) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.539999 1.016 39) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77)
    (at 145.1 125.8 180)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 3.55 180) (layer B.SilkS))
    (fp_text value STM32L011D3Px (at 0 -3.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 14 smd rect (at 2.95 1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 9 /SWCLK))
    (pad 13 smd rect (at 2.95 1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 /SWDIO))
    (pad 12 smd rect (at 2.95 0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 /WHT_LED))
    (pad 11 smd rect (at 2.95 0 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 /BLUE_LED))
    (pad 10 smd rect (at 2.95 -0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 +BATT))
    (pad 9 smd rect (at 2.95 -1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.95 -1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(U1-Pad8)"))
    (pad 7 smd rect (at -2.95 -1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at -2.95 -1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 /RED_LED1))
    (pad 5 smd rect (at -2.95 -0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 12 /RED_LED2))
    (pad 4 smd rect (at -2.95 0 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 /NRST))
    (pad 3 smd rect (at -2.95 0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at -2.95 1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at -2.95 1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module new_footprints:BATT-HLD-001 (layer B.Cu) (tedit 5BD498F7)
    (at 122.55 127.3)
    (fp_text reference BT1 (at -11.3 -4.2) (layer B.SilkS))
    (fp_text value Battery_Cell (at 0 10.16) (layer B.Fab))
    (pad 1 smd rect (at -11.45 0) (size 2.5 5.1) (layers B.Cu B.Paste B.Mask)
      (net 1 +BATT))
    (pad 1 smd rect (at 11.45 0) (size 2.5 5.1) (layers B.Cu B.Paste B.Mask)
      (net 1 +BATT))
    (pad 2 smd circle (at 0 0) (size 17.8 17.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 5BD3D205)
    (at 121.60001 113.499913 354)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45 354) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 0 1.55 354) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 354) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 354) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 139.7 128.131 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.25 0 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +BATT))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 5BD3D217)
    (at 128.369826 118.909419 354)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45 354) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 0 1.55 354) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 354) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 354) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 150.6 124.55 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.196 -0.022) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 /NRST))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 5BD3D20D)
    (at 164.8 116.2 353)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45 353) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 0 1.55 353) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 353) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 353) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module new_footprints:1.8mm_Hole (layer F.Cu) (tedit 5BE793C5)
    (at 136.144 103.251)
    (fp_text reference REF** (at 0 -3) (layer F.SilkS) hide)
    (fp_text value 1.3mm_Hole (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.762 0.762) (drill 0.762) (layers *.Mask F.Cu))
  )
  (module new_footprints:enterprise_230dpi_silk (layer F.Cu) (tedit 5BE78F6F)
    (at 138.3 124.7)
    (fp_text reference G*** (at 26.546 12.968) (layer F.SilkS) hide)
    (fp_text value LOGO (at 26.546 15) (layer F.SilkS) hide)
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 146.673 130.1115 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.012 -1.4605 180) (layer B.SilkS))
    (fp_text value 520 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 11 /RED_LED1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 155.829 125.6665 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.1463 -0.0254 180) (layer B.SilkS))
    (fp_text value 520 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 12 /RED_LED2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 137.795 127.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.2932 0.127) (layer B.SilkS))
    (fp_text value 520 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 13 /BLUE_LED))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 139 124.25 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.5 180) (layer B.SilkS))
    (fp_text value 520 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 14 /WHT_LED))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 136.9 102.5) (end 136.7028 102.7684) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.89 104.267) (end 136.0424 103.9876) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.4 105.1) (end 135.89 104.267) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.2 101.9) (end 143.5 101.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.9 102.3) (end 143.2 101.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.5 101.9) (end 141.9 102.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.2 101.7) (end 141.5 101.9) (layer Edge.Cuts) (width 0.15))
  (gr_text "Audrey 2018" (at 175.133 111.633 38) (layer B.Cu))
  (gr_text "Built from the compartment." (at 171.832413 109.473168 30) (layer B.SilkS))
  (gr_line (start 154.3304 134.366) (end 154.0764 134.5184) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 134.2136) (end 154.3304 134.366) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.3116 133.8072) (end 154.94 134.2136) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.1912 133.1976) (end 156.3116 133.8072) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.766 132.5372) (end 158.1912 133.1976) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.4932 131.6736) (end 159.766 132.5372) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.2552 131.2164) (end 161.4932 131.6736) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.0172 130.6068) (end 162.2552 131.2164) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.6268 129.9464) (end 163.0172 130.6068) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.592 128.6764) (end 163.6268 129.9464) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.4048 127.3556) (end 164.592 128.6764) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.7096 126.6444) (end 165.4048 127.3556) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.862 126.0856) (end 165.7096 126.6444) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.9636 125.476) (end 165.862 126.0856) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.8112 124.7648) (end 165.9636 125.476) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.5572 124.1552) (end 165.8112 124.7648) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.1 123.5964) (end 165.5572 124.1552) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.3888 123.0376) (end 165.1 123.5964) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.7632 122.1232) (end 164.3888 123.0376) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.7124 122.0216) (end 162.7632 122.1232) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.83 120.8532) (end 162.7124 122.0216) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.6936 120.0404) (end 163.83 120.8532) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.0492 119.7864) (end 164.6936 120.0404) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.5064 119.634) (end 165.0492 119.7864) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 119.5832) (end 165.5064 119.634) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.3352 119.5832) (end 166.37 119.5832) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.9448 119.0752) (end 167.3352 119.5832) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.3512 118.7704) (end 167.9448 119.0752) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.656 118.6688) (end 168.3512 118.7704) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.1132 118.618) (end 168.656 118.6688) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.3164 118.5672) (end 169.1132 118.618) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.672 118.3132) (end 169.3164 118.5672) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.434 117.602) (end 169.672 118.3132) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.1452 116.7892) (end 170.434 117.602) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.704 115.9764) (end 171.1452 116.7892) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.1612 115.57) (end 171.704 115.9764) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.8884 114.3) (end 172.1612 115.57) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.4096 110.7948) (end 173.8884 114.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.7972 108.9152) (end 178.4096 110.7948) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.6608 108.2548) (end 180.7972 108.9152) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.118 107.8992) (end 181.6608 108.2548) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.4736 107.5436) (end 182.118 107.8992) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.88 107.0356) (end 182.4736 107.5436) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.134 106.426) (end 182.88 107.0356) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.3372 105.5624) (end 183.134 106.426) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.388 104.7496) (end 183.3372 105.5624) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.2864 104.0892) (end 183.388 104.7496) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.9816 103.5812) (end 183.2864 104.0892) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.4736 103.124) (end 182.9816 103.5812) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.9148 102.87) (end 182.4736 103.124) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.5592 102.7684) (end 181.9148 102.87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.848 102.7176) (end 181.5592 102.7684) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.2384 102.8192) (end 180.848 102.7176) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.5272 103.0732) (end 180.2384 102.8192) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.9176 103.4288) (end 179.5272 103.0732) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.6128 103.632) (end 178.9176 103.4288) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.4604 103.5812) (end 178.6128 103.632) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.2572 103.3272) (end 178.4604 103.5812) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.0032 103.0732) (end 178.2572 103.3272) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.5968 102.87) (end 178.0032 103.0732) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.1396 102.87) (end 177.5968 102.87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.5808 103.0224) (end 177.1396 102.87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.0728 103.2256) (end 176.5808 103.0224) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.514 103.5304) (end 176.0728 103.2256) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.0568 103.8352) (end 175.514 103.5304) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.5996 104.2416) (end 175.0568 103.8352) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.1584 105.41) (end 174.5996 104.2416) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.1584 105.5624) (end 175.1584 105.41) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.6588 110.8964) (end 175.1584 105.5624) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.9824 111.8108) (end 165.6588 110.8964) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.2712 112.268) (end 163.9824 111.8108) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.7124 112.7252) (end 163.2712 112.268) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.4076 113.0808) (end 162.7124 112.7252) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.1536 113.4872) (end 162.4076 113.0808) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.7472 114.554) (end 162.1536 113.4872) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.544 115.4684) (end 161.7472 114.554) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.5948 116.2812) (end 161.544 115.4684) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.798 116.8908) (end 161.5948 116.2812) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.0012 117.348) (end 161.798 116.8908) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.3568 117.9576) (end 162.0012 117.348) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.7632 118.618) (end 162.3568 117.9576) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.798 119.5832) (end 162.7632 118.618) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.7312 120.5992) (end 161.798 119.5832) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.3756 120.8532) (end 160.7312 120.5992) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.0708 120.9548) (end 160.3756 120.8532) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.766 120.9548) (end 160.0708 120.9548) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.242 120.4976) (end 159.766 120.9548) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.9052 119.9388) (end 158.242 120.4976) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.7716 119.4816) (end 155.9052 119.9388) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.7396 119.126) (end 153.7716 119.4816) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.114 118.872) (end 151.7396 119.126) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.2852 118.618) (end 150.114 118.872) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.5928 118.3132) (end 148.2852 118.618) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.0528 118.0592) (end 145.5928 118.3132) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.6464 117.9576) (end 143.0528 118.0592) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.494 117.8052) (end 142.6464 117.9576) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 117.6528) (end 142.494 117.8052) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.7828 117.602) (end 142.24 117.6528) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.5796 117.5512) (end 141.7828 117.602) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.3764 117.3988) (end 141.5796 117.5512) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.0716 117.3988) (end 141.3764 117.3988) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.7668 117.4496) (end 141.0716 117.3988) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.3604 117.6528) (end 140.7668 117.4496) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.954 117.8052) (end 140.3604 117.6528) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.5984 117.856) (end 139.954 117.8052) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.8364 117.8052) (end 139.5984 117.856) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.1252 117.7544) (end 138.8364 117.8052) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.4648 117.6528) (end 138.1252 117.7544) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 117.5004) (end 137.4648 117.6528) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.9568 117.348) (end 137.16 117.5004) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.4836 115.6208) (end 136.9568 117.348) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 113.0808) (end 135.4836 115.6208) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.9436 112.5728) (end 133.35 113.0808) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.842 112.3696) (end 132.9436 112.5728) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.9436 112.268) (end 132.842 112.3696) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.6548 111.9124) (end 132.9436 112.268) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.906 110.4392) (end 133.6548 111.9124) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.7828 108.204) (end 136.906 110.4392) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.8308 106.934) (end 141.7828 108.204) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.4912 106.6292) (end 144.8308 106.934) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.8976 106.3244) (end 145.4912 106.6292) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.2532 105.8672) (end 145.8976 106.3244) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.6088 105.156) (end 146.2532 105.8672) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.9644 104.3432) (end 146.6088 105.156) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.1168 103.7336) (end 146.9644 104.3432) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.1168 103.124) (end 147.1168 103.7336) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.9136 102.5144) (end 147.1168 103.124) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.558 102.0572) (end 146.9136 102.5144) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.9992 101.7016) (end 146.558 102.0572) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.6436 101.5492) (end 145.9992 101.7016) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.1356 101.4984) (end 145.6436 101.5492) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.6276 101.5492) (end 145.1356 101.4984) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.8656 101.7016) (end 144.6276 101.5492) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.5 101.8) (end 143.8656 101.7016) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 136.144 103.251) (end 136.7028 102.7684) (angle -221.3316956) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.7 101.5) (end 141.2 101.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.2 101.5) (end 140.7 101.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.6 101.6) (end 140.2 101.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.2 102) (end 139.6 101.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.1 102.4) (end 138.2 102) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.9 102.5) (end 137.1 102.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.7 107) (end 133.4 105.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.3 108.8) (end 127.7 107) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121 109.2) (end 122.3 108.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.3 109.6) (end 121 109.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.7 110.2) (end 120.3 109.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119 111) (end 119.7 110.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.7 111.6) (end 119 111) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.5 112.2) (end 118.7 111.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.4 113.2) (end 118.5 112.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.5 114.2) (end 118.4 113.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.7 114.7) (end 118.5 114.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.1 115.3) (end 118.7 114.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.6 115.8) (end 119.1 115.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.2 116.2) (end 119.6 115.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121 116.5) (end 120.2 116.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.9 116.7) (end 121 116.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.9 116.8) (end 121.9 116.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.6472 116.7892) (end 122.9 116.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.8504 117.6528) (end 123.6472 116.7892) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.7 117.7) (end 123.8504 117.6528) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.5 117.8) (end 122.7 117.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.6 118) (end 120.5 117.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.4 118.3) (end 117.6 118) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.1 118.7) (end 114.4 118.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.3 119.3) (end 111.1 118.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.4 119.9) (end 107.3 119.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 120.6) (end 104.4 119.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.2 121.3) (end 101.6 120.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.5 121.9) (end 99.2 121.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96 122.6) (end 97.5 121.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.9 123.3) (end 96 122.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.1 123.9) (end 94.9 123.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.6 124.5) (end 94.1 123.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.2 125.2) (end 93.6 124.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.1 125.8) (end 93.2 125.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.1 126.3) (end 93.1 125.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.2 126.6) (end 93.1 126.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.6 127.4) (end 93.2 126.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.5 128.8) (end 93.6 127.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.6 130.1) (end 94.5 128.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.4 131) (end 95.6 130.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.9 132.1) (end 96.4 131) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.4 133.1) (end 97.9 132.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.3 133.8) (end 100.4 133.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.1 134.3) (end 102.3 133.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.6 135.1) (end 104.1 134.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.2 135.9) (end 107.6 135.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.5 136.5) (end 112.2 135.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.2 136.7) (end 117.5 136.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 136.8) (end 120.2 136.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.6 136.9) (end 122 136.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.3 137) (end 126.6 136.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.3 137.2) (end 132.3 137) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.2 137.4) (end 132.3 137.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132 137.7) (end 132.2 137.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.5 138.1) (end 132 137.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.2 138.4) (end 131.5 138.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.1 138.7) (end 131.2 138.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131 139.2) (end 131.1 138.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.6 140.1) (end 131 139.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.4 141.1) (end 130.6 140.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.4 142.3) (end 130.4 141.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.6 143.4) (end 130.4 142.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.1 144.5) (end 130.6 143.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.9 145.5) (end 131.1 144.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.8 146.4) (end 131.9 145.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.6 147) (end 132.8 146.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.4 147.4) (end 133.6 147) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.5 147.6) (end 134.4 147.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.3 147.6) (end 135.5 147.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.2 147.5) (end 136.3 147.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.8 147) (end 137.2 147.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.3 146.8) (end 138.8 147) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 146.4) (end 139.3 146.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.4 146.2) (end 140 146.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.4 145.9) (end 140.4 146.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.5 145.5) (end 141.4 145.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.4 145) (end 142.5 145.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.2 144.4) (end 143.4 145) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.5 143.4) (end 144.2 144.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.9 142.2) (end 145.5 143.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.2 140.1) (end 146.9 142.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.5 137.7) (end 149.2 140.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.0764 134.5184) (end 151.5 137.7) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.834 96.266) (xy 86.614 96.52) (xy 86.36 152.4) (xy 195.58 152.4) (xy 196.088 96.266)
      )
    )
  )
)
