<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="30.15" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="30.46" y2="0" width="0" layer="20"/>
<wire x1="30.46" y1="0" x2="31.73" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="31.73" y1="1.27" x2="31.73" y2="30.15" width="0" layer="20"/>
<wire x1="31.73" y1="30.15" x2="30.46" y2="31.42" width="0" layer="20" curve="90"/>
<wire x1="30.46" y1="31.42" x2="1.27" y2="31.42" width="0" layer="20"/>
<wire x1="1.27" y1="31.42" x2="0" y2="30.15" width="0" layer="20" curve="90"/>
<wire x1="12.7" y1="20.32" x2="12.7" y2="29.21" width="0.254" layer="20"/>
<wire x1="12.7" y1="29.21" x2="11.43" y2="29.21" width="0.254" layer="20"/>
<wire x1="11.43" y1="29.21" x2="11.43" y2="20.32" width="0.254" layer="20"/>
<wire x1="3.429" y1="10.668" x2="17.907" y2="10.668" width="0.254" layer="20"/>
<wire x1="17.907" y1="10.668" x2="20.32" y2="8.255" width="0.254" layer="20"/>
<wire x1="20.32" y1="8.255" x2="26.162" y2="8.255" width="0.254" layer="20"/>
<wire x1="26.162" y1="8.255" x2="26.162" y2="6.985" width="0.254" layer="20"/>
<wire x1="26.162" y1="6.985" x2="19.685" y2="6.985" width="0.254" layer="20"/>
<wire x1="19.685" y1="6.985" x2="17.272" y2="9.398" width="0.254" layer="20"/>
<wire x1="17.272" y1="9.398" x2="3.429" y2="9.398" width="0.254" layer="20"/>
<wire x1="3.429" y1="9.398" x2="3.429" y2="10.668" width="0.254" layer="20"/>
<wire x1="19.05" y1="20.32" x2="19.05" y2="29.21" width="0.254" layer="20"/>
<wire x1="19.05" y1="29.21" x2="17.78" y2="29.21" width="0.254" layer="20"/>
<wire x1="17.78" y1="29.21" x2="17.78" y2="20.32" width="0.254" layer="20"/>
<wire x1="12.7" y1="20.32" x2="17.78" y2="20.32" width="0.254" layer="20"/>
<wire x1="11.43" y1="20.32" x2="3.429" y2="20.32" width="0.254" layer="20"/>
<wire x1="3.429" y1="20.32" x2="3.429" y2="19.05" width="0.254" layer="20"/>
<wire x1="3.429" y1="19.05" x2="21.844" y2="19.05" width="0.254" layer="20"/>
<wire x1="21.844" y1="19.05" x2="24.892" y2="22.098" width="0.254" layer="20"/>
<wire x1="24.892" y1="22.098" x2="28.448" y2="22.098" width="0.254" layer="20"/>
<wire x1="28.448" y1="22.098" x2="28.448" y2="23.368" width="0.254" layer="20"/>
<wire x1="28.448" y1="23.368" x2="24.384" y2="23.368" width="0.254" layer="20"/>
<wire x1="24.384" y1="23.368" x2="21.336" y2="20.32" width="0.254" layer="20"/>
<wire x1="21.336" y1="20.32" x2="19.05" y2="20.32" width="0.254" layer="20"/>
<text>CUTOUT</text>
<text>CUTOUT</text>
<text>CUTOUT</text>
<text>CUTOUT</text>
<text>RNX0381K00</text>
<text>Protection Board</text>
<text>GLC 2019  Rev 1.0</text>
<text>41 Volt</text>
<hole x="4.064" y="19.685" drill="1.27"/>
<hole x="12.065" y="28.575" drill="1.27"/>
<hole x="18.415" y="28.575" drill="1.27"/>
<hole x="27.813" y="22.733" drill="1.27"/>
<hole x="25.527" y="7.62" drill="1.27"/>
<hole x="4.064" y="10.033" drill="1.27"/>
<text>CUTOUT</text>
<text>CUTOUT</text>
</plain>
<libraries>
<library name="supressor">
<description>&lt;b&gt;MOV, GDT and Spark Gap Surge Supressors&lt;/b&gt;&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2009, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="CG5350L">
<description>GDT SURGE ARRESTER&lt;p&gt;
Littelfuse, Inc.</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,17/1,3">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ptc-ntc">
<description>&lt;b&gt;PTC and NTC Resistors&lt;/b&gt;&lt;p&gt;
Siemens, Philips, Valvo&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B57164">
<description>&lt;b&gt;SIEMENS NTC&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="varistor">
<description>&lt;b&gt;Varistors/Thermistors&lt;/b&gt;&lt;p&gt;
Block, Siemens and generic&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="S05K11">
<description>&lt;b&gt;VARISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GDT1" library="supressor" package="CG5350L" value="GDT-CG5350L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+IN" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="-IN" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+OUT" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="-OUT" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="ptc-ntc" package="B57164" value="YQD100N1000">
<attribute name="OC_FARNELL" value="9753451"/>
<attribute name="MPN" value="B57164K474K52"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="29M3118"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.6" value="1K HV">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="varistor" package="S05K11" value="MOV-07D560K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="+IN" pad="1"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="+OUT" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="GDT1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="-OUT" pad="1"/>
<contactref element="-IN" pad="1"/>
<contactref element="GDT1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
