(kicad_pcb (version 20171130) (host pcbnew 5.1.9)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 16)
    (zones 0)
    (modules 17)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J0-Pad16)")
  (net 2 "Net-(J0-Pad15)")
  (net 3 "Net-(J0-Pad14)")
  (net 4 "Net-(J0-Pad13)")
  (net 5 "Net-(J0-Pad12)")
  (net 6 "Net-(J0-Pad11)")
  (net 7 "Net-(J0-Pad10)")
  (net 8 "Net-(J0-Pad9)")
  (net 9 "Net-(J0-Pad8)")
  (net 10 "Net-(J0-Pad7)")
  (net 11 "Net-(J0-Pad6)")
  (net 12 "Net-(J0-Pad5)")
  (net 13 "Net-(J0-Pad4)")
  (net 14 "Net-(J0-Pad3)")
  (net 15 "Net-(J0-Pad2)")
  (net 16 "Net-(J0-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net "Net-(J0-Pad1)")
    (add_net "Net-(J0-Pad10)")
    (add_net "Net-(J0-Pad11)")
    (add_net "Net-(J0-Pad12)")
    (add_net "Net-(J0-Pad13)")
    (add_net "Net-(J0-Pad14)")
    (add_net "Net-(J0-Pad15)")
    (add_net "Net-(J0-Pad16)")
    (add_net "Net-(J0-Pad2)")
    (add_net "Net-(J0-Pad3)")
    (add_net "Net-(J0-Pad4)")
    (add_net "Net-(J0-Pad5)")
    (add_net "Net-(J0-Pad6)")
    (add_net "Net-(J0-Pad7)")
    (add_net "Net-(J0-Pad8)")
    (add_net "Net-(J0-Pad9)")
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 154.178 92.71 90)
    (fp_text reference 16 (at 0.762 0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J0-Pad16)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 154.178 95.25 90)
    (fp_text reference 15 (at 0.762 0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J0-Pad15)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 154.178 97.79 90)
    (fp_text reference 14 (at 0.762 0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J0-Pad14)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 154.178 100.33 90)
    (fp_text reference 13 (at 0.762 0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J0-Pad13)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 154.178 102.87 90)
    (fp_text reference 12 (at 0.762 0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J0-Pad12)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 154.178 105.41 90)
    (fp_text reference 11 (at 0.762 0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J0-Pad11)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 154.178 107.95 90)
    (fp_text reference 10 (at 0.762 0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J0-Pad10)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 154.178 110.49 90)
    (fp_text reference 9 (at 0.762 0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J0-Pad9)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 150.622 110.49 90)
    (fp_text reference 8 (at 0.762 -0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J0-Pad8)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 150.622 107.95 90)
    (fp_text reference 7 (at 0.762 -0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J0-Pad7)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 150.622 105.41 90)
    (fp_text reference 6 (at 0.762 -0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J0-Pad6)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 150.622 102.87 90)
    (fp_text reference 5 (at 0.762 -0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J0-Pad5)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 150.622 100.33 90)
    (fp_text reference 4 (at 0.762 -0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J0-Pad4)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 150.622 97.79 90)
    (fp_text reference 3 (at 0.762 -0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J0-Pad3)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 150.622 95.25 90)
    (fp_text reference 2 (at 0.762 -0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J0-Pad2)"))
  )
  (module scm1-puck:sample-pad (layer F.Cu) (tedit 602ED875)
    (at 150.622 92.71 90)
    (fp_text reference 1 (at 0.762 -0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 0.75 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J0-Pad1)"))
  )
  (module scm1-puck:simple-DIP-16 (layer F.Cu) (tedit 602EF263)
    (at 152.4 101.6)
    (fp_text reference J0 (at 0 0) (layer F.SilkS) hide)
    (fp_text value Conn_02x08_Counter_Clockwise (at 0 11.43) (layer F.Fab) hide)
    (pad 16 thru_hole circle (at 3.81 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(J0-Pad16)"))
    (pad 15 thru_hole circle (at 3.81 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(J0-Pad15)"))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(J0-Pad14)"))
    (pad 13 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(J0-Pad13)"))
    (pad 12 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J0-Pad12)"))
    (pad 11 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J0-Pad11)"))
    (pad 10 thru_hole circle (at 3.81 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(J0-Pad10)"))
    (pad 9 thru_hole circle (at 3.81 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(J0-Pad9)"))
    (pad 8 thru_hole circle (at -3.81 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(J0-Pad8)"))
    (pad 7 thru_hole circle (at -3.81 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(J0-Pad7)"))
    (pad 6 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(J0-Pad6)"))
    (pad 5 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(J0-Pad5)"))
    (pad 4 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(J0-Pad4)"))
    (pad 3 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(J0-Pad3)"))
    (pad 2 thru_hole circle (at -3.81 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(J0-Pad2)"))
    (pad 1 thru_hole circle (at -3.81 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(J0-Pad1)"))
  )
  (gr_text "SCM-1 Rotator Puck v1.0\nUse Digikey part #\n1175-1521-5-ND" (at 152.4 101.6 90) (layer B.SilkS))
  (gr_line (start 156.464 91.44) (end 148.336 91.44) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.48 92.456) (end 156.464 91.44) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.48 110.744) (end 157.48 92.456) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.464 111.76) (end 157.48 110.744) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.336 111.76) (end 156.464 111.76) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.32 110.744) (end 148.336 111.76) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.32 92.456) (end 147.32 110.744) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.336 91.44) (end 147.32 92.456) (layer Edge.Cuts) (width 0.05))
)
