(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu15.10.1-stable)
  (general
    (links 22)
    (no_connects 0)
    (area 149.424999 65.824999 193.875001 110.975001)
    (thickness 1.6)
    (drawings 98)
    (tracks 73)
    (zones 0)
    (modules 13)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber2/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(D4-Pad2)")
  (net 8 "Net-(P1-Pad1)")
  (net 9 "Net-(P1-Pad2)")
  (net 10 "Net-(P1-Pad3)")
  (net 11 "Net-(P1-Pad4)")
  (net 12 "Net-(P1-Pad5)")
  (net 13 "Net-(P1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58F0EF35)
    (at 187.2 75.2 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.7 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58F0EE86)
    (at 153 85.9 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -2.8 0.1 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58F0EE9D)
    (at 190.5 85.9 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -2.9 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58F0EEA8)
    (at 190.5 98.9 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 2.9 0.1 360) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58F0EE90)
    (at 153 98.9 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 2.8 -0.1 360) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58F0EF6A)
    (at 162.8 69.3 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 20.11 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 156.2 86.2 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 187.2 86.1 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58F0EEF6)
    (at 187.2 98.6 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58F0EF18)
    (at 156.2 98.7 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -0.1 -1.8 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(P1-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Artwork_4chord-midi:craplab-flask (layer B.Cu) (tedit 0)
    (at 171.8 86.3 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Artwork_4chord-midi:craplab (layer B.Cu) (tedit 0)
    (at 171.7 93.9 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Nokia_5110-3310_LCD:Nokia_5110-3310_LCD (layer F.Cu) (tedit 5940F11B)
    (at 171.7 72.85)
    (fp_text reference U1 (at 0 6) (layer F.SilkS))
    (fp_text value Nokia_5110_LCD (at 0 8) (layer F.Fab))
    (pad "" thru_hole circle (at 17.25 32.5) (size 2 2) (drill 2) (layers *.Cu))
    (pad "" np_thru_hole circle (at 20.25 23) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 21.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 23.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 22) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 23.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 21.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 3.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 3.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 1.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 1.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 23.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 21.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 3) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" smd rect (at 19 2.5) (size 1.5 3) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 19 22.5) (size 1.5 3) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at -19 22.5) (size 1.5 3) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at -19 2.5) (size 1.5 3) (layers B.Cu B.Paste B.Mask))
    (pad "" np_thru_hole oval (at 20.25 22.5) (size 2 4.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole oval (at -20.25 22.5) (size 2 4.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole oval (at 20.25 2.5) (size 2 4.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole oval (at -20.25 2.5) (size 2 4.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad 9 smd rect (at 4 2.5) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P1-Pad6)"))
    (pad 8 smd rect (at 3 2.5) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P1-Pad5)"))
    (pad 7 smd rect (at 2 2.5) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P1-Pad4)"))
    (pad 6 smd rect (at 1 2.5) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P1-Pad3)"))
    (pad 1 smd rect (at -4 2.5) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at -3 2.5) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at 0 2.5) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P1-Pad2)"))
    (pad 4 smd rect (at -1 2.5) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P1-Pad6)"))
    (pad 3 smd rect (at -2 2.5) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 20.25 1.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 3.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 1.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" thru_hole circle (at -17.25 6) (size 2 2) (drill 2) (layers *.Cu))
  )
  (gr_text +3.3V (at 161.1 103.4) (layer F.SilkS))
  (gr_text "7 LIGHT -> GND" (at 172.6 99.5) (layer F.SilkS))
  (gr_text "VCC 6" (at 161.1 99.4) (layer F.SilkS))
  (gr_text "Bill of Materials\n\n- 1 Nokia 5110 LCD in clippable frame\n- 4 0805 180 Ohm resistor (YMMV)\n- 4 0805 LEDs (e.g. white)\n- 1 0805 100nF capacitor\n- 1 8pin header" (at 157.4 88.3) (layer F.SilkS))
  (gr_text "Revision A 05/17      Released under MIT License" (at 171.7 106.5) (layer B.SilkS))
  (gr_text "Nokia 5110 LCD breakout board" (at 171.7 104.1) (layer B.SilkS))
  (gr_text GND (at 180.6 72.7 90) (layer B.SilkS))
  (gr_text LIGHT (at 178.1 73.2 90) (layer B.SilkS))
  (gr_text VCC (at 175.7 72.7 90) (layer B.SilkS))
  (gr_text SCLK (at 173.1 73.1 90) (layer B.SilkS))
  (gr_text SDIN (at 170.6 72.9 90) (layer B.SilkS))
  (gr_text D/~C (at 168 72.7 90) (layer B.SilkS))
  (gr_text CE (at 165.4 72.2 90) (layer B.SilkS))
  (gr_text ~RST (at 162.9 72.6 90) (layer B.SilkS))
  (gr_line (start 149.5 110.9) (end 149.5 65.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.8 110.9) (end 149.5 110.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.8 65.9) (end 193.8 110.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.5 65.9) (end 193.8 65.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.7 110.8) (xy 149.6 110.8) (xy 149.6 66) (xy 193.7 66) (xy 193.7 110.8)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.7 110.8) (xy 149.6 110.8) (xy 149.6 66) (xy 193.7 66) (xy 193.7 110.8)
      )
    )
  )
)
