(kicad_pcb (version 20171130) (host pcbnew 5.1.2)
  (general
    (thickness 1.6)
    (drawings 32)
    (tracks 239)
    (zones 0)
    (modules 25)
    (nets 34)
  )
  (page A4)
  (title_block
    (title "ft231xs USB-to-serial")
    (date 19/11/2017)
    (rev rev2)
    (company flabbergast)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "output"))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad7)")
  (net 2 "Net-(U1-Pad5)")
  (net 3 "Net-(U1-Pad8)")
  (net 4 "Net-(U1-Pad9)")
  (net 5 "Net-(U1-Pad19)")
  (net 6 "Net-(C1-Pad1)")
  (net 7 GND)
  (net 8 "Net-(C2-Pad1)")
  (net 9 "Net-(C3-Pad1)")
  (net 10 +5V)
  (net 11 "Net-(J1-Pad6)")
  (net 12 "Net-(J1-Pad4)")
  (net 13 "Net-(R1-Pad2)")
  (net 14 "Net-(R2-Pad1)")
  (net 15 "Net-(R3-Pad2)")
  (net 16 "Net-(R4-Pad2)")
  (net 17 "Net-(U2-Pad4)")
  (net 18 +3V3)
  (net 19 "Net-(SW1-Pad2)")
  (net 20 PWR_OUT)
  (net 21 "Net-(R5-Pad1)")
  (net 22 "Net-(R5-Pad2)")
  (net 23 "Net-(R6-Pad1)")
  (net 24 "Net-(R6-Pad2)")
  (net 25 "Net-(R7-Pad1)")
  (net 26 "Net-(R7-Pad2)")
  (net 27 "Net-(R8-Pad1)")
  (net 28 "Net-(R8-Pad2)")
  (net 29 "Net-(D3-Pad2)")
  (net 30 "Net-(R3-Pad1)")
  (net 31 "Net-(R4-Pad1)")
  (net 32 "Net-(SJ1-Pad2)")
  (net 33 "Net-(SJ1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(SJ1-Pad2)")
    (add_net "Net-(SJ1-Pad3)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad4)")
    (add_net PWR_OUT)
  )
  (module Package_SSOP:QSOP-20_3.9x8.7mm_P0.635mm (layer F.Cu) (tedit 59F1B616)
    (at 217.805 112.395 270)
    (descr "20-Lead Plastic Shrink Small Outline Narrow Body (http://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf)")
    (tags "QSOP 0.635")
    (attr smd)
    (fp_text reference U1 (at 1.27 -3.302) (layer F.Fab))
    (fp_text value FT231XS (at -0.127 -0.254) (layer F.Fab))
    (fp_text user %R (at 1.143 1.905) (layer F.Fab))
    (pad 14 smd rect (at 2.6543 0.9525 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C3-Pad1)"))
    (pad 15 smd rect (at 2.6543 0.3175 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 7 smd rect (at -2.6543 0.9525 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at -2.6543 0.3175 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 17 smd rect (at 2.6543 -0.9525 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R3-Pad2)"))
    (pad 16 smd rect (at 2.6543 -0.3175 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at -2.6543 -0.3175 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -2.6543 -0.9525 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at -2.6543 -2.8575 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R8-Pad2)"))
    (pad 2 smd rect (at -2.6543 -2.2225 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R7-Pad2)"))
    (pad 3 smd rect (at -2.6543 -1.5875 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D3-Pad2)"))
    (pad 8 smd rect (at -2.6543 1.5875 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -2.6543 2.2225 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at -2.6543 2.8575 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R4-Pad2)"))
    (pad 11 smd rect (at 2.6543 2.8575 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R2-Pad1)"))
    (pad 12 smd rect (at 2.6543 2.2225 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (pad 13 smd rect (at 2.6543 1.5875 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C3-Pad1)"))
    (pad 18 smd rect (at 2.6543 -1.5875 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(SJ1-Pad3)"))
    (pad 19 smd rect (at 2.6543 -2.2225 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 2.6543 -2.8575 270) (size 1.6 0.41) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Package_SSOP.3dshapes/QSOP-20_3.9x8.7mm_P0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B642)
    (at 211.455 115.57)
    (attr smd)
    (fp_text reference C1 (at 0 -0.127 90) (layer F.Fab))
    (fp_text value 47pF (at 0 0) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B5EB)
    (at 211.455 109.855)
    (attr smd)
    (fp_text reference C2 (at 0 0 90) (layer F.Fab))
    (fp_text value 47pF (at 0 0) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B658)
    (at 219.71 117.475)
    (attr smd)
    (fp_text reference C3 (at 0 0 90) (layer F.Fab))
    (fp_text value 0.1uF (at 0 0) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:USB_microB_2TH_OSHPARK (layer F.Cu) (tedit 59F1B636)
    (at 205.232 112.522 270)
    (descr "USB microB 4pads THT")
    (tags "USB microB")
    (fp_text reference J1 (at 0 -1.27 270) (layer F.Fab))
    (fp_text value USB_mini_micro_B (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user "PCB edge" (at -0.05 1.45 270) (layer F.SilkS) hide)
    (pad 6 thru_hole circle (at 2.825 0 270) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at 1.3 -3 90) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (clearance 0.1))
    (pad 4 smd rect (at 0.65 -3 90) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad4)") (clearance 0.1))
    (pad 3 smd rect (at 0 -3 90) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)") (clearance 0.1))
    (pad 2 smd rect (at -0.65 -3 90) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)") (clearance 0.1))
    (pad 1 smd rect (at -1.3 -3 90) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V) (clearance 0.1))
    (pad 6 thru_hole circle (at -2.825 0 270) (size 2.15 2.15) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad6)"))
    (pad "" np_thru_hole circle (at 1.95 -2.15 90) (size 0.55 0.55) (drill 0.55) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.95 -2.15 90) (size 0.55 0.55) (drill 0.55) (layers *.Cu *.Mask F.SilkS))
    (pad "" smd rect (at -0.9 0 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 0.9 0 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B5F5)
    (at 211.455 111.76)
    (attr smd)
    (fp_text reference R1 (at 0 0 90) (layer F.Fab))
    (fp_text value 27R (at 0 0) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B601)
    (at 211.455 113.665 180)
    (attr smd)
    (fp_text reference R2 (at -0.127 0 270) (layer F.Fab))
    (fp_text value 27R (at 0 0 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B5B5)
    (at 224.155 115.57 180)
    (attr smd)
    (fp_text reference R3 (at 0 0 270) (layer F.Fab))
    (fp_text value 390R (at 0 0 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R3-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B5A3)
    (at 224.155 109.22 180)
    (attr smd)
    (fp_text reference R4 (at 0 0 270) (layer F.Fab))
    (fp_text value 390R (at 0 0 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R4-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 59F1B5D4)
    (at 210.693 106.68)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0.635 0.127 90) (layer F.Fab))
    (fp_text value ap2112k-3.3 (at 0 -2.286) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SP3T_PCM13 (layer B.Cu) (tedit 59F1B889)
    (at 214.63 118.11 180)
    (descr "Ultraminiature Surface Mount Slide Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -0.508 180) (layer F.Fab))
    (fp_text value pwr_sel (at 0 -4.25 180) (layer B.Fab))
    (fp_text user %R (at 0.127 -0.508 180) (layer B.Fab))
    (pad "" np_thru_hole circle (at -2.5 -0.33 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.5 -0.33 180) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -3 1.43 180) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at -1.5 1.43 180) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(SW1-Pad2)"))
    (pad 3 smd rect (at 1.5 1.43 180) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 20 PWR_OUT))
    (pad 4 smd rect (at 3 1.43 180) (size 0.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 18 +3V3))
    (pad "" smd rect (at -5.15 -1.43 180) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 5.15 -1.43 180) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 5.15 0.78 180) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at -5.15 0.78 180) (size 1 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SP3T_PCM13.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:M06_LOCK_NOSILK (layer F.Cu) (tedit 5728A903)
    (at 227.965 118.745 90)
    (attr virtual)
    (fp_text reference Y1 (at 1.778 -2.032 90) (layer Cmts.User) hide)
    (fp_text value FTDI (at 1.778 2.032 90) (layer Cmts.User) hide)
    (pad 1 thru_hole circle (at 0 -0.127 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 2.54 0.127 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(SJ1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 -0.127 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 PWR_OUT))
    (pad 4 thru_hole circle (at 7.62 0.127 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(R5-Pad2)"))
    (pad 5 thru_hole circle (at 10.16 -0.127 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(R6-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 0.127 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(R8-Pad1)"))
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B64E)
    (at 214.63 117.475 180)
    (attr smd)
    (fp_text reference C4 (at 0 0 270) (layer F.Fab))
    (fp_text value 0.1uF (at 0 0 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B5E1)
    (at 207.01 106.68 90)
    (attr smd)
    (fp_text reference C5 (at -0.127 0 180) (layer F.Fab))
    (fp_text value 10uF (at 0 0 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B59C)
    (at 214.249 106.553 270)
    (attr smd)
    (fp_text reference C6 (at 0 0) (layer F.Fab))
    (fp_text value 10uF (at 0 0 270) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B5AD)
    (at 224.155 113.665)
    (attr smd)
    (fp_text reference R5 (at 0 0 90) (layer F.Fab))
    (fp_text value 390R (at 0 0) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R5-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B5A6)
    (at 224.155 111.125 180)
    (attr smd)
    (fp_text reference R6 (at 0 0 270) (layer F.Fab))
    (fp_text value 390R (at 0 0 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R6-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B5B9)
    (at 224.155 118.745 180)
    (attr smd)
    (fp_text reference R7 (at -0.127 0 270) (layer F.Fab))
    (fp_text value 1kR (at 0 0 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R7-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B5BF)
    (at 224.155 106.045 180)
    (attr smd)
    (fp_text reference R8 (at 0 0 270) (layer F.Fab))
    (fp_text value 390R (at 0 0 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R8-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F1B61D)
    (at 220.726 106.553 90)
    (attr smd)
    (fp_text reference R9 (at 0 0 180) (layer F.Fab))
    (fp_text value 390R (at 0 0 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 PWR_OUT))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:0603 (layer F.Cu) (tedit 59F47698)
    (at 210.058 118.11 270)
    (attr smd)
    (fp_text reference R10 (at 0 0) (layer F.Fab))
    (fp_text value 1kR (at 0 0 270) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (model smd\capacitors\C0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOT-23_ANK (layer F.Cu) (tedit 59F48152)
    (at 217.551 106.68 180)
    (descr "SOT-23, Single Diode")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D3 (at 0.381 1.016 180) (layer F.Fab))
    (fp_text value D_Schottky (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0.381 1.016 180) (layer F.Fab))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D3-Pad2)"))
    (pad "" smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:LED-0603 (layer F.Cu) (tedit 5A120E7D)
    (at 224.155 117.094)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference RXL1 (at -2.094 -0.224 90) (layer F.Fab))
    (fp_text value RED_LED (at 0 -1.2065) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 PWR_OUT))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R3-Pad1)"))
  )
  (module flabbergast:GS3 (layer B.Cu) (tedit 5A6BA13E)
    (at 224.79 112.522)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference SJ1 (at -1.7 0 90) (layer F.Fab))
    (fp_text value R/C (at -1.778 0 270) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(SJ1-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(SJ1-Pad3)"))
  )
  (module flabbergast:LED-0603 (layer F.Cu) (tedit 5A120E2D)
    (at 224.155 107.823)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference TXL1 (at -1.905 -0.635 90) (layer F.Fab))
    (fp_text value AMBER_LED (at 0 -1.2065) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 PWR_OUT))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R4-Pad1)"))
  )
  (gr_text cb0 (at 224.79 109.982) (layer B.SilkS))
  (gr_text rts (at 224.79 115.062 180) (layer B.SilkS))
  (gr_text RXL (at 221.996 116.459 90) (layer F.SilkS))
  (gr_text TXL (at 221.996 108.839 90) (layer F.SilkS))
  (gr_text rev2 (at 206.375 112.522 270) (layer B.SilkS))
  (gr_text "when NO, target MUST\nsupply voltage" (at 215.9 111.252) (layer B.SilkS))
  (gr_text black (at 226.06 118.491 90) (layer B.SilkS))
  (gr_text green (at 226.06 106.807 90) (layer B.SilkS))
  (gr_text "(c) 2017 flabbergast" (at 215.773 108.712) (layer B.SilkS))
  (gr_text "FT231X USB-to-ser" (at 215.392 106.934) (layer B.SilkS))
  (gr_text NO (at 214.63 114.808) (layer B.SilkS))
  (gr_text 3V3 (at 209.296 115.824) (layer B.SilkS))
  (gr_text 5V (at 219.583 115.697) (layer B.SilkS))
  (gr_text r/c (at 226.187 116.205 90) (layer F.SilkS))
  (gr_text pwr (at 226.187 113.792 90) (layer F.SilkS))
  (gr_text tx (at 226.187 111.125 90) (layer F.SilkS))
  (gr_text rx (at 226.187 108.585 90) (layer F.SilkS))
  (gr_text dtr (at 226.187 106.172 90) (layer F.SilkS))
  (gr_text gnd (at 226.187 118.872 90) (layer F.SilkS))
  (gr_circle (center 207.143 117.492) (end 208.293 117.492) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.835 116.967) (end 203.835 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207.264 120.396) (end 203.835 116.967) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207.518 120.396) (end 207.264 120.396) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207.772 120.396) (end 207.518 120.396) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 228.219 120.396) (end 207.772 120.396) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 229.235 119.38) (end 228.219 120.396) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.835 106.68) (end 203.835 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 205.74 104.775) (end 203.835 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 228.6 104.775) (end 205.74 104.775) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 229.235 105.41) (end 228.6 104.775) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 229.235 119.38) (end 229.235 105.41) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 227.838 120.142) (xy 207.391 120.015) (xy 204.343 117.094) (xy 204.343 106.807) (xy 205.994 105.156)
        (xy 227.965 105.029)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 227.838 120.142) (xy 207.391 120.015) (xy 204.343 117.094) (xy 204.343 106.807) (xy 205.994 105.156)
        (xy 227.965 105.029)
      )
    )
  )
)
