(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 8)
    (no_connects 0)
    (area 144.704999 106.604999 155.523001 116.661001)
    (thickness 1.6)
    (drawings 7)
    (tracks 7)
    (zones 0)
    (modules 3)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5BCA7B45)
    (at 155.194 115.062 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at -2.54 4.064 360) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81 360) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module USBVERT:USB_MICROB_MALE_VERTICAL (layer F.Cu) (tedit 5BCA6D6F)
    (at 150.114 108.204 180)
    (fp_text reference J1 (at 0 9 180) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 -9 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 8.275 -2.23 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 3.325 -3.15 180) (size 1.9 1.9) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 3.325 0 180) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.3 0 180) (size 0.4 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 0 180) (size 0.4 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 0 180) (size 0.4 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -0.65 0 180) (size 0.4 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.3 0 180) (size 0.4 2.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 6 thru_hole circle (at -3.325 0 180) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -3.325 -3.15 180) (size 1.9 1.9) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at -8.275 -2.23 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module USBVERT:QR_Code (layer B.Cu) (tedit 0)
    (at 150.114 110.49)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text GND (at 147.574 113.284) (layer F.SilkS))
  (gr_text D+ (at 150.114 113.284) (layer F.SilkS))
  (gr_text D- (at 152.908 113.284) (layer F.SilkS))
  (gr_line (start 155.448 106.68) (end 155.448 116.586) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 106.68) (end 155.448 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 116.586) (end 144.78 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.448 116.586) (end 144.78 116.586) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.956 117.094) (xy 144.272 117.094) (xy 144.272 106.426) (xy 155.956 106.426)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.956 117.094) (xy 144.272 117.094) (xy 144.272 106.426) (xy 155.956 106.426)
      )
    )
  )
)
