(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 41)
    (no_connects 1)
    (area 86.964599 74.854999 178.510001 131.501933)
    (thickness 1.6)
    (drawings 32)
    (tracks 183)
    (zones 0)
    (modules 32)
    (nets 36)
  )
  (page A4)
  (title_block
    (company "This design uses a KiCad DIP template created by Jenner at Wickerbox Electronics")
    (comment 1 "Released under the CERN Open Hardware License v1.2")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.7874)
    (via_drill 0.5334)
    (via_min_size 0.762)
    (via_min_drill 0.508)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.1524)
    (pcb_text_size 0.762 0.762)
    (mod_edge_width 0.15)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.1524)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFEEF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory test-board-gerbers))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /D15)
  (net 4 /D0)
  (net 5 /D1)
  (net 6 /D2)
  (net 7 /D3)
  (net 8 /D4)
  (net 9 /D5)
  (net 10 /D6)
  (net 11 /D7)
  (net 12 /D8)
  (net 13 /D9)
  (net 14 /CLK)
  (net 15 /D11)
  (net 16 /D12)
  (net 17 "/D17(VIN)")
  (net 18 /PROG)
  (net 19 /DAC)
  (net 20 /CS)
  (net 21 /D16)
  (net 22 /D18)
  (net 23 /D17)
  (net 24 /D22)
  (net 25 /D21)
  (net 26 /D20)
  (net 27 /D19)
  (net 28 /D23)
  (net 29 /D14)
  (net 30 /EIN)
  (net 31 /DISP)
  (net 32 /EMO)
  (net 33 /3V3)
  (net 34 /3VO)
  (net 35 /SDO)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.7874)
    (via_drill 0.5334)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net /3V3)
    (add_net /3VO)
    (add_net /CLK)
    (add_net /CS)
    (add_net /D0)
    (add_net /D1)
    (add_net /D11)
    (add_net /D12)
    (add_net /D14)
    (add_net /D15)
    (add_net /D16)
    (add_net /D17)
    (add_net "/D17(VIN)")
    (add_net /D18)
    (add_net /D19)
    (add_net /D2)
    (add_net /D20)
    (add_net /D21)
    (add_net /D22)
    (add_net /D23)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /DAC)
    (add_net /DISP)
    (add_net /EIN)
    (add_net /EMO)
    (add_net /PROG)
    (add_net /SDO)
    (add_net GND)
  )
  (module TEENSY-LC (layer F.Cu) (tedit 5797B473)
    (at 123.1265 108.1405 270)
    (fp_text reference J1 (at -7.62 20.066 360) (layer F.SilkS) hide)
    (fp_text value TEENSY-LC (at -2.54 20.32 450) (layer F.Fab))
    (fp_text user "TEENSY LC" (at -2.7813 -12.6111 270) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at -10.16 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /D0))
    (pad 1 thru_hole circle (at -10.16 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D1))
    (pad 2 thru_hole circle (at -10.16 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D2))
    (pad 3 thru_hole circle (at -10.16 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D3))
    (pad 4 thru_hole circle (at -10.16 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D4))
    (pad 5 thru_hole circle (at -10.16 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D5))
    (pad 6 thru_hole circle (at -10.16 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D6))
    (pad 7 thru_hole circle (at -10.16 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D7))
    (pad 8 thru_hole circle (at -10.16 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D8))
    (pad 9 thru_hole circle (at -10.16 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /D9))
    (pad 10 thru_hole circle (at -10.16 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /CLK))
    (pad 11 thru_hole circle (at -10.16 20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D11))
    (pad 12 thru_hole circle (at -10.16 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /D12))
    (pad 17A thru_hole circle (at -7.62 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "/D17(VIN)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad G2 thru_hole circle (at -2.54 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad PGM thru_hole circle (at 0 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /PROG))
    (pad DAC thru_hole circle (at 2.54 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /DAC))
    (pad 13 thru_hole circle (at 5.08 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /CS))
    (pad 16 thru_hole circle (at 5.08 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D16))
    (pad 3V2 thru_hole circle (at 5.08 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 18 thru_hole circle (at 5.08 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /D18))
    (pad 17 thru_hole circle (at 5.08 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /D17))
    (pad G3 thru_hole circle (at 5.08 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 22 thru_hole circle (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /D22))
    (pad VIN thru_hole circle (at 5.08 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 21 thru_hole circle (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /D21))
    (pad 20 thru_hole circle (at 5.08 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /D20))
    (pad 19 thru_hole circle (at 5.08 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /D19))
    (pad 23 thru_hole circle (at 5.08 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D23))
    (pad 14 thru_hole circle (at 5.08 20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D14))
    (pad 15 thru_hole circle (at 5.08 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /D15))
  )
  (module Wickerlib:CAPSENSE-CIRCLE-D10MM (layer F.Cu) (tedit 5797B262)
    (at 95.504 122.6312 270)
    (fp_text reference CAP15 (at -0.2032 0.1524 360) (layer F.SilkS))
    (fp_text value CAP15 (at 0.025 7.325 270) (layer F.Fab))
    (pad 1 smd circle (at 0 0 270) (size 10.16 10.16) (layers F.Cu)
      (net 3 /D15) (clearance 0.508))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B77B)
    (at 133.0198 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D0 (at 2.54 -0.0762 360) (layer F.SilkS))
    (fp_text value D0 (at 0 -0.127 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /D0))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B775)
    (at 129.4638 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D1 (at 2.4892 -0.0762 360) (layer F.SilkS))
    (fp_text value D1 (at 0 -0.127 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D1))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B771)
    (at 125.9078 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D2 (at 2.54 -0.0762 360) (layer F.SilkS))
    (fp_text value D2 (at 0.127 -0.127 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D2))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B76D)
    (at 122.3518 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D3 (at 2.5908 0.0254 360) (layer F.SilkS))
    (fp_text value D3 (at 0.127 -0.127 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D3))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B769)
    (at 118.7958 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D4 (at 2.4892 -0.127 360) (layer F.SilkS))
    (fp_text value D4 (at 0.127 -0.127 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D4))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B766)
    (at 115.2398 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D5 (at 2.54 -0.0762 360) (layer F.SilkS))
    (fp_text value D5 (at 0.127 -0.127 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D5))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B763)
    (at 111.6838 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D6 (at 2.4892 -0.0254 360) (layer F.SilkS))
    (fp_text value D6 (at 0.127 -0.127 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D6))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B760)
    (at 108.1278 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D7 (at 2.4892 0.0254 360) (layer F.SilkS))
    (fp_text value D7 (at 0 -0.127 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D7))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B75D)
    (at 104.5718 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D8 (at 2.4892 0.1778 360) (layer F.SilkS))
    (fp_text value D8 (at 0 -0.127 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D8))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B759)
    (at 101.0158 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D9 (at 2.54 0.2286 360) (layer F.SilkS))
    (fp_text value D9 (at 0 -0.127 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /D9))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1F3)
    (at 92.71 98.679 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D12 (at 0.127 2.794 270) (layer F.SilkS))
    (fp_text value D12 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /D12))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1C0)
    (at 108.5596 119.5324 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D14 (at 2.54 -0.0508 360) (layer F.SilkS))
    (fp_text value D14 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D14))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1C5)
    (at 112.0648 119.5324 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D16 (at 2.5908 -0.0508 360) (layer F.SilkS))
    (fp_text value D16 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D16))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1C8)
    (at 115.57 119.5324 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D17 (at 2.54 -0.1524 360) (layer F.SilkS))
    (fp_text value D17 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /D17))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1CC)
    (at 119.0752 119.5324 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D20 (at 2.5908 0 360) (layer F.SilkS))
    (fp_text value D20 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /D20))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1D5)
    (at 126.0856 119.5324 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D21 (at 2.6924 0 360) (layer F.SilkS))
    (fp_text value D21 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /D21))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1D1)
    (at 122.5804 119.5324 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D22 (at 2.6416 0 360) (layer F.SilkS))
    (fp_text value D22 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /D22))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1DA)
    (at 129.5908 119.5324 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference D23 (at 2.581 0.035 360) (layer F.SilkS))
    (fp_text value D23 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D23))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1F7)
    (at 92.71 102.235 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 17A (at 0 2.667 270) (layer F.SilkS))
    (fp_text value 17A (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "/D17(VIN)"))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B22E)
    (at 92.71 112.903 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference DAC (at 0 2.667 270) (layer F.SilkS))
    (fp_text value DAC (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /DAC))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B229)
    (at 92.71 109.347 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference PGM (at 0 2.667 270) (layer F.SilkS))
    (fp_text value PGM (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /PROG))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B21E)
    (at 92.71 105.791 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference GND (at 0 2.667 270) (layer F.SilkS))
    (fp_text value PGM (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1E2)
    (at 133.096 119.5324 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 3V3 (at 2.4892 0.1524 360) (layer F.SilkS))
    (fp_text value 3v3 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B1BC)
    (at 105.0544 119.5324 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CS (at 2.54 -0.1524 360) (layer F.SilkS))
    (fp_text value CS (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /CS))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B752)
    (at 93.9038 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference DI (at 2.4892 0.0254 360) (layer F.SilkS))
    (fp_text value DI (at 0.127 0 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D11))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 5797B756)
    (at 97.4598 92.2528 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CLK (at 2.4892 -0.0254 360) (layer F.SilkS))
    (fp_text value CLK (at 0.127 0 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /CLK))
    (model Pin_Headers.3dshapes/CONN-HEADER-STRAIGHT-P2.54MM-1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x07 (layer F.Cu) (tedit 5797AC86)
    (at 125.3236 126.3396 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference I2C-BMP180 (at 2.9845 8.0645 360) (layer F.SilkS))
    (fp_text value I2C-BMP180 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /3VO))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /D19))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /SDO))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /D18))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /CS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x09 (layer F.Cu) (tedit 5797B48A)
    (at 103.0478 83.82 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "SHARP Memory Display" (at 2.7432 10.541 180) (layer F.SilkS))
    (fp_text value SHARP-MEM-DISP (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /EIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /DISP))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /EMO))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /CS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D11))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /CLK))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /3V3))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x09.wrl
      (at (xyz 0 -0.4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module teensy-big-oled:osh-park-logo-200dpi-norm-silk (layer F.Cu) (tedit 0)
    (at 95.3516 122.7836)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 5797B710)
    (at 95.6564 121.3612 180)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 4.38912 180) (layer B.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 -6.56082 180) (layer B.Fab))
  )
  (gr_text "Drew Fustini  <drew@oshpark.com>" (at 114.554 88.5444) (layer F.SilkS))
  (gr_text "SHARP Memory Display + Teensy LC\nhttps://github.com/pdp7/memory-display\nby Drew Fustini\n<drew@oshpark.com>" (at 118.2116 106.172) (layer B.SilkS))
  (gr_circle (center 129.8956 84.328) (end 132.0292 85.2932) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 96.9772 84.2772) (end 99.1108 85.2424) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.9132 130.4036) (end 130.4036 130.4036) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.8116 130.302) (end 92.9132 130.4036) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.0976 79.6544) (end 95.1992 79.6544) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.0872 86.6648) (end 95.0976 79.6544) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.0872 90.0684) (end 88.0872 86.6648) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.0872 125.5776) (end 88.0872 90.0684) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.8116 130.302) (end 88.0872 125.5776) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.9568 123.8504) (end 130.3528 130.4544) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.9568 85.852) (end 136.9568 123.8504) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 79.6544) (end 136.9568 85.8012) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.1992 79.6544) (end 130.81 79.6544) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.5708 80.9244) (xy 129.6416 80.9752) (xy 131.1656 81.026) (xy 132.7404 82.1436) (xy 134.2136 84.2772)
        (xy 136.2964 86.2584) (xy 136.0932 123.5456) (xy 130.048 129.794) (xy 93.5228 129.8448) (xy 88.7476 125.222)
        (xy 88.7984 87.376) (xy 89.5096 86.36) (xy 91.7448 84.0232) (xy 94.7928 81.0768) (xy 95.9104 80.9244)
        (xy 96.5708 80.9244)
      )
    )
  )
)
