(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 244)
    (zones 0)
    (modules 21)
    (nets 55)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 SOLENOID2_PIN)
  (net 3 GND)
  (net 4 SOLENOID1_PIN)
  (net 5 PULSE1_PIN)
  (net 6 "Net-(XA1-PadVIN)")
  (net 7 "Net-(XA1-Pad3V3)")
  (net 8 "Net-(XA1-PadRST1)")
  (net 9 "Net-(XA1-PadIORF)")
  (net 10 "Net-(XA1-PadD0)")
  (net 11 "Net-(XA1-PadD1)")
  (net 12 "Net-(XA1-PadD4)")
  (net 13 "Net-(XA1-PadD6)")
  (net 14 "Net-(XA1-PadD7)")
  (net 15 "Net-(XA1-PadD8)")
  (net 16 "Net-(XA1-PadD9)")
  (net 17 "Net-(XA1-PadD10)")
  (net 18 "Net-(XA1-PadSCL)")
  (net 19 "Net-(XA1-PadSDA)")
  (net 20 "Net-(XA1-PadAREF)")
  (net 21 "Net-(XA1-PadD13)")
  (net 22 PULSE2_PIN)
  (net 23 "Net-(XA1-PadA2)")
  (net 24 "Net-(XA1-PadA3)")
  (net 25 "Net-(XA1-PadA4)")
  (net 26 "Net-(XA1-PadA5)")
  (net 27 /S1_PATH)
  (net 28 /S2_PATH)
  (net 29 "Net-(SW1-Pad3)")
  (net 30 VCC)
  (net 31 /D13)
  (net 32 /D12)
  (net 33 /D11)
  (net 34 /D10)
  (net 35 /D9)
  (net 36 /D8)
  (net 37 /D7)
  (net 38 /D6)
  (net 39 /D4)
  (net 40 /AREF)
  (net 41 /RXI)
  (net 42 /TX0)
  (net 43 /DTR)
  (net 44 /A2)
  (net 45 /A3)
  (net 46 /A4)
  (net 47 /A5)
  (net 48 /A6)
  (net 49 /A7)
  (net 50 "Net-(XA1-PadD12)")
  (net 51 "Net-(XA1-PadD11)")
  (net 52 /INLET)
  (net 53 STATUS_LED)
  (net 54 "Net-(D3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /AREF)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D4)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /DTR)
    (add_net /RXI)
    (add_net /TX0)
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(SW1-Pad3)")
    (add_net "Net-(XA1-Pad3V3)")
    (add_net "Net-(XA1-PadA2)")
    (add_net "Net-(XA1-PadA3)")
    (add_net "Net-(XA1-PadA4)")
    (add_net "Net-(XA1-PadA5)")
    (add_net "Net-(XA1-PadAREF)")
    (add_net "Net-(XA1-PadD0)")
    (add_net "Net-(XA1-PadD1)")
    (add_net "Net-(XA1-PadD10)")
    (add_net "Net-(XA1-PadD11)")
    (add_net "Net-(XA1-PadD12)")
    (add_net "Net-(XA1-PadD13)")
    (add_net "Net-(XA1-PadD4)")
    (add_net "Net-(XA1-PadD6)")
    (add_net "Net-(XA1-PadD7)")
    (add_net "Net-(XA1-PadD8)")
    (add_net "Net-(XA1-PadD9)")
    (add_net "Net-(XA1-PadIORF)")
    (add_net "Net-(XA1-PadRST1)")
    (add_net "Net-(XA1-PadSCL)")
    (add_net "Net-(XA1-PadSDA)")
    (add_net "Net-(XA1-PadVIN)")
    (add_net PULSE1_PIN)
    (add_net PULSE2_PIN)
    (add_net SOLENOID1_PIN)
    (add_net SOLENOID2_PIN)
    (add_net STATUS_LED)
  )
  (net_class "Device Power" ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 2.4)
    (via_drill 1.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VCC)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 2)
    (via_dia 4.8)
    (via_drill 3.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /INLET)
    (add_net /S1_PATH)
    (add_net /S2_PATH)
    (add_net GND)
  )
  (module Arduino:Arduino_Uno_Shield (layer F.Cu) (tedit 5BCD6302)
    (at 120.65 113.03)
    (descr https://store.arduino.cc/arduino-uno-rev3)
    (fp_text reference XA1 (at 2.54 -54.356) (layer F.SilkS))
    (fp_text value Arduino_Uno_Shield (at 15.494 -54.356) (layer F.Fab))
    (pad A5 thru_hole oval (at 63.5 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(XA1-PadA5)"))
    (pad A4 thru_hole oval (at 60.96 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(XA1-PadA4)"))
    (pad A3 thru_hole oval (at 58.42 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(XA1-PadA3)"))
    (pad A2 thru_hole oval (at 55.88 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(XA1-PadA2)"))
    (pad A1 thru_hole oval (at 53.34 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 PULSE2_PIN))
    (pad "" thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D11 thru_hole oval (at 34.036 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "Net-(XA1-PadD11)"))
    (pad D12 thru_hole oval (at 31.496 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 "Net-(XA1-PadD12)"))
    (pad D13 thru_hole oval (at 28.956 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(XA1-PadD13)"))
    (pad AREF thru_hole oval (at 23.876 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(XA1-PadAREF)"))
    (pad SDA thru_hole oval (at 21.336 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(XA1-PadSDA)"))
    (pad SCL thru_hole oval (at 18.796 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(XA1-PadSCL)"))
    (pad "" np_thru_hole circle (at 13.97 -2.54) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 15.24 -50.8) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 66.04 -35.56) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 66.04 -7.62) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad D10 thru_hole oval (at 36.576 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(XA1-PadD10)"))
    (pad D9 thru_hole oval (at 39.116 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(XA1-PadD9)"))
    (pad D8 thru_hole oval (at 41.656 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(XA1-PadD8)"))
    (pad GND1 thru_hole oval (at 26.416 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad D7 thru_hole oval (at 45.72 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(XA1-PadD7)"))
    (pad D6 thru_hole oval (at 48.26 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(XA1-PadD6)"))
    (pad D5 thru_hole oval (at 50.8 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 STATUS_LED))
    (pad D4 thru_hole oval (at 53.34 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(XA1-PadD4)"))
    (pad D3 thru_hole oval (at 55.88 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 SOLENOID2_PIN))
    (pad D2 thru_hole oval (at 58.42 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 SOLENOID1_PIN))
    (pad D1 thru_hole oval (at 60.96 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(XA1-PadD1)"))
    (pad D0 thru_hole oval (at 63.5 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(XA1-PadD0)"))
    (pad IORF thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(XA1-PadIORF)"))
    (pad RST1 thru_hole oval (at 33.02 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(XA1-PadRST1)"))
    (pad 3V3 thru_hole oval (at 35.56 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(XA1-Pad3V3)"))
    (pad 5V1 thru_hole oval (at 38.1 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad GND2 thru_hole oval (at 40.64 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad GND3 thru_hole oval (at 43.18 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad VIN thru_hole oval (at 45.72 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(XA1-PadVIN)"))
    (pad A0 thru_hole oval (at 50.8 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 PULSE1_PIN))
  )
  (module 1101M2S3CQE2:1101M2S3CQE2 (layer F.Cu) (tedit 5BD0E365)
    (at 151.13 97.282 90)
    (fp_text reference SW1 (at 4.318 -4.826 180) (layer F.SilkS))
    (fp_text value SW_SPDT (at -2.54 -3.302) (layer F.SilkS))
    (fp_text user * (at -2.921 -9.398 90) (layer F.Fab))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 3 thru_hole circle (at 0 0 90) (size 2.794 2.794) (drill 2.286) (layers *.Cu *.Mask)
      (net 29 "Net-(SW1-Pad3)"))
    (pad 2 thru_hole circle (at 0 -4.699 90) (size 2.794 2.794) (drill 2.286) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 1 thru_hole rect (at 0 -9.398 90) (size 2.794 2.794) (drill 2.286) (layers *.Cu *.Mask)
      (net 52 /INLET))
  )
  (module SRH05S05:SRH05S05 (layer F.Cu) (tedit 5BC807B4)
    (at 160.02 98.298 270)
    (fp_text reference U1 (at -4.572 1.778 180) (layer F.SilkS))
    (fp_text value "SRH05S05 / SRH05S3V3" (at 2.54 2.54 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 153.162 84.582)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D1 (at 18.161 -0.127 -180) (layer F.SilkS))
    (fp_text value SB5100E-G (at 7.62 3.66) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 15.24 0) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 27 /S1_PATH))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 132.08 84.582)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 18.161 -0.127) (layer F.SilkS))
    (fp_text value SB5100E-G (at 7.62 3.66) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 15.24 0) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 28 /S2_PATH))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 165.608 97.028)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.27 -3.556) (layer F.SilkS))
    (fp_text value 0.33uF (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 165.608 105.156)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1.27 -4.318) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 4.46) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 VCC))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_MKDS1.5-4pol (layer F.Cu) (tedit 59FF0755)
    (at 177.8 81.28 90)
    (descr "4-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J1 (at -3.556 0) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x04 (at 7.5 -6.6 90) (layer F.Fab))
    (fp_text user %R (at 7.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 27 /S1_PATH))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 3 thru_hole circle (at 10 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 4 thru_hole circle (at 15 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 28 /S2_PATH))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS1.5-4pol.wrl
      (offset (xyz 7.50061988735199 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_B3B-PH-K_03x2.00mm_Straight (layer F.Cu) (tedit 58D3FE4F)
    (at 179.705 100.33 180)
    (descr "JST PH series connector, B3B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J2 (at 7.366 0 180) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 2 3.8 180) (layer F.Fab))
    (fp_text user %R (at 2 1.5 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 4 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 PULSE1_PIN))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 30 VCC))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B3B-PH-K_03x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_B3B-PH-K_03x2.00mm_Straight (layer F.Cu) (tedit 58D3FE4F)
    (at 179.705 106.68 180)
    (descr "JST PH series connector, B3B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J3 (at 7.366 0 180) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 2 3.8 180) (layer F.Fab))
    (fp_text user %R (at 2 1.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 4 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 22 PULSE2_PIN))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B3B-PH-K_03x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Barrel_Jack_CUI_PJ-102AH (layer F.Cu) (tedit 59BC552D)
    (at 142.24 104.14)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J4 (at 5.842 0 -180) (layer F.SilkS))
    (fp_text value Barrel_Jack (at -5.5 6.2 -270) (layer F.Fab))
    (fp_text user %R (at 0 6.5) (layer F.Fab))
    (pad 3 thru_hole circle (at 4.7 3) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 0 6) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 52 /INLET))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Barrel_Jack_CUI_PJ-102AH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 132.334 78.232 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.31 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 SOLENOID1_PIN))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 152.908 78.232 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 SOLENOID2_PIN))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-263-2 (layer B.Cu) (tedit 590079C0)
    (at 142.554 75.165)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference Q1 (at -5.775 4.445) (layer B.SilkS))
    (fp_text value FQB30N06LTM (at 9.084 -0.235 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 27 /S1_PATH))
    (pad 2 smd rect (at 5.8 2.775) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 27 /S1_PATH))
    (pad 2 smd rect (at 0.95 2.775) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 27 /S1_PATH))
    (pad 2 smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 27 /S1_PATH))
    (pad 2 smd rect (at 3.375 0) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 27 /S1_PATH))
    (pad 3 smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -5.775 2.54) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 4 SOLENOID1_PIN))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-263-2 (layer B.Cu) (tedit 590079C0)
    (at 163.195 75.184)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference Q2 (at -5.515 4.445) (layer B.SilkS))
    (fp_text value FQB30N06LTM (at 9.271 -0.254 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -5.775 2.54) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 2 SOLENOID2_PIN))
    (pad 3 smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 3.375 0) (size 9.4 10.8) (layers B.Cu B.Mask)
      (net 28 /S2_PATH))
    (pad 2 smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 28 /S2_PATH))
    (pad 2 smd rect (at 0.95 2.775) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 28 /S2_PATH))
    (pad 2 smd rect (at 5.8 2.775) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 28 /S2_PATH))
    (pad 2 smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers B.Cu B.Paste)
      (net 28 /S2_PATH))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 130.81 97.282)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -4.064) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 STATUS_LED))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Barrel_Jack_CUI_PJ-102AH (layer F.Cu) (tedit 59BC552D)
    (at 177.038 91.186 90)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J7 (at 5.75 8.45 180) (layer F.SilkS))
    (fp_text value Barrel_Jack (at -5.5 6.2 180) (layer F.Fab))
    (fp_text user %R (at 0 6.5 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 4.7 3 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 0 6 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 52 /INLET))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Barrel_Jack_CUI_PJ-102AH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 137.414 93.98 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at -1.524 0) (layer F.SilkS))
    (fp_text value 220 (at 3.81 2.31 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(D3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 132.08 90.17 90)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J5 (at 0 35.56 90) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 0 35.35 90) (layer F.Fab))
    (fp_text user %R (at 0 16.51 180) (layer F.Fab))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D13))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D12))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /D11))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /D10))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /D9))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /D8))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /D7))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /D6))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 STATUS_LED))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /D4))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 SOLENOID2_PIN))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SOLENOID1_PIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 132.08 67.31 90)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J6 (at 0 35.56 90) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 0 35.35 90) (layer F.Fab))
    (fp_text user %R (at 0 16.51 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /AREF))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /RXI))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /TX0))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /DTR))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 PULSE1_PIN))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 PULSE2_PIN))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /A2))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /A3))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /A4))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /A5))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /A6))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /A7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Polarity_Center_Positive_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 142.24 105.41)
    (descr "Polarity Logo, Center Positive")
    (tags "Logo Polarity Center Positive")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value Polarity_Center_Positive_6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (gr_text "version 1" (at 185.42 91.44 90) (layer B.SilkS))
  (gr_text "for support email dev@esologic.com" (at 187.96 91.44 90) (layer B.SilkS))
  (gr_text "SRH05S05 for Uno" (at 155.702 100.838 90) (layer F.SilkS))
  (gr_text "SRH05S3V3 for Fio" (at 158.242 100.838 90) (layer F.SilkS))
  (gr_text 2 (at 183.515 106.045 90) (layer F.SilkS))
  (gr_text "Arduino Fio Header" (at 160.02 64.77) (layer F.SilkS))
  (gr_text MOS2 (at 142.24 75.438) (layer F.SilkS))
  (gr_text MOS1 (at 163.322 75.438) (layer F.SilkS))
  (gr_text VCC (at 129.54 90.17 90) (layer F.SilkS))
  (gr_text GND (at 129.54 67.31 90) (layer F.SilkS))
  (gr_line (start 132.08 59.69) (end 185.42 59.69) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.42 113.03) (end 132.08 113.03) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.23 72.39) (end 189.23 74.93) (layer Edge.Cuts) (width 0.15))
  (gr_text "cadence & going/staying driver" (at 186.69 91.44 90) (layer B.SilkS))
  (gr_text 1 (at 183.515 99.695 90) (layer F.SilkS))
  (gr_text SOL2 (at 183.642 67.945 90) (layer F.SilkS))
  (gr_text SOL1 (at 183.642 78.74 90) (layer F.SilkS))
  (gr_line (start 189.23 72.39) (end 189.23 63.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 185.42 109.22) (end 185.42 113.03) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 63.5) (end 128.27 109.22) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 185.42 63.5) (end 189.23 63.5) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.08 63.5) (end 132.08 59.69) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.08 109.22) (end 128.27 109.22) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.23 74.93) (end 189.23 109.22) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.262 57.15) (xy 191.262 115.824) (xy 127.254 117.856) (xy 125.476 55.118)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.548 57.15) (xy 193.294 119.126) (xy 120.396 120.142) (xy 123.19 55.88)
      )
    )
  )
)
