(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 1.6)
    (drawings 54)
    (tracks 727)
    (zones 0)
    (modules 35)
    (nets 126)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.381)
    (user_trace_width 1.524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.381)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 0.285)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 0 0)
    (grid_origin 48.641 162.7505)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(U1-Pad1)")
  (net 4 "Net-(U1-Pad5)")
  (net 5 "Net-(e1-Pad16)")
  (net 6 "Net-(e1-Pad12)")
  (net 7 "Net-(e1-Pad11)")
  (net 8 "/Pressure regulators/PR1_OUT")
  (net 9 "/Pressure regulators/PR2_OUT")
  (net 10 "Net-(e1-Pad2)")
  (net 11 +3V3)
  (net 12 "Net-(e1-Pad21)")
  (net 13 "Net-(e1-Pad23)")
  (net 14 "Net-(e1-Pad24)")
  (net 15 "Net-(U6-Pad56)")
  (net 16 "Net-(U6-Pad30)")
  (net 17 "Net-(e1-Pad29)")
  (net 18 "Net-(e1-Pad30)")
  (net 19 "Net-(e1-Pad31)")
  (net 20 "Net-(e1-Pad34)")
  (net 21 "Net-(e1-Pad35)")
  (net 22 "Net-(e1-Pad37)")
  (net 23 +12V)
  (net 24 +24V)
  (net 25 "Net-(J3-Pad3)")
  (net 26 "Net-(J3-Pad4)")
  (net 27 "Net-(J3-Pad5)")
  (net 28 "Net-(J3-Pad6)")
  (net 29 "Net-(J3-Pad7)")
  (net 30 "Net-(J3-Pad8)")
  (net 31 "Net-(J3-Pad9)")
  (net 32 "Net-(J3-Pad10)")
  (net 33 "Net-(J4-Pad3)")
  (net 34 "Net-(J4-Pad4)")
  (net 35 "Net-(J4-Pad5)")
  (net 36 "Net-(J4-Pad6)")
  (net 37 "Net-(J4-Pad7)")
  (net 38 "Net-(J4-Pad8)")
  (net 39 "Net-(J4-Pad9)")
  (net 40 "Net-(J4-Pad10)")
  (net 41 "Net-(J5-Pad3)")
  (net 42 "Net-(J5-Pad4)")
  (net 43 "Net-(J5-Pad5)")
  (net 44 "Net-(J5-Pad6)")
  (net 45 "Net-(J5-Pad7)")
  (net 46 "Net-(J5-Pad8)")
  (net 47 "Net-(J5-Pad9)")
  (net 48 "Net-(J5-Pad10)")
  (net 49 "Net-(J6-Pad2)")
  (net 50 "Net-(J7-Pad2)")
  (net 51 "Net-(J8-Pad3)")
  (net 52 "Net-(J8-Pad4)")
  (net 53 "Net-(J8-Pad5)")
  (net 54 "Net-(J8-Pad6)")
  (net 55 "Net-(J8-Pad7)")
  (net 56 "Net-(J8-Pad8)")
  (net 57 "Net-(J8-Pad9)")
  (net 58 "Net-(J8-Pad10)")
  (net 59 "Net-(J9-Pad2)")
  (net 60 "Net-(J9-Pad3)")
  (net 61 "Net-(J10-Pad2)")
  (net 62 "Net-(J10-Pad3)")
  (net 63 "Net-(U2-Pad1)")
  (net 64 "Net-(U2-Pad2)")
  (net 65 "Net-(U2-Pad3)")
  (net 66 "Net-(U2-Pad4)")
  (net 67 "Net-(U2-Pad5)")
  (net 68 "Net-(U2-Pad6)")
  (net 69 "Net-(U2-Pad7)")
  (net 70 "Net-(U2-Pad8)")
  (net 71 "Net-(U3-Pad1)")
  (net 72 "Net-(U3-Pad2)")
  (net 73 "Net-(U3-Pad3)")
  (net 74 "Net-(U3-Pad4)")
  (net 75 "Net-(U3-Pad5)")
  (net 76 "Net-(U3-Pad6)")
  (net 77 "Net-(U3-Pad7)")
  (net 78 "Net-(U3-Pad8)")
  (net 79 "Net-(U4-Pad1)")
  (net 80 "Net-(U4-Pad2)")
  (net 81 "Net-(U4-Pad3)")
  (net 82 "Net-(U4-Pad4)")
  (net 83 "Net-(U4-Pad5)")
  (net 84 "Net-(U4-Pad6)")
  (net 85 "Net-(U4-Pad7)")
  (net 86 "Net-(U4-Pad8)")
  (net 87 "Net-(U5-Pad1)")
  (net 88 "Net-(U5-Pad2)")
  (net 89 "Net-(U5-Pad3)")
  (net 90 "Net-(U5-Pad4)")
  (net 91 "Net-(U5-Pad5)")
  (net 92 "Net-(U5-Pad6)")
  (net 93 "Net-(U5-Pad7)")
  (net 94 "Net-(U5-Pad8)")
  (net 95 "Net-(U6-Pad45)")
  (net 96 "Net-(U6-Pad47)")
  (net 97 "Net-(U6-Pad48)")
  (net 98 "Net-(U6-Pad49)")
  (net 99 "Net-(U6-Pad50)")
  (net 100 "Net-(U6-Pad52)")
  (net 101 "Net-(U6-Pad53)")
  (net 102 "Net-(U6-Pad54)")
  (net 103 "Net-(U6-Pad55)")
  (net 104 "/Pressure regulators/PR1_SET")
  (net 105 "/Pressure regulators/PR2_SET")
  (net 106 "Net-(U8-Pad12)")
  (net 107 "Net-(U8-Pad13)")
  (net 108 "Net-(U8-Pad14)")
  (net 109 "Net-(e1-Pad27)")
  (net 110 "Net-(e1-Pad28)")
  (net 111 "Net-(e1-Pad18)")
  (net 112 "Net-(e1-Pad17)")
  (net 113 "Net-(e1-Pad20)")
  (net 114 "Net-(e1-Pad22)")
  (net 115 "Net-(e1-Pad25)")
  (net 116 "Net-(e1-Pad26)")
  (net 117 "Net-(e1-Pad6)")
  (net 118 "/Pressure regulators/SDA")
  (net 119 "Net-(e1-Pad5)")
  (net 120 "/Pressure regulators/SCL")
  (net 121 "Net-(U8-Pad8)")
  (net 122 "Net-(U8-Pad9)")
  (net 123 "Net-(U8-Pad10)")
  (net 124 "Net-(R3-Pad2)")
  (net 125 "Net-(R4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +24V)
    (add_net +3V3)
    (add_net +5V)
    (add_net "/Pressure regulators/PR1_OUT")
    (add_net "/Pressure regulators/PR1_SET")
    (add_net "/Pressure regulators/PR2_OUT")
    (add_net "/Pressure regulators/PR2_SET")
    (add_net "/Pressure regulators/SCL")
    (add_net "/Pressure regulators/SDA")
    (add_net GND)
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J10-Pad3)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J4-Pad9)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J5-Pad9)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J8-Pad10)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(J8-Pad5)")
    (add_net "Net-(J8-Pad6)")
    (add_net "Net-(J8-Pad7)")
    (add_net "Net-(J8-Pad8)")
    (add_net "Net-(J8-Pad9)")
    (add_net "Net-(J9-Pad2)")
    (add_net "Net-(J9-Pad3)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U6-Pad30)")
    (add_net "Net-(U6-Pad45)")
    (add_net "Net-(U6-Pad47)")
    (add_net "Net-(U6-Pad48)")
    (add_net "Net-(U6-Pad49)")
    (add_net "Net-(U6-Pad50)")
    (add_net "Net-(U6-Pad52)")
    (add_net "Net-(U6-Pad53)")
    (add_net "Net-(U6-Pad54)")
    (add_net "Net-(U6-Pad55)")
    (add_net "Net-(U6-Pad56)")
    (add_net "Net-(U8-Pad10)")
    (add_net "Net-(U8-Pad12)")
    (add_net "Net-(U8-Pad13)")
    (add_net "Net-(U8-Pad14)")
    (add_net "Net-(U8-Pad8)")
    (add_net "Net-(U8-Pad9)")
    (add_net "Net-(e1-Pad11)")
    (add_net "Net-(e1-Pad12)")
    (add_net "Net-(e1-Pad16)")
    (add_net "Net-(e1-Pad17)")
    (add_net "Net-(e1-Pad18)")
    (add_net "Net-(e1-Pad2)")
    (add_net "Net-(e1-Pad20)")
    (add_net "Net-(e1-Pad21)")
    (add_net "Net-(e1-Pad22)")
    (add_net "Net-(e1-Pad23)")
    (add_net "Net-(e1-Pad24)")
    (add_net "Net-(e1-Pad25)")
    (add_net "Net-(e1-Pad26)")
    (add_net "Net-(e1-Pad27)")
    (add_net "Net-(e1-Pad28)")
    (add_net "Net-(e1-Pad29)")
    (add_net "Net-(e1-Pad30)")
    (add_net "Net-(e1-Pad31)")
    (add_net "Net-(e1-Pad34)")
    (add_net "Net-(e1-Pad35)")
    (add_net "Net-(e1-Pad37)")
    (add_net "Net-(e1-Pad5)")
    (add_net "Net-(e1-Pad6)")
  )
  (net_class 1.2A ""
    (clearance 0.1524)
    (trace_width 0.381)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class 3.5A ""
    (clearance 0.1524)
    (trace_width 1.524)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module connectors_ufcs:PJ-063AH (layer F.Cu) (tedit 5BE0C952)
    (at 148.971 91.6305)
    (descr "DC Power Jack")
    (tags "barrel jack dc")
    (fp_text reference J1 (at 0 9.39) (layer F.SilkS) hide)
    (fp_text value BARREL_JACK (at -0.3175 -4.961) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 6) (size 4.4 2) (drill oval 3.7 1.3) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole rect (at 0 0) (size 3.7 2) (drill oval 3 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole rect (at 4.5 -1) (size 2 4) (drill oval 1.3 3.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -3) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole rect (at -4.5 -1) (size 2 4) (drill oval 1.3 3.3) (layers *.Cu *.Mask))
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/barrel_jack.wrl"
      (offset (xyz 0 -6.47699990272522 4.495799932479859))
      (scale (xyz 4 4 4))
      (rotate (xyz 270 0 180))
    )
    (model C:/Users/Craig/BoxSync/ufcs/hardware/kicad/libs/CUI_INC_PJ-063AH/CUI_INC_PJ-063AH.step
      (offset (xyz 0 6 5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429)
    (at 135.763 140.6525 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J11 (at 0.254 10.668 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 10.39 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 120 "/Pressure regulators/SCL"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 "/Pressure regulators/SDA"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429)
    (at 135.763 120.8405 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J10 (at 0 10.2235 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 10.39 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J10-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(J10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 +24V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module esp32:ESP32_devkit (layer F.Cu) (tedit 5BD75027)
    (at 110.363 111.0615 90)
    (fp_text reference e1 (at -25.16 0 180) (layer F.SilkS))
    (fp_text value esp32-shield (at 0 0 90) (layer F.Fab))
    (fp_text user 3V3 (at -22.75 17 90) (layer F.SilkS))
    (fp_text user EN (at -20.25 17 90) (layer F.SilkS))
    (fp_text user IO36 (at -17.75 17 90) (layer F.SilkS))
    (fp_text user IO39 (at -15.25 17 90) (layer F.SilkS))
    (fp_text user IO34 (at -12.75 17 90) (layer F.SilkS))
    (fp_text user IO35 (at -10.25 17 90) (layer F.SilkS))
    (fp_text user IO32 (at -7.5 17 90) (layer F.SilkS))
    (fp_text user IO33 (at -5 17 90) (layer F.SilkS))
    (fp_text user IO25 (at -2.5 17 90) (layer F.SilkS))
    (fp_text user IO26 (at 0 17 90) (layer F.SilkS))
    (fp_text user IO27 (at 2.5 17 90) (layer F.SilkS))
    (fp_text user IO14 (at 5 17 90) (layer F.SilkS))
    (fp_text user IO12 (at 7.75 17 90) (layer F.SilkS))
    (fp_text user GND (at 10.25 17 90) (layer F.SilkS))
    (fp_text user IO13 (at 12.75 17 90) (layer F.SilkS))
    (fp_text user IO9 (at 15.25 17 90) (layer F.SilkS))
    (fp_text user IO10 (at 17.75 17 90) (layer F.SilkS))
    (fp_text user IO11 (at 20.25 17 90) (layer F.SilkS))
    (fp_text user 5V (at 22.75 17 90) (layer F.SilkS))
    (fp_text user IO6 (at 22.86 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO7 (at 20.32 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO8 (at 17.78 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO15 (at 15.24 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO2 (at 12.7 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO0 (at 10.16 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO4 (at 7.62 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO16 (at 5.08 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO17 (at 2.54 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO5 (at 0 -17 270 unlocked) (layer F.SilkS))
    (fp_text user IO18 (at -2.54 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO19 (at -5.08 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user GND (at -7.62 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user SDA (at -10.16 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO3 (at -12.7 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO1 (at -15.24 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user SCL (at -17.78 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user IO23 (at -20.32 -17.018 270 unlocked) (layer F.SilkS))
    (fp_text user GND (at -22.86 -17.018 270 unlocked) (layer F.SilkS))
    (pad 19 thru_hole oval (at 22.86 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 20 thru_hole oval (at 22.86 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "Net-(e1-Pad20)"))
    (pad 18 thru_hole oval (at 20.32 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(e1-Pad18)"))
    (pad 21 thru_hole oval (at 20.32 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(e1-Pad21)"))
    (pad 17 thru_hole oval (at 17.78 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(e1-Pad17)"))
    (pad 22 thru_hole oval (at 17.78 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "Net-(e1-Pad22)"))
    (pad 16 thru_hole oval (at 15.24 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(e1-Pad16)"))
    (pad 23 thru_hole oval (at 15.24 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(e1-Pad23)"))
    (pad 15 thru_hole oval (at 12.7 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U6-Pad56)"))
    (pad 24 thru_hole oval (at 12.7 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(e1-Pad24)"))
    (pad 14 thru_hole oval (at 10.16 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole oval (at 10.16 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "Net-(e1-Pad25)"))
    (pad 13 thru_hole oval (at 7.62 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U6-Pad30)"))
    (pad 26 thru_hole oval (at 7.62 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "Net-(e1-Pad26)"))
    (pad 12 thru_hole oval (at 5.08 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(e1-Pad12)"))
    (pad 27 thru_hole oval (at 5.08 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "Net-(e1-Pad27)"))
    (pad 11 thru_hole oval (at 2.54 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(e1-Pad11)"))
    (pad 28 thru_hole oval (at 2.54 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(e1-Pad28)"))
    (pad 10 thru_hole oval (at 0 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "/Pressure regulators/PR2_SET"))
    (pad 29 thru_hole oval (at 0 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(e1-Pad29)"))
    (pad 9 thru_hole oval (at -2.54 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "/Pressure regulators/PR1_SET"))
    (pad 30 thru_hole oval (at -2.54 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(e1-Pad30)"))
    (pad 8 thru_hole oval (at -5.08 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad5)"))
    (pad 31 thru_hole oval (at -5.08 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(e1-Pad31)"))
    (pad 7 thru_hole oval (at -7.62 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad1)"))
    (pad 32 thru_hole oval (at -7.62 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -10.16 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(e1-Pad6)"))
    (pad 33 thru_hole oval (at -10.16 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "/Pressure regulators/SDA"))
    (pad 5 thru_hole oval (at -12.7 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(e1-Pad5)"))
    (pad 34 thru_hole oval (at -12.7 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(e1-Pad34)"))
    (pad 4 thru_hole oval (at -15.24 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "/Pressure regulators/PR2_OUT"))
    (pad 35 thru_hole oval (at -15.24 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(e1-Pad35)"))
    (pad 3 thru_hole oval (at -17.78 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/Pressure regulators/PR1_OUT"))
    (pad 36 thru_hole oval (at -17.78 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 "/Pressure regulators/SCL"))
    (pad 2 thru_hole oval (at -20.32 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(e1-Pad2)"))
    (pad 37 thru_hole oval (at -20.32 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(e1-Pad37)"))
    (pad 1 thru_hole oval (at -22.86 12.7 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 +3V3))
    (pad 38 thru_hole oval (at -22.86 -12.75 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 38 thru_hole oval (at -22.86 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 37 thru_hole oval (at -20.32 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(e1-Pad37)"))
    (pad 36 thru_hole oval (at -17.78 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 "/Pressure regulators/SCL"))
    (pad 35 thru_hole oval (at -15.24 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(e1-Pad35)"))
    (pad 34 thru_hole oval (at -12.7 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(e1-Pad34)"))
    (pad 33 thru_hole oval (at -10.16 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "/Pressure regulators/SDA"))
    (pad 32 thru_hole oval (at -7.62 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at -5.08 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(e1-Pad31)"))
    (pad 30 thru_hole oval (at -2.54 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(e1-Pad30)"))
    (pad 29 thru_hole oval (at 0 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(e1-Pad29)"))
    (pad 28 thru_hole oval (at 2.54 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(e1-Pad28)"))
    (pad 27 thru_hole oval (at 5.08 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "Net-(e1-Pad27)"))
    (pad 26 thru_hole oval (at 7.62 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "Net-(e1-Pad26)"))
    (pad 25 thru_hole oval (at 10.16 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "Net-(e1-Pad25)"))
    (pad 24 thru_hole oval (at 12.7 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(e1-Pad24)"))
    (pad 23 thru_hole oval (at 15.24 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(e1-Pad23)"))
    (pad 22 thru_hole oval (at 17.78 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "Net-(e1-Pad22)"))
    (pad 21 thru_hole oval (at 20.32 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(e1-Pad21)"))
    (pad 20 thru_hole oval (at 22.86 -15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "Net-(e1-Pad20)"))
    (pad 1 thru_hole oval (at -22.86 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 +3V3))
    (pad 2 thru_hole oval (at -20.32 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(e1-Pad2)"))
    (pad 3 thru_hole oval (at -17.78 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/Pressure regulators/PR1_OUT"))
    (pad 4 thru_hole oval (at -15.24 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "/Pressure regulators/PR2_OUT"))
    (pad 5 thru_hole oval (at -12.7 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(e1-Pad5)"))
    (pad 6 thru_hole oval (at -10.16 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(e1-Pad6)"))
    (pad 7 thru_hole oval (at -7.62 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad1)"))
    (pad 8 thru_hole oval (at -5.08 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad5)"))
    (pad 9 thru_hole oval (at -2.54 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "/Pressure regulators/PR1_SET"))
    (pad 10 thru_hole oval (at 0 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "/Pressure regulators/PR2_SET"))
    (pad 11 thru_hole oval (at 2.54 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(e1-Pad11)"))
    (pad 12 thru_hole oval (at 5.08 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(e1-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U6-Pad30)"))
    (pad 14 thru_hole oval (at 10.16 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 12.7 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U6-Pad56)"))
    (pad 16 thru_hole oval (at 15.24 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(e1-Pad16)"))
    (pad 17 thru_hole oval (at 17.78 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(e1-Pad17)"))
    (pad 18 thru_hole oval (at 20.32 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(e1-Pad18)"))
    (pad 19 thru_hole oval (at 22.86 15.29 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model "${KIPRJMOD}/libs/esp-32-dev-board-1.snapshot.2/ESP-32-DEV Assembly.stp"
      (offset (xyz -14.2 -7.5 6))
      (scale (xyz 1.12 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module PINHEAD1-3 (layer F.Cu) (tedit 5BD86F29)
    (at 139.0015 104.8385 180)
    (fp_text reference J2 (at 7.3025 2.54 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 2.54 3.81 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 24 +24V))
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/single_header_pin/AB2_HDR_M01-1V.x3d"
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/single_header_pin/AB2_HDR_M01-1V.x3d"
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/single_header_pin/AB2_HDR_M01-1V.x3d"
      (offset (xyz 5.079999923706055 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593EC116)
    (at 196.088 90.1065)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593EC108)
    (at 90.043 90.1065)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593EC10D)
    (at 90.043 142.8115)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593EC111)
    (at 196.088 142.8115)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 593ED485)
    (at 137.9982 112.5093)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module connectors_ufcs:IDC_Header_Straight_10pins (layer F.Cu) (tedit 593ED1DF)
    (at 187.198 136.4615 180)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference J3 (at 16.4592 -0.9525 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at 5.08 4.445 180) (layer F.Fab))
    (fp_text user 1 (at 0.02 1.72 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad10)"))
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/2x5_pin_connector/AB2_HDR_M05-2V-S-3M.x3d"
      (offset (xyz 5.079999923706055 1.269999980926514 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module connectors_ufcs:IDC_Header_Straight_10pins (layer F.Cu) (tedit 593ED1DF)
    (at 187.198 121.2215 180)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference J4 (at 16.4592 -0.9525 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at 5.08 4.445 180) (layer F.Fab))
    (fp_text user 1 (at 0.02 1.72 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(J4-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(J4-Pad10)"))
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/2x5_pin_connector/AB2_HDR_M05-2V-S-3M.x3d"
      (offset (xyz 5.079999923706055 1.269999980926514 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module connectors_ufcs:IDC_Header_Straight_10pins (layer F.Cu) (tedit 593ED1DF)
    (at 187.198 106.6165 180)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference J5 (at 16.4592 -0.9525 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at 5.08 4.445 180) (layer F.Fab))
    (fp_text user 1 (at 0.02 1.72 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(J5-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 "Net-(J5-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "Net-(J5-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 "Net-(J5-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 "Net-(J5-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 "Net-(J5-Pad10)"))
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/2x5_pin_connector/AB2_HDR_M05-2V-S-3M.x3d"
      (offset (xyz 5.079999923706055 1.269999980926514 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module connectors_ufcs:IDC_Header_Straight_10pins (layer F.Cu) (tedit 593ED1DF)
    (at 187.198 92.0115 180)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference J8 (at 16.4592 -0.9525 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at 5.08 4.445 180) (layer F.Fab))
    (fp_text user 1 (at 0.02 1.72 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "Net-(J8-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 "Net-(J8-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 "Net-(J8-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 "Net-(J8-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 "Net-(J8-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 "Net-(J8-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 "Net-(J8-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 "Net-(J8-Pad10)"))
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/2x5_pin_connector/AB2_HDR_M05-2V-S-3M.x3d"
      (offset (xyz 5.079999923706055 1.269999980926514 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module connectors_ufcs:PINHEAD1-2 (layer F.Cu) (tedit 5BD78D1F)
    (at 149.1234 138.6205)
    (fp_text reference J6 (at 3.1496 -3.81) (layer F.SilkS))
    (fp_text value PUMP (at 1.27 2.3495) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J6-Pad2)"))
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/single_header_pin/AB2_HDR_M01-1V.x3d"
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/single_header_pin/AB2_HDR_M01-1V.x3d"
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module connectors_ufcs:PINHEAD1-2 (layer F.Cu) (tedit 5BD78D2D)
    (at 149.1742 129.1717)
    (fp_text reference J7 (at 3.0988 -3.7592) (layer F.SilkS))
    (fp_text value VACUUM (at 1.27 2.3495) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J7-Pad2)"))
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/single_header_pin/AB2_HDR_M01-1V.x3d"
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Craig/Box Sync/ufcs/hardware/3d/pcb_components/single_header_pin/AB2_HDR_M01-1V.x3d"
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429)
    (at 135.763 129.4765 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J9 (at 0 10.2235 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 10.39 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 +24V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(J9-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(J9-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5BD87A5B)
    (at 130.1115 114.427 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 2.4765 0.0635 90) (layer F.SilkS))
    (fp_text value 1k6 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +3V3))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 118 "/Pressure regulators/SDA"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5BD87A67)
    (at 132.6515 114.427 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 2.4765 0.0635 90) (layer F.SilkS))
    (fp_text value 1k6 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 120 "/Pressure regulators/SCL"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BD87A89)
    (at 107.823 104.0765)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -2.54 0) (layer B.SilkS))
    (fp_text value 2k7 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 124 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BD87A97)
    (at 113.3475 104.0765 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -2.6035 0 180) (layer B.SilkS))
    (fp_text value 2k7 (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BD87A8D)
    (at 107.823 105.8545)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -2.54 0) (layer B.SilkS))
    (fp_text value 1k8 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 124 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(J9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BD87AA3)
    (at 113.3475 105.8545 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -2.6035 0 180) (layer B.SilkS))
    (fp_text value 1k8 (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(J10-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BD87AD4)
    (at 130.57 129.7305)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 2.653 0) (layer B.SilkS))
    (fp_text value 1k8 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(J9-Pad3)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/Pressure regulators/PR1_OUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BD87ACC)
    (at 130.57 132.0165 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -2.653 0) (layer B.SilkS))
    (fp_text value 3k3 (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/Pressure regulators/PR1_OUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BD87AC1)
    (at 130.57 124.3965)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 2.653 0) (layer B.SilkS))
    (fp_text value 1k8 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/Pressure regulators/PR2_OUT"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(J10-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5BD87ABC)
    (at 130.57 126.4285 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -3.161 0 180) (layer B.SilkS))
    (fp_text value 3k3 (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/Pressure regulators/PR2_OUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 163.6776 138.0871)
    (descr "18-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -6.875) (layer F.SilkS))
    (fp_text value ULN2803A (at 0 6.875) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -4.7 -3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -4.7 -2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -4.7 -1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -4.7 0) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -4.7 1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -4.7 2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -4.7 3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U2-Pad8)"))
    (pad 9 smd rect (at -4.7 5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 4.7 5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +12V))
    (pad 11 smd rect (at 4.7 3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J3-Pad10)"))
    (pad 12 smd rect (at 4.7 2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J3-Pad9)"))
    (pad 13 smd rect (at 4.7 1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J3-Pad8)"))
    (pad 14 smd rect (at 4.7 0) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J3-Pad7)"))
    (pad 15 smd rect (at 4.7 -1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J3-Pad6)"))
    (pad 16 smd rect (at 4.7 -2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J3-Pad5)"))
    (pad 17 smd rect (at 4.7 -3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad4)"))
    (pad 18 smd rect (at 4.7 -5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 163.5252 108.6231)
    (descr "18-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -6.875) (layer F.SilkS))
    (fp_text value ULN2803A (at 0 6.875) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 18 smd rect (at 4.7 -5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J5-Pad3)"))
    (pad 17 smd rect (at 4.7 -3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J5-Pad4)"))
    (pad 16 smd rect (at 4.7 -2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J5-Pad5)"))
    (pad 15 smd rect (at 4.7 -1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J5-Pad6)"))
    (pad 14 smd rect (at 4.7 0) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J5-Pad7)"))
    (pad 13 smd rect (at 4.7 1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J5-Pad8)"))
    (pad 12 smd rect (at 4.7 2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J5-Pad9)"))
    (pad 11 smd rect (at 4.7 3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J5-Pad10)"))
    (pad 10 smd rect (at 4.7 5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +12V))
    (pad 9 smd rect (at -4.7 5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -4.7 3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U4-Pad8)"))
    (pad 7 smd rect (at -4.7 2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U4-Pad7)"))
    (pad 6 smd rect (at -4.7 1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U4-Pad6)"))
    (pad 5 smd rect (at -4.7 0) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U4-Pad5)"))
    (pad 4 smd rect (at -4.7 -1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U4-Pad4)"))
    (pad 3 smd rect (at -4.7 -2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U4-Pad3)"))
    (pad 2 smd rect (at -4.7 -3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U4-Pad2)"))
    (pad 1 smd rect (at -4.7 -5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U4-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 163.5506 94.0435)
    (descr "18-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 0 -6.875) (layer F.SilkS))
    (fp_text value ULN2803A (at 0 6.875) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 18 smd rect (at 4.7 -5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J8-Pad3)"))
    (pad 17 smd rect (at 4.7 -3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J8-Pad4)"))
    (pad 16 smd rect (at 4.7 -2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J8-Pad5)"))
    (pad 15 smd rect (at 4.7 -1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J8-Pad6)"))
    (pad 14 smd rect (at 4.7 0) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J8-Pad7)"))
    (pad 13 smd rect (at 4.7 1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J8-Pad8)"))
    (pad 12 smd rect (at 4.7 2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J8-Pad9)"))
    (pad 11 smd rect (at 4.7 3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J8-Pad10)"))
    (pad 10 smd rect (at 4.7 5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +12V))
    (pad 9 smd rect (at -4.7 5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -4.7 3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U5-Pad8)"))
    (pad 7 smd rect (at -4.7 2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U5-Pad7)"))
    (pad 6 smd rect (at -4.7 1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U5-Pad6)"))
    (pad 5 smd rect (at -4.7 0) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U5-Pad5)"))
    (pad 4 smd rect (at -4.7 -1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U5-Pad4)"))
    (pad 3 smd rect (at -4.7 -2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U5-Pad3)"))
    (pad 2 smd rect (at -4.7 -3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U5-Pad2)"))
    (pad 1 smd rect (at -4.7 -5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U5-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer B.Cu) (tedit 5A02F2D3)
    (at 111.3155 112.4585 270)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U8 (at 0 5.375 270) (layer B.SilkS))
    (fp_text value OpAmp-TLV2374 (at 0 -5.375 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 3.81 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(J9-Pad2)"))
    (pad 2 smd rect (at -2.7 2.54 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 124 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -2.7 1.27 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 104 "/Pressure regulators/PR1_SET"))
    (pad 4 smd rect (at -2.7 0 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at -2.7 -1.27 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 105 "/Pressure regulators/PR2_SET"))
    (pad 6 smd rect (at -2.7 -2.54 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 125 "Net-(R4-Pad2)"))
    (pad 7 smd rect (at -2.7 -3.81 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(J10-Pad2)"))
    (pad 8 smd rect (at 2.7 -3.81 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 121 "Net-(U8-Pad8)"))
    (pad 9 smd rect (at 2.7 -2.54 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 122 "Net-(U8-Pad9)"))
    (pad 10 smd rect (at 2.7 -1.27 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 123 "Net-(U8-Pad10)"))
    (pad 11 smd rect (at 2.7 0 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 2.7 1.27 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 106 "Net-(U8-Pad12)"))
    (pad 13 smd rect (at 2.7 2.54 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 107 "Net-(U8-Pad13)"))
    (pad 14 smd rect (at 2.7 3.81 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 108 "Net-(U8-Pad14)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer B.Cu) (tedit 5A02F2D3)
    (at 154.051 120.8405 270)
    (descr "18-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 6.875 270) (layer B.SilkS))
    (fp_text value ULN2803A (at 0 -6.875 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 18 smd rect (at 4.7 5.08 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(J6-Pad2)"))
    (pad 17 smd rect (at 4.7 3.81 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(J6-Pad2)"))
    (pad 16 smd rect (at 4.7 2.54 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(J6-Pad2)"))
    (pad 15 smd rect (at 4.7 1.27 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(J6-Pad2)"))
    (pad 14 smd rect (at 4.7 0 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(J7-Pad2)"))
    (pad 13 smd rect (at 4.7 -1.27 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(J7-Pad2)"))
    (pad 12 smd rect (at 4.7 -2.54 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(J7-Pad2)"))
    (pad 11 smd rect (at 4.7 -3.81 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(J7-Pad2)"))
    (pad 10 smd rect (at 4.7 -5.08 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 23 +12V))
    (pad 9 smd rect (at -4.7 -5.08 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -4.7 -3.81 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(U1-Pad5)"))
    (pad 7 smd rect (at -4.7 -2.54 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -4.7 -1.27 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(U1-Pad5)"))
    (pad 5 smd rect (at -4.7 0 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -4.7 1.27 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U1-Pad1)"))
    (pad 3 smd rect (at -4.7 2.54 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -4.7 3.81 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U1-Pad1)"))
    (pad 1 smd rect (at -4.7 5.08 270) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 163.5506 122.8725)
    (descr "18-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -6.875) (layer F.SilkS))
    (fp_text value ULN2803A (at 0 6.875) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -4.7 -3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -4.7 -2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at -4.7 -1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at -4.7 0) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -4.7 1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -4.7 2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at -4.7 3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U3-Pad8)"))
    (pad 9 smd rect (at -4.7 5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 4.7 5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +12V))
    (pad 11 smd rect (at 4.7 3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J4-Pad10)"))
    (pad 12 smd rect (at 4.7 2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J4-Pad9)"))
    (pad 13 smd rect (at 4.7 1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J4-Pad8)"))
    (pad 14 smd rect (at 4.7 0) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J4-Pad7)"))
    (pad 15 smd rect (at 4.7 -1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J4-Pad6)"))
    (pad 16 smd rect (at 4.7 -2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J4-Pad5)"))
    (pad 17 smd rect (at 4.7 -3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J4-Pad4)"))
    (pad 18 smd rect (at 4.7 -5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-56_6.1x14mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 149.098 111.379 90)
    (descr "TSSOP56: plastic thin shrink small outline package; 56 leads; body width 6.1 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot364-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U6 (at 0 -8.05 90) (layer F.SilkS))
    (fp_text value PCA9698 (at 0 8.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.75 -6.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 118 "/Pressure regulators/SDA"))
    (pad 2 smd rect (at -3.75 -6.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 120 "/Pressure regulators/SCL"))
    (pad 3 smd rect (at -3.75 -5.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U2-Pad8)"))
    (pad 4 smd rect (at -3.75 -5.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U2-Pad7)"))
    (pad 5 smd rect (at -3.75 -4.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U2-Pad6)"))
    (pad 6 smd rect (at -3.75 -4.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -3.75 -3.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U2-Pad5)"))
    (pad 8 smd rect (at -3.75 -3.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U2-Pad4)"))
    (pad 9 smd rect (at -3.75 -2.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U2-Pad3)"))
    (pad 10 smd rect (at -3.75 -2.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U2-Pad2)"))
    (pad 11 smd rect (at -3.75 -1.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -3.75 -1.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U2-Pad1)"))
    (pad 13 smd rect (at -3.75 -0.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U3-Pad8)"))
    (pad 14 smd rect (at -3.75 -0.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U3-Pad7)"))
    (pad 15 smd rect (at -3.75 0.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U3-Pad6)"))
    (pad 16 smd rect (at -3.75 0.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U3-Pad5)"))
    (pad 17 smd rect (at -3.75 1.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U3-Pad4)"))
    (pad 18 smd rect (at -3.75 1.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 19 smd rect (at -3.75 2.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U3-Pad3)"))
    (pad 20 smd rect (at -3.75 2.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U3-Pad2)"))
    (pad 21 smd rect (at -3.75 3.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U3-Pad1)"))
    (pad 22 smd rect (at -3.75 3.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U4-Pad8)"))
    (pad 23 smd rect (at -3.75 4.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at -3.75 4.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U4-Pad7)"))
    (pad 25 smd rect (at -3.75 5.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U4-Pad6)"))
    (pad 26 smd rect (at -3.75 5.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U4-Pad5)"))
    (pad 27 smd rect (at -3.75 6.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at -3.75 6.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at 3.75 6.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 3.75 6.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U6-Pad30)"))
    (pad 31 smd rect (at 3.75 5.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U4-Pad4)"))
    (pad 32 smd rect (at 3.75 5.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U4-Pad3)"))
    (pad 33 smd rect (at 3.75 4.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U4-Pad2)"))
    (pad 34 smd rect (at 3.75 4.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 35 smd rect (at 3.75 3.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U4-Pad1)"))
    (pad 36 smd rect (at 3.75 3.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U5-Pad8)"))
    (pad 37 smd rect (at 3.75 2.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U5-Pad7)"))
    (pad 38 smd rect (at 3.75 2.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U5-Pad6)"))
    (pad 39 smd rect (at 3.75 1.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at 3.75 1.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U5-Pad5)"))
    (pad 41 smd rect (at 3.75 0.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U5-Pad4)"))
    (pad 42 smd rect (at 3.75 0.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U5-Pad3)"))
    (pad 43 smd rect (at 3.75 -0.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U5-Pad2)"))
    (pad 44 smd rect (at 3.75 -0.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U5-Pad1)"))
    (pad 45 smd rect (at 3.75 -1.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U6-Pad45)"))
    (pad 46 smd rect (at 3.75 -1.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 47 smd rect (at 3.75 -2.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(U6-Pad47)"))
    (pad 48 smd rect (at 3.75 -2.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U6-Pad48)"))
    (pad 49 smd rect (at 3.75 -3.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(U6-Pad49)"))
    (pad 50 smd rect (at 3.75 -3.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(U6-Pad50)"))
    (pad 51 smd rect (at 3.75 -4.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 52 smd rect (at 3.75 -4.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(U6-Pad52)"))
    (pad 53 smd rect (at 3.75 -5.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(U6-Pad53)"))
    (pad 54 smd rect (at 3.75 -5.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(U6-Pad54)"))
    (pad 55 smd rect (at 3.75 -6.25 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(U6-Pad55)"))
    (pad 56 smd rect (at 3.75 -6.75 90) (size 1 0.285) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U6-Pad56)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-56_6.1x14mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT (layer F.Cu) (tedit 5B741BB0)
    (at 138.303 95.9485 90)
    (descr "DCDC-Converter, RECOM, RECOM_R-78E-0.5, SIP-3, pitch 2.54mm, package size 11.6x8.5x10.4mm^3, https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf")
    (tags "dc-dc recom buck sip-3 pitch 2.54mm")
    (fp_text reference U7 (at 2.54 -7.56 90) (layer F.SilkS))
    (fp_text value R-78 (at 2.54 3 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -2.25 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 23 +12V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_RECOM_R-78E-0.5_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 144.907 145.2245) (layer F.SilkS))
  (gr_text 12V (at 141.097 145.2245) (layer F.SilkS))
  (gr_text SDA (at 137.795 145.2245) (layer F.SilkS))
  (gr_text SCL (at 134.493 145.2245) (layer F.SilkS))
  (gr_text Digital (at 131.699 141.6685 90) (layer F.SilkS))
  (gr_text "Analog (Parker)" (at 131.445 125.1585 90) (layer F.SilkS))
  (gr_text "Pressure regulators" (at 128.905 132.0165 90) (layer F.SilkS))
  (gr_text "12-24V\nstep-up" (at 142.367 103.5685 90) (layer F.SilkS))
  (gr_text "LBNC, EPFL\nSenyo Lab, CWRU" (at 88.9 136.8425 270) (layer F.SilkS))
  (gr_text GND (at 148.971 93.5355) (layer F.SilkS))
  (gr_text +12V (at 148.971 95.4405) (layer F.SilkS))
  (gr_text ESP32-DevKitC (at 110.236 112.3315) (layer F.SilkS))
  (gr_text "Microfluidics Control System v1.1\nCraig F. Watson, 2018\ncraig.watson@case.edu\n" (at 89.2175 95.631 270) (layer F.SilkS))
  (gr_line (start 85.598 86.2965) (end 199.898 86.2965) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.898 146.6215) (end 85.598 146.6215) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.898 146.6215) (end 199.898 86.2965) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.598 86.2965) (end 85.598 146.6215) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 143.891 134.5565) (layer F.SilkS))
  (gr_text PV (at 140.716 134.5565) (layer F.SilkS))
  (gr_text SP (at 138.176 134.5565) (layer F.SilkS))
  (gr_text 24V (at 135.001 134.5565) (layer F.SilkS))
  (gr_text R-78 (at 135.636 93.5355 270) (layer F.SilkS))
  (gr_text 5V (at 141.605 90.3605 90) (layer F.SilkS))
  (gr_text GND (at 141.605 93.4085 90) (layer F.SilkS))
  (gr_text 12V (at 141.605 96.7105 90) (layer F.SilkS))
  (gr_text GND (at 136.271 109.093) (layer F.SilkS))
  (gr_text 12V (at 139.7635 109.0295) (layer F.SilkS))
  (gr_text 24V (at 132.5245 109.093) (layer F.SilkS))
  (gr_text PV (at 140.716 125.2855) (layer F.SilkS))
  (gr_text SP (at 138.176 125.2855) (layer F.SilkS))
  (gr_text GND (at 143.891 125.2855) (layer F.SilkS))
  (gr_text 24V (at 135.001 125.2855) (layer F.SilkS))
  (gr_text 2 (at 133.223 120.8405) (layer F.SilkS))
  (gr_text 1 (at 132.969 129.7305) (layer F.SilkS))
  (gr_text - (at 151.892 143.1925) (layer F.SilkS))
  (gr_text - (at 152.019 133.4135) (layer F.SilkS))
  (gr_text + (at 149.1615 143.129) (layer F.SilkS))
  (gr_text + (at 149.2885 133.4135) (layer F.SilkS))
  (gr_text "Pump 2" (at 154.94 128.3335 90) (layer F.SilkS))
  (gr_text "Pump 1" (at 154.8765 138.684 90) (layer F.SilkS))
  (gr_text "Valves 25-32" (at 182.118 99.6315) (layer F.SilkS))
  (gr_text "Valves 17-24" (at 182.118 114.2365) (layer F.SilkS))
  (gr_text "Valves 9-16" (at 181.483 128.8415) (layer F.SilkS))
  (gr_text "Valves 1-8" (at 181.483 144.0815) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.201 84.0105) (xy 203.581 84.0105) (xy 203.581 150.0505) (xy 84.201 150.0505)
      )
    )
  )
)
