(kicad_pcb (version 20190331) (host pcbnew "(5.1.0-218-ge90452d)")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 3)
    (zones 0)
    (modules 29)
    (nets 56)
  )
  (page "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user)
    (33 "F.Adhes" user)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user)
    (37 "F.SilkS" user)
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user)
    (41 "Cmts.User" user)
    (42 "Eco1.User" user)
    (43 "Eco2.User" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user)
    (47 "F.CrtYd" user)
    (48 "B.Fab" user)
    (49 "F.Fab" user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad48)")
  (net 2 "Net-(U1-Pad47)")
  (net 3 "Net-(U1-Pad46)")
  (net 4 "Net-(U1-Pad45)")
  (net 5 "Net-(U1-Pad44)")
  (net 6 "Net-(U1-Pad43)")
  (net 7 "Net-(U1-Pad42)")
  (net 8 "Net-(U1-Pad41)")
  (net 9 "Net-(U1-Pad40)")
  (net 10 "Net-(U1-Pad39)")
  (net 11 "Net-(U1-Pad38)")
  (net 12 "Net-(U1-Pad37)")
  (net 13 "Net-(U1-Pad36)")
  (net 14 "Net-(U1-Pad35)")
  (net 15 "Net-(U1-Pad34)")
  (net 16 "Net-(U1-Pad32)")
  (net 17 "Net-(U1-Pad31)")
  (net 18 "Net-(U1-Pad28)")
  (net 19 "Net-(U1-Pad25)")
  (net 20 "Net-(U1-Pad23)")
  (net 21 "Net-(U1-Pad21)")
  (net 22 "Net-(U1-Pad20)")
  (net 23 "Net-(U1-Pad19)")
  (net 24 "Net-(U1-Pad18)")
  (net 25 "Net-(U1-Pad13)")
  (net 26 "Net-(U1-Pad12)")
  (net 27 "Net-(U1-Pad11)")
  (net 28 "Net-(U1-Pad10)")
  (net 29 "Net-(U1-Pad9)")
  (net 30 "Net-(U1-Pad8)")
  (net 31 "Net-(U1-Pad7)")
  (net 32 "Net-(U1-Pad6)")
  (net 33 "Net-(U1-Pad4)")
  (net 34 "Net-(U1-Pad3)")
  (net 35 "Net-(U1-Pad2)")
  (net 36 "GND")
  (net 37 "+5V")
  (net 38 "+3V3")
  (net 39 "+1V2")
  (net 40 "Net-(C10-Pad1)")
  (net 41 "Net-(D1-Pad1)")
  (net 42 "Net-(U2-Pad4)")
  (net 43 "Net-(U3-Pad4)")
  (net 44 "Net-(R2-Pad1)")
  (net 45 "Net-(U4-Pad7)")
  (net 46 "Net-(U4-Pad3)")
  (net 47 "Net-(J?1555295715-Pad3)")
  (net 48 "Net-(R?1555303253-Pad1)")
  (net 49 "Net-(J?1555295715-Pad2)")
  (net 50 "Net-(R?1555309571-Pad1)")
  (net 51 "/ICE40_SPI_SI")
  (net 52 "/ICE40_SPI_SS")
  (net 53 "/ICE40_SPI_SCK")
  (net 54 "/ICE40_SPI_SO")
  (net 55 "Net-(J?1555295715-Pad4)")
  (net_class "Default" "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "+1V2")
    (add_net "+3V3")
    (add_net "+5V")
    (add_net "/ICE40_SPI_SCK")
    (add_net "/ICE40_SPI_SI")
    (add_net "/ICE40_SPI_SO")
    (add_net "/ICE40_SPI_SS")
    (add_net "GND")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J?1555295715-Pad2)")
    (add_net "Net-(J?1555295715-Pad3)")
    (add_net "Net-(J?1555295715-Pad4)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R?1555303253-Pad1)")
    (add_net "Net-(R?1555309571-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad7)")
  )
  (module "latchup-badge:logo_1" (layer "F.Cu") (tedit 0)
    (at 127 104.14)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (module "latchup-badge:logo" (layer "F.Cu") (tedit 0)
    (at 127 104.14)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (module "Connector_USB:USB_Micro-B_Molex-105017-0001" (layer "B.Cu") (tedit 5A1DC0BE)
    (at 79.29372 78.2447 90)
    (descr "http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf")
    (tags "Micro-USB SMD Typ-B")
    (attr smd)
    (fp_text reference "J1" (at 0 3.1125 270) (layer "B.SilkS"))
    (fp_text value "USB_B_Micro" (at 0.3 -4.3375 270) (layer "B.Fab"))
    (fp_text user "%R" (at 0 -0.8875 270) (layer "B.Fab"))
    (fp_text user "PCB Edge" (at 0 -2.6875 270) (layer "Dwgs.User"))
    (pad "6" smd rect (at -2.9 -1.2375 90) (size 1.2 1.9) (layers "B.Cu" "B.Mask")
      (net 36 "GND"))
    (pad "6" smd rect (at 2.9 -1.2375 90) (size 1.2 1.9) (layers "B.Cu" "B.Mask")
      (net 36 "GND"))
    (pad "6" thru_hole oval (at 3.5 -1.2375 90) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 36 "GND"))
    (pad "6" thru_hole oval (at -3.5 -1.2375 270) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 36 "GND"))
    (pad "6" smd rect (at -1 -1.2375 90) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "GND"))
    (pad "6" thru_hole circle (at 2.5 1.4625 90) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 36 "GND"))
    (pad "3" smd rect (at 0 1.4625 90) (size 0.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "Net-(J?1555295715-Pad3)"))
    (pad "4" smd rect (at 0.65 1.4625 90) (size 0.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "Net-(J?1555295715-Pad4)"))
    (pad "5" smd rect (at 1.3 1.4625 90) (size 0.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "GND"))
    (pad "1" smd rect (at -1.3 1.4625 90) (size 0.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "+5V"))
    (pad "2" smd rect (at -0.65 1.4625 90) (size 0.4 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "Net-(J?1555295715-Pad2)"))
    (pad "6" thru_hole circle (at -2.5 1.4625 90) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 36 "GND"))
    (pad "6" smd rect (at 1 -1.2375 90) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "GND"))
    (model "${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex-105017-0001.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBD)
    (at 106.02214 68.28536 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R5" (at -2.06756 -0.10922 270) (layer "B.SilkS"))
    (fp_text value "1.5K" (at 0 -1.17 270) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 270) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(R?1555303253-Pad1)"))
    (pad "1" smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(U1-Pad25)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBD)
    (at 84.99602 78.9305 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R4" (at -0.00254 -1.28524) (layer "B.SilkS"))
    (fp_text value "25" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(J?1555295715-Pad2)"))
    (pad "1" smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R?1555309571-Pad1)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBD)
    (at 84.99602 77.89164 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 1.17) (layer "B.SilkS"))
    (fp_text value "25" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(J?1555295715-Pad3)"))
    (pad "1" smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(R?1555303253-Pad1)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Package_SO:SOIJ-8_5.3x5.3mm_P1.27mm" (layer "B.Cu") (tedit 5A02F2D3)
    (at 118.04396 75.00112)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference "U4" (at 0 3.68) (layer "B.SilkS"))
    (fp_text value "M25PX32-VMW" (at 0 -3.68) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "8" smd rect (at 3.65 1.905) (size 1.7 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "+3V3"))
    (pad "7" smd rect (at 3.65 0.635) (size 1.7 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "Net-(U4-Pad7)"))
    (pad "6" smd rect (at 3.65 -0.635) (size 1.7 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "/ICE40_SPI_SCK"))
    (pad "5" smd rect (at 3.65 -1.905) (size 1.7 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "/ICE40_SPI_SO"))
    (pad "4" smd rect (at -3.65 -1.905) (size 1.7 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "GND"))
    (pad "3" smd rect (at -3.65 -0.635) (size 1.7 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "Net-(U4-Pad3)"))
    (pad "2" smd rect (at -3.65 0.635) (size 1.7 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "/ICE40_SPI_SI"))
    (pad "1" smd rect (at -3.65 1.905) (size 1.7 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "/ICE40_SPI_SS"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIJ-8_5.3x5.3mm_P1.27mm.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 124.78258 76.84262 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C15" (at 0 1.17) (layer "B.SilkS"))
    (fp_text value ".1uF" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (pad "1" smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Oscillator:Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm" (layer "B.Cu") (tedit 58CD3344)
    (at 104.275241 59.809039)
    (descr "Miniature Crystal Clock Oscillator Abracon ASE series, http://www.abracon.com/Oscillators/ASEseries.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal oscillator")
    (attr smd)
    (fp_text reference "X1" (at 0 2.45 180) (layer "B.SilkS"))
    (fp_text value "ASE-12.000MHz" (at 0 -2.45 180) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 180) (layer "B.Fab"))
    (pad "4" smd rect (at -1.05 0.825) (size 1.3 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "+3V3"))
    (pad "3" smd rect (at 1.05 0.825) (size 1.3 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "Net-(U1-Pad35)"))
    (pad "2" smd rect (at 1.05 -0.825) (size 1.3 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "GND"))
    (pad "1" smd rect (at -1.05 -0.825) (size 1.3 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "Net-(R2-Pad1)"))
    (model "${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBD)
    (at 104.02824 57.34304)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.143 180) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.17 180) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 180) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (pad "1" smd roundrect (at -0.485 0) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(R2-Pad1)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 101.36124 59.88304 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0 1.17 90) (layer "B.SilkS"))
    (fp_text value ".1uF" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 90) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (pad "1" smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Package_TO_SOT_SMD:SOT-23-5" (layer "B.Cu") (tedit 5A02FF57)
    (at 93.258392 82.697579 270)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (attr smd)
    (fp_text reference "U3" (at -0.002799 2.727712 90) (layer "B.SilkS"))
    (fp_text value "TLV70033_SOT23-5" (at 0 -2.9 90) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "5" smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "+3V3"))
    (pad "4" smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "Net-(U3-Pad4)"))
    (pad "3" smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "+5V"))
    (pad "2" smd rect (at -1.1 0 270) (size 1.06 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "GND"))
    (pad "1" smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "+5V"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Package_TO_SOT_SMD:SOT-23-5" (layer "B.Cu") (tedit 5A02FF57)
    (at 99.608392 82.697579 270)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (attr smd)
    (fp_text reference "U2" (at -0.002799 2.727712 90) (layer "B.SilkS"))
    (fp_text value "TLV70012_SOT23-5" (at 0 -2.9 90) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "5" smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "+1V2"))
    (pad "4" smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "Net-(U2-Pad4)"))
    (pad "3" smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "+5V"))
    (pad "2" smd rect (at -1.1 0 270) (size 1.06 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "GND"))
    (pad "1" smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "+5V"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBD)
    (at 104.28224 67.37604 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R1" (at 2.03708 0.09144) (layer "B.SilkS"))
    (fp_text value "100" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C10-Pad1)"))
    (pad "1" smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V2"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Diode_SMD:D_0603_1608Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 107.71124 72.58304 270)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (attr smd)
    (fp_text reference "D1" (at 2.3875 0 90) (layer "B.SilkS"))
    (fp_text value "CDBU0520" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 90) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(D1-Pad1)"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 117.49024 63.82004 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C13" (at -3.048 0) (layer "B.SilkS"))
    (fp_text value ".1uF" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (pad "1" smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 117.49024 64.96304)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C12" (at 3.048 0 180) (layer "B.SilkS"))
    (fp_text value ".1uF" (at 0 -1.17 180) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 180) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (pad "1" smd roundrect (at -0.485 0) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V2"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 117.49013 66.339846)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C11" (at 3.048 0 180) (layer "B.SilkS"))
    (fp_text value "10uF" (at 0 -1.43 180) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 180) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V2"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 104.28224 68.39204 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C10" (at 2.4384 -0.33274) (layer "B.SilkS"))
    (fp_text value ".1uF" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (pad "1" smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C10-Pad1)"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 104.28478 65.65138 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C9" (at 2.11582 0.01016) (layer "B.SilkS"))
    (fp_text value ".1uF" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (pad "1" smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V2"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 97.9805 68.38696 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C8" (at 2.54 0) (layer "B.SilkS"))
    (fp_text value "10uF" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C10-Pad1)"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 98.87966 65.6209 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C7" (at 2.54 -0.020194) (layer "B.SilkS"))
    (fp_text value "10uF" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V2"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 109.23524 72.58304 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C6" (at -2.39 0 270) (layer "B.SilkS"))
    (fp_text value ".1uF" (at 0 -1.17 270) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 270) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (pad "1" smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 93.258392 85.872579)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 1.43 180) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.43 180) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 180) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 99.608392 85.872579)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 1.43 180) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.43 180) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 180) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V2"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 104.282129 63.799845)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C3" (at -1.968389 0.037975 180) (layer "B.SilkS"))
    (fp_text value ".1uF" (at 0 -1.17 180) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 180) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.485 0) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (pad "1" smd roundrect (at -0.485 0) (size 0.59 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 93.258392 79.522579)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0.066288 -1.399799 180) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.43 180) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 180) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "+5V"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu") (tedit 5B301BBE)
    (at 99.608392 79.522579)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0.066288 -1.399799 180) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.43 180) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0 180) (layer "B.Fab"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "GND"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "+5V"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm" (layer "B.Cu") (tedit 5C26A111)
    (at 111.072129 66.023846 180)
    (descr "QFN, 48 Pin (http://www.st.com/resource/en/datasheet/stm32f042k6.pdf#page=94), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference "U1" (at 0 4.82) (layer "B.SilkS"))
    (fp_text value "ICE40UP5K-SG48ITR" (at 0 -4.82) (layer "B.Fab"))
    (fp_text user "%R" (at 0 0) (layer "B.Fab"))
    (pad "48" smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad48)"))
    (pad "47" smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(U1-Pad47)"))
    (pad "46" smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U1-Pad46)"))
    (pad "45" smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U1-Pad45)"))
    (pad "44" smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(U1-Pad44)"))
    (pad "43" smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U1-Pad43)"))
    (pad "42" smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(U1-Pad42)"))
    (pad "41" smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(U1-Pad41)"))
    (pad "40" smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(U1-Pad40)"))
    (pad "39" smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U1-Pad39)"))
    (pad "38" smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1-Pad38)"))
    (pad "37" smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(U1-Pad37)"))
    (pad "36" smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U1-Pad36)"))
    (pad "35" smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U1-Pad35)"))
    (pad "34" smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U1-Pad34)"))
    (pad "33" smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (pad "32" smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U1-Pad32)"))
    (pad "31" smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U1-Pad31)"))
    (pad "30" smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V2"))
    (pad "29" smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C10-Pad1)"))
    (pad "28" smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(U1-Pad28)"))
    (pad "27" smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(R?1555303253-Pad1)"))
    (pad "26" smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R?1555309571-Pad1)"))
    (pad "25" smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(U1-Pad25)"))
    (pad "24" smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(D1-Pad1)"))
    (pad "23" smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(U1-Pad23)"))
    (pad "22" smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (pad "21" smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U1-Pad21)"))
    (pad "20" smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U1-Pad20)"))
    (pad "19" smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U1-Pad19)"))
    (pad "18" smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U1-Pad18)"))
    (pad "17" smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/ICE40_SPI_SI"))
    (pad "16" smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "/ICE40_SPI_SS"))
    (pad "15" smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "/ICE40_SPI_SCK"))
    (pad "14" smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "/ICE40_SPI_SO"))
    (pad "13" smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U1-Pad13)"))
    (pad "12" smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U1-Pad12)"))
    (pad "11" smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U1-Pad11)"))
    (pad "10" smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(U1-Pad10)"))
    (pad "9" smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U1-Pad9)"))
    (pad "8" smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(U1-Pad8)"))
    (pad "7" smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U1-Pad7)"))
    (pad "6" smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(U1-Pad6)"))
    (pad "5" smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V2"))
    (pad "4" smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(U1-Pad4)"))
    (pad "3" smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(U1-Pad3)"))
    (pad "2" smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(U1-Pad2)"))
    (pad "1" smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "+3V3"))
    (pad "" smd roundrect (at 2.1 -2.1 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 2.1 -0.7 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 2.1 0.7 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 2.1 2.1 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.7 -2.1 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.7 -0.7 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.7 0.7 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.7 2.1 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.7 -2.1 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.7 -0.7 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.7 0.7 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.7 2.1 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -2.1 -2.1 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -2.1 -0.7 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -2.1 0.7 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -2.1 2.1 180) (size 1.13 1.13) (layers "B.Paste") (roundrect_rratio 0.221239))
    (pad "49" smd roundrect (at 0 0 180) (size 5.6 5.6) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.044643)
      (net 36 "GND"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MY NAME IS" (at 128.27 63.5) (layer "F.SilkS"))
  (gr_text "HELLO" (at 128.27 57.15) (layer "F.SilkS"))
  (gr_line (start 165.1 59.055) (end 172.72 59.055) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 165.1 55.88) (end 165.1 52.705) (angle -180) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 172.72 55.88) (end 172.72 59.055) (angle -180) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 165.1 52.705) (end 172.72 52.705) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 81.28 59.055) (end 88.9 59.055) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 81.28 52.705) (end 88.9 52.705) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 88.9 55.88) (end 88.9 59.055) (angle -180) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 81.28 55.88) (end 81.28 52.705) (angle -180) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 81.28 55.88) (end 81.28 50.8) (angle -90) (layer "Edge.Cuts") (width 0.12))
  (gr_arc (start 81.28 116.84) (end 76.2 116.84) (angle -90) (layer "Edge.Cuts") (width 0.12))
  (gr_arc (start 172.72 116.84) (end 172.72 121.92) (angle -90) (layer "Edge.Cuts") (width 0.12))
  (gr_arc (start 172.72 55.88) (end 177.8 55.88) (angle -90) (layer "Edge.Cuts") (width 0.12))
  (gr_line (start 76.2 116.84) (end 76.2 55.88) (layer "Edge.Cuts") (width 0.12))
  (gr_line (start 81.28 121.92) (end 172.72 121.92) (layer "Edge.Cuts") (width 0.12))
  (gr_line (start 177.8 55.88) (end 177.8 116.84) (layer "Edge.Cuts") (width 0.12))
  (gr_line (start 81.28 50.8) (end 172.72 50.8) (layer "Edge.Cuts") (width 0.12))
  (zone (net 36) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 121.92) (xy 177.8 121.92) (xy 177.8 50.8) (xy 76.2 50.8)
      )
    )
  )
  (zone (net 38) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 121.92) (xy 177.8 121.92) (xy 177.8 50.8) (xy 76.2 50.8)
      )
    )
  )
)
