(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 43)
    (tracks 45)
    (zones 0)
    (modules 5)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(J2-Pad2)")
  (net 6 "Net-(J2-Pad3)")
  (net 7 "Net-(J2-Pad4)")
  (net 8 "Net-(J3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J3-Pad2)")
    (add_net VCC)
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 157.115 97.18 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:2_tiny_pads (layer F.Cu) (tedit 5E63B89E)
    (at 143.06 99.47 90)
    (fp_text reference J1 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd circle (at -1.27 2.54 90) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd circle (at 1.27 2.54 90) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
  )
  (module Connector:4_tiny_pads (layer F.Cu) (tedit 5E63B90D)
    (at 151.41 100.56)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Female (at 0 -0.5) (layer F.Fab))
    (pad 1 smd circle (at -3.81 2.54) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 smd circle (at -1.27 2.54) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 3 smd circle (at 1.27 2.54) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 4 smd circle (at 3.81 2.54) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad4)"))
  )
  (module Connector:2_tiny_pads (layer F.Cu) (tedit 5E63B89E)
    (at 159.84 100.17 270)
    (fp_text reference J3 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0 -0.5 90) (layer F.Fab))
    (pad 2 smd circle (at 1.27 2.54 270) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (pad 1 smd circle (at -1.27 2.54 270) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Package_SO:SOIJ-8_5.3x5.3mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 151.424999 99.224999 180)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -3.68) (layer F.SilkS) hide)
    (fp_text value ATtiny85-20SU (at 0 3.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (pad 2 smd rect (at -3.65 -0.635 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at -3.65 0.635 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at -3.65 1.905 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 3.65 1.905 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 6 smd rect (at 3.65 0.635 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 7 smd rect (at 3.65 -0.635 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 8 smd rect (at 3.65 -1.905 180) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIJ-8_5.3x5.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text ATtiny85 (at 151.45 99.25) (layer F.SilkS))
  (gr_text int (at 145.575 96.8) (layer F.SilkS))
  (gr_text 5/rst (at 157.275 103.75) (layer F.SilkS))
  (gr_text 4 (at 153.7 103.775) (layer F.SilkS))
  (gr_text 1 (at 149.125 103.775) (layer F.SilkS))
  (gr_text 0 (at 146.525 103.8) (layer F.SilkS))
  (gr_text 2 (at 144.325 98.225) (layer F.SilkS))
  (gr_text + (at 144.325 100.775) (layer F.SilkS))
  (gr_text 3 (at 158.6 101.5) (layer F.SilkS))
  (gr_text ⏚ (at 158.625 98.85) (layer F.SilkS))
  (gr_text ⏚ (at 157.3 98.95) (layer B.SilkS))
  (gr_text "… or do, I’m a\npcb, not a cop" (at 151.6 99.9) (layer B.SilkS))
  (gr_text "do not ingest" (at 151.6 98.1) (layer B.SilkS))
  (gr_text 5 (at 155.2 103.2) (layer B.SilkS))
  (gr_text 4 (at 152.7 103.2) (layer B.SilkS))
  (gr_text 1 (at 150.1 103.1) (layer B.SilkS))
  (gr_text 0 (at 147.5 103.2) (layer B.SilkS))
  (gr_text 3 (at 157.275 101.425) (layer B.SilkS))
  (gr_text 2 (at 145.6 98.2) (layer B.SilkS))
  (gr_text + (at 145.59 100.66) (layer B.SilkS))
  (gr_line (start 159.1 95.9) (end 159.1 104.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.875 95.875) (end 159.1 95.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.875 104.3) (end 143.875 95.875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.1 104.3) (end 143.875 104.3) (layer Edge.Cuts) (width 0.1))
)
