(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 100)
    (no_connects 0)
    (area 76.150001 56.3 213.85 100.700001)
    (thickness 1.6)
    (drawings 21)
    (tracks 622)
    (zones 0)
    (modules 29)
    (nets 98)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (trace_clearance 0.22)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory PDF/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 HT)
  (net 3 CLK)
  (net 4 DATA)
  (net 5 ~LE)
  (net 6 ~BL)
  (net 7 +12V)
  (net 8 "Net-(NE1-Pad1)")
  (net 9 HRP)
  (net 10 "Net-(NE2-Pad1)")
  (net 11 LRP)
  (net 12 "Net-(NE3-Pad1)")
  (net 13 HLP)
  (net 14 "Net-(NE4-Pad1)")
  (net 15 LLP)
  (net 16 "Net-(R1-Pad2)")
  (net 17 "Net-(R2-Pad2)")
  (net 18 "Net-(R3-Pad2)")
  (net 19 "Net-(R4-Pad2)")
  (net 20 "Net-(R5-Pad2)")
  (net 21 "Net-(R6-Pad2)")
  (net 22 HH7)
  (net 23 HH6)
  (net 24 HH5)
  (net 25 HH4)
  (net 26 HH3)
  (net 27 HH2)
  (net 28 HH1)
  (net 29 HH0)
  (net 30 HH9)
  (net 31 HH8)
  (net 32 "Net-(U1-Pad12)")
  (net 33 LH7)
  (net 34 LH6)
  (net 35 LH5)
  (net 36 LH4)
  (net 37 LH3)
  (net 38 LH2)
  (net 39 LH1)
  (net 40 LH0)
  (net 41 LH9)
  (net 42 LH8)
  (net 43 "Net-(U2-Pad12)")
  (net 44 HM7)
  (net 45 HM6)
  (net 46 HM5)
  (net 47 HM4)
  (net 48 HM3)
  (net 49 HM2)
  (net 50 HM1)
  (net 51 HM0)
  (net 52 HM9)
  (net 53 HM8)
  (net 54 "Net-(U3-Pad12)")
  (net 55 LM7)
  (net 56 LM6)
  (net 57 LM5)
  (net 58 LM4)
  (net 59 LM3)
  (net 60 LM2)
  (net 61 LM1)
  (net 62 LM0)
  (net 63 LM9)
  (net 64 LM8)
  (net 65 "Net-(U4-Pad12)")
  (net 66 HS7)
  (net 67 HS6)
  (net 68 HS5)
  (net 69 HS4)
  (net 70 HS3)
  (net 71 HS2)
  (net 72 HS1)
  (net 73 HS0)
  (net 74 HS9)
  (net 75 HS8)
  (net 76 "Net-(U5-Pad12)")
  (net 77 LS7)
  (net 78 LS6)
  (net 79 LS5)
  (net 80 LS4)
  (net 81 LS3)
  (net 82 LS2)
  (net 83 LS1)
  (net 84 LS0)
  (net 85 LS9)
  (net 86 LS8)
  (net 87 "Net-(U6-Pad12)")
  (net 88 "Net-(U7-Pad23)")
  (net 89 "Net-(U7-Pad24)")
  (net 90 "Net-(U7-Pad25)")
  (net 91 "Net-(U7-Pad26)")
  (net 92 "Net-(U7-Pad32)")
  (net 93 "Net-(U7-Pad34)")
  (net 94 "Net-(U8-Pad24)")
  (net 95 "Net-(U8-Pad25)")
  (net 96 "Net-(U8-Pad26)")
  (net 97 "Net-(U8-Pad34)")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.22)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +12V)
    (add_net CLK)
    (add_net DATA)
    (add_net GND)
    (add_net HH0)
    (add_net HH1)
    (add_net HH2)
    (add_net HH3)
    (add_net HH4)
    (add_net HH5)
    (add_net HH6)
    (add_net HH7)
    (add_net HH8)
    (add_net HH9)
    (add_net HLP)
    (add_net HM0)
    (add_net HM1)
    (add_net HM2)
    (add_net HM3)
    (add_net HM4)
    (add_net HM5)
    (add_net HM6)
    (add_net HM7)
    (add_net HM8)
    (add_net HM9)
    (add_net HRP)
    (add_net HS0)
    (add_net HS1)
    (add_net HS2)
    (add_net HS3)
    (add_net HS4)
    (add_net HS5)
    (add_net HS6)
    (add_net HS7)
    (add_net HS8)
    (add_net HS9)
    (add_net HT)
    (add_net LH0)
    (add_net LH1)
    (add_net LH2)
    (add_net LH3)
    (add_net LH4)
    (add_net LH5)
    (add_net LH6)
    (add_net LH7)
    (add_net LH8)
    (add_net LH9)
    (add_net LLP)
    (add_net LM0)
    (add_net LM1)
    (add_net LM2)
    (add_net LM3)
    (add_net LM4)
    (add_net LM5)
    (add_net LM6)
    (add_net LM7)
    (add_net LM8)
    (add_net LM9)
    (add_net LRP)
    (add_net LS0)
    (add_net LS1)
    (add_net LS2)
    (add_net LS3)
    (add_net LS4)
    (add_net LS5)
    (add_net LS6)
    (add_net LS7)
    (add_net LS8)
    (add_net LS9)
    (add_net "Net-(NE1-Pad1)")
    (add_net "Net-(NE2-Pad1)")
    (add_net "Net-(NE3-Pad1)")
    (add_net "Net-(NE4-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U6-Pad12)")
    (add_net "Net-(U7-Pad23)")
    (add_net "Net-(U7-Pad24)")
    (add_net "Net-(U7-Pad25)")
    (add_net "Net-(U7-Pad26)")
    (add_net "Net-(U7-Pad32)")
    (add_net "Net-(U7-Pad34)")
    (add_net "Net-(U8-Pad24)")
    (add_net "Net-(U8-Pad25)")
    (add_net "Net-(U8-Pad26)")
    (add_net "Net-(U8-Pad34)")
    (add_net ~BL)
    (add_net ~LE)
  )
  (module Housings_QFP:PQFP-44_10x10mm_Pitch0.8mm (layer B.Cu) (tedit 5B422098)
    (at 127 80 90)
    (descr "44-Lead Plastic Quad Flatpack - 10x10x2.5mm Body (http://www.onsemi.com/pub/Collateral/122BK.PDF)")
    (tags "PQFP 0.8")
    (attr smd)
    (fp_text reference U7 (at 1.2 -0.2 180) (layer B.SilkS))
    (fp_text value HV5522PG (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -6.75 4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 39 LH1))
    (pad 2 smd rect (at -6.75 3.2 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 38 LH2))
    (pad 3 smd rect (at -6.75 2.4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 37 LH3))
    (pad 4 smd rect (at -6.75 1.6 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 36 LH4))
    (pad 5 smd rect (at -6.75 0.8 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 35 LH5))
    (pad 6 smd rect (at -6.75 0 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 34 LH6))
    (pad 7 smd rect (at -6.75 -0.8 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 33 LH7))
    (pad 8 smd rect (at -6.75 -1.6 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 42 LH8))
    (pad 9 smd rect (at -6.75 -2.4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 41 LH9))
    (pad 10 smd rect (at -6.75 -3.2 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 40 LH0))
    (pad 11 smd rect (at -6.75 -4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 28 HH1))
    (pad 12 smd rect (at -4 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 27 HH2))
    (pad 13 smd rect (at -3.2 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 26 HH3))
    (pad 14 smd rect (at -2.4 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 25 HH4))
    (pad 15 smd rect (at -1.6 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 24 HH5))
    (pad 16 smd rect (at -0.8 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 23 HH6))
    (pad 17 smd rect (at 0 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 22 HH7))
    (pad 18 smd rect (at 0.8 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 31 HH8))
    (pad 19 smd rect (at 1.6 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 30 HH9))
    (pad 20 smd rect (at 2.4 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 29 HH0))
    (pad 21 smd rect (at 3.2 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 15 LLP))
    (pad 22 smd rect (at 4 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 13 HLP))
    (pad 23 smd rect (at 6.75 -4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 88 "Net-(U7-Pad23)"))
    (pad 24 smd rect (at 6.75 -3.2 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 89 "Net-(U7-Pad24)"))
    (pad 25 smd rect (at 6.75 -2.4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 90 "Net-(U7-Pad25)"))
    (pad 26 smd rect (at 6.75 -1.6 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 91 "Net-(U7-Pad26)"))
    (pad 27 smd rect (at 6.75 -0.8 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 7 +12V))
    (pad 28 smd rect (at 6.75 0 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 3 CLK))
    (pad 29 smd rect (at 6.75 0.8 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 6.75 1.6 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 7 +12V))
    (pad 31 smd rect (at 6.75 2.4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 5 ~LE))
    (pad 32 smd rect (at 6.75 3.2 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 92 "Net-(U7-Pad32)"))
    (pad 33 smd rect (at 6.75 4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 6 ~BL))
    (pad 34 smd rect (at 4 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 93 "Net-(U7-Pad34)"))
    (pad 35 smd rect (at 3.2 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 50 HM1))
    (pad 36 smd rect (at 2.4 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 49 HM2))
    (pad 37 smd rect (at 1.6 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 48 HM3))
    (pad 38 smd rect (at 0.8 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 47 HM4))
    (pad 39 smd rect (at 0 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 46 HM5))
    (pad 40 smd rect (at -0.8 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 45 HM6))
    (pad 41 smd rect (at -1.6 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 44 HM7))
    (pad 42 smd rect (at -2.4 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 53 HM8))
    (pad 43 smd rect (at -3.2 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 52 HM9))
    (pad 44 smd rect (at -4 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 51 HM0))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/PQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:PQFP-44_10x10mm_Pitch0.8mm (layer B.Cu) (tedit 59A9B33B)
    (at 173.05 80 90)
    (descr "44-Lead Plastic Quad Flatpack - 10x10x2.5mm Body (http://www.onsemi.com/pub/Collateral/122BK.PDF)")
    (tags "PQFP 0.8")
    (attr smd)
    (fp_text reference U8 (at 1.7 1.85 180) (layer B.SilkS))
    (fp_text value HV5522PG (at 0 -4.1 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -6.75 4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 72 HS1))
    (pad 2 smd rect (at -6.75 3.2 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 71 HS2))
    (pad 3 smd rect (at -6.75 2.4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 70 HS3))
    (pad 4 smd rect (at -6.75 1.6 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 69 HS4))
    (pad 5 smd rect (at -6.75 0.8 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 68 HS5))
    (pad 6 smd rect (at -6.75 0 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 67 HS6))
    (pad 7 smd rect (at -6.75 -0.8 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 66 HS7))
    (pad 8 smd rect (at -6.75 -1.6 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 75 HS8))
    (pad 9 smd rect (at -6.75 -2.4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 74 HS9))
    (pad 10 smd rect (at -6.75 -3.2 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 73 HS0))
    (pad 11 smd rect (at -6.75 -4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 61 LM1))
    (pad 12 smd rect (at -4 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 60 LM2))
    (pad 13 smd rect (at -3.2 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 59 LM3))
    (pad 14 smd rect (at -2.4 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 58 LM4))
    (pad 15 smd rect (at -1.6 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 57 LM5))
    (pad 16 smd rect (at -0.8 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 56 LM6))
    (pad 17 smd rect (at 0 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 55 LM7))
    (pad 18 smd rect (at 0.8 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 64 LM8))
    (pad 19 smd rect (at 1.6 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 63 LM9))
    (pad 20 smd rect (at 2.4 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 62 LM0))
    (pad 21 smd rect (at 3.2 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 11 LRP))
    (pad 22 smd rect (at 4 -6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 9 HRP))
    (pad 23 smd rect (at 6.75 -4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 92 "Net-(U7-Pad32)"))
    (pad 24 smd rect (at 6.75 -3.2 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 94 "Net-(U8-Pad24)"))
    (pad 25 smd rect (at 6.75 -2.4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 95 "Net-(U8-Pad25)"))
    (pad 26 smd rect (at 6.75 -1.6 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 96 "Net-(U8-Pad26)"))
    (pad 27 smd rect (at 6.75 -0.8 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 7 +12V))
    (pad 28 smd rect (at 6.75 0 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 3 CLK))
    (pad 29 smd rect (at 6.75 0.8 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 6.75 1.6 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 7 +12V))
    (pad 31 smd rect (at 6.75 2.4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 5 ~LE))
    (pad 32 smd rect (at 6.75 3.2 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 4 DATA))
    (pad 33 smd rect (at 6.75 4 90) (size 1.5 0.52) (layers B.Cu B.Mask)
      (net 6 ~BL))
    (pad 34 smd rect (at 4 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 97 "Net-(U8-Pad34)"))
    (pad 35 smd rect (at 3.2 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 83 LS1))
    (pad 36 smd rect (at 2.4 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 82 LS2))
    (pad 37 smd rect (at 1.6 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 81 LS3))
    (pad 38 smd rect (at 0.8 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 80 LS4))
    (pad 39 smd rect (at 0 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 79 LS5))
    (pad 40 smd rect (at -0.8 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 78 LS6))
    (pad 41 smd rect (at -1.6 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 77 LS7))
    (pad 42 smd rect (at -2.4 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 86 LS8))
    (pad 43 smd rect (at -3.2 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 85 LS9))
    (pad 44 smd rect (at -4 6.75 90) (size 0.52 1.5) (layers B.Cu B.Mask)
      (net 84 LS0))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/PQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 102 77.54)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 3 -4.54) (layer B.SilkS))
    (fp_text value Conn_01x02_Male (at 0 -4.87) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 HT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 198 85)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at -2.2 1.3) (layer B.SilkS))
    (fp_text value Conn_01x05_Male (at 0 -12.49) (layer B.Fab))
    (fp_text user %R (at 0 -5.08 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 CLK))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 DATA))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 ~LE))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 ~BL))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 102 82.46 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at -3 -4.54 180) (layer B.SilkS))
    (fp_text value Conn_01x02_Male (at 0 -4.87 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +12V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 116.9 73.8)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.7) (layer B.SilkS))
    (fp_text value 27K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 HT))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 16 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 120.15 88.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.05 -1.7) (layer B.SilkS))
    (fp_text value 27K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 HT))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 17 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 149.5 74.1)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.7) (layer B.SilkS))
    (fp_text value 27K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0.0036) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 HT))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 18 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 159.85 74.1)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.7) (layer B.SilkS))
    (fp_text value 27K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 HT))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 19 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 179.95 88.7 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 27K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 HT))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 20 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 188.15 88.7 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 27K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 HT))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 21 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 148.1 88.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.7) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 8 "Net-(NE1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 HT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 166.4 88.7)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -1.8) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 10 "Net-(NE2-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 HT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 135.15 88.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -0.15 -1.6) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 12 "Net-(NE3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 HT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 140.3 88.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -1.8) (layer B.SilkS))
    (fp_text value 220K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 14 "Net-(NE4-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 HT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module topfootprints:LD8007 (layer F.Cu) (tedit 5B420050)
    (at 114 80)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value LD8007 (at 0 -6.6) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 4.1) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 22 HH7))
    (pad 2 smd trapezoid (at -2.1 3.5 330) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 23 HH6))
    (pad 3 smd trapezoid (at -3.6 2 300) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 24 HH5))
    (pad 4 smd trapezoid (at -4.1 0 270) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 25 HH4))
    (pad 5 smd trapezoid (at -3.6 -2 240) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 26 HH3))
    (pad 6 smd trapezoid (at -2.1 -3.5 210) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 27 HH2))
    (pad 7 smd trapezoid (at 0 -4.1 180) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 28 HH1))
    (pad 8 smd trapezoid (at 2 -3.6 150) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 16 "Net-(R1-Pad2)"))
    (pad 9 smd trapezoid (at 3.5 -2.1 120) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 29 HH0))
    (pad 10 smd trapezoid (at 4.1 0 90) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 30 HH9))
    (pad 11 smd trapezoid (at 3.5 2.1 60) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 31 HH8))
    (pad 12 smd trapezoid (at 2 3.6 30) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 32 "Net-(U1-Pad12)"))
  )
  (module topfootprints:LD8007 (layer F.Cu) (tedit 5B420050)
    (at 126 80)
    (fp_text reference U2 (at 0 0) (layer F.SilkS))
    (fp_text value LD8007 (at 0 -6.6) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 4.1) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 33 LH7))
    (pad 2 smd trapezoid (at -2.1 3.5 330) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 34 LH6))
    (pad 3 smd trapezoid (at -3.6 2 300) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 35 LH5))
    (pad 4 smd trapezoid (at -4.1 0 270) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 36 LH4))
    (pad 5 smd trapezoid (at -3.6 -2 240) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 37 LH3))
    (pad 6 smd trapezoid (at -2.1 -3.5 210) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 38 LH2))
    (pad 7 smd trapezoid (at 0 -4.1 180) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 39 LH1))
    (pad 8 smd trapezoid (at 2 -3.6 150) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 17 "Net-(R2-Pad2)"))
    (pad 9 smd trapezoid (at 3.5 -2.1 120) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 40 LH0))
    (pad 10 smd trapezoid (at 4.1 0 90) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 41 LH9))
    (pad 11 smd trapezoid (at 3.5 2.1 60) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 42 LH8))
    (pad 12 smd trapezoid (at 2 3.6 30) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 43 "Net-(U2-Pad12)"))
  )
  (module topfootprints:LD8007 (layer F.Cu) (tedit 5B420050)
    (at 144 80)
    (fp_text reference U3 (at 0 0) (layer F.SilkS))
    (fp_text value LD8007 (at 0 -6.6) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 4.1) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 44 HM7))
    (pad 2 smd trapezoid (at -2.1 3.5 330) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 45 HM6))
    (pad 3 smd trapezoid (at -3.6 2 300) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 46 HM5))
    (pad 4 smd trapezoid (at -4.1 0 270) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 47 HM4))
    (pad 5 smd trapezoid (at -3.6 -2 240) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 48 HM3))
    (pad 6 smd trapezoid (at -2.1 -3.5 210) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 49 HM2))
    (pad 7 smd trapezoid (at 0 -4.1 180) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 50 HM1))
    (pad 8 smd trapezoid (at 2 -3.6 150) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 18 "Net-(R3-Pad2)"))
    (pad 9 smd trapezoid (at 3.5 -2.1 120) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 51 HM0))
    (pad 10 smd trapezoid (at 4.1 0 90) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 52 HM9))
    (pad 11 smd trapezoid (at 3.5 2.1 60) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 53 HM8))
    (pad 12 smd trapezoid (at 2 3.6 30) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 54 "Net-(U3-Pad12)"))
  )
  (module topfootprints:LD8007 (layer F.Cu) (tedit 5B420050)
    (at 156 80)
    (fp_text reference U4 (at 0 0) (layer F.SilkS))
    (fp_text value LD8007 (at 0 -6.6) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 4.1) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 55 LM7))
    (pad 2 smd trapezoid (at -2.1 3.5 330) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 56 LM6))
    (pad 3 smd trapezoid (at -3.6 2 300) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 57 LM5))
    (pad 4 smd trapezoid (at -4.1 0 270) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 58 LM4))
    (pad 5 smd trapezoid (at -3.6 -2 240) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 59 LM3))
    (pad 6 smd trapezoid (at -2.1 -3.5 210) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 60 LM2))
    (pad 7 smd trapezoid (at 0 -4.1 180) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 61 LM1))
    (pad 8 smd trapezoid (at 2 -3.6 150) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 19 "Net-(R4-Pad2)"))
    (pad 9 smd trapezoid (at 3.5 -2.1 120) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 62 LM0))
    (pad 10 smd trapezoid (at 4.1 0 90) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 63 LM9))
    (pad 11 smd trapezoid (at 3.5 2.1 60) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 64 LM8))
    (pad 12 smd trapezoid (at 2 3.6 30) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 65 "Net-(U4-Pad12)"))
  )
  (module topfootprints:LD8007 (layer F.Cu) (tedit 5B420050)
    (at 174 80)
    (fp_text reference U5 (at 0 0) (layer F.SilkS))
    (fp_text value LD8007 (at 0 -6.6) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 4.1) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 66 HS7))
    (pad 2 smd trapezoid (at -2.1 3.5 330) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 67 HS6))
    (pad 3 smd trapezoid (at -3.6 2 300) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 68 HS5))
    (pad 4 smd trapezoid (at -4.1 0 270) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 69 HS4))
    (pad 5 smd trapezoid (at -3.6 -2 240) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 70 HS3))
    (pad 6 smd trapezoid (at -2.1 -3.5 210) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 71 HS2))
    (pad 7 smd trapezoid (at 0 -4.1 180) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 72 HS1))
    (pad 8 smd trapezoid (at 2 -3.6 150) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 20 "Net-(R5-Pad2)"))
    (pad 9 smd trapezoid (at 3.5 -2.1 120) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 73 HS0))
    (pad 10 smd trapezoid (at 4.1 0 90) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 74 HS9))
    (pad 11 smd trapezoid (at 3.5 2.1 60) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 75 HS8))
    (pad 12 smd trapezoid (at 2 3.6 30) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 76 "Net-(U5-Pad12)"))
  )
  (module topfootprints:LD8007 (layer F.Cu) (tedit 5B420050)
    (at 186 80)
    (fp_text reference U6 (at 0 0) (layer F.SilkS))
    (fp_text value LD8007 (at 0 -6.6) (layer F.Fab) hide)
    (pad 1 smd trapezoid (at 0 4.1) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 77 LS7))
    (pad 2 smd trapezoid (at -2.1 3.5 330) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 78 LS6))
    (pad 3 smd trapezoid (at -3.6 2 300) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 79 LS5))
    (pad 4 smd trapezoid (at -4.1 0 270) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 80 LS4))
    (pad 5 smd trapezoid (at -3.6 -2 240) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 81 LS3))
    (pad 6 smd trapezoid (at -2.1 -3.5 210) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 82 LS2))
    (pad 7 smd trapezoid (at 0 -4.1 180) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 83 LS1))
    (pad 8 smd trapezoid (at 2 -3.6 150) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 21 "Net-(R6-Pad2)"))
    (pad 9 smd trapezoid (at 3.5 -2.1 120) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 84 LS0))
    (pad 10 smd trapezoid (at 4.1 0 90) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 85 LS9))
    (pad 11 smd trapezoid (at 3.5 2.1 60) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 86 LS8))
    (pad 12 smd trapezoid (at 2 3.6 30) (size 1.5 2) (rect_delta 0 0.4 ) (layers F.Cu F.Mask)
      (net 87 "Net-(U6-Pad12)"))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B431D51)
    (at 102 71)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 1 -4.6) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B4208CB)
    (at 102 89)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B4208D6)
    (at 198 89)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B4208D2)
    (at 198 71)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-R_EIA-2012-12_Reflow (layer F.Cu) (tedit 58CC8C08)
    (at 164.975 74.4)
    (descr "Tantalum capacitor, Case R, EIA 2012-12, 2.0x1.3x1.2mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference NE1 (at -0.975 0) (layer F.SilkS))
    (fp_text value Lamp_Neon (at 0 2.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.175 0) (size 1.55 1.8) (layers F.Cu F.Mask)
      (net 8 "Net-(NE1-Pad1)"))
    (pad 2 smd rect (at 1.175 0) (size 1.55 1.8) (layers F.Cu F.Mask)
      (net 9 HRP))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-R_EIA-2012-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-R_EIA-2012-12_Reflow (layer F.Cu) (tedit 58CC8C08)
    (at 164.975 77.6)
    (descr "Tantalum capacitor, Case R, EIA 2012-12, 2.0x1.3x1.2mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference NE2 (at -0.975 0) (layer F.SilkS))
    (fp_text value Lamp_Neon (at 0 2.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.175 0) (size 1.55 1.8) (layers F.Cu F.Mask)
      (net 10 "Net-(NE2-Pad1)"))
    (pad 2 smd rect (at 1.175 0) (size 1.55 1.8) (layers F.Cu F.Mask)
      (net 11 LRP))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-R_EIA-2012-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-R_EIA-2012-12_Reflow (layer F.Cu) (tedit 58CC8C08)
    (at 135 74.4)
    (descr "Tantalum capacitor, Case R, EIA 2012-12, 2.0x1.3x1.2mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference NE3 (at -0.975 0) (layer F.SilkS))
    (fp_text value Lamp_Neon (at 0 2.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.175 0) (size 1.55 1.8) (layers F.Cu F.Mask)
      (net 12 "Net-(NE3-Pad1)"))
    (pad 2 smd rect (at 1.175 0) (size 1.55 1.8) (layers F.Cu F.Mask)
      (net 13 HLP))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-R_EIA-2012-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-R_EIA-2012-12_Reflow (layer F.Cu) (tedit 58CC8C08)
    (at 135 77.6)
    (descr "Tantalum capacitor, Case R, EIA 2012-12, 2.0x1.3x1.2mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference NE4 (at -0.975 0) (layer F.SilkS))
    (fp_text value Lamp_Neon (at 0 2.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.175 0) (size 1.55 1.8) (layers F.Cu F.Mask)
      (net 14 "Net-(NE4-Pad1)"))
    (pad 2 smd rect (at 1.175 0) (size 1.55 1.8) (layers F.Cu F.Mask)
      (net 15 LLP))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-R_EIA-2012-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text mini-nixie (at 108.5 89) (layer F.Mask))
  (gr_text pierremuth.wordpress.com (at 187 89) (layer F.Mask))
  (dimension 7 (width 0.3) (layer Cmts.User)
    (gr_text "7,000 mm" (at 92.65 72.5 90) (layer Cmts.User))
    (feature1 (pts (xy 100 69) (xy 91.3 69)))
    (feature2 (pts (xy 100 76) (xy 91.3 76)))
    (crossbar (pts (xy 94 76) (xy 94 69)))
    (arrow1a (pts (xy 94 69) (xy 94.586421 70.126504)))
    (arrow1b (pts (xy 94 69) (xy 93.413579 70.126504)))
    (arrow2a (pts (xy 94 76) (xy 94.586421 74.873496)))
    (arrow2b (pts (xy 94 76) (xy 93.413579 74.873496)))
  )
  (dimension 35 (width 0.3) (layer Cmts.User)
    (gr_text "35.000 mm" (at 182.5 62.65) (layer Cmts.User))
    (feature1 (pts (xy 200 69) (xy 200 61.3)))
    (feature2 (pts (xy 165 69) (xy 165 61.3)))
    (crossbar (pts (xy 165 64) (xy 200 64)))
    (arrow1a (pts (xy 200 64) (xy 198.873496 64.586421)))
    (arrow1b (pts (xy 200 64) (xy 198.873496 63.413579)))
    (arrow2a (pts (xy 165 64) (xy 166.126504 64.586421)))
    (arrow2b (pts (xy 165 64) (xy 166.126504 63.413579)))
  )
  (dimension 35 (width 0.3) (layer Cmts.User)
    (gr_text "35.000 mm" (at 117.5 63.65) (layer Cmts.User))
    (feature1 (pts (xy 100 69) (xy 100 62.3)))
    (feature2 (pts (xy 135 69) (xy 135 62.3)))
    (crossbar (pts (xy 135 65) (xy 100 65)))
    (arrow1a (pts (xy 100 65) (xy 101.126504 64.413579)))
    (arrow1b (pts (xy 100 65) (xy 101.126504 65.586421)))
    (arrow2a (pts (xy 135 65) (xy 133.873496 64.413579)))
    (arrow2b (pts (xy 135 65) (xy 133.873496 65.586421)))
  )
  (dimension 2 (width 0.3) (layer Cmts.User)
    (gr_text "2.000 mm" (at 207.35 90 90) (layer Cmts.User))
    (feature1 (pts (xy 200 89) (xy 208.7 89)))
    (feature2 (pts (xy 200 91) (xy 208.7 91)))
    (crossbar (pts (xy 206 91) (xy 206 89)))
    (arrow1a (pts (xy 206 89) (xy 206.586421 90.126504)))
    (arrow1b (pts (xy 206 89) (xy 205.413579 90.126504)))
    (arrow2a (pts (xy 206 91) (xy 206.586421 89.873496)))
    (arrow2b (pts (xy 206 91) (xy 205.413579 89.873496)))
  )
  (dimension 11 (width 0.3) (layer Cmts.User)
    (gr_text "11.000 mm" (at 207.35 74.5 270) (layer Cmts.User))
    (feature1 (pts (xy 200 80) (xy 208.7 80)))
    (feature2 (pts (xy 200 69) (xy 208.7 69)))
    (crossbar (pts (xy 206 69) (xy 206 80)))
    (arrow1a (pts (xy 206 80) (xy 205.413579 78.873496)))
    (arrow1b (pts (xy 206 80) (xy 206.586421 78.873496)))
    (arrow2a (pts (xy 206 69) (xy 205.413579 70.126504)))
    (arrow2b (pts (xy 206 69) (xy 206.586421 70.126504)))
  )
  (dimension 12 (width 0.3) (layer Cmts.User)
    (gr_text "12.000 mm" (at 180 95.35) (layer Cmts.User))
    (feature1 (pts (xy 186 91) (xy 186 96.7)))
    (feature2 (pts (xy 174 91) (xy 174 96.7)))
    (crossbar (pts (xy 174 94) (xy 186 94)))
    (arrow1a (pts (xy 186 94) (xy 184.873496 94.586421)))
    (arrow1b (pts (xy 186 94) (xy 184.873496 93.413579)))
    (arrow2a (pts (xy 174 94) (xy 175.126504 94.586421)))
    (arrow2b (pts (xy 174 94) (xy 175.126504 93.413579)))
  )
  (dimension 18 (width 0.3) (layer Cmts.User)
    (gr_text "18.000 mm" (at 165 99.35) (layer Cmts.User))
    (feature1 (pts (xy 174 91) (xy 174 100.7)))
    (feature2 (pts (xy 156 91) (xy 156 100.7)))
    (crossbar (pts (xy 156 98) (xy 174 98)))
    (arrow1a (pts (xy 174 98) (xy 172.873496 98.586421)))
    (arrow1b (pts (xy 174 98) (xy 172.873496 97.413579)))
    (arrow2a (pts (xy 156 98) (xy 157.126504 98.586421)))
    (arrow2b (pts (xy 156 98) (xy 157.126504 97.413579)))
  )
  (dimension 12 (width 0.3) (layer Cmts.User)
    (gr_text "12.000 mm" (at 150 95.35) (layer Cmts.User))
    (feature1 (pts (xy 156 91) (xy 156 96.7)))
    (feature2 (pts (xy 144 91) (xy 144 96.7)))
    (crossbar (pts (xy 144 94) (xy 156 94)))
    (arrow1a (pts (xy 156 94) (xy 154.873496 94.586421)))
    (arrow1b (pts (xy 156 94) (xy 154.873496 93.413579)))
    (arrow2a (pts (xy 144 94) (xy 145.126504 94.586421)))
    (arrow2b (pts (xy 144 94) (xy 145.126504 93.413579)))
  )
  (dimension 18 (width 0.3) (layer Cmts.User)
    (gr_text "18.000 mm" (at 135 99.35) (layer Cmts.User))
    (feature1 (pts (xy 144 91) (xy 144 100.7)))
    (feature2 (pts (xy 126 91) (xy 126 100.7)))
    (crossbar (pts (xy 126 98) (xy 144 98)))
    (arrow1a (pts (xy 144 98) (xy 142.873496 98.586421)))
    (arrow1b (pts (xy 144 98) (xy 142.873496 97.413579)))
    (arrow2a (pts (xy 126 98) (xy 127.126504 98.586421)))
    (arrow2b (pts (xy 126 98) (xy 127.126504 97.413579)))
  )
  (dimension 12 (width 0.3) (layer Cmts.User)
    (gr_text "12.000 mm" (at 120 95.35) (layer Cmts.User))
    (feature1 (pts (xy 126 91) (xy 126 96.7)))
    (feature2 (pts (xy 114 91) (xy 114 96.7)))
    (crossbar (pts (xy 114 94) (xy 126 94)))
    (arrow1a (pts (xy 126 94) (xy 124.873496 94.586421)))
    (arrow1b (pts (xy 126 94) (xy 124.873496 93.413579)))
    (arrow2a (pts (xy 114 94) (xy 115.126504 94.586421)))
    (arrow2b (pts (xy 114 94) (xy 115.126504 93.413579)))
  )
  (dimension 14 (width 0.3) (layer Cmts.User)
    (gr_text "14.000 mm" (at 193 99.349999) (layer Cmts.User))
    (feature1 (pts (xy 186 91) (xy 186 100.699999)))
    (feature2 (pts (xy 200 91) (xy 200 100.699999)))
    (crossbar (pts (xy 200 97.999999) (xy 186 97.999999)))
    (arrow1a (pts (xy 186 97.999999) (xy 187.126504 97.413578)))
    (arrow1b (pts (xy 186 97.999999) (xy 187.126504 98.58642)))
    (arrow2a (pts (xy 200 97.999999) (xy 198.873496 97.413578)))
    (arrow2b (pts (xy 200 97.999999) (xy 198.873496 98.58642)))
  )
  (dimension 14 (width 0.3) (layer Cmts.User)
    (gr_text "14.000 mm" (at 107 99.35) (layer Cmts.User))
    (feature1 (pts (xy 114 91) (xy 114 100.7)))
    (feature2 (pts (xy 100 91) (xy 100 100.7)))
    (crossbar (pts (xy 100 98) (xy 114 98)))
    (arrow1a (pts (xy 114 98) (xy 112.873496 98.586421)))
    (arrow1b (pts (xy 114 98) (xy 112.873496 97.413579)))
    (arrow2a (pts (xy 100 98) (xy 101.126504 98.586421)))
    (arrow2b (pts (xy 100 98) (xy 101.126504 97.413579)))
  )
  (dimension 22 (width 0.3) (layer Cmts.User)
    (gr_text "22.000 mm" (at 82.65 80 90) (layer Cmts.User))
    (feature1 (pts (xy 100 69) (xy 81.3 69)))
    (feature2 (pts (xy 100 91) (xy 81.3 91)))
    (crossbar (pts (xy 84 91) (xy 84 69)))
    (arrow1a (pts (xy 84 69) (xy 84.586421 70.126504)))
    (arrow1b (pts (xy 84 69) (xy 83.413579 70.126504)))
    (arrow2a (pts (xy 84 91) (xy 84.586421 89.873496)))
    (arrow2b (pts (xy 84 91) (xy 83.413579 89.873496)))
  )
  (dimension 100 (width 0.3) (layer Cmts.User)
    (gr_text "100.000 mm" (at 150 57.65) (layer Cmts.User))
    (feature1 (pts (xy 200 69) (xy 200 56.3)))
    (feature2 (pts (xy 100 69) (xy 100 56.3)))
    (crossbar (pts (xy 100 59) (xy 200 59)))
    (arrow1a (pts (xy 200 59) (xy 198.873496 59.586421)))
    (arrow1b (pts (xy 200 59) (xy 198.873496 58.413579)))
    (arrow2a (pts (xy 100 59) (xy 101.126504 59.586421)))
    (arrow2b (pts (xy 100 59) (xy 101.126504 58.413579)))
  )
  (gr_line (start 100 91) (end 100 69) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200 91) (end 100 91) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200 69) (end 200 91) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 69) (end 200 69) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.5 69.5) (xy 100.5 69.5) (xy 100.5 90.5) (xy 199.5 90.5)
      )
    )
  )
)
