(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 14)
    (no_connects 0)
    (area 134.556499 85.280499 156.527501 106.489501)
    (thickness 1.6)
    (drawings 37)
    (tracks 34)
    (zones 0)
    (modules 10)
    (nets 7)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.99898 1.99898)
    (pad_drill 1)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x011fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(IC1-Pad2)")
  (net 4 "Net-(IC1-Pad3)")
  (net 5 "Net-(IC1-Pad5)")
  (net 6 "Net-(IC1-Pad6)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.3)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net VCC)
  )
  (module BRICE:DS18B20 placed (layer Top) (tedit 590DDBD6)
    (at 153.924 100.584 90)
    (fp_text reference Sonde (at -4.064 0 180) (layer F.SilkS))
    (fp_text value DS18B20 (at 0 4.826 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad2)"))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer Top) (tedit 590DE427)
    (at 149.606 90.17 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference "C1 10uF" (at 1.25 -3.56 90) (layer F.SilkS))
    (fp_text value 10uF (at 7.112 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module BRICE:ATTINY85-P (layer Top) (tedit 590DE499)
    (at 145.796 97.282)
    (descr "PDIP-8 Standard 300mil 8pin Dual In Line Package")
    (tags "Power Integrations P Package")
    (fp_text reference ATTINY85-P (at 0.635 0) (layer F.SilkS))
    (fp_text value ATTINY85-P (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1.27 3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 3.81 -3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 -3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole circle (at -1.27 -3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -3.81 -3.81) (size 1.905 1.905) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
  )
  (module BRICE:Power_Pad_2x_1mmDrill (layer Top) (tedit 590DD653)
    (at 153.924 89.154 90)
    (fp_text reference 5vcc (at 0 1.524 90) (layer F.SilkS))
    (fp_text value Power (at 0 4.826 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer Top) (tedit 590DD65A)
    (at 153.924 93.98 90)
    (fp_text reference pb0 (at 1.016 -1.524 90) (layer F.SilkS))
    (fp_text value pb0 (at 0.762 4.826 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.016 0 90) (size 1.99898 1.99898) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad5)"))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer Top) (tedit 590DD469)
    (at 153.924 96.266 270)
    (fp_text reference pb1 (at -1.016 1.524 270) (layer F.SilkS))
    (fp_text value pb1 (at 0 -4.318 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.762 0 270) (size 1.99898 1.99898) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad6)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer Top) (tedit 590DE47E)
    (at 139.954 104.14)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "R1 4,7 KOhms" (at 5.08 0) (layer F.SilkS))
    (fp_text value 4700 (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module BRICE:FS1000A (layer Top) (tedit 590DE41C)
    (at 137.16 96.012 90)
    (fp_text reference "RF 433" (at -4.318 0 180) (layer F.SilkS))
    (fp_text value FS1000A (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad3)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer Top) (tedit 590DCC15)
    (at 140.462 88.9 90)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0.508 -6.604 90) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0 90) (layer F.Fab) hide)
  )
  (module Symbols:WEEE-Logo_4.2x6mm_SilkScreen (layer Bottom) (tedit 0)
    (at 139.954 88.392 270)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value WEEE-Logo_4.2x6mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (gr_line (start 137.16 85.344) (end 153.924 85.344) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 153.924 106.426) (end 137.16 106.426) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 156.464 103.886) (end 156.464 87.884) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 134.62 87.884) (end 134.62 103.886) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_text "DESIGN IN FRENCH" (at 139.954 96.266 90) (layer B.SilkS))
  (gr_text https://easydomoticz.com (at 144.526 102.87 180) (layer B.SilkS))
  (gr_arc (start 153.924 87.884) (end 153.924 85.344) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 153.924 103.886) (end 156.464 103.886) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 137.16 87.884) (end 134.62 87.884) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 137.16 103.886) (end 137.16 106.426) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_text 2017 (at 148.844 97.536 90) (layer B.SilkS))
  (gr_text + (at 152.4 90.424) (layer F.SilkS))
  (gr_text - (at 152.4 87.884 90) (layer F.SilkS))
  (gr_text DATA (at 152.4 100.584 90) (layer F.SilkS))
  (gr_text GND (at 152.4 103.124 90) (layer F.SilkS))
  (gr_text VCC (at 152.4 98.044 90) (layer F.SilkS))
  (gr_text "ZIONIII SONDE B V2.1" (at 151.892 93.218 90) (layer B.SilkS))
  (gr_text DATA (at 138.684 98.552 90) (layer F.SilkS))
  (gr_text VCC (at 138.684 96.012 90) (layer F.SilkS))
  (gr_text GND (at 138.684 93.472 90) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.62 85.344) (xy 156.464 85.344) (xy 156.464 106.426) (xy 134.62 106.426)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.62 85.344) (xy 156.464 85.344) (xy 156.464 106.426) (xy 134.62 106.426)
      )
    )
  )
)
