(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 0)
    (no_connects 1)
    (area 118.669459 81.840159 154.379461 108.025161)
    (thickness 1.6)
    (drawings 9)
    (tracks 65)
    (zones 0)
    (modules 13)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.6096)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.6256)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.9144)
    (via_drill 0.508)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.9144)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 GND)
  (net 6 VCC)
  (net 7 "Net-(Q1-Pad2)")
  (net 8 "Net-(Q2-Pad2)")
  (net 9 "Net-(P1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.9144)
    (via_drill 0.508)
    (uvia_dia 0.9144)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Angled_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 150.49446 95.25016)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference P1 (at 0.25 -2.413) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 4.315 7.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 122.68146 96.26616 180)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference SW2 (at 0 4.826 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 4.315 4.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5570F7EA)
    (at 145.03346 88.39216 90)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D1 (at -2.36 0 180) (layer F.SilkS))
    (fp_text value Led_Small (at 1.524 -3.937 90) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5570F7EA)
    (at 138.17546 88.39216 90)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D2 (at -2.36 0 180) (layer F.SilkS))
    (fp_text value Led_Small (at 1.524 -3.937 90) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58610935)
    (at 132.46046 99.69516)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.54 3.22 180) (layer F.SilkS))
    (fp_text value Q_PNP_EBC (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58610935)
    (at 132.46046 94.74216)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value Q_PNP_EBC (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 126.23746 103.50516 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 12.59 0.507 180) (layer F.SilkS))
    (fp_text value 1k (at 5.08 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 146.68446 103.50516 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at -2.36 0 180) (layer F.SilkS))
    (fp_text value 470 (at 5.08 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 140.33446 103.50516 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at -2.36 0 180) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(P1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 143.50946 103.50516 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at -2.36 0 180) (layer F.SilkS))
    (fp_text value 470 (at 5.08 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 129.66646 93.34516 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at -2.43 -0.078 360) (layer F.SilkS))
    (fp_text value 1k (at 5.08 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(Q2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 122.68146 102.36216 180)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference SW1 (at -0.063 -2.27 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 4.315 4.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 58B67C2A)
    (at 123.74446 86.91516)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0.588 -3.91) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "SIG\nVCC\nGND" (at 151.38346 104.72216) (layer F.SilkS))
  (gr_text 2 (at 134.11146 87.19616) (layer F.SilkS))
  (gr_text 1 (at 149.35146 87.19616) (layer F.SilkS))
  (dimension 5 (width 0.3) (layer Dwgs.User)
    (gr_text "5.000 mm" (at 114.39446 84.41516 90) (layer Dwgs.User))
    (feature1 (pts (xy 123.74446 81.91516) (xy 113.04446 81.91516)))
    (feature2 (pts (xy 123.74446 86.91516) (xy 113.04446 86.91516)))
    (crossbar (pts (xy 115.74446 86.91516) (xy 115.74446 81.91516)))
    (arrow1a (pts (xy 115.74446 81.91516) (xy 116.330881 83.041664)))
    (arrow1b (pts (xy 115.74446 81.91516) (xy 115.158039 83.041664)))
    (arrow2a (pts (xy 115.74446 86.91516) (xy 116.330881 85.788656)))
    (arrow2b (pts (xy 115.74446 86.91516) (xy 115.158039 85.788656)))
  )
  (dimension 5 (width 0.3) (layer Dwgs.User)
    (gr_text "5.000 mm" (at 121.24446 79.56516) (layer Dwgs.User))
    (feature1 (pts (xy 118.74446 86.91516) (xy 118.74446 78.21516)))
    (feature2 (pts (xy 123.74446 86.91516) (xy 123.74446 78.21516)))
    (crossbar (pts (xy 123.74446 80.91516) (xy 118.74446 80.91516)))
    (arrow1a (pts (xy 118.74446 80.91516) (xy 119.870964 80.328739)))
    (arrow1b (pts (xy 118.74446 80.91516) (xy 119.870964 81.501581)))
    (arrow2a (pts (xy 123.74446 80.91516) (xy 122.617956 80.328739)))
    (arrow2b (pts (xy 123.74446 80.91516) (xy 122.617956 81.501581)))
  )
  (gr_line (start 118.74446 81.91516) (end 118.74446 107.95016) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.30446 81.91516) (end 118.74446 81.91516) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.30446 107.95016) (end 154.30446 81.91516) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.74446 107.95016) (end 154.30446 107.95016) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.745 107.95) (xy 154.305 107.95) (xy 154.305 81.915) (xy 118.745 81.915)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.745 107.95) (xy 154.305 107.95) (xy 154.305 81.915) (xy 118.745 81.915)
      )
    )
  )
)
