(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 42)
    (no_connects 0)
    (area 139.194999 93.394999 168.405001 110.305001)
    (thickness 1.6002)
    (drawings 10)
    (tracks 175)
    (zones 0)
    (modules 11)
    (nets 32)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.01)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.35 1.35)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 DTR)
  (net 3 RESET)
  (net 4 VCC)
  (net 5 +3V3)
  (net 6 INT1)
  (net 7 "Net-(IC1-Pad2)")
  (net 8 "Net-(IC1-Pad7)")
  (net 9 "Net-(IC1-Pad8)")
  (net 10 "Net-(IC1-Pad9)")
  (net 11 "Net-(IC1-Pad10)")
  (net 12 "Net-(IC1-Pad11)")
  (net 13 NRCE)
  (net 14 NRSS)
  (net 15 SEL)
  (net 16 CMD)
  (net 17 DAT)
  (net 18 CLK)
  (net 19 "Net-(IC1-Pad19)")
  (net 20 "Net-(IC1-Pad22)")
  (net 21 "Net-(IC1-Pad23)")
  (net 22 "Net-(IC1-Pad24)")
  (net 23 "Net-(IC1-Pad25)")
  (net 24 "Net-(IC1-Pad26)")
  (net 25 SDA)
  (net 26 SCL)
  (net 27 RX)
  (net 28 TX)
  (net 29 INT0)
  (net 30 "Net-(J1-Pad8)")
  (net 31 "Net-(IC1-Pad20)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net CLK)
    (add_net CMD)
    (add_net DAT)
    (add_net DTR)
    (add_net GND)
    (add_net INT0)
    (add_net INT1)
    (add_net NRCE)
    (add_net NRSS)
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(J1-Pad8)")
    (add_net RESET)
    (add_net RX)
    (add_net SCL)
    (add_net SDA)
    (add_net SEL)
    (add_net TX)
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.00mm (layer Top) (tedit 58BAAB81)
    (at 140.6 109 180)
    (descr "Through hole straight pin header, 1x06, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.00mm single row")
    (fp_text reference J4 (at 0 -2.12 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X05 (at 0 12.12 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 DTR))
    (pad 2 thru_hole oval (at 0 2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 TX))
    (pad 3 thru_hole oval (at 0 4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 RX))
    (pad 4 thru_hole oval (at 0 6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 5 thru_hole oval (at 0 8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer Bottom) (tedit 58BAB068)
    (at 148.5 108.9)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers Bottom B.Mask)
      (net 2 DTR))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers Bottom B.Mask)
      (net 3 RESET))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer Top) (tedit 58BAADBD)
    (at 147.9 96.3 225)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -0.070711 -0.070711 225) (layer F.SilkS))
    (fp_text value 10uF (at 0 2 225) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 225) (layer F.Fab))
    (pad 1 smd rect (at -2 0 225) (size 2 1.6) (layers Top F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 2 0 225) (size 2 1.6) (layers Top F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer Top) (tedit 58BAADB4)
    (at 150.4 98 225)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 0 225) (layer F.SilkS))
    (fp_text value 10uF (at 0 2 225) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 225) (layer F.Fab))
    (pad 1 smd rect (at -2 0 225) (size 2 1.6) (layers Top F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 2 0 225) (size 2 1.6) (layers Top F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer Top) (tedit 58BAB030)
    (at 154.6 103.5 135)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 0 135) (layer F.SilkS))
    (fp_text value ATMEGA328P-A (at 0 6.05 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 6 INT1))
    (pad 2 smd rect (at -4.25 -2 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 7 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 -0.4 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 5 +3V3))
    (pad 5 smd rect (at -4.25 0.4 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -4.25 1.2 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 5 +3V3))
    (pad 7 smd rect (at -4.25 2 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 8 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 9 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 10 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -2 4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 11 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 12 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 13 NRCE))
    (pad 13 smd rect (at 0.4 4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 14 NRSS))
    (pad 14 smd rect (at 1.2 4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 15 SEL))
    (pad 15 smd rect (at 2 4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 16 CMD))
    (pad 16 smd rect (at 2.8 4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 17 DAT))
    (pad 17 smd rect (at 4.25 2.8 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 18 CLK))
    (pad 18 smd rect (at 4.25 2 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 5 +3V3))
    (pad 19 smd rect (at 4.25 1.2 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 19 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 31 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 4.25 -1.2 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 20 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 21 "Net-(IC1-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8 135) (size 1.6 0.55) (layers Top F.Mask)
      (net 22 "Net-(IC1-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 23 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 24 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 25 SDA))
    (pad 28 smd rect (at 0.4 -4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 26 SCL))
    (pad 29 smd rect (at -0.4 -4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 3 RESET))
    (pad 30 smd rect (at -1.2 -4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 27 RX))
    (pad 31 smd rect (at -2 -4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 28 TX))
    (pad 32 smd rect (at -2.8 -4.25 225) (size 1.6 0.55) (layers Top F.Mask)
      (net 29 INT0))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.00mm (layer Top) (tedit 58BAAE1A)
    (at 167 107 270)
    (descr "Through hole straight pin header, 2x04, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.00mm double row")
    (fp_text reference J1 (at 1 -2.12 270) (layer F.SilkS) hide)
    (fp_text value CONN_02X04 (at 1 8.12 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 3 thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 NRCE))
    (pad 4 thru_hole oval (at 2 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 NRSS))
    (pad 5 thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 DAT))
    (pad 6 thru_hole oval (at 2 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 CMD))
    (pad 7 thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 CLK))
    (pad 8 thru_hole oval (at 2 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.00mm (layer Top) (tedit 58BAAE15)
    (at 164.1 96 270)
    (descr "Through hole straight pin header, 2x03, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.00mm double row")
    (fp_text reference J2 (at 1 -2.12 270) (layer F.SilkS) hide)
    (fp_text value CONN_02X03 (at 1 6.12 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 SEL))
    (pad 4 thru_hole oval (at 2 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 DAT))
    (pad 5 thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 CMD))
    (pad 6 thru_hole oval (at 2 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 CLK))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.00mm (layer Top) (tedit 58BAADF1)
    (at 143.6 99)
    (descr "Through hole straight pin header, 1x06, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.00mm single row")
    (fp_text reference J3 (at 0 -2.12) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 12.12) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 SDA))
    (pad 4 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 SCL))
    (pad 5 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 INT0))
    (pad 6 thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 INT1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.00mm (layer Top) (tedit 58BAADE2)
    (at 143.6 95)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (fp_text reference J5 (at -0.2 -2.3) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.12) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer Bottom) (tedit 58BAB05C)
    (at 154.6 102.2 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 1.85 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers Bottom B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers Bottom B.Mask)
      (net 3 RESET))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing_Handsoldering (layer Bottom) (tedit 58BAA307)
    (at 149.4 98.2 270)
    (descr "SOT89-3, Housing, Handsoldering,")
    (tags "SOT89-3 Housing Handsoldering ")
    (attr smd)
    (fp_text reference REG1 (at 4.9 2.3 270) (layer B.SilkS) hide)
    (fp_text value HT7333 (at 0.5 -3.15 270) (layer B.Fab))
    (pad 1 smd rect (at -1.98 1.5) (size 1 2.5) (layers Bottom B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.98 0) (size 1 2.5) (layers Bottom B.Mask)
      (net 4 VCC))
    (pad 3 smd rect (at -1.98 -1.5) (size 1 2.5) (layers Bottom B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.98 0) (size 2 4) (layers Bottom B.Mask)
      (net 4 VCC))
    (pad 2 smd trapezoid (at -0.37 0 180) (size 1.5 0.75) (rect_delta 0 -0.5 ) (layers Bottom B.Mask)
      (net 4 VCC))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing_Handsoldering.wrl
      (at (xyz 0.02 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "WirelessController\nv0.1" (at 162.1 101.9) (layer B.SilkS))
  (gr_text FTDI (at 140.6 97.2) (layer F.SilkS))
  (gr_text ADXL345 (at 145.4 105 90) (layer F.SilkS))
  (gr_text PS2 (at 162.1 94.2) (layer F.SilkS))
  (gr_text nRF24L01+ (at 164.6 105.2) (layer F.SilkS))
  (gr_line (start 139.2 110.3) (end 168.4 110.3) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 139.2 93.4) (end 139.2 110.3) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 168.4 93.4) (end 139.2 93.4) (angle 90) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 168.4 110.3) (end 168.4 93.4) (angle 90) (layer Edge.Cuts) (width 0.01))
  (dimension 17 (width 0.3) (layer Eco1.User)
    (gr_text "17.000 mm" (at 127.65 102 270) (layer Eco1.User))
    (feature1 (pts (xy 181.6 110.5) (xy 126.3 110.5)))
    (feature2 (pts (xy 181.6 93.5) (xy 126.3 93.5)))
    (crossbar (pts (xy 129 93.5) (xy 129 110.5)))
    (arrow1a (pts (xy 129 110.5) (xy 128.413579 109.373496)))
    (arrow1b (pts (xy 129 110.5) (xy 129.586421 109.373496)))
    (arrow2a (pts (xy 129 93.5) (xy 128.413579 94.626504)))
    (arrow2b (pts (xy 129 93.5) (xy 129.586421 94.626504)))
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.4 110.3) (xy 139.2 110.3) (xy 139.2 93.4) (xy 168.4 93.4)
      )
    )
  )
  (zone (net 4) (net_name VCC) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.4 110.3) (xy 139.2 110.3) (xy 139.2 93.4) (xy 168.4 93.4)
      )
    )
  )
)
