(kicad_pcb (version 20190331) (host pcbnew "(5.1.0-373-ge808c7f95)")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 0)
    (modules 2)
    (nets 1)
  )
  (page "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user)
    (33 "F.Adhes" user)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user)
    (37 "F.SilkS" user)
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user)
    (41 "Cmts.User" user)
    (42 "Eco1.User" user)
    (43 "Eco2.User" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user)
    (47 "F.CrtYd" user)
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class "Default" "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "oshpark:OSH_small" (layer "F.Cu") (tedit 5D3E8195)
    (at 144.4752 72.39)
    (descr "Imported from OSHPARK.svg")
    (tags "svg2mod")
    (attr smd)
    (fp_text reference "OSH_small" (at 0 -11.457835) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 11.457835) (layer "F.SilkS") hide)
  )
  (module "oshpark:OSH_small" (layer "F.Cu") (tedit 5CD3FE0B)
    (at 144.4752 72.39)
    (descr "Imported from OSHPARK.svg")
    (tags "svg2mod")
    (attr smd)
    (fp_text reference "OSH_small" (at 0 -11.457835) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 11.457835) (layer "F.SilkS") hide)
  )
  (gr_text "drew@oshpark.com" (at 144.3736 78.8416) (layer "B.Cu"))
  (gr_text "Drew Fustini" (at 144.526 73.2028) (layer "B.Cu"))
  (gr_text "OSH Park\n2 layer Flexible PCB" (at 144.272 65.8368) (layer "B.Cu"))
  (gr_text "Drew Fustini" (at 144.526 73.2028) (layer "B.Mask"))
  (gr_text "OSH Park\n2 layer Flexible PCB" (at 144.272 65.8368) (layer "B.Mask"))
  (gr_line (start 126.746 66.294) (end 126.6952 77.9272) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 157.988 82.4992) (end 131.2672 82.4992) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 162.56 66.294) (end 162.56 77.9272) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 131.318 61.722) (end 157.988 61.722) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 157.988 77.9272) (end 157.988 82.4992) (angle -90) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 131.2672 77.9272) (end 126.6952 77.9272) (angle -90) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 131.318 66.294) (end 131.318 61.722) (angle -90) (layer "Edge.Cuts") (width 0.05))
  (gr_text "drew@oshpark.com" (at 144.3736 78.8416) (layer "B.Mask"))
  (gr_arc (start 157.988 66.294) (end 162.56 66.294) (angle -90) (layer "Edge.Cuts") (width 0.05))
)
