(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 7)
    (no_connects 0)
    (area 47.498 88.392 87.122 127)
    (thickness 1.6)
    (drawings 35)
    (tracks 43)
    (zones 0)
    (modules 2)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad0)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(J1-Pad5)")
  (net 7 "Net-(J1-Pad6)")
  (net 8 "Net-(J1-Pad7)")
  (net 9 "Net-(J1-Pad8)")
  (net 10 "Net-(J1-Pad17A)")
  (net 11 "Net-(J1-Pad3V1)")
  (net 12 "Net-(J1-PadG2)")
  (net 13 "Net-(J1-PadPGM)")
  (net 14 "Net-(J1-PadDAC)")
  (net 15 "Net-(J1-Pad16)")
  (net 16 "Net-(J1-Pad18)")
  (net 17 "Net-(J1-Pad17)")
  (net 18 "Net-(J1-PadG3)")
  (net 19 "Net-(J1-Pad22)")
  (net 20 "Net-(J1-PadVIN)")
  (net 21 "Net-(J1-Pad21)")
  (net 22 "Net-(J1-Pad20)")
  (net 23 "Net-(J1-Pad19)")
  (net 24 "Net-(J1-Pad23)")
  (net 25 "Net-(J1-Pad14)")
  (net 26 "Net-(J1-Pad15)")
  (net 27 "Net-(J2-Pad7)")
  (net 28 /OLED_GND)
  (net 29 /MOSI)
  (net 30 /CLK)
  (net 31 /DC)
  (net 32 /CS)
  (net 33 /OLED_VIN)
  (net 34 /RST)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CLK)
    (add_net /CS)
    (add_net /DC)
    (add_net /MOSI)
    (add_net /OLED_GND)
    (add_net /OLED_VIN)
    (add_net /RST)
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad17A)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad3V1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadG2)")
    (add_net "Net-(J1-PadG3)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVIN)")
    (add_net "Net-(J2-Pad7)")
  )
  (module TEENSY-LC (layer B.Cu) (tedit 573A94F4)
    (at 60.706 101.092 270)
    (fp_text reference "" (at -2.032 9.906 270) (layer B.SilkS))
    (fp_text value TEENSY-LC (at -2.54 -20.32 450) (layer B.Fab))
    (pad G1 thru_hole circle (at -10.16 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 28 /OLED_GND))
    (pad 0 thru_hole circle (at -10.16 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 "Net-(J1-Pad0)"))
    (pad 1 thru_hole circle (at -10.16 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 -12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 -15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 29 /MOSI))
    (pad 10 thru_hole circle (at -10.16 -17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 30 /CLK))
    (pad 11 thru_hole circle (at -10.16 -20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 31 /DC))
    (pad 12 thru_hole circle (at -10.16 -22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 32 /CS))
    (pad 17A thru_hole circle (at -7.62 -22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 10 "Net-(J1-Pad17A)"))
    (pad 3V1 thru_hole circle (at -5.08 -22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 "Net-(J1-Pad3V1)"))
    (pad G2 thru_hole circle (at -2.54 -22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(J1-PadG2)"))
    (pad PGM thru_hole circle (at 0 -22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 -22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 14 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 -22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 34 /RST))
    (pad 16 thru_hole circle (at 5.08 -15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 "Net-(J1-Pad16)"))
    (pad 3V2 thru_hole circle (at 5.08 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 33 /OLED_VIN))
    (pad 18 thru_hole circle (at 5.08 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 16 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 5.08 -12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 17 "Net-(J1-Pad17)"))
    (pad G3 thru_hole circle (at 5.08 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 18 "Net-(J1-PadG3)"))
    (pad 22 thru_hole circle (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 19 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 20 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 22 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 23 "Net-(J1-Pad19)"))
    (pad 23 thru_hole circle (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 24 "Net-(J1-Pad23)"))
    (pad 14 thru_hole circle (at 5.08 -20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 25 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 -17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 26 "Net-(J1-Pad15)"))
  )
  (module Wickerlib:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 573AA435)
    (at 58.166 111.506 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value OLED (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /CS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /RST))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /DC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CLK))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /MOSI))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /OLED_VIN))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /OLED_GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 85.598 115.062) (end 87.122 115.062) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 46.482 112.776) (end 46.482 113.538) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "DREW FUSTINI" (at 58.42 98.806 180) (layer B.Mask))
  (gr_text "DREW FUSTINI" (at 86.106 98.806 90) (layer F.Mask))
  (gr_text oshpark.com (at 47.752 99.06 90) (layer F.SilkS))
  (gr_text "OSH\nPark" (at 51.054 111.506) (layer F.Mask))
  (gr_text drew@oshpark.com (at 66.548 86.868) (layer F.Cu))
  (gr_text drew@oshpark.com (at 66.548 86.868) (layer B.Mask))
  (gr_text drew@oshpark.com (at 66.548 86.868) (layer F.Mask))
  (gr_circle (center 84.836 86.868) (end 84.328 86.106) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 49.276 86.868) (end 48.768 86.106) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.63 114.554) (end 87.122 115.062) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.63 113.792) (end 87.63 114.554) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.63 86.868) (end 87.63 113.792) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.106 85.344) (end 87.63 86.868) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.09 85.344) (end 86.106 85.344) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.82 85.344) (end 85.09 85.344) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.26 85.344) (end 83.82 85.344) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 46.482 87.122) (end 48.26 85.344) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 46.482 113.03) (end 46.482 87.122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.006 115.062) (end 85.598 115.062) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 46.482 113.538) (end 48.006 115.062) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text drew@oshpark.com (at 60.706 95.25) (layer F.Mask))
  (gr_text drew@oshpark.com (at 60.706 96.774 180) (layer B.SilkS))
  (zone (net 33) (net_name /OLED_VIN) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47.498 88.392) (xy 86.868 88.392) (xy 86.868 114.808) (xy 47.498 114.808)
      )
    )
  )
  (zone (net 28) (net_name /OLED_GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.006 88.9) (xy 85.852 88.9) (xy 85.852 114.3) (xy 48.006 114.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.962 88.392) (xy 55.626 88.392) (xy 55.88 85.852) (xy 77.216 85.852) (xy 77.216 87.884)
      )
    )
  )
)
