(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 54)
    (no_connects 0)
    (area 73.214048 68.875 131.477143 103.31)
    (thickness 1.6)
    (drawings 26)
    (tracks 289)
    (zones 0)
    (modules 26)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C4-Pad2)")
  (net 5 "Net-(C10-Pad1)")
  (net 6 "Net-(C2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C4-Pad2)")
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585C37F9)
    (at 98.425 76.2 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value C1 (at 0.635 28.575 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585C3801)
    (at 98.425 85.725 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 4.445 0 360) (layer F.SilkS))
    (fp_text value C2 (at 3.81 24.13 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585C381D)
    (at 95.885 95.25 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 1.905 2.54 360) (layer F.SilkS))
    (fp_text value C3 (at 0 20.955 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585C3806)
    (at 103.505 85.725 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value C4 (at 1.905 23.495 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585C37EE)
    (at 103.505 76.2 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value C5 (at 1.905 24.13 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585C37FC)
    (at 98.425 77.47 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 1.905 29.21 90) (layer F.SilkS))
    (fp_text value C1 (at 1.905 29.21 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585C3808)
    (at 98.425 84.455 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 1.905 -28.575 270) (layer F.SilkS))
    (fp_text value C2 (at 5.715 24.13 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585C37AC)
    (at 95.885 93.98 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at 2.54 21.59 270) (layer F.SilkS))
    (fp_text value C3 (at 1.27 20.955 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585C380B)
    (at 103.505 86.995 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C9 (at 2.54 24.13 90) (layer F.SilkS))
    (fp_text value C4 (at 3.81 24.13 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585C37F3)
    (at 103.505 77.47 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C10 (at 1.905 23.495 90) (layer F.SilkS))
    (fp_text value C5 (at 3.175 23.495 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585C378D)
    (at 85.725 78.74)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L1 (at -1.27 -0.635) (layer F.SilkS))
    (fp_text value L1 (at -11.43 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 -5.08) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585C37A8)
    (at 89.535 80.645 270)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L2 (at 11.43 -0.635 360) (layer F.SilkS))
    (fp_text value L2 (at 6.35 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 -5.08 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad1)"))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585C37BE)
    (at 108.585 92.71 180)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L3 (at -1.27 -4.445 180) (layer F.SilkS))
    (fp_text value L3 (at -19.05 1.905 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 -5.08 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585C37D2)
    (at 107.315 80.645 270)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L4 (at 11.43 -4.445 360) (layer F.SilkS))
    (fp_text value L4 (at 3.175 -19.685 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 -5.08 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(C10-Pad1)"))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585C37D9)
    (at 106.045 78.74)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L5 (at 11.43 -0.635) (layer F.SilkS))
    (fp_text value L5 (at 20.955 1.905) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 -5.08) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Libraries:SMA_Vertical_Or_Edge (layer F.Cu) (tedit 585C3798)
    (at 83.185 85.725 270)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference P1 (at 1.27 8.89 270) (layer F.SilkS))
    (fp_text value BNC (at 0 8.89 270) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 smd rect (at 2.54 1.778 270) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at 0 1.524 270) (size 1.524 5.588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.54 1.778 270) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.54 1.778 270) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.54 1.778 270) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Connect.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:SMA_Vertical_Or_Edge (layer F.Cu) (tedit 585C37C5)
    (at 118.745 85.725 90)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference P2 (at -0.635 8.89 90) (layer F.SilkS))
    (fp_text value BNC (at 0.635 8.89 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 smd rect (at 2.54 1.778 90) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at 0 1.524 90) (size 1.524 5.588) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -2.54 1.778 90) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.54 1.778 90) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.54 1.778 90) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Connect.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585C378A)
    (at 90.805 76.2 90)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L6 (at 0 -16.51 90) (layer F.SilkS))
    (fp_text value L1 (at -0.635 -16.51 90) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 90) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.6 0 90) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585C3794)
    (at 92.075 85.725)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L7 (at -17.145 -5.08) (layer F.SilkS))
    (fp_text value L2 (at -17.78 -3.175) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.6 0) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C2-Pad1)"))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585C37BC)
    (at 103.505 95.25 270)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L8 (at 0 -24.13 270) (layer F.SilkS))
    (fp_text value L3 (at -1.905 -24.13 270) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 270) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.6 0 270) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585C380F)
    (at 109.855 85.725)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L9 (at 17.78 -1.905) (layer F.SilkS))
    (fp_text value L4 (at 17.145 2.54) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1.6 0) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C10-Pad1)"))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585C37E2)
    (at 111.125 76.2 90)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L10 (at 0 16.51 90) (layer F.SilkS))
    (fp_text value L5 (at -0.635 15.875 90) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 90) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.6 0 90) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585C39D3)
    (at 80.01 74.93)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at -1.27 -5.08) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 3.81 -5.08) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585C39DD)
    (at 80.01 96.52)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 1.905 5.08) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 6.35 5.08) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585C39D8)
    (at 121.92 96.52)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0.635 5.715) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 5.08) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585C39D1)
    (at 121.92 74.93)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at -1.27 -5.08) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at -6.35 -5.08) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text O (at 86.995 90.805) (layer B.Mask))
  (gr_text O (at 90.17 92.71) (layer B.Mask))
  (gr_text o (at 88.265 95.25) (layer B.Mask))
  (gr_text <>< (at 91.44 95.885) (layer B.Mask))
  (gr_text ><> (at 86.995 97.79) (layer B.Mask))
  (gr_text "mark@halibut.com  SmittyHalibut" (at 83.82 71.755) (layer F.SilkS))
  (gr_text "BY-NC-SA 2016 Mark Smith" (at 83.82 99.695) (layer F.SilkS))
  (gr_text "HPF v1.0a" (at 83.82 97.79) (layer F.SilkS))
  (gr_arc (start 78.74 97.79) (end 78.74 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.19 97.79) (end 125.73 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.19 73.66) (end 123.19 71.12) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 78.74 73.66) (end 76.2 73.66) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 71.12) (end 78.74 71.12) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 81.915) (end 125.73 73.66) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 81.915) (end 125.73 81.915) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 89.535) (end 123.19 81.915) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 89.535) (end 123.19 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 97.79) (end 125.73 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.74 100.33) (end 123.19 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.2 89.535) (end 76.2 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.74 89.535) (end 76.2 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.74 81.915) (end 78.74 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.2 81.915) (end 78.74 81.915) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.2 73.66) (end 76.2 81.915) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 71.12) (xy 125.73 71.12) (xy 125.73 100.33) (xy 76.2 100.33)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 71.12) (xy 125.73 71.12) (xy 125.73 100.33) (xy 76.2 100.33)
      )
    )
  )
)
