(kicad_pcb (version 20170123) (host pcbnew "(2017-05-02 revision e4d2924ee)-makepkg")
  (general
    (links 42)
    (no_connects 6)
    (area 154.7525 50.699999 220.412143 96.620001)
    (thickness 1.6)
    (drawings 8)
    (tracks 215)
    (zones 0)
    (modules 15)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.762)
    (user_trace_width 1.524)
    (trace_clearance 0.2)
    (zone_clearance 0.3302)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.1016)
    (pad_to_paste_clearance_ratio -0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(AE1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D3-Pad1)")
  (net 5 "Net-(D4-Pad1)")
  (net 6 "Net-(D5-Pad1)")
  (net 7 "Net-(U1-Pad2)")
  (net 8 "Net-(U1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(AE1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad6)")
  )
  (module FritzLib:ANT1204 (layer F.Cu) (tedit 59912E10)
    (at 177.165 57.15)
    (fp_text reference AE1 (at 0 -4.31) (layer F.SilkS))
    (fp_text value ANT1204LL05R0915A (at 0 -5.31) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 4.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(AE1-Pad1)"))
    (pad 2 smd rect (at 12.2 0) (size 2 4.5) (layers F.Cu F.Paste F.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 167.91 59.055)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value CM1214A (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(AE1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 168.005 75.438)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value CM1214A (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 168.005 91.948)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D3 (at 0 -2.5) (layer F.SilkS))
    (fp_text value CM1214A (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 186.055 71.816 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D4 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value CM1214A (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 186.055 88.265 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D5 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value CM1214A (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FritzLib:J502 (layer F.Cu) (tedit 5990A428)
    (at 161.29 61.595 90)
    (fp_text reference J1 (at -1.27 4.445 90) (layer F.SilkS))
    (fp_text value SMA (at 0 -5.58 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0 90) (size 2.6162 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 8.763 0 90) (size 2.6162 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 4.318 0 90) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(AE1-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 2.6162 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 8.763 0 90) (size 2.6162 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module FritzLib:J502 (layer F.Cu) (tedit 5990A428)
    (at 161.29 77.978 90)
    (fp_text reference J2 (at -2.032 4.445 90) (layer F.SilkS))
    (fp_text value SMA (at 0 -5.58 90) (layer F.Fab))
    (pad 2 smd rect (at 8.763 0 90) (size 2.6162 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 0 90) (size 2.6162 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 4.318 0 90) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 8.763 0 90) (size 2.6162 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 0 90) (size 2.6162 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module FritzLib:J502 (layer F.Cu) (tedit 5990A428)
    (at 193.04 77.978 90)
    (fp_text reference J3 (at 0 -4.58 90) (layer F.SilkS))
    (fp_text value SMA (at 0 -5.58 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0 90) (size 2.6162 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 8.763 0 90) (size 2.6162 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 4.318 0 90) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 2.6162 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 8.763 0 90) (size 2.6162 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module FritzLib:J502 (layer F.Cu) (tedit 5990A428)
    (at 161.29 94.488 90)
    (fp_text reference J4 (at -0.762 4.445 90) (layer F.SilkS))
    (fp_text value SMA (at 0 -5.58 90) (layer F.Fab))
    (pad 2 smd rect (at 8.763 0 90) (size 2.6162 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 0 90) (size 2.6162 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 4.318 0 90) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 8.763 0 90) (size 2.6162 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 0 90) (size 2.6162 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module FritzLib:J502 (layer F.Cu) (tedit 5990A428)
    (at 193.04 94.488 90)
    (fp_text reference J5 (at 0 -4.58 90) (layer F.SilkS))
    (fp_text value SMA (at 0 -5.58 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0 90) (size 2.6162 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 8.763 0 90) (size 2.6162 5.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 4.318 0 90) (size 2.286 5.08) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 2.6162 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 8.763 0 90) (size 2.6162 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 58E0A804)
    (at 173.355 91.821 270)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R1 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value 53.6 (at 0 2.4 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 58E0A804)
    (at 177.165 89.535 180)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R2 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value 620R (at 0 2.4 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 58E0A804)
    (at 180.975 91.821 270)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R3 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value 53.6 (at 0 2.4 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FritzLib:0915LP (layer F.Cu) (tedit 59913000)
    (at 177.165 73.66)
    (fp_text reference U1 (at 0 -2) (layer F.Fab))
    (fp_text value 0915LP (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.65 -0.9) (size 0.35 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 -0.9) (size 0.35 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -0.65 -0.9) (size 0.35 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -1.275 0 90) (size 0.35 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 5 smd rect (at -0.65 0.9) (size 0.35 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0 0.9) (size 0.35 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at 0.65 0.9) (size 0.35 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 1.275 0 90) (size 0.35 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad1)"))
  )
  (gr_text "915 MHz Chip Antenna" (at 180.975 62.865) (layer F.SilkS))
  (gr_text "928 MHz LPF" (at 177.165 68.58) (layer F.SilkS))
  (gr_text "28 dB Attenuator" (at 177.165 84.455) (layer F.SilkS))
  (gr_text "60 mil trace width\n13 mil space" (at 198.755 73.66) (layer Cmts.User))
  (gr_line (start 196.215 50.8) (end 158.115 50.8) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 196.215 96.52) (end 196.215 50.8) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 158.115 96.52) (end 196.215 96.52) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 158.115 50.8) (end 158.115 96.52) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.99 51.435) (xy 158.75 51.435) (xy 158.75 65.405) (xy 173.99 65.405)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.58 66.675) (xy 158.75 66.675) (xy 158.75 80.645) (xy 195.58 80.645)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.58 81.915) (xy 158.75 81.915) (xy 158.75 95.885) (xy 195.58 95.885)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3302))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.513566 66.675) (xy 158.683566 66.675) (xy 158.683566 80.645) (xy 195.513566 80.645)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3302))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.58 81.915) (xy 158.75 81.915) (xy 158.75 95.885) (xy 195.58 95.885)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3302))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.99 51.435) (xy 158.75 51.435) (xy 158.75 65.405) (xy 173.99 65.405)
      )
    )
  )
  (zone (net 3) (net_name "Net-(D2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 174.625 72.898) (xy 176.403 73.406) (xy 176.403 73.914) (xy 174.625 74.422)
      )
    )
  )
  (zone (net 4) (net_name "Net-(D3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 174.117 89.408) (xy 175.26 88.265) (xy 175.768 88.265) (xy 175.768 90.932) (xy 175.26 90.932)
        (xy 174.625 90.932) (xy 172.085 90.932) (xy 171.577 90.932) (xy 171.577 89.408)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D4-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 180.213 74.422) (xy 177.950962 73.962703) (xy 177.950962 73.454703) (xy 180.213 72.898)
      )
    )
  )
  (zone (net 6) (net_name "Net-(D5-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 178.689 88.265) (xy 179.07 88.265) (xy 179.832 89.408) (xy 183.515 89.408) (xy 183.515 90.424)
        (xy 182.372 91.059) (xy 180.213 91.059) (xy 179.705 91.059) (xy 178.689 91.059)
      )
    )
  )
)
