(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 0)
    (area 23.594287 80.422593 253.97879 150.02)
    (thickness 1.6002)
    (drawings 25)
    (tracks 3720)
    (zones 0)
    (modules 73)
    (nets 77)
  )
  (page A)
  (title_block
    (title "Interactive Rainbow")
    (date 2017-03-29)
    (rev 1.0.1)
    (company "Sembazuru Circuits (for Barrel of Makers)")
    (comment 1 "1.0.0 Initial layout.")
    (comment 2 "1.0.1 Add KiCad logo.")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 0.889)
    (user_trace_width 1.016)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.7874)
    (via_drill 0.381)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 38.1 139.7)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.076200)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /Out1)
  (net 3 /In1)
  (net 4 /Out2)
  (net 5 /In2)
  (net 6 /Out3)
  (net 7 /In3)
  (net 8 /Out4)
  (net 9 /In4)
  (net 10 /Out5)
  (net 11 /In5)
  (net 12 /Out6)
  (net 13 /In6)
  (net 14 /Out7)
  (net 15 /In7)
  (net 16 /Out8)
  (net 17 /In8)
  (net 18 /~SS)
  (net 19 /MOSI)
  (net 20 /MISO)
  (net 21 /SCK)
  (net 22 "+5V(1)")
  (net 23 "+5V(2)")
  (net 24 /~IR_Osc+)
  (net 25 /~IR_Osc-)
  (net 26 /In1+)
  (net 27 /Out1+)
  (net 28 /Out1-)
  (net 29 /In1-)
  (net 30 /In2+)
  (net 31 /Out2+)
  (net 32 /Out2-)
  (net 33 /In2-)
  (net 34 /In3+)
  (net 35 /Out3+)
  (net 36 /Out3-)
  (net 37 /In3-)
  (net 38 /In4+)
  (net 39 /Out4+)
  (net 40 /Out4-)
  (net 41 /In4-)
  (net 42 /In5+)
  (net 43 /Out5+)
  (net 44 /Out5-)
  (net 45 /In5-)
  (net 46 /In6+)
  (net 47 /Out6+)
  (net 48 /Out6-)
  (net 49 /In6-)
  (net 50 /In7+)
  (net 51 /Out7+)
  (net 52 /Out7-)
  (net 53 /In7-)
  (net 54 /In8+)
  (net 55 /Out8+)
  (net 56 /Out8-)
  (net 57 /In8-)
  (net 58 /~SS+)
  (net 59 /~SS-)
  (net 60 /MISO+)
  (net 61 /MOSI+)
  (net 62 /MOSI-)
  (net 63 /MISO-)
  (net 64 /SCK+)
  (net 65 /SCK-)
  (net 66 /~SS'+)
  (net 67 /~SS'-)
  (net 68 /MISO'+)
  (net 69 /MOSI'+)
  (net 70 /MOSI'-)
  (net 71 /MISO'-)
  (net 72 /SCK'+)
  (net 73 /SCK'-)
  (net 74 /SS)
  (net 75 /MOSI')
  (net 76 /MISO')
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.7874)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /In1)
    (add_net /In2)
    (add_net /In3)
    (add_net /In4)
    (add_net /In5)
    (add_net /In6)
    (add_net /In7)
    (add_net /In8)
    (add_net /MISO)
    (add_net /MISO')
    (add_net /MOSI)
    (add_net /MOSI')
    (add_net /Out1)
    (add_net /Out2)
    (add_net /Out3)
    (add_net /Out4)
    (add_net /Out5)
    (add_net /Out6)
    (add_net /Out7)
    (add_net /Out8)
    (add_net /SCK)
    (add_net /SS)
    (add_net /~SS)
  )
  (net_class 3A_Power ""
    (clearance 0.1524)
    (trace_width 0.889)
    (via_dia 0.889)
    (via_drill 0.4572)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "+5V(1)")
    (add_net GND)
  )
  (net_class 5A_Power ""
    (clearance 0.1524)
    (trace_width 1.778)
    (via_dia 1.778)
    (via_drill 0.889)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "+5V(2)")
  )
  (net_class Differential ""
    (clearance 0.14986)
    (trace_width 0.1524)
    (via_dia 0.7874)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /In1+)
    (add_net /In1-)
    (add_net /In2+)
    (add_net /In2-)
    (add_net /In3+)
    (add_net /In3-)
    (add_net /In4+)
    (add_net /In4-)
    (add_net /In5+)
    (add_net /In5-)
    (add_net /In6+)
    (add_net /In6-)
    (add_net /In7+)
    (add_net /In7-)
    (add_net /In8+)
    (add_net /In8-)
    (add_net /MISO'+)
    (add_net /MISO'-)
    (add_net /MISO+)
    (add_net /MISO-)
    (add_net /MOSI'+)
    (add_net /MOSI'-)
    (add_net /MOSI+)
    (add_net /MOSI-)
    (add_net /Out1+)
    (add_net /Out1-)
    (add_net /Out2+)
    (add_net /Out2-)
    (add_net /Out3+)
    (add_net /Out3-)
    (add_net /Out4+)
    (add_net /Out4-)
    (add_net /Out5+)
    (add_net /Out5-)
    (add_net /Out6+)
    (add_net /Out6-)
    (add_net /Out7+)
    (add_net /Out7-)
    (add_net /Out8+)
    (add_net /Out8-)
    (add_net /SCK'+)
    (add_net /SCK'-)
    (add_net /SCK+)
    (add_net /SCK-)
    (add_net /~IR_Osc+)
    (add_net /~IR_Osc-)
    (add_net /~SS'+)
    (add_net /~SS'-)
    (add_net /~SS+)
    (add_net /~SS-)
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 116.84 102.235 180)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J3 (at -1.27 -4.445 180) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.445 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /~IR_Osc+))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /~IR_Osc-))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 /In3+))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 /Out3+))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 /Out3-))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 /In3-))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 208.915 102.235 180)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J8 (at -1.27 -4.445 180) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.45 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /~IR_Osc+))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /~IR_Osc-))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 /In8+))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 /Out8+))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 /Out8-))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 57 /In8-))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS762W45P254L1016H508Q8 (layer F.Cu) (tedit 587D1F93)
    (at 213.36 118.11)
    (descr "DIP for Socket, 300 mil lead span, 100 mil pitch; 8 pin, 400 mil L X 255.9 mil W X 200 mil H body")
    (fp_text reference XU10 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value IC_Socket08 (at 3.81 -3.81) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-8__300.wrl
      (at (xyz 0.15 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS762W45P254L1016H508Q8 (layer F.Cu) (tedit 587D1F93)
    (at 213.36 129.54)
    (descr "DIP for Socket, 300 mil lead span, 100 mil pitch; 8 pin, 400 mil L X 255.9 mil W X 200 mil H body")
    (fp_text reference XU9 (at 1.27 -1.27) (layer F.SilkS))
    (fp_text value IC_Socket08 (at 3.81 -3.81) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-8__300.wrl
      (at (xyz 0.15 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS762W45P254L1016H508Q8 (layer F.Cu) (tedit 587D1F93)
    (at 58.42 116.84)
    (descr "DIP for Socket, 300 mil lead span, 100 mil pitch; 8 pin, 400 mil L X 255.9 mil W X 200 mil H body")
    (fp_text reference XU8 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value IC_Socket08 (at 3.81 -3.81) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-8__300.wrl
      (at (xyz 0.15 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS762W45P254L1016H508Q8 (layer F.Cu) (tedit 587D1F93)
    (at 58.42 132.08)
    (descr "DIP for Socket, 300 mil lead span, 100 mil pitch; 8 pin, 400 mil L X 255.9 mil W X 200 mil H body")
    (fp_text reference XU7 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value IC_Socket08 (at 3.81 -3.81) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-8__300.wrl
      (at (xyz 0.15 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS794W45P254L1969H508Q16 (layer F.Cu) (tedit 58157D96)
    (at 186.69 117.475)
    (descr "DIP for Socket, 7.94 mm lead span, 2.54 mm pitch; 16 pin, 19.69 mm L X 6.60 mm W X 5.08 mm H body")
    (fp_text reference XU6 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value IC_Socket16 (at 8.89 -3.81) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-16__300.wrl
      (at (xyz 0.35 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS794W45P254L1969H508Q16 (layer F.Cu) (tedit 58157D96)
    (at 149.86 117.475)
    (descr "DIP for Socket, 7.94 mm lead span, 2.54 mm pitch; 16 pin, 19.69 mm L X 6.60 mm W X 5.08 mm H body")
    (fp_text reference XU5 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value IC_Socket16 (at 8.89 -3.81) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-16__300.wrl
      (at (xyz 0.35 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS794W45P254L1969H508Q16 (layer F.Cu) (tedit 58157D96)
    (at 113.03 117.475)
    (descr "DIP for Socket, 7.94 mm lead span, 2.54 mm pitch; 16 pin, 19.69 mm L X 6.60 mm W X 5.08 mm H body")
    (fp_text reference XU4 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value IC_Socket16 (at 8.89 -3.81) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-16__300.wrl
      (at (xyz 0.35 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS794W45P254L1969H508Q16 (layer F.Cu) (tedit 58157D96)
    (at 76.2 117.475)
    (descr "DIP for Socket, 7.94 mm lead span, 2.54 mm pitch; 16 pin, 19.69 mm L X 6.60 mm W X 5.08 mm H body")
    (fp_text reference XU3 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value IC_Socket16 (at 8.89 -3.81) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-16__300.wrl
      (at (xyz 0.35 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS794W45P254L1969H508Q16 (layer F.Cu) (tedit 58157D96)
    (at 114.3 137.16)
    (descr "DIP for Socket, 7.94 mm lead span, 2.54 mm pitch; 16 pin, 19.69 mm L X 6.60 mm W X 5.08 mm H body")
    (fp_text reference XU2 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value IC_Socket16 (at 8.89 -3.81) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-16__300.wrl
      (at (xyz 0.35 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS794W45P254L1969H508Q16 (layer F.Cu) (tedit 58157D96)
    (at 147.32 137.16)
    (descr "DIP for Socket, 7.94 mm lead span, 2.54 mm pitch; 16 pin, 19.69 mm L X 6.60 mm W X 5.08 mm H body")
    (fp_text reference XU1 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value IC_Socket16 (at 8.89 -3.81) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-16__300.wrl
      (at (xyz 0.35 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L1003H508Q8 (layer F.Cu) (tedit 587D45C5)
    (at 213.36 118.11)
    (descr "DIPS, 300 mil lead span, 100 mil pitch; 8 pin, 395 mil L X 400 mil W X 200 mil H body")
    (fp_text reference U10 (at 1.27 1.905) (layer F.SilkS))
    (fp_text value DS8921 (at 3.81 -5.715) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 76 /MISO'))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 75 /MOSI'))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 70 /MOSI'-))
    (pad 6 thru_hole circle (at 5.08 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 69 /MOSI'+))
    (pad 7 thru_hole circle (at 2.54 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 71 /MISO'-))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 68 /MISO'+))
    (model dil/sockets/dil_socket_8.wrl
      (at (xyz 0.15 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L1003H508Q8 (layer F.Cu) (tedit 587D45C5)
    (at 213.36 129.54)
    (descr "DIPS, 300 mil lead span, 100 mil pitch; 8 pin, 395 mil L X 400 mil W X 200 mil H body")
    (fp_text reference U9 (at 0.635 2.286) (layer F.SilkS))
    (fp_text value uA9638C (at 3.81 -5.715) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 18 /~SS))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 21 /SCK))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 73 /SCK'-))
    (pad 6 thru_hole circle (at 5.08 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 72 /SCK'+))
    (pad 7 thru_hole circle (at 2.54 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 67 /~SS'-))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 66 /~SS'+))
    (model dil/sockets/dil_socket_8.wrl
      (at (xyz 0.15 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L1003H508Q8 (layer F.Cu) (tedit 587D45C5)
    (at 58.42 116.84)
    (descr "DIPS, 300 mil lead span, 100 mil pitch; 8 pin, 395 mil L X 400 mil W X 200 mil H body")
    (fp_text reference U8 (at 0.635 2.54) (layer F.SilkS))
    (fp_text value DS8921 (at 3.81 -5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 19 /MOSI))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 20 /MISO))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 63 /MISO-))
    (pad 6 thru_hole circle (at 5.08 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 60 /MISO+))
    (pad 7 thru_hole circle (at 2.54 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 62 /MOSI-))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 61 /MOSI+))
    (model dil/sockets/dil_socket_8.wrl
      (at (xyz 0.15 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L1003H508Q8 (layer F.Cu) (tedit 587D45C5)
    (at 58.42 132.08)
    (descr "DIPS, 300 mil lead span, 100 mil pitch; 8 pin, 395 mil L X 400 mil W X 200 mil H body")
    (fp_text reference U7 (at 0.635 2.54) (layer F.SilkS))
    (fp_text value uA9637AC (at 3.81 -5.715) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 18 /~SS))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 21 /SCK))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 65 /SCK-))
    (pad 6 thru_hole circle (at 5.08 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 64 /SCK+))
    (pad 7 thru_hole circle (at 2.54 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 59 /~SS-))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 58 /~SS+))
    (model dil/sockets/dil_socket_8.wrl
      (at (xyz 0.15 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L2019H508Q16 (layer F.Cu) (tedit 58157D65)
    (at 186.69 117.475)
    (descr "DIPS, 7.62 mm lead span, 2.54 mm pitch; 16 pin, 20.19 mm L X 10.16 mm W X 5.08 mm H body")
    (fp_text reference U6 (at -2.54 0) (layer F.SilkS))
    (fp_text value 75C1168 (at 8.89 -5.715) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 53 /In7-))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 50 /In7+))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 15 /In7))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 17 /In8))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 54 /In8+))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 57 /In8-))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Out8))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 55 /Out8+))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 56 /Out8-))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 52 /Out7-))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 51 /Out7+))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 14 /Out7))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (model dil/sockets/dil_socket_16.wrl
      (at (xyz 0.35 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L2019H508Q16 (layer F.Cu) (tedit 58157D65)
    (at 149.86 117.475)
    (descr "DIPS, 7.62 mm lead span, 2.54 mm pitch; 16 pin, 20.19 mm L X 10.16 mm W X 5.08 mm H body")
    (fp_text reference U5 (at -2.54 0) (layer F.SilkS))
    (fp_text value 75C1168 (at 8.89 -5.715) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 45 /In5-))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 42 /In5+))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 11 /In5))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 13 /In6))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 46 /In6+))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 49 /In6-))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 12 /Out6))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 47 /Out6+))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 48 /Out6-))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 44 /Out5-))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 43 /Out5+))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Out5))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (model dil/sockets/dil_socket_16.wrl
      (at (xyz 0.35 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L2019H508Q16 (layer F.Cu) (tedit 58157D65)
    (at 113.03 117.475)
    (descr "DIPS, 7.62 mm lead span, 2.54 mm pitch; 16 pin, 20.19 mm L X 10.16 mm W X 5.08 mm H body")
    (fp_text reference U4 (at -2.54 0) (layer F.SilkS))
    (fp_text value 75C1168 (at 8.89 -5.715) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 37 /In3-))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 34 /In3+))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 7 /In3))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 9 /In4))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 38 /In4+))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 41 /In4-))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 8 /Out4))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 39 /Out4+))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 40 /Out4-))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 36 /Out3-))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 35 /Out3+))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Out3))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (model dil/sockets/dil_socket_16.wrl
      (at (xyz 0.35 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L2019H508Q16 (layer F.Cu) (tedit 58157D65)
    (at 76.2 117.475)
    (descr "DIPS, 7.62 mm lead span, 2.54 mm pitch; 16 pin, 20.19 mm L X 10.16 mm W X 5.08 mm H body")
    (fp_text reference U3 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 75C1168 (at 8.89 -5.715) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 29 /In1-))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 26 /In1+))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 3 /In1))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 5 /In2))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 30 /In2+))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 33 /In2-))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Out2))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 31 /Out2+))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 32 /Out2-))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 28 /Out1-))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 27 /Out1+))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 2 /Out1))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (model dil/sockets/dil_socket_16.wrl
      (at (xyz 0.35 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L2019H508Q16 (layer F.Cu) (tedit 58157D65)
    (at 114.3 137.16)
    (descr "DIPS, 7.62 mm lead span, 2.54 mm pitch; 16 pin, 20.19 mm L X 10.16 mm W X 5.08 mm H body")
    (fp_text reference U2 (at -2.54 1.651) (layer F.SilkS))
    (fp_text value 74HC165 (at 8.89 -5.715) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 74 /SS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SCK))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 11 /In5))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 13 /In6))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 15 /In7))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 17 /In8))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 20 /MISO))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 76 /MISO'))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 3 /In1))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 5 /In2))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 7 /In3))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 9 /In4))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 18 /~SS))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (model dil/sockets/dil_socket_16.wrl
      (at (xyz 0.35 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L2019H508Q16 (layer F.Cu) (tedit 58157D65)
    (at 147.32 137.16)
    (descr "DIPS, 7.62 mm lead span, 2.54 mm pitch; 16 pin, 20.19 mm L X 10.16 mm W X 5.08 mm H body")
    (fp_text reference U1 (at -2.54 0) (layer F.SilkS))
    (fp_text value 74HC595 (at 8.89 -5.715) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Out2))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Out3))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 8 /Out4))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Out5))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 12 /Out6))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 14 /Out7))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Out8))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 17.78 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 75 /MOSI'))
    (pad 10 thru_hole circle (at 15.24 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 11 thru_hole circle (at 12.7 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SCK))
    (pad 12 thru_hole circle (at 10.16 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 18 /~SS))
    (pad 13 thru_hole circle (at 7.62 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole circle (at 5.08 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 19 /MOSI))
    (pad 15 thru_hole circle (at 2.54 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 2 /Out1))
    (pad 16 thru_hole circle (at 0 -7.62) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (model dil/sockets/dil_socket_16.wrl
      (at (xyz 0.35 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESAD1016W56L681D259 (layer F.Cu) (tedit 5815799F)
    (at 101.6 137.16)
    (descr "Resistor, Axial; 400 mil C X 22 mil W 268 mil L X 102 mil Dia body - Standard 1/4W Resistor")
    (tags "RES 0.25 1/4")
    (fp_text reference R1 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 1kΩ (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.53 1.53) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.53 1.53) (drill 0.8128) (layers *.Cu *.Mask)
      (net 74 /SS))
    (model unused_3d.3dshapes/discret.resistors.horizontal.r_h_1k.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:TO92184P520H734-3 (layer F.Cu) (tedit 58157AC6)
    (at 108.07866 134.6215)
    (descr "TO-92, 1.8415 mm pitch; 3 pin, 5.207 mm W X 7.341 mm H body")
    (tags "TO92 TO-92")
    (fp_text reference Q1 (at -2.03366 -0.0015) (layer F.SilkS))
    (fp_text value VN3205 (at 1.77634 -3.8115) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.00166 -0.0015) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.83984 -2.07175) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 18 /~SS))
    (pad 3 thru_hole circle (at 3.68134 -0.0015) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 74 /SS))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Wide.wrl
      (at (xyz 0.072435 -0.000315 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 -90))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 228.6 124.46 90)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J14 (at -5.08 -3.175 180) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.445 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 66 /~SS'+))
    (pad 2 thru_hole circle (at 1.27 -2.54 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 67 /~SS'-))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 68 /MISO'+))
    (pad 4 thru_hole circle (at 3.81 -2.54 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 69 /MOSI'+))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 70 /MOSI'-))
    (pad 6 thru_hole circle (at 6.35 -2.54 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 71 /MISO'-))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 72 /SCK'+))
    (pad 8 thru_hole circle (at 8.89 -2.54 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 73 /SCK'-))
    (pad "" np_thru_hole circle (at 10.165 6.35 90) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 90) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 193.04 134.62 90)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J13 (at -2.54 -5.715 180) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.445 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 1.27 -2.54 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 4 thru_hole circle (at 3.81 -2.54 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /~IR_Osc+))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /~IR_Osc-))
    (pad 6 thru_hole circle (at 6.35 -2.54 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 8.89 -2.54 90) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 90) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 90) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:KYCON_KLDVHCX-0202-x_CirHole (layer F.Cu) (tedit 587EDFE8)
    (at 231.14 94.16 90)
    (descr "DC Power Jack Kycon# KLDVHCX-0202-x")
    (tags "PWR DC")
    (fp_text reference J12 (at -6.17 4.445 180) (layer F.SilkS))
    (fp_text value KLDVHCX-0202-A (at 5.895 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -4.9 0 180) (size 4.5 4.5) (drill 3.5) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 2 thru_hole circle (at -1.4 5.6 90) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 1.4 2.8 90) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ipc-7251TH-connectors.3dshapes/KYCON_KLDVHCX-0202-x.wrl
      (at (xyz 0 -0.255906 0.562992))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 50.8 116.84 270)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J11 (at -5.08 -3.048 360) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 3.81 13.97 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 /~SS+))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 59 /~SS-))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 60 /MISO+))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 61 /MOSI+))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 62 /MOSI-))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 63 /MISO-))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 64 /SCK+))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 65 /SCK-))
    (pad "" np_thru_hole circle (at 10.165 6.35 270) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 270) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 83.82 127 270)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J10 (at -4.445 -3.175 360) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.445 13.97 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /~IR_Osc+))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /~IR_Osc-))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 270) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 270) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:KYCON_KLDVHCX-0202-x_CirHole (layer F.Cu) (tedit 588D96C7)
    (at 45.72 93.98 90)
    (descr "DC Power Jack Kycon# KLDVHCX-0202-x")
    (tags "PWR DC")
    (fp_text reference J9 (at -5.715 4.445 180) (layer F.SilkS))
    (fp_text value KLDVHCX-0202-A (at 5.715 0.635 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -4.9 0 180) (size 4.5 4.5) (drill 3.5) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 2 thru_hole circle (at -1.4 5.6 90) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 1.4 2.8 90) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ipc-7251TH-connectors.3dshapes/KYCON_KLDVHCX-0202-x.wrl
      (at (xyz 0 -0.255906 0.562992))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 190.5 102.235 180)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J7 (at -1.27 -4.445 180) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.445 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /~IR_Osc+))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /~IR_Osc-))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 /In7+))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 /Out7+))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 /Out7-))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 /In7-))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 172.085 102.235 180)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J6 (at -0.635 -4.445 180) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.445 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /~IR_Osc+))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /~IR_Osc-))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 /In6+))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 /Out6+))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 /Out6-))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 /In6-))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 153.67 102.235 180)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J5 (at -1.27 -4.445 180) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.445 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /~IR_Osc+))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /~IR_Osc-))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 /In5+))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 /Out5+))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 /Out5-))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 /In5-))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 135.255 102.235 180)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J4 (at -1.27 -4.445 180) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.45 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /~IR_Osc+))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /~IR_Osc-))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 /In4+))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 /Out4+))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 /Out4-))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 /In4-))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 98.425 102.235 180)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J2 (at -1.27 -4.445 180) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.445 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /~IR_Osc+))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /~IR_Osc-))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 /In2+))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 /Out2+))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 /Out2-))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 /In2-))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 80.01 102.235 180)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J1 (at -1.27 -4.445 180) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.445 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /~IR_Osc+))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /~IR_Osc-))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 /In1+))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 /Out1+))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 /Out1-))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 /In1-))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 180) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-standard:CAPPRD254W50D500H850 (layer F.Cu) (tedit 58157DD8)
    (at 184.15 132.08 90)
    (descr "Capacitor, Polarized, Radial (Dipped, Round); 2.54 mm C X 5.00 mm Dia X 8.50 mm H body")
    (fp_text reference C18 (at -2.54 -1.27 180) (layer F.SilkS))
    (fp_text value 10µF (at 4.445 -1.905 180) (layer F.Fab))
    (fp_text user + (at -1.27 -1.905 90) (layer F.SilkS))
    (fp_text user + (at -1.778 -1.016 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.05 0 0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 187.96 132.08 90)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C17 (at -2.54 -0.635 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 4.445 -1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPPRD254W50D500H850 (layer F.Cu) (tedit 58157DD8)
    (at 218.44 96.52 90)
    (descr "Capacitor, Polarized, Radial (Dipped, Round); 2.54 mm C X 5.00 mm Dia X 8.50 mm H body")
    (fp_text reference C16 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10µF (at 5.08 0 180) (layer F.Fab))
    (fp_text user + (at -1.27 -1.905 90) (layer F.SilkS))
    (fp_text user + (at -1.778 -1.016 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.05 0 0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 223.52 96.52 90)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C15 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 88.9 129.54 270)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C14 (at -2.54 -0.635 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 4.445 -0.635 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPPRD254W50D500H850 (layer F.Cu) (tedit 58157DD8)
    (at 92.71 129.54 270)
    (descr "Capacitor, Polarized, Radial (Dipped, Round); 2.54 mm C X 5.00 mm Dia X 8.50 mm H body")
    (fp_text reference C13 (at -2.54 -0.635 360) (layer F.SilkS))
    (fp_text value 10µF (at 4.445 -1.905 360) (layer F.Fab))
    (fp_text user + (at -1.27 -1.905 270) (layer F.SilkS))
    (fp_text user + (at -1.778 -1.016 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.05 0 0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 55.88 96.52 90)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C12 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPPRD254W50D500H850 (layer F.Cu) (tedit 58157DD8)
    (at 60.325 96.52 90)
    (descr "Capacitor, Polarized, Radial (Dipped, Round); 2.54 mm C X 5.00 mm Dia X 8.50 mm H body")
    (fp_text reference C11 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10µF (at 5.08 0 180) (layer F.Fab))
    (fp_text user + (at -1.27 1.905 90) (layer F.SilkS))
    (fp_text user + (at -1.778 -1.016 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 23 "+5V(2)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.05 0 0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 210.82 118.11 90)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C10 (at -2.54 -0.635 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 4.445 -0.635 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 210.82 129.54 90)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C9 (at 0 -3.048 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 4.445 -0.635 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 55.88 116.84 90)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C8 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 55.88 132.08 90)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C7 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 4.445 -0.635 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 184.15 109.855 270)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C6 (at -2.54 0 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.27 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 147.32 109.855 270)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C5 (at -2.54 0 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.27 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 110.49 109.855 270)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C4 (at -2.54 0 540) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.27 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 73.66 109.855 270)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C3 (at 5.08 0 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.27 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 114.3 127)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C2 (at -3.175 0) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.27 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 58157E65)
    (at 144.145 129.54 270)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C1 (at -2.54 0 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 5.08 0.635 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 22 "+5V(1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 58.42 121.92)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R2 (at -2.54 0) (layer F.SilkS))
    (fp_text value 100Ω (at 1.27 -1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 58 /~SS+))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 59 /~SS-))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 58.42 106.68)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R3 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 100Ω (at 3.175 -1.905) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 61 /MOSI+))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 62 /MOSI-))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 63.5 121.92)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R4 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 100Ω (at 3.175 -1.905) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 64 /SCK+))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 65 /SCK-))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 213.36 107.95)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R5 (at 1.27 0) (layer F.SilkS))
    (fp_text value 100Ω (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 68 /MISO'+))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 71 /MISO'-))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 76.2 120.015)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R6 (at -2.54 0) (layer F.SilkS))
    (fp_text value 100Ω (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 29 /In1-))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 26 /In1+))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 88.9 120.015)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R7 (at -2.54 0) (layer F.SilkS))
    (fp_text value 100Ω (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 30 /In2+))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 33 /In2-))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 113.03 120.015)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R8 (at -2.54 0) (layer F.SilkS))
    (fp_text value 100Ω (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 37 /In3-))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 34 /In3+))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 125.73 120.015)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R9 (at -2.54 0) (layer F.SilkS))
    (fp_text value 100Ω (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 38 /In4+))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 41 /In4-))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 149.86 120.015)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R10 (at -3.175 0) (layer F.SilkS))
    (fp_text value 100Ω (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 45 /In5-))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 42 /In5+))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 162.56 120.015)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R11 (at -3.175 0) (layer F.SilkS))
    (fp_text value 100Ω (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 46 /In6+))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 49 /In6-))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 186.69 120.015)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R12 (at -3.175 0) (layer F.SilkS))
    (fp_text value 100Ω (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 53 /In7-))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 50 /In7+))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 588192A7)
    (at 199.39 120.015)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R13 (at -3.175 0) (layer F.SilkS))
    (fp_text value 100Ω (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 54 /In8+))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 57 /In8-))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:OSHW_03mm_copper_noMask (layer B.Cu) (tedit 0)
    (at 217.932 135.89 180)
    (fp_text reference G*** (at 0 -1.77038 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 1.77038 180) (layer B.SilkS) hide)
  )
  (module logos:crane_0.40in_silkscreen (layer B.Cu) (tedit 0)
    (at 226.695 132.715 180)
    (fp_text reference G*** (at 0 -3.64236 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 3.64236 180) (layer B.SilkS) hide)
  )
  (module ipc-7251TH-standard:MTGP794H326V8P (layer F.Cu) (tedit 549A50E1)
    (at 43.18 134.62)
    (descr "Mounting Hole, Plated, #4 Free Fit")
    (tags MTGP#4Free)
    (fp_text reference MH1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "#4 PTH" (at 0 0) (layer F.SilkS) hide)
    (pad 0 thru_hole rect (at 0 0) (size 7.94 7.94) (drill 3.26) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole rect (at 0 3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole rect (at 3.556 3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole rect (at 3.556 0) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole rect (at 3.556 -3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole rect (at 0 -3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole rect (at -3.556 -3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole rect (at -3.556 0) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole rect (at -3.556 3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module ipc-7251TH-standard:MTGNP794H326Z794P (layer F.Cu) (tedit 549A53B9)
    (at 236.22 134.62)
    (descr "Mounting Hole, Not Plated, #4 Free Fit")
    (tags MTGNP#4Free)
    (fp_text reference MH2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "#4 NPTH" (at 0 0) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.26 3.26) (drill 3.26) (layers *.Cu *.Mask)
      (clearance 2.34))
  )
  (module ipc-7251TH-standard:MTGNP794H326Z794P (layer F.Cu) (tedit 549A53B9)
    (at 236.22 106.68)
    (descr "Mounting Hole, Not Plated, #4 Free Fit")
    (tags MTGNP#4Free)
    (fp_text reference MH3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "#4 NPTH" (at 0 0) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.26 3.26) (drill 3.26) (layers *.Cu *.Mask)
      (clearance 2.34))
  )
  (module ipc-7251TH-standard:MTGNP794H326Z794P (layer F.Cu) (tedit 549A53B9)
    (at 43.18 106.68)
    (descr "Mounting Hole, Not Plated, #4 Free Fit")
    (tags MTGNP#4Free)
    (fp_text reference MH4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "#4 NPTH" (at 0 0) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.26 3.26) (drill 3.26) (layers *.Cu *.Mask)
      (clearance 2.34))
  )
  (module Symbols:Symbol_KiCAD-Logo_CopperAndSilkScreenTop (layer B.Cu) (tedit 0)
    (at 219.456 102.108 180)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference REF** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "KiCAD Logo" (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (dimension 5.08 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 238.76 144.225) (layer Dwgs.User))
    (feature1 (pts (xy 241.3 140.335) (xy 241.3 145.575)))
    (feature2 (pts (xy 236.22 140.335) (xy 236.22 145.575)))
    (crossbar (pts (xy 236.22 142.875) (xy 241.3 142.875)))
    (arrow1a (pts (xy 241.3 142.875) (xy 240.173496 143.461421)))
    (arrow1b (pts (xy 241.3 142.875) (xy 240.173496 142.288579)))
    (arrow2a (pts (xy 236.22 142.875) (xy 237.346504 143.461421)))
    (arrow2b (pts (xy 236.22 142.875) (xy 237.346504 142.288579)))
  )
  (dimension 17.78 (width 0.3) (layer Dwgs.User)
    (gr_text "0.7000 in" (at 33.575 97.79 90) (layer Dwgs.User))
    (feature1 (pts (xy 37.465 88.9) (xy 32.225 88.9)))
    (feature2 (pts (xy 37.465 106.68) (xy 32.225 106.68)))
    (crossbar (pts (xy 34.925 106.68) (xy 34.925 88.9)))
    (arrow1a (pts (xy 34.925 88.9) (xy 35.511421 90.026504)))
    (arrow1b (pts (xy 34.925 88.9) (xy 34.338579 90.026504)))
    (arrow2a (pts (xy 34.925 106.68) (xy 35.511421 105.553496)))
    (arrow2b (pts (xy 34.925 106.68) (xy 34.338579 105.553496)))
  )
  (dimension 33.02 (width 0.3) (layer Dwgs.User)
    (gr_text "1.3000 in" (at 29.13 123.19 90) (layer Dwgs.User))
    (feature1 (pts (xy 37.465 106.68) (xy 27.78 106.68)))
    (feature2 (pts (xy 37.465 139.7) (xy 27.78 139.7)))
    (crossbar (pts (xy 30.48 139.7) (xy 30.48 106.68)))
    (arrow1a (pts (xy 30.48 106.68) (xy 31.066421 107.806504)))
    (arrow1b (pts (xy 30.48 106.68) (xy 29.893579 107.806504)))
    (arrow2a (pts (xy 30.48 139.7) (xy 31.066421 138.573496)))
    (arrow2b (pts (xy 30.48 139.7) (xy 29.893579 138.573496)))
  )
  (dimension 27.94 (width 0.3) (layer Dwgs.User)
    (gr_text "1.1000 in" (at 33.575 120.65 90) (layer Dwgs.User))
    (feature1 (pts (xy 37.465 106.68) (xy 32.225 106.68)))
    (feature2 (pts (xy 37.465 134.62) (xy 32.225 134.62)))
    (crossbar (pts (xy 34.925 134.62) (xy 34.925 106.68)))
    (arrow1a (pts (xy 34.925 106.68) (xy 35.511421 107.806504)))
    (arrow1b (pts (xy 34.925 106.68) (xy 34.338579 107.806504)))
    (arrow2a (pts (xy 34.925 134.62) (xy 35.511421 133.493496)))
    (arrow2b (pts (xy 34.925 134.62) (xy 34.338579 133.493496)))
  )
  (dimension 5.08 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 33.575 137.16 90) (layer Dwgs.User))
    (feature1 (pts (xy 37.465 134.62) (xy 32.225 134.62)))
    (feature2 (pts (xy 37.465 139.7) (xy 32.225 139.7)))
    (crossbar (pts (xy 34.925 139.7) (xy 34.925 134.62)))
    (arrow1a (pts (xy 34.925 134.62) (xy 35.511421 135.746504)))
    (arrow1b (pts (xy 34.925 134.62) (xy 34.338579 135.746504)))
    (arrow2a (pts (xy 34.925 139.7) (xy 35.511421 138.573496)))
    (arrow2b (pts (xy 34.925 139.7) (xy 34.338579 138.573496)))
  )
  (dimension 193.04 (width 0.3) (layer Dwgs.User)
    (gr_text "7.6000 in" (at 139.7 144.224999) (layer Dwgs.User))
    (feature1 (pts (xy 236.22 140.335) (xy 236.22 145.574999)))
    (feature2 (pts (xy 43.18 140.335) (xy 43.18 145.574999)))
    (crossbar (pts (xy 43.18 142.874999) (xy 236.22 142.874999)))
    (arrow1a (pts (xy 236.22 142.874999) (xy 235.093496 143.46142)))
    (arrow1b (pts (xy 236.22 142.874999) (xy 235.093496 142.288578)))
    (arrow2a (pts (xy 43.18 142.874999) (xy 44.306504 143.46142)))
    (arrow2b (pts (xy 43.18 142.874999) (xy 44.306504 142.288578)))
  )
  (dimension 198.12 (width 0.3) (layer Dwgs.User)
    (gr_text "7.8000 in" (at 137.16 148.669999) (layer Dwgs.User))
    (feature1 (pts (xy 236.22 140.335) (xy 236.22 150.019999)))
    (feature2 (pts (xy 38.1 140.335) (xy 38.1 150.019999)))
    (crossbar (pts (xy 38.1 147.319999) (xy 236.22 147.319999)))
    (arrow1a (pts (xy 236.22 147.319999) (xy 235.093496 147.90642)))
    (arrow1b (pts (xy 236.22 147.319999) (xy 235.093496 146.733578)))
    (arrow2a (pts (xy 38.1 147.319999) (xy 39.226504 147.90642)))
    (arrow2b (pts (xy 38.1 147.319999) (xy 39.226504 146.733578)))
  )
  (dimension 5.08 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 40.64 144.225) (layer Dwgs.User))
    (feature1 (pts (xy 43.18 140.335) (xy 43.18 145.575)))
    (feature2 (pts (xy 38.1 140.335) (xy 38.1 145.575)))
    (crossbar (pts (xy 38.1 142.875) (xy 43.18 142.875)))
    (arrow1a (pts (xy 43.18 142.875) (xy 42.053496 143.461421)))
    (arrow1b (pts (xy 43.18 142.875) (xy 42.053496 142.288579)))
    (arrow2a (pts (xy 38.1 142.875) (xy 39.226504 143.461421)))
    (arrow2b (pts (xy 38.1 142.875) (xy 39.226504 142.288579)))
  )
  (gr_text "LED Pwr" (at 220.345 90.805) (layer F.SilkS))
  (gr_text "LED Pwr" (at 58.42 90.805) (layer F.SilkS))
  (gr_text "Osc\nIn" (at 90.297 136.652) (layer F.SilkS))
  (gr_text "Osc\nOut" (at 186.055 124.587) (layer F.SilkS))
  (gr_text "SPI\nOut" (at 228.092 107.823) (layer F.SilkS))
  (gr_text "SPI\nIn" (at 50.165 108.585) (layer F.SilkS))
  (gr_text "Sch V2.0.2\nPcb V1.0.0" (at 219.456 103.251) (layer F.SilkS))
  (gr_text "TrippyRGB\nI&O Expander" (at 220.472 136.017) (layer F.SilkS))
  (gr_text "Sembazuru\nCircuits" (at 227.076 137.668) (layer B.SilkS))
  (gr_text "DIY DE" (at 208.915 137.795) (layer B.SilkS))
  (gr_text BoM (at 208.915 133.985) (layer B.SilkS))
  (dimension 50.8 (width 0.3) (layer Dwgs.User)
    (gr_text "2.0000 in" (at 248.443075 114.3 270) (layer Dwgs.User))
    (feature1 (pts (xy 242.013075 139.7) (xy 249.793075 139.7)))
    (feature2 (pts (xy 242.013075 88.9) (xy 249.793075 88.9)))
    (crossbar (pts (xy 247.093075 88.9) (xy 247.093075 139.7)))
    (arrow1a (pts (xy 247.093075 139.7) (xy 246.506654 138.573496)))
    (arrow1b (pts (xy 247.093075 139.7) (xy 247.679496 138.573496)))
    (arrow2a (pts (xy 247.093075 88.9) (xy 246.506654 90.026504)))
    (arrow2b (pts (xy 247.093075 88.9) (xy 247.679496 90.026504)))
  )
  (dimension 203.2 (width 0.3) (layer Dwgs.User)
    (gr_text "8.0000 in" (at 139.7 81.772593) (layer Dwgs.User))
    (feature1 (pts (xy 241.3 88.202593) (xy 241.3 80.422593)))
    (feature2 (pts (xy 38.1 88.202593) (xy 38.1 80.422593)))
    (crossbar (pts (xy 38.1 83.122593) (xy 241.3 83.122593)))
    (arrow1a (pts (xy 241.3 83.122593) (xy 240.173496 83.709014)))
    (arrow1b (pts (xy 241.3 83.122593) (xy 240.173496 82.536172)))
    (arrow2a (pts (xy 38.1 83.122593) (xy 39.226504 83.709014)))
    (arrow2b (pts (xy 38.1 83.122593) (xy 39.226504 82.536172)))
  )
  (gr_line (start 241.3 88.9) (end 38.1 88.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 241.3 139.7) (end 241.3 88.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 38.1 139.7) (end 241.3 139.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 38.1 88.9) (end 38.1 139.7) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.5842))
    (polygon
      (pts
        (xy 38.354 89.154) (xy 38.354 139.446) (xy 241.046 139.446) (xy 241.046 89.154)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.439 133.731) (xy 82.931 134.239) (xy 82.931 135.001) (xy 83.439 135.509) (xy 84.201 135.509)
        (xy 84.709 135.001) (xy 84.709 134.239) (xy 84.201 133.731)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.979 132.461) (xy 85.471 132.969) (xy 85.471 133.731) (xy 85.979 134.239) (xy 86.741 134.239)
        (xy 87.249 133.731) (xy 87.249 132.969) (xy 86.741 132.461)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.979 135.001) (xy 85.471 135.509) (xy 85.471 136.271) (xy 85.979 136.779) (xy 86.741 136.779)
        (xy 87.249 136.271) (xy 87.249 135.509) (xy 86.741 135.001)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.519 131.318) (xy 88.138 131.699) (xy 88.138 132.461) (xy 88.519 132.842) (xy 89.281 132.842)
        (xy 89.662 132.461) (xy 89.662 131.699) (xy 89.281 131.318)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.119 124.841) (xy 189.611 125.349) (xy 189.611 126.111) (xy 190.119 126.619) (xy 190.881 126.619)
        (xy 191.389 126.111) (xy 191.389 125.349) (xy 190.881 124.841)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 192.659 126.111) (xy 192.151 126.619) (xy 192.151 127.381) (xy 192.659 127.889) (xy 193.421 127.889)
        (xy 193.929 127.381) (xy 193.929 126.619) (xy 193.421 126.111)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.119 127.381) (xy 189.611 127.889) (xy 189.611 128.651) (xy 190.119 129.159) (xy 190.881 129.159)
        (xy 191.389 128.651) (xy 191.389 127.889) (xy 190.881 127.381)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.579 128.778) (xy 187.198 129.159) (xy 187.198 129.921) (xy 187.579 130.302) (xy 188.341 130.302)
        (xy 188.722 129.921) (xy 188.722 129.159) (xy 188.341 128.778)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.725 128.905) (xy 213.995 128.905) (xy 213.995 130.175) (xy 212.725 130.175)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.725 117.475) (xy 213.995 117.475) (xy 213.995 118.745) (xy 212.725 118.745)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.309 109.093) (xy 187.071 109.093) (xy 187.452 109.474) (xy 187.452 110.236) (xy 187.071 110.617)
        (xy 186.309 110.617) (xy 185.928 110.236) (xy 185.928 109.474)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.479 109.093) (xy 150.241 109.093) (xy 150.622 109.474) (xy 150.622 110.236) (xy 150.241 110.617)
        (xy 149.479 110.617) (xy 149.098 110.236) (xy 149.098 109.474)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.649 109.093) (xy 113.411 109.093) (xy 113.792 109.474) (xy 113.792 110.236) (xy 113.411 110.617)
        (xy 112.649 110.617) (xy 112.268 110.236) (xy 112.268 109.474)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.819 109.093) (xy 76.581 109.093) (xy 76.962 109.474) (xy 76.962 110.236) (xy 76.581 110.617)
        (xy 75.819 110.617) (xy 75.438 110.236) (xy 75.438 109.474)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.785 116.205) (xy 59.055 116.205) (xy 59.055 117.475) (xy 57.785 117.475)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.785 131.445) (xy 59.055 131.445) (xy 59.055 132.715) (xy 57.785 132.715)
      )
    )
  )
  (zone (net 22) (net_name "+5V(1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.5842))
    (polygon
      (pts
        (xy 38.354 96.52) (xy 38.354 139.446) (xy 241.046 139.446) (xy 241.046 96.52)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.439 128.651) (xy 82.931 129.159) (xy 82.931 129.921) (xy 83.439 130.429) (xy 84.201 130.429)
        (xy 84.709 129.921) (xy 84.709 129.159) (xy 84.201 128.651)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.979 127.381) (xy 85.471 127.889) (xy 85.471 128.651) (xy 85.979 129.159) (xy 86.741 129.159)
        (xy 87.249 128.651) (xy 87.249 127.889) (xy 86.741 127.381)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.931 126.111) (xy 82.931 127.889) (xy 84.709 127.889) (xy 84.709 126.111) (xy 84.709 126.111)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.138 128.778) (xy 88.138 130.302) (xy 89.662 130.302) (xy 89.662 128.778) (xy 89.662 128.778)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.119 132.51997) (xy 189.611 132.969) (xy 189.611 133.731) (xy 190.119 134.239) (xy 190.881 134.239)
        (xy 191.389 133.731) (xy 191.389 132.969) (xy 190.881 132.51997)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 192.659 131.191) (xy 192.151 131.699) (xy 192.151 132.461) (xy 192.659 132.969) (xy 193.421 132.969)
        (xy 193.929 132.461) (xy 193.929 131.699) (xy 193.421 131.191)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 192.151 133.731) (xy 192.151 135.509) (xy 193.929 135.509) (xy 193.929 133.731) (xy 193.929 133.731)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.198 131.318) (xy 187.198 132.842) (xy 188.722 132.842) (xy 188.722 131.318) (xy 188.722 131.318)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.919 128.651) (xy 114.681 128.651) (xy 115.189 129.159) (xy 115.189 129.921) (xy 114.681 130.429)
        (xy 113.919 130.429) (xy 113.411 129.921) (xy 113.411 129.159)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.939 128.651) (xy 147.701 128.651) (xy 148.209 129.159) (xy 148.209 129.921) (xy 147.701 130.429)
        (xy 146.939 130.429) (xy 146.431 129.921) (xy 146.431 129.159)
      )
    )
  )
)
