(kicad_pcb (version 20171130) (host pcbnew 5.1.10-88a1d61d58~88~ubuntu20.10.1)
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 315)
    (zones 0)
    (modules 9)
    (nets 33)
  )
  (page USLetter)
  (title_block
    (title "29F010 to 23C1000")
    (date 2021-05-09)
    (rev 005)
    (company "Brian K. White - b.kenyon.w@gmail.com")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.18)
    (user_trace_width 0.16)
    (user_trace_width 0.3)
    (trace_clearance 0.16)
    (zone_clearance 0.16)
    (zone_45_only no)
    (trace_min 0.16)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (uvia_size 0.5)
    (uvia_drill 0.3)
    (uvias_allowed no)
    (uvia_min_size 0.5)
    (uvia_min_drill 0.3)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 1.2)
    (pad_drill 0.58)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (aux_axis_origin 0 0)
    (grid_origin 150 97.46)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_FLASH_23C1000"))
  )
  (net 0 "")
  (net 1 /A14)
  (net 2 /D2)
  (net 3 /A13)
  (net 4 /D1)
  (net 5 /A8)
  (net 6 /D0)
  (net 7 /A9)
  (net 8 /A0)
  (net 9 /A11)
  (net 10 /A1)
  (net 11 /~OE)
  (net 12 /A2)
  (net 13 /A10)
  (net 14 /A3)
  (net 15 /~CE)
  (net 16 /A4)
  (net 17 /D7)
  (net 18 /A5)
  (net 19 /D6)
  (net 20 /A6)
  (net 21 /D5)
  (net 22 /A7)
  (net 23 /D4)
  (net 24 /A12)
  (net 25 /D3)
  (net 26 /~WE)
  (net 27 /A16)
  (net 28 /A15)
  (net 29 /VCC)
  (net 30 /GND)
  (net 31 /A16_~OE)
  (net 32 /VPP)
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.18)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.5)
    (uvia_drill 0.3)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A16_~OE)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /GND)
    (add_net /VCC)
    (add_net /VPP)
    (add_net /~CE)
    (add_net /~OE)
    (add_net /~WE)
  )
  (module 000_LOCAL:NPTH_3mm (layer F.Cu) (tedit 5F9F8D8C)
    (at 150 77.775)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value NPTH_3mm (at 0 -2.54) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module 000_LOCAL:DIP32_0.6_pcb_sil_pins (layer F.Cu) (tedit 5FC98C84)
    (at 150 97.46)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference J1 (at 0 -21.38) (layer F.SilkS) hide)
    (fp_text value "uPD23C1000 / FLASH" (at 0 21.59) (layer F.Fab))
    (fp_text user %R (at 0.27 0.58) (layer F.Fab))
    (pad 32 thru_hole circle (at 7.62 -19.05) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 29 /VCC))
    (pad 31 thru_hole circle (at 7.62 -16.51) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 26 /~WE))
    (pad 15 thru_hole circle (at -7.62 16.51) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 /D2))
    (pad 16 thru_hole circle (at -7.62 19.05) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 30 /GND))
    (pad 1 thru_hole roundrect (at -7.62 -19.05) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 32 /VPP))
    (pad 29 thru_hole circle (at 7.62 -11.43) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 /A14))
    (pad 2 thru_hole circle (at -7.62 -16.51) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 27 /A16))
    (pad 30 thru_hole circle (at 7.62 -13.97) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 29 /VCC))
    (pad 3 thru_hole roundrect (at -7.62 -13.97) (size 1.2 1.2) (drill 0.58) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 28 /A15))
    (pad 17 thru_hole circle (at 7.62 19.05) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 25 /D3))
    (pad 4 thru_hole circle (at -7.62 -11.43) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 24 /A12))
    (pad 18 thru_hole circle (at 7.62 16.51) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 23 /D4))
    (pad 5 thru_hole circle (at -7.62 -8.89) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 22 /A7))
    (pad 19 thru_hole circle (at 7.62 13.97) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 21 /D5))
    (pad 6 thru_hole circle (at -7.62 -6.35) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 20 /A6))
    (pad 20 thru_hole circle (at 7.62 11.43) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 19 /D6))
    (pad 7 thru_hole circle (at -7.62 -3.81) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 18 /A5))
    (pad 21 thru_hole circle (at 7.62 8.89) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 /D7))
    (pad 8 thru_hole circle (at -7.62 -1.27) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 /A4))
    (pad 22 thru_hole circle (at 7.62 6.35) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 /~CE))
    (pad 9 thru_hole circle (at -7.62 1.27) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 /A3))
    (pad 23 thru_hole circle (at 7.62 3.81) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 /A10))
    (pad 10 thru_hole circle (at -7.62 3.81) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 12 /A2))
    (pad 24 thru_hole circle (at 7.62 1.27) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 31 /A16_~OE))
    (pad 11 thru_hole circle (at -7.62 6.35) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 /A1))
    (pad 25 thru_hole circle (at 7.62 -1.27) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 9 /A11))
    (pad 12 thru_hole circle (at -7.62 8.89) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 /A0))
    (pad 26 thru_hole circle (at 7.62 -3.81) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 /A9))
    (pad 13 thru_hole circle (at -7.62 11.43) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 /D0))
    (pad 27 thru_hole circle (at 7.62 -6.35) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 /A8))
    (pad 14 thru_hole circle (at -7.62 13.97) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 /D1))
    (pad 28 thru_hole circle (at 7.62 -8.89) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 /A13))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 19.05 0.18034))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -19.05 0.18034))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 19.05 0.18034))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -19.05 0.18034))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:Pin_Header_Angled_1x03_Pitch2.54mm_12shorted (layer F.Cu) (tedit 5E67F9D5)
    (at 155.715 115.24 180)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 4.385 -2.27) (layer F.SilkS) hide)
    (fp_text value RUN/PROGRAM (at 4.385 7.35) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 27 /A16))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 31 /A16_~OE))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 11 /~OE))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/PinHeader_1x03_P2.54mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/Jumper.stp
      (offset (xyz 4.064 -3.7592 0.1016))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 90))
    )
  )
  (module 000_LOCAL:R_0805 (layer F.Cu) (tedit 5F9E65BE)
    (at 146.19 80.95 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -0.0508 -0.0127 180) (layer F.SilkS))
    (fp_text value 47K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 32 /VPP))
    (pad 2 smd roundrect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 29 /VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/R_0805_2012Metric.step_x
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:R_0805 (layer F.Cu) (tedit 5F9E65BE)
    (at 153.81 80.95 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 0 180) (layer F.SilkS))
    (fp_text value 47K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 26 /~WE))
    (pad 2 smd roundrect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 29 /VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:R_0805 (layer F.Cu) (tedit 5F9E65BE)
    (at 155.75 106.35 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.0381 -0.0254) (layer F.SilkS))
    (fp_text value 47k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 11 /~OE))
    (pad 2 smd roundrect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 30 /GND))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:TSOP32-14mm (layer F.Cu) (tedit 5F970953)
    (at 150 100.46 180)
    (descr "Module CMS TSOP 32 pins")
    (tags "CMS TSOP")
    (attr smd)
    (fp_text reference U2 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value "29F010 sTSOP-32 14mm" (at 0.15 -1.35 180) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 1 smd roundrect (at -3.75 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /A11))
    (pad 2 smd roundrect (at -3.25 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /A9))
    (pad 3 smd roundrect (at -2.75 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /A8))
    (pad 4 smd roundrect (at -2.25 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /A13))
    (pad 5 smd roundrect (at -1.75 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /A14))
    (pad 6 smd roundrect (at -1.25 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -0.75 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /~WE))
    (pad 8 smd roundrect (at -0.25 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /VCC))
    (pad 9 smd roundrect (at 0.25 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /VPP))
    (pad 10 smd roundrect (at 0.75 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /A16))
    (pad 11 smd roundrect (at 1.25 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /A15))
    (pad 12 smd roundrect (at 1.75 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /A12))
    (pad 13 smd roundrect (at 2.25 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /A7))
    (pad 14 smd roundrect (at 2.75 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /A6))
    (pad 15 smd roundrect (at 3.25 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /A5))
    (pad 16 smd roundrect (at 3.75 6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /A4))
    (pad 17 smd roundrect (at 3.75 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /A3))
    (pad 18 smd roundrect (at 3.25 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A2))
    (pad 19 smd roundrect (at 2.75 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A1))
    (pad 20 smd roundrect (at 2.25 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /A0))
    (pad 21 smd roundrect (at 1.75 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /D0))
    (pad 22 smd roundrect (at 1.25 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /D1))
    (pad 23 smd roundrect (at 0.75 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /D2))
    (pad 24 smd roundrect (at 0.25 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /GND))
    (pad 25 smd roundrect (at -0.25 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /D3))
    (pad 26 smd roundrect (at -0.75 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /D4))
    (pad 27 smd roundrect (at -1.25 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /D5))
    (pad 28 smd roundrect (at -1.75 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /D6))
    (pad 29 smd roundrect (at -2.25 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /D7))
    (pad 30 smd roundrect (at -2.75 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /~CE))
    (pad 31 smd roundrect (at -3.25 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A10))
    (pad 32 smd roundrect (at -3.75 -6.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /~OE))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/TSOP32_8x14.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module 000_LOCAL:PLCC32_7x9 (layer F.Cu) (tedit 5F9708DD)
    (at 150 97.46)
    (descr "PLCC, 32 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/doc0015.pdf), generated with kicad-footprint-generator ipc_plcc_jLead_generator.py")
    (tags "PLCC LCC")
    (attr smd)
    (fp_text reference U3 (at 0 -8.52) (layer F.SilkS) hide)
    (fp_text value "29F010 PLCC 7x9" (at 0 8.52) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 32 smd roundrect (at 1.27 -6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /VCC))
    (pad 31 smd roundrect (at 2.54 -6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /~WE))
    (pad 30 smd roundrect (at 3.81 -6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 29 smd roundrect (at 5.5625 -5.08) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /A14))
    (pad 28 smd roundrect (at 5.5625 -3.81) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /A13))
    (pad 27 smd roundrect (at 5.5625 -2.54) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /A8))
    (pad 26 smd roundrect (at 5.5625 -1.27) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /A9))
    (pad 25 smd roundrect (at 5.5625 0) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /A11))
    (pad 24 smd roundrect (at 5.5625 1.27) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /~OE))
    (pad 23 smd roundrect (at 5.5625 2.54) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A10))
    (pad 22 smd roundrect (at 5.5625 3.81) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /~CE))
    (pad 21 smd roundrect (at 5.5625 5.08) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /D7))
    (pad 20 smd roundrect (at 3.81 6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /D6))
    (pad 19 smd roundrect (at 2.54 6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /D5))
    (pad 18 smd roundrect (at 1.27 6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /D4))
    (pad 17 smd roundrect (at 0 6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /D3))
    (pad 16 smd roundrect (at -1.27 6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /GND))
    (pad 15 smd roundrect (at -2.54 6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /D2))
    (pad 14 smd roundrect (at -3.81 6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /D1))
    (pad 13 smd roundrect (at -5.5625 5.08) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /D0))
    (pad 12 smd roundrect (at -5.5625 3.81) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /A0))
    (pad 11 smd roundrect (at -5.5625 2.54) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A1))
    (pad 10 smd roundrect (at -5.5625 1.27) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A2))
    (pad 9 smd roundrect (at -5.5625 0) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /A3))
    (pad 8 smd roundrect (at -5.5625 -1.27) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /A4))
    (pad 7 smd roundrect (at -5.5625 -2.54) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /A5))
    (pad 6 smd roundrect (at -5.5625 -3.81) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /A6))
    (pad 5 smd roundrect (at -5.5625 -5.08) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /A7))
    (pad 4 smd roundrect (at -3.81 -6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /A12))
    (pad 3 smd roundrect (at -2.54 -6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /A15))
    (pad 2 smd roundrect (at -1.27 -6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /A16))
    (pad 1 smd roundrect (at 0 -6.8375) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /VPP))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/PLCC32_7x9.step_x
      (offset (xyz 0 0 0.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:TSOP32-20mm (layer F.Cu) (tedit 5F970990)
    (at 150 97.46 180)
    (descr "Module CMS TSOP 32 pins")
    (tags "CMS TSOP")
    (attr smd)
    (fp_text reference U1 (at 0 -5 180) (layer F.SilkS) hide)
    (fp_text value "29F010 TSOP-32 20mm" (at 0 5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -3.75 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /A11))
    (pad 2 smd roundrect (at -3.25 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /A9))
    (pad 3 smd roundrect (at -2.75 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /A8))
    (pad 4 smd roundrect (at -2.25 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /A13))
    (pad 5 smd roundrect (at -1.75 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /A14))
    (pad 6 smd roundrect (at -1.25 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -0.75 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /~WE))
    (pad 8 smd roundrect (at -0.25 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /VCC))
    (pad 9 smd roundrect (at 0.25 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /VPP))
    (pad 10 smd roundrect (at 0.75 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /A16))
    (pad 11 smd roundrect (at 1.25 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /A15))
    (pad 12 smd roundrect (at 1.75 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /A12))
    (pad 13 smd roundrect (at 2.25 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /A7))
    (pad 14 smd roundrect (at 2.75 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /A6))
    (pad 15 smd roundrect (at 3.25 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /A5))
    (pad 16 smd roundrect (at 3.75 9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /A4))
    (pad 17 smd roundrect (at 3.75 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /A3))
    (pad 18 smd roundrect (at 3.25 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A2))
    (pad 19 smd roundrect (at 2.75 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A1))
    (pad 20 smd roundrect (at 2.25 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /A0))
    (pad 21 smd roundrect (at 1.75 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /D0))
    (pad 22 smd roundrect (at 1.25 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /D1))
    (pad 23 smd roundrect (at 0.75 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /D2))
    (pad 24 smd roundrect (at 0.25 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /GND))
    (pad 25 smd roundrect (at -0.25 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /D3))
    (pad 26 smd roundrect (at -0.75 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /D4))
    (pad 27 smd roundrect (at -1.25 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /D5))
    (pad 28 smd roundrect (at -1.75 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /D6))
    (pad 29 smd roundrect (at -2.25 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /D7))
    (pad 30 smd roundrect (at -2.75 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /~CE))
    (pad 31 smd roundrect (at -3.25 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /A10))
    (pad 32 smd roundrect (at -3.75 -9.75 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /~OE))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/TSOP32_8X20.step_x
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_text 29F010 (at 145.809 78.7275) (layer F.SilkS))
  (gr_text "29F010\n28C010\n27C010" (at 150 98.71 -90) (layer F.SilkS))
  (gr_text "Place board in programmer ZIF socket" (at 148.59 80.01 90) (layer B.SilkS))
  (gr_text 23C1000 (at 150 85.395) (layer F.SilkS))
  (gr_line (start 141.745 77.775) (end 158.255 77.775) (layer Edge.Cuts) (width 0.05))
  (gr_text github.com/bkw777/aDIPters (at 155.75 97.46 90) (layer B.SilkS))
  (gr_text "R1, R2: 47k" (at 152.4 107.95 90) (layer B.SilkS))
  (gr_text "Legs: TE 1544210" (at 153.67 107.95 90) (layer B.SilkS))
  (gr_text "Move the jumper from RUN to PRG" (at 147.32 80.01 90) (layer B.SilkS))
  (gr_text "To program:" (at 146.05 78.74 90) (layer B.SilkS))
  (gr_text PRG (at 144.285 109.525 -90) (layer F.SilkS))
  (gr_text RUN (at 144.285 115.875 -90) (layer F.SilkS))
  (gr_line (start 141.745 117.145) (end 141.745 77.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.255 77.775) (end 158.255 117.145) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.745 117.145) (end 158.255 117.145) (layer Edge.Cuts) (width 0.05))
  (zone (net 30) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 158.255 117.145) (xy 141.745 117.145) (xy 141.745 77.775) (xy 158.255 77.775)
      )
    )
  )
  (zone (net 30) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 158.255 117.145) (xy 141.745 117.145) (xy 141.745 77.775) (xy 158.255 77.775)
      )
    )
  )
)
