(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND1")
  (net 2 "+12L")
  (net 3 "+12V")
  (net 4 "-12V")
  (net 5 "Net-(PS1-+V)")
  (net 6 "Net-(PS1--V)")
  (net 7 "Net-(U2-Vreg2)")
  (net 8 "Net-(PS1-Vin)")
  (net 9 "Net-(U2-Vreg1)")
  (net 10 "Net-(U3C-+)")
  (net 11 "Net-(U3C--)")
  (net 12 "-12VA")
  (net 13 "Net-(U1C-+)")
  (net 14 "Net-(U2-Ref1)")
  (net 15 "Net-(U3A--)")
  (net 16 "Net-(U3B--)")
  (net 17 "Net-(U3D-+)")
  (net 18 "Net-(U3D--)")
  (net 19 "Net-(J3-In)")
  (net 20 "Net-(U1D-+)")
  (net 21 "Net-(R6-Pad2)")
  (net 22 "Net-(R7-Pad2)")
  (net 23 "Net-(U1B--)")
  (net 24 "Net-(U1A--)")
  (net 25 "unconnected-(RV2-Pad1)")
  (net 26 "unconnected-(U2-NC-Pad5)")
  (net 27 "unconnected-(U2-EAout2-Pad6)")
  (net 28 "Net-(U2-Comp)")
  (net 29 "GND2")
  (net 30 "/Vdiff1")
  (net 31 "/Vlp1")
  (net 32 "/Vo2")
  (net 33 "/Voff2")
  (net 34 "/Vin+")
  (net 35 "/Vin-")
  (net 36 "Net-(U2-Ref2)")
  (net 37 "/Voff1")
  (net 38 "/Vin1")
  (net 39 "Net-(U1D--)")
  (net 40 "Net-(R14-Pad2)")
  (net 41 "Net-(R15-Pad2)")
  (net 42 "Net-(R24-Pad2)")
  (net 43 "/V-")
  (net 44 "/V+")
  (footprint "_es_RLC:R_THT_1W" (layer "F.Cu")
    (at 105.918 93.98 -90)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (property "MPN" "RNCP1206FTD1K00")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R2" (at -9.398 0 -180) (layer "F.SilkS"))
    (fp_text value "1k" (at 7.62 3.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -7.874 0 270) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 34 "/Vin+") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.874 0 270) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 44 "/V+") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/CMF601K0000FHEK.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 162.052 99.568)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RNCP1206FTD1K00")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R14" (at 0.026 -1.524) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(U2-Ref1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 40 "Net-(R14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (at 88.138 107.95)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 118.11 91.44 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RMCF1206FT20K0")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R7" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 24 "Net-(U1A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 22 "Net-(R7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 130.81 101.6)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R12" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "301" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(U1C-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 36 "Net-(U2-Ref2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 135.636 84.074 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "CL31B334KBHWPNE")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C7" (at 2.794 0) (layer "F.SilkS"))
    (fp_text value "0.33u" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "GND2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "Net-(PS1-+V)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 179.324 83.82)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R25" (at 2.794 0 90) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 42 "Net-(R24-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 19 "Net-(J3-In)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 144.526 100.838 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "CL31B105KCHNNNE")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C9" (at -2.794 0) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 29 "GND2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 155.194 100.838 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "CL31B105KCHNNNE")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C13" (at 3.048 0 -180) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "+12L") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_RLC:L_Murata_82473C" (layer "F.Cu")
    (at 132.08 78.994 180)
    (descr "Murata 82xx series SMT inductor")
    (property "MPN" "82154C")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor, small symbol")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L2" (at 0 2.286 unlocked) (layer "F.SilkS"))
    (fp_text value "150u" (at 0.381 4.064 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.127 2.794 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.143 0 180) (size 1.524 3.048) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(PS1--V)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.143 -0.006835 180) (size 1.524 3.048) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-12V") (pintype "passive"))
    (model "C:/Users/stiers/Google Drive/Work Projects/_KiCad Lib/3D Models/mps_mag_8200_smt_a.step"
      (offset (xyz 25.0698 136.0932 0.9652))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 130.81 104.14 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RNCP1206FTD1K00")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R13" (at -3.048 0 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "GND2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(U1C-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_RLC:R_THT_1W" (layer "F.Cu")
    (at 101.6 93.98 90)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (property "MPN" "RNCP1206FTD1K00")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 9.398 0 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 7.62 3.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -7.874 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 35 "/Vin-") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.874 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 43 "/V-") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/CMF601K0000FHEK.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "_es_RLC:Potentiometer_Nidec_ST4_Vertical" (layer "F.Cu")
    (at 172.688 80.144 180)
    (descr "Potentiometer, vertical, Vishay TS53YJ, https://www.vishay.com/docs/51008/ts53.pdf")
    (tags "Potentiometer vertical Vishay TS53YJ")
    (property "MPN" "ST-4ETA202")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Trim-potentiometer, US symbol")
    (property "ki_keywords" "resistor variable trimpot trimmer")
    (attr smd)
    (fp_text reference "RV2" (at -3.588 1.658 270) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect (at 2 -1.15 180) (size 2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "unconnected-(RV2-Pad1)") (pinfunction "1") (pintype "passive+no_connect"))
    (pad "2" smd rect (at -2 0 180) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(R24-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 2 1.15 180) (size 2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(U3D--)") (pinfunction "3") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/ST-4ETA2k_(202).stp"
      (offset (xyz 0 0 2.286))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 124.968 101.6 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R5" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "Rg" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 24 "Net-(U1A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 23 "Net-(U1B--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Mechanical:40mil PTH" (layer "F.Cu")
    (at 144.78 109.982)
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "PTH1" (at 0 -1.524 unlocked) (layer "F.SilkS") hide)
    (fp_text value "GND2" (at 0 1.778 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.048 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 29 "GND2") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 130.81 96.52)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "C1206C102J2GAC7800")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C4" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "390p" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 20 "Net-(U1D-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 33 "/Voff2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 153.162 78.994 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "CL31B334KBHWPNE")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C12" (at -2.794 0 -180) (layer "F.SilkS"))
    (fp_text value "0.33u" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 8 "Net-(PS1-Vin)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (at 195.58 80.01)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 128.524 78.994 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "CL31B334KBHWPNE")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C6" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "0.33u" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 4 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "GND2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 160.274 78.994 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "CL31B334KBHWPNE")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C15" (at -2.794 0 -180) (layer "F.SilkS"))
    (fp_text value "0.33u" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "+12L") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 189.738 76.2)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Power" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "+12L") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "-12VA") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 179.2855 88.9)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "GRM31C5C2A104JA01L")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C17" (at 2.8325 0 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 12 "-12VA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 166.116 93.98)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RMCF1206FT20K0")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R19" (at -2.794 0 90) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(U3C--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 30 "/Vdiff1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 118.11 88.9)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RMCF1206FT20K0")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R9" (at -3.048 0 90) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 22 "Net-(R7-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 20 "Net-(U1D-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 130.81 88.9)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RNCP1206FTD1K00")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R10" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 39 "Net-(U1D--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 32 "/Vo2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 179.324 91.44)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R20" (at 2.794 0 90) (layer "F.SilkS"))
    (fp_text value "500" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 30 "/Vdiff1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 31 "/Vlp1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 166.116 88.9)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "GRM31C5C2A104JA01L")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C16" (at -2.794 0 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "+12L") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 130.81 93.98)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "GRM31C5C2A104JA01L")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 29 "GND2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 118.11 93.98)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "GRM31C5C2A104JA01L")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at -3.048 0 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 29 "GND2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm" (layer "F.Cu")
    (at 149.86 96.52 180)
    (descr "16-Lead Plastic Shrink Small Outline Narrow Body (QR)-.150\" Body [QSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.635")
    (property "MPN" "ADUM3190ARQZ")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "2500V isolation amplifier")
    (attr smd)
    (fp_text reference "U2" (at -2.54 -3.556) (layer "F.SilkS"))
    (fp_text value "ADUM3190ARQZ" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.6543 -2.2225 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+12L") (pinfunction "Vdd1") (pintype "power_in"))
    (pad "2" smd rect (at -2.6543 -1.5875 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND1") (pinfunction "GND1") (pintype "power_in"))
    (pad "3" smd rect (at -2.6543 -0.9525 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(U2-Vreg1)") (pinfunction "Vreg1") (pintype "power_out"))
    (pad "4" smd rect (at -2.6543 -0.3175 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(U2-Ref1)") (pinfunction "Ref1") (pintype "power_out"))
    (pad "5" smd rect (at -2.6543 0.3175 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "unconnected-(U2-NC-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd rect (at -2.6543 0.9525 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "unconnected-(U2-EAout2-Pad6)") (pinfunction "EAout2") (pintype "output+no_connect"))
    (pad "7" smd rect (at -2.6543 1.5875 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/Vin1") (pinfunction "EAout") (pintype "output"))
    (pad "8" smd rect (at -2.6543 2.2225 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND1") (pinfunction "GND1") (pintype "power_in"))
    (pad "9" smd rect (at 2.6543 2.2225 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "GND2") (pinfunction "GND2") (pintype "power_in"))
    (pad "10" smd rect (at 2.6543 1.5875 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(U2-Comp)") (pinfunction "Comp") (pintype "output"))
    (pad "11" smd rect (at 2.6543 0.9525 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(U2-Comp)") (pinfunction "Vin-") (pintype "input"))
    (pad "12" smd rect (at 2.6543 0.3175 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/Vo2") (pinfunction "Vin+") (pintype "input"))
    (pad "13" smd rect (at 2.6543 -0.3175 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(U2-Ref2)") (pinfunction "Ref2") (pintype "power_out"))
    (pad "14" smd rect (at 2.6543 -0.9525 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(U2-Vreg2)") (pinfunction "Vreg2") (pintype "power_out"))
    (pad "15" smd rect (at 2.6543 -1.5875 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "GND2") (pinfunction "GND2") (pintype "power_in"))
    (pad "16" smd rect (at 2.6543 -2.2225 180) (size 1.6 0.41) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12V") (pinfunction "Vdd2") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/QSOP-16_3.9x4.9mm_P0.635mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Power Supply:CUI PEME1-S DC-DC Converter" (layer "F.Cu")
    (at 155.956 87.63 180)
    (property "MPN" "NKA1212SC")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "12V in, ±12V out")
    (attr through_hole)
    (fp_text reference "PS1" (at -1.524 -2.032 unlocked) (layer "F.SilkS"))
    (fp_text value "NKA1212SC" (at 8.89 5.715 180 unlocked) (layer "F.Fab"))
    (fp_text user "+V" (at 15.24 1.268571 90 unlocked) (layer "B.SilkS"))
    (fp_text user "GND" (at 2.525079 1.268571 90 unlocked) (layer "B.SilkS"))
    (fp_text user "Vin" (at 0 1.27 90 unlocked) (layer "B.SilkS"))
    (fp_text user "-V" (at 10.16 1.27 90 unlocked) (layer "B.SilkS"))
    (fp_text user "0V" (at 12.7 1.268571 90 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 9.525 6.985 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(PS1-Vin)") (pinfunction "Vin") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 1 "GND1") (pinfunction "GND") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.168572 0 180) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(PS1--V)") (pinfunction "-V") (pintype "power_out"))
    (pad "6" thru_hole circle (at 12.708572 0 180) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 29 "GND2") (pinfunction "0V") (pintype "power_out"))
    (pad "7" thru_hole circle (at 15.248572 0 180) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(PS1-+V)") (pinfunction "+V") (pintype "power_out"))
    (model "${STIERS_3DMODEL_DIR}/CUI_PEME1-S12-D12-S.step"
      (offset (xyz 7.62 -2.1082 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 179.324 93.98)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R21" (at 2.794 0 90) (layer "F.SilkS"))
    (fp_text value "500" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 31 "/Vlp1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 17 "Net-(U3D-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 166.116 86.36 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "C1206C102J2GAC7800")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C18" (at 2.794 0 90) (layer "F.SilkS"))
    (fp_text value "390p" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 10 "Net-(U3C-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 162.052 102.108)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 1.524) (layer "F.SilkS"))
    (fp_text value "6.81k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 41 "Net-(R15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 173.228 94.996)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "GRM31C5C2A104JA01L")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C20" (at -3.048 0 90) (layer "F.SilkS"))
    (fp_text value "DNP" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 31 "/Vlp1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 179.324 81.28 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RMCF1206FT20K0")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R22" (at -2.794 0 90) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 18 "Net-(U3D--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 128.524 84.074 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "CL31B334KBHWPNE")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C5" (at 2.794 0) (layer "F.SilkS"))
    (fp_text value "0.33u" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "GND2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 172.72 88.9)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "MPN" "LF347DT")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at -3.302 -5.08) (layer "F.SilkS"))
    (fp_text value "LF347" (at 0 5.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U3A--)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U3A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/Vin1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+12L") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/Voff1") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U3B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U3B--)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/Vdiff1") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U3C--)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U3C-+)") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "-12VA") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(U3D-+)") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(U3D--)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(R24-Pad2)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1812_4532Metric_Pad1.30x3.40mm_HandSolder" (layer "F.Cu")
    (at 149.86 91.186)
    (descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "CHV1812N3K0271JCT")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C11" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "270p, 3kV" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.225 0) (size 1.3 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "GND2") (pintype "passive"))
    (pad "2" smd roundrect (at 2.225 0) (size 1.3 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 130.81 91.44)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "C1206C102J2GAC7800")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C3" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "390p" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 39 "Net-(U1D--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 32 "/Vo2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 166.09 84.074 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RNCP1206FTD1K00")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R16" (at 2.768 0 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 15 "Net-(U3A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 10 "Net-(U3C-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 166.116 96.52)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "C1206C102J2GAC7800")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C19" (at -2.794 0 90) (layer "F.SilkS"))
    (fp_text value "390p" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 11 "Net-(U3C--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 30 "/Vdiff1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Connector:BNC_Horizontal_ThruHole" (layer "F.Cu")
    (at 95.758 93.98 90)
    (property "MPN" "031-5431-10RFX")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J1" (at -8.636 1.778 unlocked) (layer "F.SilkS"))
    (fp_text value "Vin" (at 0 5.08 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.254 3.556 90 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at -5.08 -5.08 90) (size 3.5 7) (drill 2.01) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole oval (at 5.08 -5.08 90) (size 3.5 7) (drill 2.01) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole oval (at 0 0 90) (size 1.6 2.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 34 "/Vin+") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 90) (size 1.6 2.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 35 "/Vin-") (pinfunction "Ext") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/31-5431-10RFX.stp"
      (offset (xyz 0 -1.3462 0.9144))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (at 195.58 107.95)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "_es_RLC:Potentiometer_Nidec_ST4_Vertical" (layer "F.Cu")
    (at 167.894 100.838 180)
    (descr "Potentiometer, vertical, Vishay TS53YJ, https://www.vishay.com/docs/51008/ts53.pdf")
    (tags "Potentiometer vertical Vishay TS53YJ")
    (property "MPN" "ST-4ETA202")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Trim-potentiometer, US symbol")
    (property "ki_keywords" "resistor variable trimpot trimmer")
    (attr smd)
    (fp_text reference "RV1" (at -3.81 1.778 90) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect (at 2 -1.15 180) (size 2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(R15-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2 0 180) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/Voff1") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 2 1.15 180) (size 2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(R14-Pad2)") (pinfunction "3") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/ST-4ETA2k_(202).stp"
      (offset (xyz 0 0 2.286))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 135.636 78.994 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "CL31B334KBHWPNE")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C8" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "0.33u" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(PS1--V)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "GND2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 166.116 81.534 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RMCF1206FT20K0")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R18" (at 2.794 0 90) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 10 "Net-(U3C-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 118.11 96.774 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RMCF1206FT20K0")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R6" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 23 "Net-(U1B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 21 "Net-(R6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 124.46 93.98)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "MPN" "LF347DT")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -5.28) (layer "F.SilkS"))
    (fp_text value "LF347" (at 0 5.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(R7-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U1A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/V+") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+12V") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/V-") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U1B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(R6-Pad2)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/Voff2") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/Voff2") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U1C-+)") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(U1D-+)") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(U1D--)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/Vo2") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Connector:BNC_Horizontal_ThruHole" (layer "F.Cu")
    (at 187.96 93.98 -90)
    (property "MPN" "031-5431-10RFX")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J3" (at -5.715 3.556 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "Vout" (at 0 5.08 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.254 3.556 -90 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at -5.08 -5.08 270) (size 3.5 7) (drill 2.01) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole oval (at 5.08 -5.08 270) (size 3.5 7) (drill 2.01) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole oval (at 0 0 270) (size 1.6 2.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J3-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 270) (size 1.6 2.5) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 1 "GND1") (pinfunction "Ext") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/31-5431-10RFX.stp"
      (offset (xyz 0 -1.3462 0.9144))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 179.324 86.36 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R24" (at -2.794 0 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 42 "Net-(R24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.5mm" (layer "F.Cu")
    (at 88.138 80.01)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 179.324 96.52)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RMCF1206FT20K0")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R23" (at 2.794 0 90) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 17 "Net-(U3D-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 118.11 99.314)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RMCF1206FT20K0")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R8" (at -3.048 0 90) (layer "F.SilkS"))
    (fp_text value "20k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 21 "Net-(R6-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 39 "Net-(U1D--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 166.116 91.44 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RNCP1206FTD1K00")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R17" (at 2.794 0 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 16 "Net-(U3B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(U3C--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_RLC:L_Murata_82473C" (layer "F.Cu")
    (at 156.718 79.756)
    (descr "Murata 82xx series SMT inductor")
    (property "MPN" "82154C")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor, small symbol")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L3" (at 1.016 -2.286 unlocked) (layer "F.SilkS"))
    (fp_text value "150u" (at 0.381 4.064 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.127 2.794 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.143 0) (size 1.524 3.048) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(PS1-Vin)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.143 -0.006835) (size 1.524 3.048) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+12L") (pintype "passive"))
    (model "C:/Users/stiers/Google Drive/Work Projects/_KiCad Lib/3D Models/mps_mag_8200_smt_a.step"
      (offset (xyz 25.0698 136.0932 0.9652))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 109.728 102.87 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R4" (at -1.524 0 180) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "/V+") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "GND2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Mechanical:40mil PTH" (layer "F.Cu")
    (at 154.686 109.982)
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "PTH2" (at 0 -1.524 unlocked) (layer "F.SilkS") hide)
    (fp_text value "GND1" (at 0 1.778 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.048 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 1 "GND1") (pintype "passive"))
  )
  (footprint "_es_RLC:L_Murata_82473C" (layer "F.Cu")
    (at 132.08 84.074)
    (descr "Murata 82xx series SMT inductor")
    (property "MPN" "82154C")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor, small symbol")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L1" (at 0 2.413 unlocked) (layer "F.SilkS"))
    (fp_text value "150u" (at 0.381 4.064 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.127 2.794 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.143 0) (size 1.524 3.048) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.143 -0.006835) (size 1.524 3.048) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(PS1-+V)") (pintype "passive"))
    (model "C:/Users/stiers/Google Drive/Work Projects/_KiCad Lib/3D Models/mps_mag_8200_smt_a.step"
      (offset (xyz 25.0698 136.0932 0.9652))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 109.728 92.71 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "MPN" "-")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 9.144 0 180) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "GND2") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "/V-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Uncommon:STS321150B100" (layer "F.Cu")
    (at 112.014 93.98 90)
    (descr "TVS diode, 15V")
    (property "MPN" "STS321150B100")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "15V, 450W Discrete Bidirectional TVS Diode, SOD-323")
    (property "ki_keywords" "transient voltage suppressor thyrector transil")
    (attr smd)
    (fp_text reference "D1" (at 2.286 0 unlocked) (layer "F.SilkS"))
    (fp_text value "STS321150B100" (at 0 2.286 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.556 90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1 0 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/V+") (pinfunction "A1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 1.1 0 90) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/V-") (pinfunction "A2") (pintype "passive") (thermal_bridge_angle 45))
    (model "${STIERS_3DMODEL_DIR}/SOD-323.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${STIERS_3DMODEL_DIR}/SOD323_DIO.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 158.242 100.838 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "CL31B105KCHNNNE")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C14" (at 3.048 0 -180) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.85 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 9 "Net-(U2-Vreg1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 141.732 100.838 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "MPN" "CL31B105KCHNNNE")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C10" (at -2.794 0) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 29 "GND2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 7 "Net-(U2-Vreg2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 130.81 99.06)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RNCP1206FTD1K00")
    (property "Sheetfile" "Isoamp v4 prototype.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R11" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 20 "Net-(U1D-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 33 "/Voff2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 151.13 101.6) (end 151.13 81.28)
    (layer "Edge.Cuts"))
  (gr_arc (start 88.138 113.03) (mid 84.545898 111.542102) (end 83.058 107.95)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.59 81.28) (mid 149.86 80.01) (end 151.13 81.28)
    (layer "Edge.Cuts"))
  (gr_arc (start 151.13 101.6) (mid 149.86 102.87) (end 148.59 101.6)
    (layer "Edge.Cuts"))
  (gr_line (start 83.058 80.01) (end 83.058 107.95)
    (layer "Edge.Cuts"))
  (gr_line (start 195.58 74.93) (end 88.138 74.93)
    (layer "Edge.Cuts"))
  (gr_line (start 200.66 107.95) (end 200.66 80.01)
    (layer "Edge.Cuts"))
  (gr_line (start 148.59 81.28) (end 148.59 101.6)
    (layer "Edge.Cuts"))
  (gr_arc (start 83.058 80.01) (mid 84.545898 76.417898) (end 88.138 74.93)
    (layer "Edge.Cuts"))
  (gr_arc (start 195.58 74.93) (mid 199.172102 76.417898) (end 200.66 80.01)
    (layer "Edge.Cuts"))
  (gr_line (start 88.138 113.03) (end 195.58 113.03)
    (layer "Edge.Cuts"))
  (gr_arc (start 200.66 107.95) (mid 199.172102 111.542102) (end 195.58 113.03)
    (layer "Edge.Cuts"))
  (gr_text "+12V" (at 123.444 86.36) (layer "F.SilkS"))
  (gr_text "V-" (at 101.6 82.042) (layer "F.SilkS"))
  (gr_text "OFFSET" (at 167.894 104.394) (layer "F.SilkS"))
  (gr_text "GND" (at 188.214 78.74) (layer "F.SilkS"))
  (gr_text "Voff1" (at 174.244 100.838) (layer "F.SilkS"))
  (gr_text "ADuM3190 Isolation Amplifier Prototype v4\nE. Stiers / K. Kim\n19 July, 2024" (at 99.568 112.014) (layer "F.SilkS"))
  (gr_text "Ref1" (at 137.541 101.6) (layer "F.SilkS"))
  (gr_text "12V" (at 155.829 75.946) (layer "F.SilkS"))
  (gr_text "GND1" (at 154.686 108.204) (layer "F.SilkS"))
  (gr_text "+12V" (at 188.214 76.327) (layer "F.SilkS"))
  (gr_text "Rg" (at 124.968 103.632) (layer "F.SilkS"))
  (gr_text "-12V" (at 123.444 78.232) (layer "F.SilkS"))
  (gr_text "GND" (at 188.281 81.31) (layer "F.SilkS"))
  (gr_text "GND2" (at 144.78 108.204) (layer "F.SilkS"))
  (gr_text "Vin-" (at 101.6 104.648) (layer "F.SilkS"))
  (gr_text "Ref1" (at 160.274 96.52) (layer "F.SilkS"))
  (gr_text "V-" (at 113.284 85.09) (layer "F.SilkS"))
  (gr_text "GAIN" (at 170.688 84.074) (layer "F.SilkS"))
  (gr_text "V+" (at 105.918 104.648) (layer "F.SilkS"))
  (gr_text "Vo2" (at 137.16 91.44) (layer "F.SilkS"))
  (gr_text "Vin+" (at 105.918 82.042) (layer "F.SilkS"))
  (gr_text "Voff2" (at 137.668 99.06) (layer "F.SilkS"))
  (gr_text "-12V" (at 188.214 83.82) (layer "F.SilkS"))
  (gr_text "Cf" (at 173.228 97.028) (layer "F.SilkS"))
  (zone (net 29) (net_name "GND2") (layers "F&B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.27))
    (polygon
      (pts
        (xy 114.808 88.9)
        (xy 108.712 88.9)
        (xy 108.712 99.06)
        (xy 114.851354 99.059295)
        (xy 114.808 114.046)
        (xy 148.59 114.046)
        (xy 148.59 73.406)
        (xy 114.808 73.406)
      )
    )
  )
  (zone (net 1) (net_name "GND1") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1.27))
    (polygon
      (pts
        (xy 151.13 72.39)
        (xy 151.13 115.57)
        (xy 203.2 115.57)
        (xy 203.2 72.39)
      )
    )
  )
)
