(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (date "2024-02-25")
    (rev "2.1")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "output")
    )
  )
  (net 0 "")
  (net 1 "/Local A")
  (net 2 "/AAin A")
  (net 3 "/Ain A")
  (net 4 "Net-(D1-K)")
  (net 5 "/AD A")
  (net 6 "Net-(D1-A)")
  (net 7 "Net-(J1-Pin_1)")
  (net 8 "Net-(J1-Pin_2)")
  (net 9 "Net-(Q1-B)")
  (net 10 "/Ain B")
  (net 11 "/MSS GND")
  (net 12 "/7 A")
  (net 13 "/AAin B")
  (net 14 "Net-(D4-K)")
  (footprint "Imports:CONN_RJSBE5080_16P13X12P57_AMP" (layer "F.Cu")
    (at 114 98.8 -90)
    (tags "RJHSE-5080 ")
    (property "Label" "MSS A")
    (property "MPN" "MTJ-881X1")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RJ connector, 8P8C (8 positions 8 connected), RJ31/RJ32/RJ33/RJ34/RJ35/RJ41/RJ45/RJ49/RJ61")
    (property "ki_keywords" "8P8C RJ female connector")
    (attr through_hole)
    (fp_text reference "J2" (at -3.5 -4 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "RJ45" (at -4 -8.5 -90 unlocked) (layer "F.Fab"))
    (fp_text user "1" (at 1.397 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "2" (at 1.397 -1.778 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "8" (at -8.509 -1.778 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "7" (at -8.509 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -3.5 -6 -90 unlocked) (layer "F.Fab"))
    (fp_text user "8" (at -8.509 -1.778 -90 unlocked) (layer "F.Fab"))
    (fp_text user "7" (at -8.509 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "1" (at 1.397 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "2" (at 1.397 -1.778 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 2 "/AAin A") (pintype "passive"))
    (pad "2" thru_hole circle (at -1.016 -1.778 270) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 3 "/Ain A") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.032 0 270) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 13 "/AAin B") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.048 -1.778 270) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 1 "/Local A") (pintype "passive"))
    (pad "5" thru_hole circle (at -4.064 0 270) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 11 "/MSS GND") (pintype "passive"))
    (pad "6" thru_hole circle (at -5.08 -1.778 270) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 10 "/Ain B") (pintype "passive"))
    (pad "7" thru_hole circle (at -6.096 0 270) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 12 "/7 A") (pintype "passive"))
    (pad "8" thru_hole circle (at -7.112 -1.778 270) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 5 "/AD A") (pintype "passive"))
    (pad "9" thru_hole circle (at -9.906 2.54 270) (size 3.7592 3.7592) (drill 3.2512) (layers "*.Cu" "*.Mask"))
    (pad "10" thru_hole circle (at 2.794 2.54 270) (size 3.7592 3.7592) (drill 3.2512) (layers "*.Cu" "*.Mask"))
    (model ":KICAD_USER:Imports/3d/RJHSE-5080.step"
      (offset (xyz -3.5 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 123.8 63)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP1" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "Loop for current sense" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "myMods:Free-moNH-20" (layer "F.Cu")
    (at 151.2 73.8 90)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 90) (layer "F.SilkS") hide)
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (at 151.8 60.6)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_4.3mm_M4" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (at 110.8 112.5)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_4.3mm_M4" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 123.8 82.4)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP2" (at 0 -1.998) (layer "F.SilkS") hide)
    (fp_text value "~" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (at 110.8 60.6)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_4.3mm_M4" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (at 141.81 78 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "MPN" "1N4148FS-ND")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode, small symbol, filled shape")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D2" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "/MSS GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (at 151.8 112.5)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_4.3mm_M4" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 142.6 89.7 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (property "MPN" "FG28X7R1H474KRT06")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 0.5 2.4 90) (layer "F.SilkS"))
    (fp_text value "470n" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D4-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/MSS GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 128 83.8)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "MPN" "CF14JT470R")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "470" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(Q1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (at 141.8 66.79 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "MPN" "1N4148FS-ND")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode, small symbol, filled shape")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D3" (at 3.81 -2.12 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "/MSS GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "myMods:FIS101NL" (layer "F.Cu")
    (at 129.6 70.6)
    (descr "Current Sense Inductor")
    (property "MPN" "56300C")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L1" (at -9.8 3.8 unlocked) (layer "F.SilkS"))
    (fp_text value "Murata 56300C" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -6.35 0) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-A)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.35 0) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 11 "/MSS GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD_USER}/Imports/3d/FIS121NL.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Imports:CUI_TB003-500-P02BE" (layer "F.Cu")
    (at 150.4 93.8 90)
    (property "Label" "aux")
    (property "MPN" "TB003-500-P02BE")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J4" (at 3.6 -5 90) (layer "F.SilkS"))
    (fp_text value "2x-screw" (at 13.391 5.361 90) (layer "F.Fab"))
    (fp_text user "+" (at 4.9 5.0375 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${Label}" (at -5.6 0 90 unlocked) (layer "F.SilkS"))
    (fp_text user "-" (at 0.1 5.0375 90 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 11 "/MSS GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D4-K)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD_USER}/Imports/3d/CUI_DEVICES_TB003-500-P02BE.step"
      (offset (xyz 10 -3.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (at 138.43 87.63 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "MPN" "1N4148FS-ND")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode, small symbol, filled shape")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D4" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "/Local A") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Imports:CUI_TB003-500-P02BE" (layer "F.Cu")
    (at 112.8375 71.5 -90)
    (property "Label" "DCC")
    (property "MPN" "TB003-500-P02BE")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J1" (at -1.9 -5.1625 90) (layer "F.SilkS"))
    (fp_text value "2x-screw" (at 13.391 5.361 90) (layer "F.Fab"))
    (fp_text user "${Label}" (at 2.54 5.5755 -90 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD_USER}/Imports/3d/CUI_DEVICES_TB003-500-P02BE.step"
      (offset (xyz 10 -3.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (at 142.6 81.2 -90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "MPN" "2N3904TA")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at 2.54 -3.56 -90) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 2.54 2.79 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "/MSS GND") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(Q1-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D4-K)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Imports:CONN_RJSBE5080_16P13X12P57_AMP" (layer "F.Cu")
    (at 137.556 109.39675)
    (tags "RJHSE-5080 ")
    (property "Label" "MSS B")
    (property "MPN" "MTJ-881X1")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RJ connector, 8P8C (8 positions 8 connected), RJ31/RJ32/RJ33/RJ34/RJ35/RJ41/RJ45/RJ49/RJ61")
    (property "ki_keywords" "8P8C RJ female connector")
    (attr through_hole)
    (fp_text reference "J7" (at -3.5 -4 unlocked) (layer "F.SilkS"))
    (fp_text value "RJ45" (at -4 -8.5 unlocked) (layer "F.Fab"))
    (fp_text user "7" (at -8.509 0 unlocked) (layer "F.SilkS"))
    (fp_text user "2" (at 1.397 -1.778 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at 1.397 0 unlocked) (layer "F.SilkS"))
    (fp_text user "8" (at -8.509 -1.778 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at 1.397 0 unlocked) (layer "F.Fab"))
    (fp_text user "2" (at 1.397 -1.778 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.5 -6 unlocked) (layer "F.Fab"))
    (fp_text user "8" (at -8.509 -1.778 unlocked) (layer "F.Fab"))
    (fp_text user "7" (at -8.509 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 13 "/AAin B") (pintype "passive"))
    (pad "2" thru_hole circle (at -1.016 -1.778) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 10 "/Ain B") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.032 0) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 2 "/AAin A") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.048 -1.778) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 1 "/Local A") (pintype "passive"))
    (pad "5" thru_hole circle (at -4.064 0) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 11 "/MSS GND") (pintype "passive"))
    (pad "6" thru_hole circle (at -5.08 -1.778) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 3 "/Ain A") (pintype "passive"))
    (pad "7" thru_hole circle (at -6.096 0) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 12 "/7 A") (pintype "passive"))
    (pad "8" thru_hole circle (at -7.112 -1.778) (size 1.3716 1.3716) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 5 "/AD A") (pintype "passive"))
    (pad "9" thru_hole circle (at -9.906 2.54) (size 3.7592 3.7592) (drill 3.2512) (layers "*.Cu" "*.Mask"))
    (pad "10" thru_hole circle (at 2.794 2.54) (size 3.7592 3.7592) (drill 3.2512) (layers "*.Cu" "*.Mask"))
    (model ":KICAD_USER:Imports/3d/RJHSE-5080.step"
      (offset (xyz -3.5 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (at 131.01 78 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "MPN" "1N4148FS-ND")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode, small symbol, filled shape")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D1" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm" (layer "B.Cu")
    (at 121.2 108.6 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "mss-crossover.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Solder Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files exclude_from_bom)
    (net_tie_pad_groups "1, 2")
    (fp_text reference "JP1" (at 0 1.8) (layer "B.SilkS") hide)
    (fp_text value "MSS 7" (at 0 -1.9) (layer "B.SilkS"))
    (pad "1" smd custom (at -0.65 0 180) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 12 "/7 A") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.5 0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 180) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 11 "/MSS GND") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0 0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (gr_rect (start 105.918 55.626) (end 156.718 117.39)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "MSS" (at 115.4 107.2 315) (layer "F.SilkS"))
  (gr_text "Sense Loop" (at 109 83) (layer "F.SilkS"))
  (gr_text "MSS Crossover Node\n${ISSUE_DATE}\nRev ${REVISION}" (at 136.4 60.2) (layer "F.SilkS"))
  (gr_text "Sense Loop" (at 108.8 65.2) (layer "F.SilkS"))
)
