(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu19.04.1)
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 265)
    (zones 0)
    (modules 10)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 3.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VDD)
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(R1-Pad2)")
  (net 6 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class ad ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /VDD)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad1)")
  )
  (module Battery:BatteryHolder_Keystone_3000_1x12mm (layer B.Cu) (tedit 5E432C5A)
    (at 156.34716 107.0991 180)
    (descr http://www.keyelco.com/product-pdf.cfm?p=777)
    (tags "Keystone type 3000 coin cell retainer")
    (attr smd)
    (fp_text reference CR1220 (at 0 8 180 unlocked) (layer B.SilkS))
    (fp_text value BatteryHolder_Keystone_3000_1x12mm (at 0 -7.5) (layer B.Fab) hide)
    (fp_text user %R (at -0.13462 -3.64998) (layer B.Fab))
    (pad 2 smd circle (at 0 0 180) (size 10.2 10.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 7.9 0 180) (size 3.5 3.3) (layers B.Cu B.Paste B.Mask)
      (net 2 /VDD))
    (pad 1 smd rect (at -7.9 0 180) (size 3.5 3.3) (layers B.Cu B.Paste B.Mask)
      (net 2 /VDD))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_3000_1x12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module afterdark:OSHW-Logo2_9.8x8mm_Copper (layer B.Cu) (tedit 5E433FF0)
    (at 142.35684 106.35742)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_Copper (at 0.75 0) (layer B.Fab) hide)
  )
  (module Symbol:KiCad-Logo2_5mm_Copper (layer B.Cu) (tedit 5E433FD2)
    (at 168.96588 99.59594)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 5.08) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_5mm_Copper (at 0 -5.08) (layer B.Fab) hide)
  )
  (module afterdark:OSHW-Logo2_9.8x8mm_Copper (layer B.Cu) (tedit 5E10D1D7)
    (at 170.31462 106.40314)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_Copper (at 0.75 0) (layer B.Fab) hide)
  )
  (module digikey-footprints:SOIC-8-1EP_W3.9mm (layer B.Cu) (tedit 5E41D6CC)
    (at 157.60446 81.1911)
    (attr smd)
    (fp_text reference U1 (at 0 5.52 180 unlocked) (layer B.SilkS))
    (fp_text value 7555 (at 0 -5.85 180 unlocked) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 8 smd rect (at -1.905 2.75) (size 0.65 1.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /VDD) (solder_mask_margin 0.07))
    (pad 7 smd rect (at -0.635 2.75) (size 0.65 1.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(R1-Pad2)") (solder_mask_margin 0.07))
    (pad 6 smd rect (at 0.635 2.75) (size 0.65 1.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C1-Pad1)") (solder_mask_margin 0.07))
    (pad 5 smd rect (at 1.905 2.75) (size 0.65 1.75) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.07))
    (pad 4 smd rect (at 1.905 -2.75) (size 0.65 1.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /VDD) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 0.635 -2.75) (size 0.65 1.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(R3-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -0.635 -2.75) (size 0.65 1.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C1-Pad1)") (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.905 -2.75) (size 0.65 1.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 168.01846 94.50832 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0.06604 -1.64846 180 unlocked) (layer B.SilkS))
    (fp_text value 100 (at -0.00508 1.66116 180 unlocked) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 149.5044 94.50832)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 1.65 180 unlocked) (layer B.SilkS))
    (fp_text value 470K (at 0 -1.65 180 unlocked) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(C1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 142.38478 94.49816)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.65 180 unlocked) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.65 180 unlocked) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 /VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B4B45C9)
    (at 162.53714 94.5007)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 1.65 180 unlocked) (layer B.SilkS))
    (fp_text value LED (at 0 -1.65 180 unlocked) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 156.35478 94.50832)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 1.82 180 unlocked) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.82 180 unlocked) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 134.469497 81.709264) (end 156.46654 69.009264) (layer Edge.Cuts) (width 0.4064))
  (gr_line (start 178.463583 107.109256) (end 156.46654 119.809256) (layer Edge.Cuts) (width 0.4064))
  (gr_line (start 134.469497 107.10926) (end 134.469497 81.709264) (layer Edge.Cuts) (width 0.4064))
  (gr_line (start 156.46654 119.809256) (end 134.4695 107.10926) (layer Edge.Cuts) (width 0.4064))
  (gr_line (start 178.463583 81.70926) (end 178.463583 107.109256) (layer Edge.Cuts) (width 0.4064))
  (gr_line (start 156.46654 69.009264) (end 178.46358 81.70926) (layer Edge.Cuts) (width 0.4064))
  (gr_text "New York City" (at 146.15922 76.95184 210) (layer B.Cu))
  (gr_text "Open Hardware Summit 2020" (at 136.4107 94.62008 270) (layer B.Mask))
  (gr_text "Open Hardware Summit 2020" (at 136.4107 94.62008 270) (layer B.Cu))
  (gr_text "Getting to Blinky!" (at 165.8239 76.60386 150) (layer B.Cu))
  (gr_text contextualelectronics.com/GTB (at 176.69256 94.26194 90) (layer B.Mask))
  (gr_text contextualelectronics.com/GTB (at 176.69256 94.2594 90) (layer B.Cu))
)
