(kicad_pcb (version 3) (host pcbnew "(2013-07-07 BZR 4022)-stable")
  (general
    (links 12)
    (no_connects 0)
    (area 185.369999 86.309999 256.590001 141.020001)
    (thickness 1.6)
    (drawings 23)
    (tracks 9)
    (zones 0)
    (modules 3)
    (nets 5)
  )
  (page A3)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 1.016)
    (user_trace_width 0.254)
    (user_trace_width 1.016)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 3178497)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3.3V)
  (net 2 GND)
  (net 3 N-0000032)
  (net 4 N-0000087)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net +3.3V)
    (add_net GND)
    (add_net N-0000032)
    (add_net N-0000087)
  )
  (net_class POWER ""
    (clearance 0.254)
    (trace_width 1.016)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module conn_2x23 (layer F.Cu) (tedit 58324DA1)
    (at 192.405 90.805 90)
    (fp_text reference P8 (at -3.175 5.715 180) (layer F.SilkS) hide)
    (fp_text value CONN_23X2 (at -3.175 13.97 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 GND)
    )
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 GND)
    )
    (pad 3 thru_hole circle (at 0 2.54 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 5 thru_hole circle (at 0 5.08 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 6 thru_hole circle (at 2.54 5.08 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 7 thru_hole circle (at 0 7.62 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 8 thru_hole circle (at 2.54 7.62 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 9 thru_hole circle (at 0 10.16 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 10 thru_hole circle (at 2.54 10.16 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 11 thru_hole circle (at 0 12.7 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 12 thru_hole circle (at 2.54 12.7 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 13 thru_hole circle (at 0 15.24 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 14 thru_hole circle (at 2.54 15.24 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 15 thru_hole circle (at 0 17.78 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 16 thru_hole circle (at 2.54 17.78 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 17 thru_hole circle (at 0 20.32 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 18 thru_hole circle (at 2.54 20.32 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 19 thru_hole circle (at 0 22.86 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 20 thru_hole circle (at 2.54 22.86 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 21 thru_hole circle (at 0 25.4 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 22 thru_hole circle (at 2.54 25.4 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 23 thru_hole circle (at 0 27.94 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 24 thru_hole circle (at 2.54 27.94 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 25 thru_hole circle (at 0 30.48 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 26 thru_hole circle (at 2.54 30.48 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 27 thru_hole circle (at 0 33.02 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 28 thru_hole circle (at 2.54 33.02 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 29 thru_hole circle (at 0 35.56 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 30 thru_hole circle (at 2.54 35.56 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 31 thru_hole circle (at 0 38.1 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 32 thru_hole circle (at 2.54 38.1 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 33 thru_hole circle (at 0 40.64 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 34 thru_hole circle (at 2.54 40.64 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 35 thru_hole circle (at 0 43.18 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 36 thru_hole circle (at 2.54 43.18 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 37 thru_hole circle (at 0 45.72 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 38 thru_hole circle (at 2.54 45.72 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 39 thru_hole circle (at 0 48.26 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 40 thru_hole circle (at 2.54 48.26 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 41 thru_hole circle (at 0 50.8 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 42 thru_hole circle (at 2.54 50.8 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 43 thru_hole circle (at 0 53.34 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 44 thru_hole circle (at 2.54 53.34 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 45 thru_hole circle (at 0 55.88 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 46 thru_hole circle (at 2.54 55.88 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (module conn_2x23 (layer F.Cu) (tedit 58324E85)
    (at 192.405 139.065 90)
    (fp_text reference P9 (at 5.715 7.62 180) (layer F.SilkS) hide)
    (fp_text value CONN_23X2 (at 5.715 14.605 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 GND)
    )
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 GND)
    )
    (pad 3 thru_hole circle (at 0 2.54 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V)
    )
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V)
    )
    (pad 5 thru_hole circle (at 0 5.08 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 6 thru_hole circle (at 2.54 5.08 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 7 thru_hole circle (at 0 7.62 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 8 thru_hole circle (at 2.54 7.62 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 9 thru_hole circle (at 0 10.16 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 10 thru_hole circle (at 2.54 10.16 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 11 thru_hole circle (at 0 12.7 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 12 thru_hole circle (at 2.54 12.7 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 13 thru_hole circle (at 0 15.24 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 14 thru_hole circle (at 2.54 15.24 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 15 thru_hole circle (at 0 17.78 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 16 thru_hole circle (at 2.54 17.78 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 17 thru_hole circle (at 0 20.32 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 18 thru_hole circle (at 2.54 20.32 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 19 thru_hole circle (at 0 22.86 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 4 N-0000087)
    )
    (pad 20 thru_hole circle (at 2.54 22.86 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 N-0000032)
    )
    (pad 21 thru_hole circle (at 0 25.4 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 22 thru_hole circle (at 2.54 25.4 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 23 thru_hole circle (at 0 27.94 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 24 thru_hole circle (at 2.54 27.94 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 25 thru_hole circle (at 0 30.48 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 26 thru_hole circle (at 2.54 30.48 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 27 thru_hole circle (at 0 33.02 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 28 thru_hole circle (at 2.54 33.02 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 29 thru_hole circle (at 0 35.56 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 30 thru_hole circle (at 2.54 35.56 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 31 thru_hole circle (at 0 38.1 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 32 thru_hole circle (at 2.54 38.1 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 33 thru_hole circle (at 0 40.64 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 34 thru_hole circle (at 2.54 40.64 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 35 thru_hole circle (at 0 43.18 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 36 thru_hole circle (at 2.54 43.18 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 37 thru_hole circle (at 0 45.72 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 38 thru_hole circle (at 2.54 45.72 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 39 thru_hole circle (at 0 48.26 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 40 thru_hole circle (at 2.54 48.26 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 41 thru_hole circle (at 0 50.8 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 42 thru_hole circle (at 2.54 50.8 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 43 thru_hole circle (at 0 53.34 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 GND)
    )
    (pad 44 thru_hole circle (at 2.54 53.34 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 GND)
    )
    (pad 45 thru_hole circle (at 0 55.88 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 GND)
    )
    (pad 46 thru_hole circle (at 2.54 55.88 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 GND)
    )
  )
  (module AdafruitDS3231 (layer F.Cu) (tedit 5832603E)
    (at 208.735 102.505 90)
    (fp_text reference P1 (at 0.18 -14.13 90) (layer F.SilkS))
    (fp_text value "ADAFRUIT DS3231" (at -7.985 -17.6 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 -8.89 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V)
    )
    (pad 2 thru_hole circle (at 0 -6.35 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 2 GND)
    )
    (pad 3 thru_hole circle (at 0 -3.81 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 4 N-0000087)
    )
    (pad 4 thru_hole circle (at 0 -1.27 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
      (net 3 N-0000032)
    )
    (pad 5 thru_hole circle (at 0 1.27 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 6 thru_hole circle (at 0 3.81 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 7 thru_hole circle (at 0 6.35 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 8 thru_hole circle (at 0 8.89 90) (size 1.5 1.5) (drill 1.016)
      (layers *.Cu *.Mask F.SilkS)
    )
  )
  (gr_text 2 (at 189.23 136.525) (layer F.SilkS))
  (gr_text 2 (at 189.23 88.265) (layer F.SilkS))
  (gr_text 45 (at 252.095 90.805) (layer F.SilkS))
  (gr_text 45 (at 252.095 139.065) (layer F.SilkS))
  (gr_text 46 (at 252.095 88.265) (layer F.SilkS))
  (gr_text "P2B (P9)" (at 215.9 132.08) (layer F.SilkS))
  (gr_text "P2A (P8)" (at 216.535 95.25) (layer F.SilkS))
  (gr_text "MOUNT BATTERY UP" (at 208.915 116.205) (layer F.SilkS))
  (gr_text 46 (at 252.73 153.67) (layer F.SilkS))
  (gr_text 1 (at 189.23 91.44) (layer F.SilkS))
  (gr_text 46 (at 252.095 135.89) (layer F.SilkS))
  (gr_text 1 (at 189.23 139.065) (layer F.SilkS))
  (gr_text "RTC, DS3231, JOHN BAKER, 2016" (at 215.9 127) (layer F.SilkS))
  (gr_line (start 185.42 86.36) (end 185.42 140.97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 256.54 86.36) (end 185.42 86.36) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 256.54 140.97) (end 256.54 86.36) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.42 140.97) (end 256.54 140.97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 255.905 140.335) (xy 186.055 140.335) (xy 186.055 86.995) (xy 255.905 86.995)
      )
    )
  )
  (zone (net 1) (net_name +3.3V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 255.905 140.335) (xy 186.055 140.335) (xy 186.055 86.995) (xy 255.905 86.995)
      )
    )
  )
)
